(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.5748)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(solder_mask_min_width 0.25)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "+5V")
	(net 2 "Net-(C46-Pad1)")
	(net 3 "Net-(C19-Pad1)")
	(net 4 "Net-(C54-Pad1)")
	(net 5 "Net-(D26-Pad1)")
	(net 6 "Net-(D17-Pad2)")
	(net 7 "Net-(D17-Pad1)")
	(net 8 "Net-(D18-Pad2)")
	(net 9 "Net-(D18-Pad1)")
	(net 10 "Net-(D19-Pad2)")
	(net 11 "Net-(D19-Pad1)")
	(net 12 "Net-(D20-Pad2)")
	(net 13 "Net-(D20-Pad1)")
	(net 14 "unconnected-(H1-Pad1)")
	(net 15 "unconnected-(H1-Pad2)")
	(net 16 "unconnected-(H1-Pad3)")
	(net 17 "unconnected-(H1-Pad4)")
	(net 18 "unconnected-(H1-Pad5)")
	(net 19 "unconnected-(H1-Pad6)")
	(net 20 "unconnected-(H1-Pad7)")
	(net 21 "unconnected-(H1-Pad8)")
	(net 22 "unconnected-(H1-Pad9)")
	(net 23 "unconnected-(H1-Pad10)")
	(net 24 "unconnected-(H1-Pad11)")
	(net 25 "unconnected-(H1-Pad12)")
	(net 26 "unconnected-(H1-Pad13)")
	(net 27 "unconnected-(H1-Pad14)")
	(net 28 "unconnected-(H1-Pad15)")
	(net 29 "unconnected-(H1-Pad16)")
	(net 30 "unconnected-(H1-Pad17)")
	(net 31 "unconnected-(H1-Pad18)")
	(net 32 "unconnected-(H1-Pad19)")
	(net 33 "unconnected-(H1-Pad20)")
	(net 34 "unconnected-(H1-Pad21)")
	(net 35 "unconnected-(H1-Pad22)")
	(net 36 "unconnected-(H1-Pad23)")
	(net 37 "unconnected-(H1-Pad24)")
	(net 38 "unconnected-(H1-Pad25)")
	(net 39 "unconnected-(H1-Pad26)")
	(net 40 "unconnected-(H1-Pad27)")
	(net 41 "unconnected-(H1-Pad28)")
	(net 42 "unconnected-(H1-Pad29)")
	(net 43 "unconnected-(H1-Pad30)")
	(net 44 "PWR_LCL_3")
	(net 45 "PWR_LCL_4")
	(net 46 "unconnected-(H1-Pad35)")
	(net 47 "unconnected-(H1-Pad36)")
	(net 48 "unconnected-(H1-Pad37)")
	(net 49 "unconnected-(H1-Pad38)")
	(net 50 "unconnected-(H1-Pad39)")
	(net 51 "unconnected-(H1-Pad40)")
	(net 52 "unconnected-(H1-Pad41)")
	(net 53 "unconnected-(H1-Pad42)")
	(net 54 "unconnected-(H1-Pad43)")
	(net 55 "unconnected-(H1-Pad44)")
	(net 56 "PWR_LCL_1")
	(net 57 "PWR_LCL_2")
	(net 58 "+BATT")
	(net 59 "Net-(D25-Pad1)")
	(net 60 "ENA_LCL_4")
	(net 61 "ENA_LCL_3")
	(net 62 "unconnected-(H2-Pad1)")
	(net 63 "unconnected-(H2-Pad2)")
	(net 64 "unconnected-(H2-Pad3)")
	(net 65 "unconnected-(H2-Pad4)")
	(net 66 "unconnected-(H2-Pad5)")
	(net 67 "unconnected-(H2-Pad6)")
	(net 68 "unconnected-(H2-Pad7)")
	(net 69 "unconnected-(H2-Pad8)")
	(net 70 "unconnected-(H2-Pad9)")
	(net 71 "unconnected-(H2-Pad10)")
	(net 72 "unconnected-(H2-Pad11)")
	(net 73 "unconnected-(H2-Pad12)")
	(net 74 "unconnected-(H2-Pad13)")
	(net 75 "unconnected-(H2-Pad14)")
	(net 76 "unconnected-(H2-Pad15)")
	(net 77 "unconnected-(H2-Pad16)")
	(net 78 "unconnected-(H2-Pad17)")
	(net 79 "Net-(L1-Pad1)")
	(net 80 "Net-(L2-Pad1)")
	(net 81 "Net-(L3-Pad1)")
	(net 82 "Net-(L4-Pad1)")
	(net 83 "Net-(R50-Pad2)")
	(net 84 "Net-(R60-Pad2)")
	(net 85 "unconnected-(H2-Pad18)")
	(net 86 "unconnected-(H2-Pad19)")
	(net 87 "unconnected-(H2-Pad20)")
	(net 88 "unconnected-(H2-Pad21)")
	(net 89 "unconnected-(H2-Pad22)")
	(net 90 "unconnected-(H2-Pad23)")
	(net 91 "unconnected-(H2-Pad24)")
	(net 92 "unconnected-(H2-Pad27)")
	(net 93 "unconnected-(H2-Pad28)")
	(net 94 "unconnected-(H2-Pad33)")
	(net 95 "unconnected-(H2-Pad34)")
	(net 96 "unconnected-(H2-Pad35)")
	(net 97 "unconnected-(H2-Pad36)")
	(net 98 "unconnected-(H2-Pad47)")
	(net 99 "unconnected-(H2-Pad48)")
	(net 100 "unconnected-(H2-Pad49)")
	(net 101 "unconnected-(H2-Pad50)")
	(net 102 "unconnected-(H2-Pad51)")
	(net 103 "unconnected-(H2-Pad52)")
	(net 104 "ENA_LCL_2")
	(net 105 "ENA_LCL_1")
	(net 106 "Net-(C32-Pad1)")
	(net 107 "/Semi_Regulated_Bus")
	(net 108 "Net-(D27-Pad1)")
	(net 109 "Net-(D1-Pad2)")
	(net 110 "CHARGE")
	(net 111 "Net-(D3-Pad2)")
	(net 112 "Net-(D5-Pad2)")
	(net 113 "Net-(D7-Pad2)")
	(net 114 "Net-(D10-Pad2)")
	(net 115 "Net-(D11-Pad2)")
	(net 116 "unconnected-(U1-Pad5)")
	(net 117 "unconnected-(U2-Pad5)")
	(net 118 "unconnected-(U3-Pad5)")
	(net 119 "unconnected-(U4-Pad5)")
	(net 120 "unconnected-(U22-Pad10)")
	(net 121 "S2")
	(net 122 "unconnected-(U22-Pad12)")
	(net 123 "unconnected-(U22-Pad16)")
	(net 124 "unconnected-(U23-Pad10)")
	(net 125 "unconnected-(U23-Pad12)")
	(net 126 "unconnected-(U23-Pad16)")
	(net 127 "unconnected-(U24-Pad5)")
	(net 128 "unconnected-(U25-Pad5)")
	(net 129 "unconnected-(U26-Pad10)")
	(net 130 "unconnected-(U26-Pad12)")
	(net 131 "unconnected-(U26-Pad16)")
	(net 132 "unconnected-(U31-Pad1)")
	(net 133 "unconnected-(U31-Pad6)")
	(net 134 "unconnected-(U31-Pad11)")
	(net 135 "GND")
	(net 136 "unconnected-(U31-Pad20)")
	(net 137 "unconnected-(U33-Pad10)")
	(net 138 "unconnected-(U33-Pad12)")
	(net 139 "unconnected-(U33-Pad16)")
	(net 140 "Net-(R52-Pad1)")
	(net 141 "Net-(R62-Pad1)")
	(net 142 "unconnected-(U34-Pad1)")
	(net 143 "unconnected-(U34-Pad6)")
	(net 144 "unconnected-(U34-Pad11)")
	(net 145 "unconnected-(U34-Pad20)")
	(net 146 "Net-(D28-Pad1)")
	(net 147 "Net-(D29-Pad1)")
	(footprint "librecube_pcb_template:ESQ-126-39-x-D"
		(locked yes)
		(layer "F.Cu")
		(at 96.52 53.975)
		(descr "elevated through-hole socket strip designed for higher profile board spacing of PC/104 boards")
		(tags "PC104, connector, through-hole, socket strip")
		(property "Reference" "H1"
			(at -2.48 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_02X26"
			(at 1.27 -1.27 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(clearance 0.2)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(H1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "2" thru_hole circle
			(at 0 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(H1-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "3" thru_hole circle
			(at 2.54 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(H1-Pad3)")
			(pinfunction "Pin_3")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "4" thru_hole circle
			(at 2.54 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(H1-Pad4)")
			(pinfunction "Pin_4")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "5" thru_hole circle
			(at 5.08 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(H1-Pad5)")
			(pinfunction "Pin_5")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "6" thru_hole circle
			(at 5.08 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(H1-Pad6)")
			(pinfunction "Pin_6")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "7" thru_hole circle
			(at 7.62 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(H1-Pad7)")
			(pinfunction "Pin_7")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "8" thru_hole circle
			(at 7.62 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(H1-Pad8)")
			(pinfunction "Pin_8")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "9" thru_hole circle
			(at 10.16 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(H1-Pad9)")
			(pinfunction "Pin_9")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "10" thru_hole circle
			(at 10.16 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(H1-Pad10)")
			(pinfunction "Pin_10")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "11" thru_hole circle
			(at 12.7 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(H1-Pad11)")
			(pinfunction "Pin_11")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "12" thru_hole circle
			(at 12.7 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(H1-Pad12)")
			(pinfunction "Pin_12")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "13" thru_hole circle
			(at 15.24 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(H1-Pad13)")
			(pinfunction "Pin_13")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "14" thru_hole circle
			(at 15.24 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(H1-Pad14)")
			(pinfunction "Pin_14")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "15" thru_hole circle
			(at 17.78 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(H1-Pad15)")
			(pinfunction "Pin_15")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "16" thru_hole circle
			(at 17.78 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(H1-Pad16)")
			(pinfunction "Pin_16")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "17" thru_hole circle
			(at 20.32 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(H1-Pad17)")
			(pinfunction "Pin_17")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "18" thru_hole circle
			(at 20.32 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "unconnected-(H1-Pad18)")
			(pinfunction "Pin_18")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "19" thru_hole circle
			(at 22.86 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "unconnected-(H1-Pad19)")
			(pinfunction "Pin_19")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "20" thru_hole circle
			(at 22.86 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "unconnected-(H1-Pad20)")
			(pinfunction "Pin_20")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "21" thru_hole circle
			(at 25.4 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "unconnected-(H1-Pad21)")
			(pinfunction "Pin_21")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "22" thru_hole circle
			(at 25.4 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "unconnected-(H1-Pad22)")
			(pinfunction "Pin_22")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "23" thru_hole circle
			(at 27.94 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "unconnected-(H1-Pad23)")
			(pinfunction "Pin_23")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "24" thru_hole circle
			(at 27.94 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "unconnected-(H1-Pad24)")
			(pinfunction "Pin_24")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "25" thru_hole circle
			(at 30.48 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "unconnected-(H1-Pad25)")
			(pinfunction "Pin_25")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "26" thru_hole circle
			(at 30.48 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "unconnected-(H1-Pad26)")
			(pinfunction "Pin_26")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "27" thru_hole circle
			(at 33.02 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "unconnected-(H1-Pad27)")
			(pinfunction "Pin_27")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "28" thru_hole circle
			(at 33.02 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "unconnected-(H1-Pad28)")
			(pinfunction "Pin_28")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "29" thru_hole circle
			(at 35.56 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "unconnected-(H1-Pad29)")
			(pinfunction "Pin_29")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "30" thru_hole circle
			(at 35.56 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "unconnected-(H1-Pad30)")
			(pinfunction "Pin_30")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "31" thru_hole circle
			(at 38.1 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "CHARGE")
			(pinfunction "Pin_31")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "32" thru_hole circle
			(at 38.1 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "CHARGE")
			(pinfunction "Pin_32")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "33" thru_hole circle
			(at 40.64 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "GND")
			(pinfunction "Pin_33")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "34" thru_hole circle
			(at 40.64 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "GND")
			(pinfunction "Pin_34")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "35" thru_hole circle
			(at 43.18 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "unconnected-(H1-Pad35)")
			(pinfunction "Pin_35")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "36" thru_hole circle
			(at 43.18 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "unconnected-(H1-Pad36)")
			(pinfunction "Pin_36")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "37" thru_hole circle
			(at 45.72 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "unconnected-(H1-Pad37)")
			(pinfunction "Pin_37")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "38" thru_hole circle
			(at 45.72 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "unconnected-(H1-Pad38)")
			(pinfunction "Pin_38")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "39" thru_hole circle
			(at 48.26 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "unconnected-(H1-Pad39)")
			(pinfunction "Pin_39")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "40" thru_hole circle
			(at 48.26 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "unconnected-(H1-Pad40)")
			(pinfunction "Pin_40")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "41" thru_hole circle
			(at 50.8 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "unconnected-(H1-Pad41)")
			(pinfunction "Pin_41")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "42" thru_hole circle
			(at 50.8 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "unconnected-(H1-Pad42)")
			(pinfunction "Pin_42")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "43" thru_hole circle
			(at 53.34 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "unconnected-(H1-Pad43)")
			(pinfunction "Pin_43")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "44" thru_hole circle
			(at 53.34 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "unconnected-(H1-Pad44)")
			(pinfunction "Pin_44")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "45" thru_hole circle
			(at 55.88 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "ENA_LCL_4")
			(pinfunction "Pin_45")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "46" thru_hole circle
			(at 55.88 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "PWR_LCL_4")
			(pinfunction "Pin_46")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "47" thru_hole circle
			(at 58.42 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "ENA_LCL_3")
			(pinfunction "Pin_47")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "48" thru_hole circle
			(at 58.42 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "PWR_LCL_3")
			(pinfunction "Pin_48")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "49" thru_hole circle
			(at 60.96 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "ENA_LCL_2")
			(pinfunction "Pin_49")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "50" thru_hole circle
			(at 60.96 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "PWR_LCL_2")
			(pinfunction "Pin_50")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "51" thru_hole circle
			(at 63.5 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "ENA_LCL_1")
			(pinfunction "Pin_51")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "52" thru_hole circle
			(at 63.5 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "PWR_LCL_1")
			(pinfunction "Pin_52")
			(pintype "passive")
			(clearance 0.2)
		)
		(model "${KIPRJMOD}/librecube_pcb_template.pretty/ESQ-126-39-x-D.step"
			(offset
				(xyz 31.75 1.275 2.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "librecube_pcb_template:ESQ-126-39-x-D"
		(locked yes)
		(layer "F.Cu")
		(at 96.52 48.895)
		(descr "elevated through-hole socket strip designed for higher profile board spacing of PC/104 boards")
		(tags "PC104, connector, through-hole, socket strip")
		(property "Reference" "H2"
			(at -2.48 -1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_02X26"
			(at 1.27 -1.27 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(clearance 0.2)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "unconnected-(H2-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "2" thru_hole circle
			(at 0 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "unconnected-(H2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "3" thru_hole circle
			(at 2.54 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "unconnected-(H2-Pad3)")
			(pinfunction "Pin_3")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "4" thru_hole circle
			(at 2.54 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "unconnected-(H2-Pad4)")
			(pinfunction "Pin_4")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "5" thru_hole circle
			(at 5.08 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "unconnected-(H2-Pad5)")
			(pinfunction "Pin_5")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "6" thru_hole circle
			(at 5.08 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "unconnected-(H2-Pad6)")
			(pinfunction "Pin_6")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "7" thru_hole circle
			(at 7.62 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "unconnected-(H2-Pad7)")
			(pinfunction "Pin_7")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "8" thru_hole circle
			(at 7.62 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "unconnected-(H2-Pad8)")
			(pinfunction "Pin_8")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "9" thru_hole circle
			(at 10.16 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "unconnected-(H2-Pad9)")
			(pinfunction "Pin_9")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "10" thru_hole circle
			(at 10.16 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "unconnected-(H2-Pad10)")
			(pinfunction "Pin_10")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "11" thru_hole circle
			(at 12.7 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "unconnected-(H2-Pad11)")
			(pinfunction "Pin_11")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "12" thru_hole circle
			(at 12.7 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "unconnected-(H2-Pad12)")
			(pinfunction "Pin_12")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "13" thru_hole circle
			(at 15.24 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "unconnected-(H2-Pad13)")
			(pinfunction "Pin_13")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "14" thru_hole circle
			(at 15.24 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "unconnected-(H2-Pad14)")
			(pinfunction "Pin_14")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "15" thru_hole circle
			(at 17.78 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "unconnected-(H2-Pad15)")
			(pinfunction "Pin_15")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "16" thru_hole circle
			(at 17.78 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "unconnected-(H2-Pad16)")
			(pinfunction "Pin_16")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "17" thru_hole circle
			(at 20.32 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "unconnected-(H2-Pad17)")
			(pinfunction "Pin_17")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "18" thru_hole circle
			(at 20.32 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "unconnected-(H2-Pad18)")
			(pinfunction "Pin_18")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "19" thru_hole circle
			(at 22.86 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "unconnected-(H2-Pad19)")
			(pinfunction "Pin_19")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "20" thru_hole circle
			(at 22.86 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "unconnected-(H2-Pad20)")
			(pinfunction "Pin_20")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "21" thru_hole circle
			(at 25.4 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "unconnected-(H2-Pad21)")
			(pinfunction "Pin_21")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "22" thru_hole circle
			(at 25.4 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "unconnected-(H2-Pad22)")
			(pinfunction "Pin_22")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "23" thru_hole circle
			(at 27.94 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "unconnected-(H2-Pad23)")
			(pinfunction "Pin_23")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "24" thru_hole circle
			(at 27.94 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "unconnected-(H2-Pad24)")
			(pinfunction "Pin_24")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "25" thru_hole circle
			(at 30.48 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "Pin_25")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "26" thru_hole circle
			(at 30.48 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "Pin_26")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "27" thru_hole circle
			(at 33.02 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "unconnected-(H2-Pad27)")
			(pinfunction "Pin_27")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "28" thru_hole circle
			(at 33.02 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "unconnected-(H2-Pad28)")
			(pinfunction "Pin_28")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "29" thru_hole circle
			(at 35.56 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "GND")
			(pinfunction "Pin_29")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "30" thru_hole circle
			(at 35.56 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "GND")
			(pinfunction "Pin_30")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "31" thru_hole circle
			(at 38.1 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "GND")
			(pinfunction "Pin_31")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "32" thru_hole circle
			(at 38.1 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "GND")
			(pinfunction "Pin_32")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "33" thru_hole circle
			(at 40.64 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "unconnected-(H2-Pad33)")
			(pinfunction "Pin_33")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "34" thru_hole circle
			(at 40.64 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "unconnected-(H2-Pad34)")
			(pinfunction "Pin_34")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "35" thru_hole circle
			(at 43.18 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 96 "unconnected-(H2-Pad35)")
			(pinfunction "Pin_35")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "36" thru_hole circle
			(at 43.18 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "unconnected-(H2-Pad36)")
			(pinfunction "Pin_36")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "37" thru_hole circle
			(at 45.72 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 121 "S2")
			(pinfunction "Pin_37")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "38" thru_hole circle
			(at 45.72 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 121 "S2")
			(pinfunction "Pin_38")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "39" thru_hole circle
			(at 48.26 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 121 "S2")
			(pinfunction "Pin_39")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "40" thru_hole circle
			(at 48.26 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 121 "S2")
			(pinfunction "Pin_40")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "41" thru_hole circle
			(at 50.8 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "GND")
			(pinfunction "Pin_41")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "42" thru_hole circle
			(at 50.8 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "GND")
			(pinfunction "Pin_42")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "43" thru_hole circle
			(at 53.34 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "GND")
			(pinfunction "Pin_43")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "44" thru_hole circle
			(at 53.34 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "GND")
			(pinfunction "Pin_44")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "45" thru_hole circle
			(at 55.88 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "+BATT")
			(pinfunction "Pin_45")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "46" thru_hole circle
			(at 55.88 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "+BATT")
			(pinfunction "Pin_46")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "47" thru_hole circle
			(at 58.42 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "unconnected-(H2-Pad47)")
			(pinfunction "Pin_47")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "48" thru_hole circle
			(at 58.42 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 99 "unconnected-(H2-Pad48)")
			(pinfunction "Pin_48")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "49" thru_hole circle
			(at 60.96 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "unconnected-(H2-Pad49)")
			(pinfunction "Pin_49")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "50" thru_hole circle
			(at 60.96 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "unconnected-(H2-Pad50)")
			(pinfunction "Pin_50")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "51" thru_hole circle
			(at 63.5 0)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 102 "unconnected-(H2-Pad51)")
			(pinfunction "Pin_51")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(pad "52" thru_hole circle
			(at 63.5 -2.54)
			(size 1.365 1.365)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 103 "unconnected-(H2-Pad52)")
			(pinfunction "Pin_52")
			(pintype "passive+no_connect")
			(clearance 0.2)
		)
		(model "${KIPRJMOD}/librecube_pcb_template.pretty/ESQ-126-39-x-D.step"
			(offset
				(xyz 31.75 1.275 2.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad"
		(layer "F.Cu")
		(at 91.44 46.355)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "M1"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad"
		(layer "F.Cu")
		(at 165.1 46.355)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "M2"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad"
		(layer "F.Cu")
		(at 87.63 132.08)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "M3"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad"
		(layer "F.Cu")
		(at 167.64 132.08)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "M4"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 133.989949 62.875 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 1.778 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 133.989949 59.319 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -1.778 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "PWR_LCL_3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 144.096949 62.825 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0.254 1.778 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 140.336861 60.837632 90)
		(descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SO SO")
		(property "Reference" "U2"
			(at 0 -3.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "TPS2034"
			(at -0.576368 3.350088 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.575 -1.905 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.575 -0.635 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.575 0.635 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pinfunction "IN")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -2.575 1.905 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 60 "ENA_LCL_4")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 2.575 1.905 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 117 "unconnected-(U2-Pad5)")
			(pinfunction "/OC")
			(pintype "open_collector+no_connect")
		)
		(pad "6" smd roundrect
			(at 2.575 0.635 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "PWR_LCL_4")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at 2.575 -0.635 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "PWR_LCL_4")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at 2.575 -1.905 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "PWR_LCL_4")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 110.066861 60.862632 90)
		(descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SO SO")
		(property "Reference" "U3"
			(at 0 -3.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "TPS2034"
			(at 0 3.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.575 -1.905 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.575 -0.635 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.575 0.635 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pinfunction "IN")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -2.575 1.905 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 105 "ENA_LCL_1")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 2.575 1.905 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 118 "unconnected-(U3-Pad5)")
			(pinfunction "/OC")
			(pintype "open_collector+no_connect")
		)
		(pad "6" smd roundrect
			(at 2.575 0.635 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "PWR_LCL_1")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at 2.575 -0.635 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "PWR_LCL_1")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at 2.575 -1.905 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "PWR_LCL_1")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 130.236861 60.837632 90)
		(descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SO SO")
		(property "Reference" "U1"
			(at 0 -3.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "TPS2034"
			(at -0.626368 3.414088 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.575 -1.905 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.575 -0.635 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.575 0.635 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pinfunction "IN")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -2.575 1.905 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "ENA_LCL_3")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 2.575 1.905 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 116 "unconnected-(U1-Pad5)")
			(pinfunction "/OC")
			(pintype "open_collector+no_connect")
		)
		(pad "6" smd roundrect
			(at 2.575 0.635 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "PWR_LCL_3")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at 2.575 -0.635 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "PWR_LCL_3")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at 2.575 -1.905 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "PWR_LCL_3")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 144.096949 59.269 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -1.778 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "PWR_LCL_4")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 113.816861 62.845132 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at -0.762 1.778 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 113.816861 59.289132 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at -0.762 -1.778 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "PWR_LCL_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 120.179791 60.837264 90)
		(descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SO SO")
		(property "Reference" "U4"
			(at 0 -3.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "TPS2034"
			(at -0.492868 3.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.575 -1.905 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.575 -0.635 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.575 0.635 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pinfunction "IN")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -2.575 1.905 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 104 "ENA_LCL_2")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 2.575 1.905 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 119 "unconnected-(U4-Pad5)")
			(pinfunction "/OC")
			(pintype "open_collector+no_connect")
		)
		(pad "6" smd roundrect
			(at 2.575 0.635 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 57 "PWR_LCL_2")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at 2.575 -0.635 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 57 "PWR_LCL_2")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at 2.575 -1.905 90)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 57 "PWR_LCL_2")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 123.917791 62.850132 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0 1.778 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 123.917791 59.294132 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at -0.254 -1.778 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 57 "PWR_LCL_2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 144.78 42.926 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J9"
			(at 0 -2.33 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 0 4.87 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 121 "S2")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 122.965 115.95 -90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D9"
			(at -3.55622 -0.0924 90)
			(layer "F.SilkS")
		)
		(property "Value" "D_Schottky"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 110 "CHARGE")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 114 "Net-(D10-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 118.3 115.95 -90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D8"
			(at -3.52574 -0.1747 90)
			(layer "F.SilkS")
		)
		(property "Value" "D_Schottky"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 110 "CHARGE")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 113 "Net-(D7-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 132.4 115.95 -90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D12"
			(at -4.0185 0.05544 90)
			(layer "F.SilkS")
		)
		(property "Value" "D_Schottky"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 110 "CHARGE")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 115 "Net-(D11-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 115.965 115.95 -90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D7"
			(at -3.5105 -0.08428 90)
			(layer "F.SilkS")
		)
		(property "Value" "D_Schottky"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 110 "CHARGE")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 113 "Net-(D7-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 125.3 115.95 -90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D10"
			(at -3.99564 -0.01264 90)
			(layer "F.SilkS")
		)
		(property "Value" "D_Schottky"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 110 "CHARGE")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 114 "Net-(D10-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 125.365 120.2975 -90)
		(descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x02 2.54mm single row")
		(property "Reference" "J7"
			(at 4.385 -2.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 4.385 4.81 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 114 "Net-(D10-Pad2)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 132.365 120.2975 -90)
		(descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x02 2.54mm single row")
		(property "Reference" "J8"
			(at 4.385 -2.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 4.385 4.81 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 115 "Net-(D11-Pad2)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 118.365 120.2975 -90)
		(descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x02 2.54mm single row")
		(property "Reference" "J6"
			(at 4.385 -2.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 4.385 4.81 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 113 "Net-(D7-Pad2)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Battery:BatteryHolder_Keystone_1042_1x18650"
		(locked yes)
		(layer "F.Cu")
		(at 127.4 100.2 180)
		(descr "Battery holder for 18650 cylindrical cells http://www.keyelco.com/product.cfm/product_id/918")
		(tags "18650 Keystone 1042 Li-ion")
		(property "Reference" "BT2"
			(at -36.203 8.925 0)
			(layer "F.SilkS")
		)
		(property "Value" "Battery_Cell"
			(at 0 11.3 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -35.93 -8 180)
			(size 2.39 2.39)
			(drill 2.39)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -27.6 8 180)
			(size 3.45 3.45)
			(drill 3.45)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 27.6 -8 180)
			(size 3.45 3.45)
			(drill 3.45)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -38.5 0 180)
			(size 7.34 6.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "+BATT")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 38.5 0 180)
			(size 7.34 6.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 135 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_Keystone_1042_1x18650.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Battery:BatteryHolder_Keystone_1042_1x18650"
		(locked yes)
		(layer "F.Cu")
		(at 127.5 78.3)
		(descr "Battery holder for 18650 cylindrical cells http://www.keyelco.com/product.cfm/product_id/918")
		(tags "18650 Keystone 1042 Li-ion")
		(property "Reference" "BT1"
			(at 36.33 -8.896 0)
			(layer "F.SilkS")
		)
		(property "Value" "Battery_Cell"
			(at 0 11.3 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -35.93 -8)
			(size 2.39 2.39)
			(drill 2.39)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -27.6 8)
			(size 3.45 3.45)
			(drill 3.45)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 27.6 -8)
			(size 3.45 3.45)
			(drill 3.45)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -38.5 0)
			(size 7.34 6.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "+BATT")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 38.5 0)
			(size 7.34 6.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 135 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_Keystone_1042_1x18650.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Symbol:OSHW-Logo2_7.3x6mm_SilkScreen"
		(locked yes)
		(layer "F.Cu")
		(at 165.1 52.7)
		(descr "Open Source Hardware Symbol")
		(tags "Logo Symbol OSHW")
		(property "Reference" "REF**"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "OSHW-Logo2_7.3x6mm_SilkScreen"
			(at 0.75 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 101.896 115.9205 -90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D3"
			(at -3.5105 -0.04518 90)
			(layer "F.SilkS")
		)
		(property "Value" "D_Schottky"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 110 "CHARGE")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 111 "Net-(D3-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 97.296 120.268 -90)
		(descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x02 2.54mm single row")
		(property "Reference" "J3"
			(at 4.385 -2.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 4.385 4.81 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 109 "Net-(D1-Pad2)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 111.331 115.9205 -90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D6"
			(at -3.5105 -0.07768 90)
			(layer "F.SilkS")
		)
		(property "Value" "D_Schottky"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 110 "CHARGE")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 112 "Net-(D5-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 104.296 120.268 -90)
		(descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x02 2.54mm single row")
		(property "Reference" "J4"
			(at 4.385 -2.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 4.385 4.81 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 111 "Net-(D3-Pad2)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 104.331 115.9205 -90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D4"
			(at -3.4978 -0.04924 90)
			(layer "F.SilkS")
		)
		(property "Value" "D_Schottky"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 110 "CHARGE")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 111 "Net-(D3-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 108.896 115.9205 -90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D5"
			(at -3.5105 -0.06346 90)
			(layer "F.SilkS")
		)
		(property "Value" "D_Schottky"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 110 "CHARGE")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 112 "Net-(D5-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 97.331 115.883 -90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D2"
			(at -3.573 -0.03096 90)
			(layer "F.SilkS")
		)
		(property "Value" "D_Schottky"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 110 "CHARGE")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 109 "Net-(D1-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 111.296 120.268 -90)
		(descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x02 2.54mm single row")
		(property "Reference" "J5"
			(at 4.385 -2.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 4.385 4.81 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 112 "Net-(D5-Pad2)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "librecube_pcb_template:LibreCube_logo_22.4mm"
		(locked yes)
		(layer "F.Cu")
		(at 151.765 134.493)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 129.965 115.95 -90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D11"
			(at -4.0185 0.0214 90)
			(layer "F.SilkS")
		)
		(property "Value" "D_Schottky"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 110 "CHARGE")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 115 "Net-(D11-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 94.896 115.883 -90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D1"
			(at -3.573 -0.00812 90)
			(layer "F.SilkS")
		)
		(property "Value" "D_Schottky"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 110 "CHARGE")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 109 "Net-(D1-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 157.5 60.85 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.5k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 108 "Net-(D27-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 152.4 60.8 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.5k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 147 "Net-(D29-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 136.546949 62.825 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 60 "ENA_LCL_4")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 106.290949 62.859 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 105 "ENA_LCL_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric"
		(layer "F.Cu")
		(at 116 43)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D25"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "Net-(D25-Pad1)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric"
		(layer "F.Cu")
		(at 152.4 57.4 90)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D29"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 147 "Net-(D29-Pad1)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "PWR_LCL_4")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 116.435879 62.837632 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 104 "ENA_LCL_2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric"
		(layer "F.Cu")
		(at 160 57.4125 90)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D26"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(D26-Pad1)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "PWR_LCL_1")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 126.489949 62.875 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 61 "ENA_LCL_3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 154.95 60.85 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.5k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 146 "Net-(D28-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric"
		(layer "F.Cu")
		(at 154.95 57.4 90)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D28"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 146 "Net-(D28-Pad1)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "PWR_LCL_3")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 160 60.85 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.5k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 5 "Net-(D26-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric"
		(layer "F.Cu")
		(at 157.5 57.4 90)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D27"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 108 "Net-(D27-Pad1)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 57 "PWR_LCL_2")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 112.5 43 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "1.5k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 59 "Net-(D25-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "B.Cu")
		(at 100.619583 93.202917)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D14"
			(at 0 2 0)
			(layer "B.SilkS")
		)
		(property "Value" "D_Schottky"
			(at 0 -2.1 0)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 107 "/Semi_Regulated_Bus")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 3 "Net-(C19-Pad1)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP2.85x4mm"
		(layer "B.Cu")
		(at 113.576083 98.108958 180)
		(descr "HTSSOP, 20 Pin (https://pdfserv.maximintegrated.com/package_dwgs/21-0108.PDF U20E-1), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "HTSSOP SO")
		(property "Reference" "U31"
			(at 0 4.2 0)
			(layer "B.SilkS")
		)
		(property "Value" "bq24002"
			(at 0 -4.2 0)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "" smd roundrect
			(at 0 -1 180)
			(size 2.3 1.61)
			(layers "B.Paste")
			(roundrect_rratio 0.15528)
		)
		(pad "" smd roundrect
			(at 0 1 180)
			(size 2.3 1.61)
			(layers "B.Paste")
			(roundrect_rratio 0.15528)
		)
		(pad "1" smd roundrect
			(at -2.8625 2.925 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 132 "unconnected-(U31-Pad1)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "2" smd roundrect
			(at -2.8625 2.275 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 140 "Net-(R52-Pad1)")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.8625 1.625 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 140 "Net-(R52-Pad1)")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.8625 0.975 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.325 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 140 "Net-(R52-Pad1)")
			(pinfunction "ISNS")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at -2.8625 -0.325 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 133 "unconnected-(U31-Pad6)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "7" smd roundrect
			(at -2.8625 -0.975 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 83 "Net-(R50-Pad2)")
			(pinfunction "APG/THERM")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -2.8625 -1.625 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -2.8625 -2.275 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pinfunction "VSEL")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -2.8625 -2.925 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 2.8625 -2.925 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 134 "unconnected-(U31-Pad11)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "12" smd roundrect
			(at 2.8625 -2.275 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(C46-Pad1)")
			(pinfunction "CR")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at 2.8625 -1.625 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "TMR_SEL")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 2.8625 -0.975 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(D18-Pad1)")
			(pinfunction "STAT1")
			(pintype "output")
		)
		(pad "15" smd roundrect
			(at 2.8625 -0.325 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(D17-Pad1)")
			(pinfunction "STAT2")
			(pintype "output")
		)
		(pad "16" smd roundrect
			(at 2.8625 0.325 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "17" smd roundrect
			(at 2.8625 0.975 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 58 "+BATT")
			(pinfunction "VSENSE")
			(pintype "input")
		)
		(pad "18" smd roundrect
			(at 2.8625 1.625 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 58 "+BATT")
			(pinfunction "OUT`")
			(pintype "passive")
		)
		(pad "19" smd roundrect
			(at 2.8625 2.275 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 58 "+BATT")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(pad "20" smd roundrect
			(at 2.8625 2.925 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 136 "unconnected-(U31-Pad20)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "21" smd rect
			(at 0 0 180)
			(size 2.85 4)
			(layers "B.Cu" "B.Mask")
		)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP2.85x4mm.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 148.575 83.925 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C32"
			(at 0 1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 106 "Net-(C32-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 151.175 75.925 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C33"
			(at -3.4 0.2 90)
			(layer "B.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 113.433 82.009)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C35"
			(at 0 -1.778 180)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 107 "/Semi_Regulated_Bus")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 116.989 82.009 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C36"
			(at 0 1.778 180)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 106 "Net-(C32-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 113.3545 73.119)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C37"
			(at 0.0785 -1.778 180)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 107 "/Semi_Regulated_Bus")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 116.989 73.119 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C38"
			(at 0 1.778 180)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 106 "Net-(C32-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 111.401083 102.658958)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C46"
			(at 0 1.625 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.22uF"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(C46-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 111.426083 93.558958)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C48"
			(at 0 -1.778 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 58 "+BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "B.Cu")
		(at 100.623983 90.791037)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D13"
			(at -0.0317 -1.77708 0)
			(layer "B.SilkS")
		)
		(property "Value" "D_Schottky"
			(at 0 -2.1 0)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 107 "/Semi_Regulated_Bus")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 3 "Net-(C19-Pad1)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "B.Cu")
		(at 100.594583 100.527917)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D15"
			(at 0 -1.632 0)
			(layer "B.SilkS")
		)
		(property "Value" "D_Schottky"
			(at 0 -2.1 0)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 107 "/Semi_Regulated_Bus")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 58 "+BATT")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "B.Cu")
		(at 100.594583 103.067917)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D16"
			(at 0 2 0)
			(layer "B.SilkS")
		)
		(property "Value" "D_Schottky"
			(at 0 -2.1 0)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 107 "/Semi_Regulated_Bus")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 58 "+BATT")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric"
		(layer "B.Cu")
		(at 105.501083 96.433958 -90)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D17"
			(at -3.1642 -0.1 -90)
			(layer "B.SilkS")
		)
		(property "Value" "LED"
			(at 0 -1.65 -90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(D17-Pad1)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(D17-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric"
		(layer "B.Cu")
		(at 107.526083 96.433958 -90)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D18"
			(at -3.1675 -0.1 -90)
			(layer "B.SilkS")
		)
		(property "Value" "LED"
			(at 0 -1.65 -90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(D18-Pad1)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(D18-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric"
		(layer "B.Cu")
		(at 105.875 109.3875 -90)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D19"
			(at 0.2551 2.9188 -90)
			(layer "B.SilkS")
		)
		(property "Value" "LED"
			(at 0 -1.65 -90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(D19-Pad1)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(D19-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_10.4x10.4_H4.8"
		(layer "B.Cu")
		(at 156.072 84.129 -90)
		(descr "Choke, SMD, 10.4x10.4mm 4.8mm height")
		(tags "Choke SMD")
		(property "Reference" "L2"
			(at 4.996 6.35 90)
			(layer "B.SilkS")
		)
		(property "Value" "6.8uH"
			(at 0 -6.35 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -4.15 0 270)
			(size 2.7 3.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 80 "Net-(L2-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 4.15 0 270)
			(size 2.7 3.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 106 "Net-(C32-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_10.4x10.4_H4.8.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 118.526083 99.933958 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R50"
			(at -3.1625 -0.165 90)
			(layer "B.SilkS")
		)
		(property "Value" "309k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 83 "Net-(R50-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 117.776083 102.683958 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R51"
			(at 3.1625 0.295 0)
			(layer "B.SilkS")
		)
		(property "Value" "110k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 83 "Net-(R50-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "B.Cu")
		(at 118.676083 95.858958 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R52"
			(at 3.81 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1"
			(at 0 -1.82 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0 90)
			(size 1.25 1.75)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.2)
			(net 140 "Net-(R52-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4 0 90)
			(size 1.25 1.75)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.2)
			(net 3 "Net-(C19-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 105.501083 99.908958 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R55"
			(at -3.53492 -0.00254 -90)
			(layer "B.SilkS")
		)
		(property "Value" "1.5k"
			(at 0 -1.65 -90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(D17-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 107.526083 99.908958 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R56"
			(at -3.3325 0.02184 -90)
			(layer "B.SilkS")
		)
		(property "Value" "1.5k"
			(at 0 -1.65 -90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(D18-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3x3mm"
		(layer "B.Cu")
		(at 146.975 76.525 90)
		(descr "HTSSOP, 16 Pin (https://www.st.com/resource/en/datasheet/stp08cp05.pdf#page=20), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "HTSSOP SO")
		(property "Reference" "U23"
			(at -5.6 -2.2 90)
			(layer "B.SilkS")
		)
		(property "Value" "TPS61032"
			(at 0 -3.45 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "" smd roundrect
			(at -0.75 -0.75 90)
			(size 1.21 1.21)
			(layers "B.Paste")
			(roundrect_rratio 0.206612)
		)
		(pad "" smd roundrect
			(at -0.75 0.75 90)
			(size 1.21 1.21)
			(layers "B.Paste")
			(roundrect_rratio 0.206612)
		)
		(pad "" smd roundrect
			(at 0.75 -0.75 90)
			(size 1.21 1.21)
			(layers "B.Paste")
			(roundrect_rratio 0.206612)
		)
		(pad "" smd roundrect
			(at 0.75 0.75 90)
			(size 1.21 1.21)
			(layers "B.Paste")
			(roundrect_rratio 0.206612)
		)
		(pad "1" smd roundrect
			(at -2.875 2.275 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 80 "Net-(L2-Pad1)")
			(pinfunction "SW")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.875 1.625 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 80 "Net-(L2-Pad1)")
			(pinfunction "SW")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.875 0.975 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.875 0.325 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -2.875 -0.325 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at -2.875 -0.975 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 106 "Net-(C32-Pad1)")
			(pinfunction "VBAT")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -2.875 -1.625 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "LBI")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -2.875 -2.275 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "SYNC")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at 2.875 -2.275 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 106 "Net-(C32-Pad1)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 2.875 -1.625 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 124 "unconnected-(U23-Pad10)")
			(pinfunction "LBO")
			(pintype "output+no_connect")
		)
		(pad "11" smd roundrect
			(at 2.875 -0.975 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at 2.875 -0.325 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 125 "unconnected-(U23-Pad12)")
			(pinfunction "FB")
			(pintype "input+no_connect")
		)
		(pad "13" smd roundrect
			(at 2.875 0.325 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pinfunction "VOUT")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 2.875 0.975 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pinfunction "VOUT")
			(pintype "passive")
		)
		(pad "15" smd roundrect
			(at 2.875 1.625 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pinfunction "VOUT")
			(pintype "passive")
		)
		(pad "16" smd roundrect
			(at 2.875 2.275 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 126 "unconnected-(U23-Pad16)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "17" smd rect
			(at 0 0 90)
			(size 3 3)
			(layers "B.Cu" "B.Mask")
			(net 135 "GND")
			(pinfunction "PAD")
			(pintype "power_in")
		)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3x3mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
		(layer "B.Cu")
		(at 114.957 85.819)
		(descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SO SO")
		(property "Reference" "U24"
			(at 0 3.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "TPS2034"
			(at 0 -3.4 0)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.575 1.905)
			(size 1.75 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.575 0.635)
			(size 1.75 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 107 "/Semi_Regulated_Bus")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.575 -0.635)
			(size 1.75 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 107 "/Semi_Regulated_Bus")
			(pinfunction "IN")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -2.575 -1.905)
			(size 1.75 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 121 "S2")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 2.575 -1.905)
			(size 1.75 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 127 "unconnected-(U24-Pad5)")
			(pinfunction "/OC")
			(pintype "open_collector+no_connect")
		)
		(pad "6" smd roundrect
			(at 2.575 -0.635)
			(size 1.75 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 106 "Net-(C32-Pad1)")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at 2.575 0.635)
			(size 1.75 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 106 "Net-(C32-Pad1)")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at 2.575 1.905)
			(size 1.75 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 106 "Net-(C32-Pad1)")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
		(layer "B.Cu")
		(at 114.975 77.015)
		(descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SO SO")
		(property "Reference" "U25"
			(at 0 3.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "TPS2034"
			(at 0 -3.4 0)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.575 1.905)
			(size 1.75 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.575 0.635)
			(size 1.75 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 107 "/Semi_Regulated_Bus")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.575 -0.635)
			(size 1.75 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 107 "/Semi_Regulated_Bus")
			(pinfunction "IN")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -2.575 -1.905)
			(size 1.75 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 121 "S2")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 2.575 -1.905)
			(size 1.75 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 128 "unconnected-(U25-Pad5)")
			(pinfunction "/OC")
			(pintype "open_collector+no_connect")
		)
		(pad "6" smd roundrect
			(at 2.575 -0.635)
			(size 1.75 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 106 "Net-(C32-Pad1)")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at 2.575 0.635)
			(size 1.75 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 106 "Net-(C32-Pad1)")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at 2.575 1.905)
			(size 1.75 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 106 "Net-(C32-Pad1)")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_Tantalum_SMD:CP_EIA-7343-31_Kemet-D"
		(layer "B.Cu")
		(at 138.575 74.925)
		(descr "Tantalum Capacitor SMD Kemet-D (7343-31 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
		(tags "capacitor tantalum")
		(property "Reference" "C21"
			(at -2.54 3.683 180)
			(layer "B.SilkS")
		)
		(property "Value" "220uF"
			(at 0 -3.1 180)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -3.1125 0)
			(size 2.075 2.55)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.120482)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.1125 0)
			(size 2.075 2.55)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.120482)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-31_Kemet-D.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_Tantalum_SMD:CP_EIA-7343-31_Kemet-D"
		(layer "B.Cu")
		(at 156.975 75.125)
		(descr "Tantalum Capacitor SMD Kemet-D (7343-31 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
		(tags "capacitor tantalum")
		(property "Reference" "C23"
			(at 0 -3.4 180)
			(layer "B.SilkS")
		)
		(property "Value" "220uF"
			(at 0 -3.1 180)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -3.1125 0)
			(size 2.075 2.55)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.120482)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.1125 0)
			(size 2.075 2.55)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.120482)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-31_Kemet-D.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_Tantalum_SMD:CP_EIA-7343-31_Kemet-D"
		(layer "B.Cu")
		(at 138.1 101.2625)
		(descr "Tantalum Capacitor SMD Kemet-D (7343-31 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
		(tags "capacitor tantalum")
		(property "Reference" "C25"
			(at 0 -3.175 180)
			(layer "B.SilkS")
		)
		(property "Value" "220uF"
			(at 0 -3.1 180)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -3.1125 0)
			(size 2.075 2.55)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.120482)
			(net 3 "Net-(C19-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.1125 0)
			(size 2.075 2.55)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.120482)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-31_Kemet-D.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 129.975 83.725 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C39"
			(at 0 1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 106 "Net-(C32-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 132.775 75.525 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C40"
			(at 3.429 -0.254 90)
			(layer "B.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_10.4x10.4_H4.8"
		(layer "B.Cu")
		(at 137.575 84.125 -90)
		(descr "Choke, SMD, 10.4x10.4mm 4.8mm height")
		(tags "Choke SMD")
		(property "Reference" "L3"
			(at 4.6 6.4 90)
			(layer "B.SilkS")
		)
		(property "Value" "6.8uH"
			(at 0 -6.35 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -4.15 0 270)
			(size 2.7 3.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 81 "Net-(L3-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 4.15 0 270)
			(size 2.7 3.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 106 "Net-(C32-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_10.4x10.4_H4.8.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3x3mm"
		(layer "B.Cu")
		(at 128.375 76.525 90)
		(descr "HTSSOP, 16 Pin (https://www.st.com/resource/en/datasheet/stp08cp05.pdf#page=20), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "HTSSOP SO")
		(property "Reference" "U26"
			(at -5.6 -2 90)
			(layer "B.SilkS")
		)
		(property "Value" "TPS61032"
			(at 0 -3.45 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "" smd roundrect
			(at -0.75 -0.75 90)
			(size 1.21 1.21)
			(layers "B.Paste")
			(roundrect_rratio 0.206612)
		)
		(pad "" smd roundrect
			(at -0.75 0.75 90)
			(size 1.21 1.21)
			(layers "B.Paste")
			(roundrect_rratio 0.206612)
		)
		(pad "" smd roundrect
			(at 0.75 -0.75 90)
			(size 1.21 1.21)
			(layers "B.Paste")
			(roundrect_rratio 0.206612)
		)
		(pad "" smd roundrect
			(at 0.75 0.75 90)
			(size 1.21 1.21)
			(layers "B.Paste")
			(roundrect_rratio 0.206612)
		)
		(pad "1" smd roundrect
			(at -2.875 2.275 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 81 "Net-(L3-Pad1)")
			(pinfunction "SW")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.875 1.625 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 81 "Net-(L3-Pad1)")
			(pinfunction "SW")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.875 0.975 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.875 0.325 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -2.875 -0.325 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at -2.875 -0.975 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 106 "Net-(C32-Pad1)")
			(pinfunction "VBAT")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -2.875 -1.625 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "LBI")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -2.875 -2.275 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "SYNC")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at 2.875 -2.275 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 106 "Net-(C32-Pad1)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 2.875 -1.625 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 129 "unconnected-(U26-Pad10)")
			(pinfunction "LBO")
			(pintype "output+no_connect")
		)
		(pad "11" smd roundrect
			(at 2.875 -0.975 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at 2.875 -0.325 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 130 "unconnected-(U26-Pad12)")
			(pinfunction "FB")
			(pintype "input+no_connect")
		)
		(pad "13" smd roundrect
			(at 2.875 0.325 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pinfunction "VOUT")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 2.875 0.975 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pinfunction "VOUT")
			(pintype "passive")
		)
		(pad "15" smd roundrect
			(at 2.875 1.625 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pinfunction "VOUT")
			(pintype "passive")
		)
		(pad "16" smd roundrect
			(at 2.875 2.275 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 131 "unconnected-(U26-Pad16)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "17" smd rect
			(at 0 0 90)
			(size 3 3)
			(layers "B.Cu" "B.Mask")
			(net 135 "GND")
			(pinfunction "PAD")
			(pintype "power_in")
		)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3x3mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3x3mm"
		(layer "B.Cu")
		(at 127.925 102.6625 90)
		(descr "HTSSOP, 16 Pin (https://www.st.com/resource/en/datasheet/stp08cp05.pdf#page=20), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "HTSSOP SO")
		(property "Reference" "U33"
			(at -5.6 -2 90)
			(layer "B.SilkS")
		)
		(property "Value" "TPS61032"
			(at 0 -3.45 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "" smd roundrect
			(at -0.75 -0.75 90)
			(size 1.21 1.21)
			(layers "B.Paste")
			(roundrect_rratio 0.206612)
		)
		(pad "" smd roundrect
			(at -0.75 0.75 90)
			(size 1.21 1.21)
			(layers "B.Paste")
			(roundrect_rratio 0.206612)
		)
		(pad "" smd roundrect
			(at 0.75 -0.75 90)
			(size 1.21 1.21)
			(layers "B.Paste")
			(roundrect_rratio 0.206612)
		)
		(pad "" smd roundrect
			(at 0.75 0.75 90)
			(size 1.21 1.21)
			(layers "B.Paste")
			(roundrect_rratio 0.206612)
		)
		(pad "1" smd roundrect
			(at -2.875 2.275 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 82 "Net-(L4-Pad1)")
			(pinfunction "SW")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.875 1.625 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 82 "Net-(L4-Pad1)")
			(pinfunction "SW")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.875 0.975 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.875 0.325 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -2.875 -0.325 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at -2.875 -0.975 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 110 "CHARGE")
			(pinfunction "VBAT")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -2.875 -1.625 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "LBI")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -2.875 -2.275 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "SYNC")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at 2.875 -2.275 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 110 "CHARGE")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 2.875 -1.625 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 137 "unconnected-(U33-Pad10)")
			(pinfunction "LBO")
			(pintype "output+no_connect")
		)
		(pad "11" smd roundrect
			(at 2.875 -0.975 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at 2.875 -0.325 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 138 "unconnected-(U33-Pad12)")
			(pinfunction "FB")
			(pintype "input+no_connect")
		)
		(pad "13" smd roundrect
			(at 2.875 0.325 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pinfunction "VOUT")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 2.875 0.975 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pinfunction "VOUT")
			(pintype "passive")
		)
		(pad "15" smd roundrect
			(at 2.875 1.625 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pinfunction "VOUT")
			(pintype "passive")
		)
		(pad "16" smd roundrect
			(at 2.875 2.275 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 139 "unconnected-(U33-Pad16)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "17" smd rect
			(at 0 0 90)
			(size 3 3)
			(layers "B.Cu" "B.Mask")
			(net 135 "GND")
			(pinfunction "PAD")
			(pintype "power_in")
		)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3x3mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 132.1 102.0625 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C30"
			(at -3.4 0.2 90)
			(layer "B.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 150.7 102.0625 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C51"
			(at -3.2 0.2 90)
			(layer "B.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_10.4x10.4_H4.8"
		(layer "B.Cu")
		(at 137.0048 110.5795 -90)
		(descr "Choke, SMD, 10.4x10.4mm 4.8mm height")
		(tags "Choke SMD")
		(property "Reference" "L4"
			(at 4.483 6.35 90)
			(layer "B.SilkS")
		)
		(property "Value" "6.8uH"
			(at 0 -6.35 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -4.15 0 270)
			(size 2.7 3.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 82 "Net-(L4-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 4.15 0 270)
			(size 2.7 3.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 110 "CHARGE")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_10.4x10.4_H4.8.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 129.7 109.8625 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C50"
			(at 0 1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 110 "CHARGE")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 148.3 109.6625 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C29"
			(at 0 1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 110 "CHARGE")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_Tantalum_SMD:CP_EIA-7343-31_Kemet-D"
		(layer "B.Cu")
		(at 156.5 101.2625)
		(descr "Tantalum Capacitor SMD Kemet-D (7343-31 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
		(tags "capacitor tantalum")
		(property "Reference" "C19"
			(at -0.2 -3.2 180)
			(layer "B.SilkS")
		)
		(property "Value" "220uF"
			(at 0 -3.1 180)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -3.1125 0)
			(size 2.075 2.55)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.120482)
			(net 3 "Net-(C19-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.1125 0)
			(size 2.075 2.55)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.120482)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-31_Kemet-D.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_10.4x10.4_H4.8"
		(layer "B.Cu")
		(at 155.5 110.4625 -90)
		(descr "Choke, SMD, 10.4x10.4mm 4.8mm height")
		(tags "Choke SMD")
		(property "Reference" "L1"
			(at 4.6 6.35 90)
			(layer "B.SilkS")
		)
		(property "Value" "6.8uH"
			(at 0 -6.35 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -4.15 0 270)
			(size 2.7 3.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 79 "Net-(L1-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 4.15 0 270)
			(size 2.7 3.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 110 "CHARGE")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_10.4x10.4_H4.8.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3x3mm"
		(layer "B.Cu")
		(at 146.539 102.6105 90)
		(descr "HTSSOP, 16 Pin (https://www.st.com/resource/en/datasheet/stp08cp05.pdf#page=20), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "HTSSOP SO")
		(property "Reference" "U22"
			(at -5.452 -2.039 90)
			(layer "B.SilkS")
		)
		(property "Value" "TPS61032"
			(at 0 -3.45 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "" smd roundrect
			(at -0.75 -0.75 90)
			(size 1.21 1.21)
			(layers "B.Paste")
			(roundrect_rratio 0.206612)
		)
		(pad "" smd roundrect
			(at -0.75 0.75 90)
			(size 1.21 1.21)
			(layers "B.Paste")
			(roundrect_rratio 0.206612)
		)
		(pad "" smd roundrect
			(at 0.75 -0.75 90)
			(size 1.21 1.21)
			(layers "B.Paste")
			(roundrect_rratio 0.206612)
		)
		(pad "" smd roundrect
			(at 0.75 0.75 90)
			(size 1.21 1.21)
			(layers "B.Paste")
			(roundrect_rratio 0.206612)
		)
		(pad "1" smd roundrect
			(at -2.875 2.275 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 79 "Net-(L1-Pad1)")
			(pinfunction "SW")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.875 1.625 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 79 "Net-(L1-Pad1)")
			(pinfunction "SW")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.875 0.975 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.875 0.325 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -2.875 -0.325 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at -2.875 -0.975 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 110 "CHARGE")
			(pinfunction "VBAT")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -2.875 -1.625 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "LBI")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -2.875 -2.275 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "SYNC")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at 2.875 -2.275 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 110 "CHARGE")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 2.875 -1.625 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 120 "unconnected-(U22-Pad10)")
			(pinfunction "LBO")
			(pintype "output+no_connect")
		)
		(pad "11" smd roundrect
			(at 2.875 -0.975 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at 2.875 -0.325 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 122 "unconnected-(U22-Pad12)")
			(pinfunction "FB")
			(pintype "input+no_connect")
		)
		(pad "13" smd roundrect
			(at 2.875 0.325 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pinfunction "VOUT")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 2.875 0.975 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pinfunction "VOUT")
			(pintype "passive")
		)
		(pad "15" smd roundrect
			(at 2.875 1.625 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pinfunction "VOUT")
			(pintype "passive")
		)
		(pad "16" smd roundrect
			(at 2.875 2.275 90)
			(size 1.55 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 123 "unconnected-(U22-Pad16)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "17" smd rect
			(at 0 0 90)
			(size 3 3)
			(layers "B.Cu" "B.Mask")
			(net 135 "GND")
			(pinfunction "PAD")
			(pintype "power_in")
		)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3x3mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 115.751083 93.558958 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C45"
			(at 0 1.65 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 111.519583 106.452917)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C56"
			(at 0 -1.524 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 58 "+BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 115.837583 106.452917 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C53"
			(at 0 1.65 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric"
		(layer "B.Cu")
		(at 107.975 109.3875 -90)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D20"
			(at -0.8967 3.725 -90)
			(layer "B.SilkS")
		)
		(property "Value" "LED"
			(at 0 -1.65 -90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 13 "Net-(D20-Pad1)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(D20-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP2.85x4mm"
		(layer "B.Cu")
		(at 113.713583 111.057917 180)
		(descr "HTSSOP, 20 Pin (https://pdfserv.maximintegrated.com/package_dwgs/21-0108.PDF U20E-1), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "HTSSOP SO")
		(property "Reference" "U34"
			(at 0 4.2 0)
			(layer "B.SilkS")
		)
		(property "Value" "bq24002"
			(at 0 -4.2 0)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "" smd roundrect
			(at 0 -1 180)
			(size 2.3 1.61)
			(layers "B.Paste")
			(roundrect_rratio 0.15528)
		)
		(pad "" smd roundrect
			(at 0 1 180)
			(size 2.3 1.61)
			(layers "B.Paste")
			(roundrect_rratio 0.15528)
		)
		(pad "1" smd roundrect
			(at -2.8625 2.925 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 142 "unconnected-(U34-Pad1)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "2" smd roundrect
			(at -2.8625 2.275 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 141 "Net-(R62-Pad1)")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.8625 1.625 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 141 "Net-(R62-Pad1)")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.8625 0.975 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.325 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 141 "Net-(R62-Pad1)")
			(pinfunction "ISNS")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at -2.8625 -0.325 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 143 "unconnected-(U34-Pad6)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "7" smd roundrect
			(at -2.8625 -0.975 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 84 "Net-(R60-Pad2)")
			(pinfunction "APG/THERM")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -2.8625 -1.625 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -2.8625 -2.275 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pinfunction "VSEL")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -2.8625 -2.925 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 2.8625 -2.925 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 144 "unconnected-(U34-Pad11)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "12" smd roundrect
			(at 2.8625 -2.275 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "Net-(C54-Pad1)")
			(pinfunction "CR")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at 2.8625 -1.625 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "TMR_SEL")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 2.8625 -0.975 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 13 "Net-(D20-Pad1)")
			(pinfunction "STAT1")
			(pintype "output")
		)
		(pad "15" smd roundrect
			(at 2.8625 -0.325 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(D19-Pad1)")
			(pinfunction "STAT2")
			(pintype "output")
		)
		(pad "16" smd roundrect
			(at 2.8625 0.325 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "17" smd roundrect
			(at 2.8625 0.975 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 58 "+BATT")
			(pinfunction "VSENSE")
			(pintype "input")
		)
		(pad "18" smd roundrect
			(at 2.8625 1.625 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 58 "+BATT")
			(pinfunction "OUT`")
			(pintype "passive")
		)
		(pad "19" smd roundrect
			(at 2.8625 2.275 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 58 "+BATT")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(pad "20" smd roundrect
			(at 2.8625 2.925 180)
			(size 1.475 0.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 145 "unconnected-(U34-Pad20)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "21" smd rect
			(at 0 0 180)
			(size 2.85 4)
			(layers "B.Cu" "B.Mask")
		)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP2.85x4mm.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 118.641583 112.895917 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R60"
			(at -3.302 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "309k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 84 "Net-(R60-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 117.891583 115.595917 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R61"
			(at -3.302 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "110k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 84 "Net-(R60-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 107.975 112.925 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R66"
			(at -3.2495 0.0723 -90)
			(layer "B.SilkS")
		)
		(property "Value" "1.5k"
			(at 0 -1.65 -90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(D20-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 111.541583 115.595917)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C54"
			(at 3.302 0.137 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.22uF"
			(at -0.266583 -1.558417 0)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "Net-(C54-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 135 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "B.Cu")
		(at 118.841583 108.845917 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R62"
			(at 3.81 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1"
			(at 0 -1.82 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0 90)
			(size 1.25 1.75)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.2)
			(net 141 "Net-(R62-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4 0 90)
			(size 1.25 1.75)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.2)
			(net 3 "Net-(C19-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 105.875 112.9375 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R65"
			(at -3.3765 0.1165 -90)
			(layer "B.SilkS")
		)
		(property "Value" "1.5k"
			(at 0 -1.65 -90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C19-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(D19-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 108.8 83.1 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "1M"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pcdu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 107 "/Semi_Regulated_Bus")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 121 "S2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 172.78 136.1851)
		(mid 172.501025 136.858625)
		(end 171.8275 137.1376)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 117.7255 41.2526)
		(mid 118.399038 41.531573)
		(end 118.678 42.2051)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 83.5625 79.0478)
		(mid 84.236019 79.326781)
		(end 84.515 80.0003)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 138.0455 135.2326)
		(mid 138.719038 135.511573)
		(end 138.998 136.1851)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 171.8275 99.3424)
		(mid 172.501038 99.621373)
		(end 172.78 100.2949)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 84.515 80.0003)
		(end 84.515 98.3899)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.61 42.2051)
		(end 82.61 78.0953)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 171.8275 99.3424)
		(mid 171.154 99.063411)
		(end 170.875 98.3899)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.875 80.0003)
		(end 170.875 98.3899)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 138.998 42.2051)
		(mid 139.276986 41.531586)
		(end 139.9505 41.2526)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 83.5625 137.1376)
		(mid 82.888981 136.858619)
		(end 82.61 136.1851)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.78 42.2051)
		(end 172.78 78.0953)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 83.5625 137.1376)
		(end 117.7255 137.1376)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.9505 41.2526)
		(end 171.8275 41.2526)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 171.8275 41.2526)
		(mid 172.501038 41.531573)
		(end 172.78 42.2051)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.61 100.2949)
		(end 82.61 136.1851)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 83.5625 79.0478)
		(mid 82.888981 78.768819)
		(end 82.61 78.0953)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 170.875 80.0003)
		(mid 171.153986 79.326786)
		(end 171.8275 79.0478)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 139.9505 137.1376)
		(mid 139.277 136.858611)
		(end 138.998 136.1851)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 82.61 100.2949)
		(mid 82.888981 99.621381)
		(end 83.5625 99.3424)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 84.515 98.3899)
		(mid 84.236019 99.063419)
		(end 83.5625 99.3424)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 118.678 136.1851)
		(mid 118.956986 135.511586)
		(end 119.6305 135.2326)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 118.678 136.1851)
		(mid 118.399025 136.858625)
		(end 117.7255 137.1376)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119.6305 135.2326)
		(end 138.0455 135.2326)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 119.6305 43.1576)
		(mid 118.957 42.878611)
		(end 118.678 42.2051)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119.6305 43.1576)
		(end 138.0455 43.1576)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.78 100.2949)
		(end 172.78 136.1851)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 83.5625 41.2526)
		(end 117.7255 41.2526)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 172.78 78.0953)
		(mid 172.501025 78.768825)
		(end 171.8275 79.0478)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 138.998 42.2051)
		(mid 138.719025 42.878625)
		(end 138.0455 43.1576)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 82.61 42.2051)
		(mid 82.888981 41.531581)
		(end 83.5625 41.2526)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.9505 137.1376)
		(end 171.8275 137.1376)
		(layer "Edge.Cuts")
	)
	(gr_text "Battery\nCharger"
		(at 100.6 113.125 0)
		(layer "B.SilkS")
	)
	(gr_text "Solar Array Regulator"
		(at 145.65 117.675 0)
		(layer "B.SilkS")
	)
	(gr_text "System\nPower Switch"
		(at 108.175 79.815 270)
		(layer "B.SilkS")
	)
	(gr_text "Main Bus Power Regulator"
		(at 142.325 91.15 0)
		(layer "B.SilkS")
	)
	(gr_text "-     +"
		(at 103.006 131.418 0)
		(layer "F.SilkS")
	)
	(gr_text "-     +"
		(at 96.106 131.418 0)
		(layer "F.SilkS")
	)
	(gr_text "-     +"
		(at 110.006 131.418 0)
		(layer "F.SilkS")
	)
	(gr_text "-     +"
		(at 117.106 131.418 0)
		(layer "F.SilkS")
	)
	(gr_text "-     +"
		(at 124.006 131.418 0)
		(layer "F.SilkS")
	)
	(gr_text "Remote/Platform/Power/PCDU\nLC2201 Version 1.0.0"
		(at 151.8 129.9 0)
		(layer "F.SilkS")
	)
	(gr_text "-     +"
		(at 131.006 131.418 0)
		(layer "F.SilkS")
	)
	(zone
		(net 135)
		(net_name "GND")
		(locked yes)
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 81.845 33.0774) (xy 174.555 33.0774) (xy 174.555 137.9424) (xy 81.845 137.9424)
			)
		)
	)
	(zone
		(net 135)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
		)
		(polygon
			(pts
				(xy 146.375 80.725) (xy 146.375 83.725) (xy 147.975 83.725) (xy 147.975 80.725)
			)
		)
	)
	(zone
		(net 135)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 155.575 72.725) (xy 155.575 76.125) (xy 149.575 76.125) (xy 149.575 74.925) (xy 144.775 74.925)
				(xy 144.775 78.325) (xy 161.375 78.325) (xy 161.375 72.725)
			)
		)
	)
	(zone
		(net 135)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
		)
		(polygon
			(pts
				(xy 127.775 78.925) (xy 127.775 83.325) (xy 129.575 83.325) (xy 129.575 78.925)
			)
		)
	)
	(zone
		(net 135)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
		)
		(polygon
			(pts
				(xy 137.175 72.525) (xy 137.175 76.725) (xy 130.975 76.725) (xy 130.975 74.725) (xy 126.375 74.725)
				(xy 126.375 77.925) (xy 142.975 77.925) (xy 142.975 72.525)
			)
		)
	)
	(zone
		(net 81)
		(net_name "Net-(L3-Pad1)")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
		)
		(polygon
			(pts
				(xy 130.175 78.525) (xy 130.175 81.325) (xy 131.575 81.325) (xy 131.575 83.725) (xy 142.975 83.725)
				(xy 142.975 78.525)
			)
		)
	)
	(zone
		(net 80)
		(net_name "Net-(L2-Pad1)")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
		)
		(polygon
			(pts
				(xy 148.575 78.925) (xy 148.575 81.725) (xy 149.975 81.725) (xy 149.975 83.525) (xy 161.375 83.525)
				(xy 161.375 78.925)
			)
		)
	)
	(zone
		(net 106)
		(net_name "Net-(C32-Pad1)")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 129.375 84.525) (xy 129.375 89.725) (xy 161.375 89.725) (xy 161.375 84.525)
			)
		)
	)
	(zone
		(net 135)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 127.3 105.0625) (xy 127.3 109.4625) (xy 129.1 109.4625) (xy 129.1 105.0625)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(C19-Pad1)")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
		)
		(polygon
			(pts
				(xy 128.1 97.4625) (xy 128.1 100.4625) (xy 132.1 100.4625) (xy 132.1 101.8625) (xy 136.1 101.8625)
				(xy 136.1 97.4625)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(C19-Pad1)")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 146.9 97.6625) (xy 146.9 100.3545) (xy 149.5 100.3545) (xy 149.5 101.8625) (xy 154.5 101.8625)
				(xy 154.5 97.6625)
			)
		)
	)
	(zone
		(net 135)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
		)
		(polygon
			(pts
				(xy 136.7 98.8625) (xy 136.7 103.0625) (xy 130.5 103.0625) (xy 130.5 101.0625) (xy 125.9 101.0625)
				(xy 125.9 104.4625) (xy 142.5 104.4625) (xy 142.5 98.8625)
			)
		)
	)
	(zone
		(net 135)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 155.1 98.8625) (xy 155.1 102.4625) (xy 148.9 102.4625) (xy 148.9 101.3545) (xy 144.3 101.3545)
				(xy 144.3 104.4625) (xy 160.9 104.4625) (xy 160.9 98.8625)
			)
		)
	)
	(zone
		(net 82)
		(net_name "Net-(L4-Pad1)")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 129.72 105.1045) (xy 129.72 107.9045) (xy 130.9 107.8625) (xy 130.9 109.6625) (xy 142.3 109.6625)
				(xy 142.3 105.0625)
			)
		)
	)
	(zone
		(net 135)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
		)
		(polygon
			(pts
				(xy 146.1 106.8625) (xy 146.1 109.6625) (xy 147.7 109.6625) (xy 147.7 106.8625)
			)
		)
	)
	(zone
		(net 110)
		(net_name "CHARGE")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 128.9 110.2625) (xy 128.9 115.4625) (xy 160.9 115.4625) (xy 160.9 110.2625)
			)
		)
	)
	(zone
		(net 135)
		(net_name "GND")
		(locked yes)
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 81.765 40.3024) (xy 174.475 40.3024) (xy 174.475 145.4674) (xy 81.765 145.4674)
			)
		)
	)
	(zone
		(net 79)
		(net_name "Net-(L1-Pad1)")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 148.075 104.9875) (xy 148.075 107.7875) (xy 149.255 107.7455) (xy 149.255 109.5455) (xy 160.655 109.5455)
				(xy 160.655 104.9455)
			)
		)
	)
)
