VERSION:554370312

11,III,WLAN_BWA_UPDATE_VDEV_BW: phy_mode=%d, opmode=%d, Requested operating voltage corner=0x%x 
10,II,Static LP voltage corner = %d for phymode %d = %d 
9,II,WLAN_BWA_GET_VDEV_BW: vdev_id=%d, vdev_bw=%d [>=BW_CNT returned] 
8,IIII,WLAN_BWA_GET_VDEV_BW: vdev_id=%d, vdev_bw=%d, ACTIVE=%d, PAUSED=%d 
7,II,Static operating voltage corner = %d for phymode = %d 
6,II,WLAN_BWA_SET_PMAC_BW: mac_id=%d, pmac_bw=%d 
5,II,WLAN_BWA_SET_PMAC_BW: mac_id=%d, pmac_bw=%d [!WAL_EOK returned] 
4,II,WLAN_BWA_UPDATE_PMAC_BW: mac_id=%d, final_bw=%d 
3,II,WLAN_BWA_UPDATE_VDEV_BW: vdev_id=%d, pmac_id=%d 
2,I,WLAN_BWA_VDEV_FREE: vdev_id=%d 
1,I,WLAN_BWA_VDEV_INIT: vdev_id=%d 
14,I,Chainmask_Proxy_CHM_NOTIF: event_type = 0x%x 
13,IIII,Chainmask_Proxy_Set_Antenna_Mode:  mac_id_map = 0x%x, mac_id = %d, num_tx_chains = %d, num_rx_chains = %d 
12,IIII,Chainmask_Proxy_Set_Chainmask: band_map = 0x%x, mac_id_map = 0x%x, chainmask = %d, Tx_Rx = %d (Tx = 0, Rx = 1) 
15,II,SWBMISS_VDEV_EVT: vdev_id=%d, notif=%d 
16,IIII,SWBMISS_DELIVER_EVT: vdev_id=%d, evt_type=0x%x, bcn_rssi_avg=%d, bcn_rssi_last=%d 
17,IIIIII,SWBMISS_TIMER_FN: vdev_id=%d, curr_bmiss_bcnt=%d, pre_bmiss_detected=%d, first_bmiss_detected=%d, final_bmiss_detected=%d, b_timeout=%d 
18,IIII,SWBMISS_NULL_SEND_CMPLT: first_bmiss_bcnt = %d, final_bmiss_bcnt = %d default_prebmiss_count = %d, vbmiss_connected = %d 
19,IIIIII,SWBMISS_NULL_SEND_CMPLT: vdev_id=%d, isQosNullSuccess=%d isFinalBmiss=%d first_bmiss_detected=%d final_bmiss_detected=%d fbmiss_evnt_posted=%d 
20,II,SWBMISS_TIMER_SET: vdev_id=%d, timeout_val=%d 
21,II,SWBMISS_BCON_RECVED: vdev_id=%d, IS_HWBMISS=%d 
22,IIIIII,SWBMISS_DISABLED: vdev_id=%d, module_id=%d, bmiss_disable_bitmap_63_32=0x%x, bmiss_disable_bitmap_31_0=0x%x, curr_bmiss_bcnt=%d, cur_disable_bitmask=0x%x 
23,IIIIII,SWBMISS_ENABLED: vdev_id=%d, module_id=%d, bmiss_disable_bitmap_63_32=0x%x, bmiss_disable_bitmap_31_0=0x%x, curr_bmiss_bcnt=%d, final_bmiss_detected=%d 
24,I,SWBMISS_RESYNC_ALL_VDEV: mac_id=%d 
25,I,SWBMISS_SWITCH_2_HWBMISS: vdev_id=%d 
30,I,HWBMISS_DISABLED: vdev_id=%d 
29,IIIIII,HWBMISS_ENABLED: vdev_id=%d, pre_bmiss_detected=%d, first_bmiss_detected=%d, final_bmiss_detected=%d, curr_bmiss_bcnt=%d, curr_listen_interval=%d 
28,,HWBMISS_ENABLED: [final_bmiss_detected=1] 
27,II,HWBMISS_SWITCH_2_SWBMISS: vdev_id=%d, hwbmiss_bcnt=%u 
26,II,HWBMISS_EVENT_HANDLER: vdev_id=%d, event_type=0x%x 
31,I,WMI_PDEV_SET_MAC_CONFIG_RESP_EVENT: status=0x%x 
32,,WMI_PDEV_SET_MAC_CONFIG_RESP_EVENT: WMI Event Alloc Failed!!! 
33,I,wlan_pdev_set_hw_mode: DBSMGR_Ret_Status = 0x%x 
34,I,wlan_pdev_set_hw_mode: HW_Mode_Idx = 0x%x 
35,I,wlan_pdev_set_pcl: num_chans=%d 
36,III,wlan_pdev_set_pcl: cur_category %d: num_chans_in_category %d -> cur_idx %d 
37,II,wlan_pdev_set_pcl not match pcl_cnt=%d,supp_chan_cnt=%d 
38,IIIIIII,HCC Recv WMI_GET_TPC_POWER_CMDID in FW: %d, %d, %d, %d, %d, %d,0x%x  
39,I,wlan_pdev_resume_cmd: NOT expected to receive during wifi on, mac id=%d 
40,,wlan_pdev_resume_cmd: NOT expected to receive during wifi on 
41,,wlan_pdev_set_param: Param WMI_PDEV_GREEN_AP_PS_ENABLE_CMDID is not handled 
42,,WMI_PDEV_SET_WMM_PARAMS_CMDID DEPRECATED - use VDEV level command instead 
43,I,HCC dispatch_wlan_pdev_cmds: cmd_id:0x%x 
44,III,wlan_pdev_get_hw_mode_transition_event: old_hw_idx=0x%x, new_hw_idx=0x%x, vdev_num=%d 
45,I,wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_RX_CHAIN_MASK_5G, value=0x%x 
46,I,wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_TX_CHAIN_MASK_5G, value=0x%x 
47,I,wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_RX_CHAIN_MASK_2G, value=0x%x 
48,I,wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_TX_CHAIN_MASK_2G, value=0x%x 
49,I,wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_RX_CHAIN_MASK, value=0x%x 
50,I,wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_TX_CHAIN_MASK, value=0x%x 
51,II,wlan_dev_unit_test: cmd = WAL_PDEV_PARAM_PN_SHIFT_FACTOR, mac_id = %d, value = %d 
52,,wlan_dev_unit_test: wal_pdev is NULL 
53,I,wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_ABG_MODE_TX_CHAIN_NUM, value = 0x%x 
54,I,unit_test: sleep for %d ms 
55,II,wlan_dev_unit_test: cmd = PDEV_SET_HW_MODE, hw_mode = %d, ret_status = %d 
56,II,wlan_pdev_set_hw_mode_resp_event: status=0x%x, cfg_hw_mode_idx=0x%x 
57,,wlan_pdev_set_hw_mode_resp_event: WMI Event Alloc Failed!!! 
58,III,HCC Send EVENT: WMI_GET_TPC_POWER_EVENTID:0x%x, pwr: %d, len:%d 
59,I,wlan_get_chip_power_stats: stats_capture->num_debug_register 0x%x 
60,I,PDEV_PARAM_IOT_PATTERN=%08x 
61,I,wlan_pdev_set_param: WMI_PDEV_PARAM_RX_CHAIN_MASK_5G 0x%x 
62,I,wlan_pdev_set_param: WMI_PDEV_PARAM_TX_CHAIN_MASK_5G 0x%x 
63,I,wlan_pdev_set_param: WMI_PDEV_PARAM_RX_CHAIN_MASK_2G 0x%x 
64,I,wlan_pdev_set_param: WMI_PDEV_PARAM_TX_CHAIN_MASK_2G 0x%x 
65,I,wlan_pdev_set_param: Param WMI_PDEV_PARAM_RX_CHAIN_MASK 0x%x 
66,I,wlan_pdev_set_param: Param WMI_PDEV_PARAM_TX_CHAIN_MASK 0x%x 
67,II,WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                        curr_data_index (%d) > next_data_index %d 
68,,WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                   oui_cmd_buff_length validation failed 
69,II,WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                   num_of_oui_read %d and index of buf_data %d should be equal 
70,II,WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                     total_num_of_configured_oui (%d) < %d 
71,II,WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                    num_vendor_oui_ext (%d) > %d 
72,II,WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                    total_num_configured_element (%d) > %d 
73,II,WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                   total_length (%d) > %d 
74,II,WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                   capability length (%d) > %d 
75,II,WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                   mac address length (%d) > %d 
76,II,WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                   data length (%d) > %d 
77,II,WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                   header length (%d) > %d 
78,II,wlan_resync_imps: IMPS_ENABLED=%d, VDEV_UP_COUNT=%d 
79,I,wlan_dev_init: ant_sharing_enabled = %d 
80,IIIIIIII,WMI_PEER_PARAM_DISABLE_AGGRESSIVE_TX:peer %x value %x mac_address %x:%x:%x:%x:%x:%x 
81,I,wlan_vdev_change_minimum_allowed_mcs: minimum_allowed_mcs 0x=%x 
82,I,wlan_vdev_peer_change_phymode_internal: phymode = %x 
83,I,wlan_vdev_peer_autorate_reset: user_start_rate 0x=%x 
84,I,wlan_vdev_peer_mimo_ps_internal: valid_tx_chainmask 0x=%x 
85,I,wlan_vdev_peer_change_bw_internal: new_bw = %x 
86,II,VDEV EVT:WMI_PEER_DELETE_RESP_EVENTID send vdevId=%d time=%d 
87,II,RESOURCE_PEER_ALLOC curr_tsf_63_32=0x%x,curr_tsf_31_0=0x%x 
88,IIII,RESOURCE_PEER_ALLOC del_req_tsf_63_32=0x%x,del_req_tsf_31_0=0x%x,del_conf_tsf_63_32=0x%x,del_conf_tsf_31_0=0x%x 
89,IIII,RESOURCE_PEER_ALLOC create_by=%d,delete_by=%d,create_tsf_63_32=0x%x,create_tsf_31_0=0x%x 
90,II,RESOURCE_PEER_ALLOC  error peer_type = %d, delete_in_process:%d 
91,IIII,RESOURCE_PEER_ALLOC error vdev_id = %d mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x usage_count = %d 
92,II,update non data2, peer:0x%x, rc:0x%x 
93,III,wlan_vdev_dispatch_peer_change_bw:prev_ni_flags=%x new_ni_flags=%x new_bw = %x 
94,IIIII,PEER_ASSOC ni_legacy_rate_set= 0x%x ht_caps=0x%x vht_caps=0x%x vht_mcs_set=0x%x ht_mcs_set= 0x%x 
95,IIIII,PEER_ASSOC ni_flags=0x%x phymode=0x%x nss=0x%x mpdudensity=%d max_mpdu=%d 
96,IIIIIII,PEER_ASSOC cmd for %x:%x:%x:%x:%x:%x, num_peer_ht_rates=%d 
97,,PEER_ASSOC null peer 
98,,peer not exist. still generating PEER_DELETE_RESP_EVENTID 
99,IIIIIII,peer delete command for vdev_id %d ****%02x:%02x:%02x:%02x:%02x:%02x****
 
100,IIIIII,peer create command for ****%02x:%02x:%02x:%02x:%02x:%02x****
 
101,IIIIII,ROAM_VDEV_UPDATE_BSS_PEER error no peer for ****%02x:%02x:%02x:%02x:%02x:%02x**** 
102,IIIIIIII,ROAM_VDEV_UPDATE_BSS_PEER by find_peer_pdev for ****%02x:%02x:%02x:%02x:%02x:%02x* mac_id %d %d*** 
103,IIIIIII,ROAM_VDEV_UPDATE_BSS_PEER by find_peer for ****%02x:%02x:%02x:%02x:%02x:%02x* mac_id %d *** 
104,IIIIII,peer_update status=%d,vdevid=%d,macaddr=0x%8x0x%4x peer_type=%d,req_peer_type=%d
 
105,III,Nr=%x Nc=%x peer_nss=%x 
106,II,Nr=%x Ntx=%x 
107,I,Nc=%x
 
108,II,Nr=%x Nrx=%x 
109,I,wlan_set_peer_txbfcap vht_caps=%x 
110,III,RESOURCE_PEER_NBRHOOD_MGMT_INFO  nbrhood_peers_ctxt/mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x num_valid_peers = %d 
111,II,RESOURCE_PEER_NBRHOOD_MGMT_INFO  nbrhood_peers_ctxt/mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x 
112,I,wlan_peer_send_peer_info_event num_valid_peers=%d 
113,II,wlan_peer_send_peer_info_event j=%d, peer=%p 
114,II,wlan_peer_send_peer_info_event bss_peer=%p, self_peer=%p 
115,I,RESOURCE_PEER_NBRHOOD_MGMT_INFO  nbrhood_peers_ctxt/mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x 
116,I,RESOURCE_PEER_NBRHOOD_MGMT_ALLOC  nbrhood_peers_ctxt = 0x%x 
117,II,RESOURCE_PEER_NBRHOOD_MGMT_ALLOC  nbrhood_peers_ctxt = 0x%x var2 = %d 
118,II,VDEV EVT PEER: wlan_free_peer del_resp=%d, wal_peer:0x%x 
119,IIII,VDEV EVT:RESOURCE_PEER_FREE vdev_id = %d mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x usage_count = %d 
120,IIIII,wal peer allocaton status = %d vdev_id_8/mac_id_8 = 0x%x mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x peer_type = %d 
120,IIIII,wal peer allocaton status = %d vdev_id_8/mac_id_8 = 0x%x mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x peer_type = %d 
121,IIIIII,RESOURCE_PEER_ALLOC duplicate PEER_TYPE_BSS vdev_id = %d mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x mac_id = %d/%d peer=0x%x 
122,,MAWC_UNREGISTER_NOTIFY_FAIL entry not found 
123,,MAWC_REGISTER_NOTIFY_FAIL alloc failed 
124,,MAWC_REGISTER_NOTIFY_FAIL already registered 
125,,MAWC_REGISTER_NOTIFY_FAIL pool is not initialized 
126,I,MAWC_ENABLE_SENSOR enable = %d (0 = disable, 1 = enable) 
127,,MAWC_ALLOC_EVENT_FAIL no buffer 
128,I,MAWC_SENSOR_ERROR error = %d 
129,II,MAWC_MOTION_STATE_UPDATE cur_motion_state = %d new_motion_state = %d (0:unknown,1:stationary,2:walk,3:transit) 
130,II,[MAWC] WMI_MAWC_SENSOR_REPORT_IND_CMDID motion_state = %d(0:Unknown,1:Stationary,2:Walk,3:Transit), status = %d 
131,,MAWC] dispatch_cmds() MAWC context or buffer is NULL 
132,IIII,MAWC_UNIT_TEST_GEN_SENSOR_REPORT vdev_id = %d motion_state = %d sensor_status = %d num_args = %d 
133,I,LOCAL MGMT DEAUTH-DISASSOC tx compl. status 0x%x 
134,,IEEE80211_FC0_SUBTYPE_NDPA 
135,III,mac id mismatch:rx:%x vdev:%x, frame: %x
 
135,III,mac id mismatch:rx:%x vdev:%x, frame: %x
 
136,IIIII,MGMT_TXRX_FORWARD_TO_HOST: not mgmt pkt, Ch_VdevActCnt_ToHost=0x%08x Type_Subtype=0x%04x Seq=%d(0x%x) RssiComb_Chain0_1_MacId=0x%08x 
137,IIIIIII,MGMT_TXRX_FORWARD_TO_HOST: mgmt pkt, Ch_VdevActCnt_ToHost=0x%08x Type_Subtype=0x%04x Seq=%04d(0x%03x) Addr2=0x%04x 0x%08x RssiComb_Chain0_1_MacId=0x%08x 
138,III,_wlan_mgmt_local_send_nullfunc() get nullfunc failed: peer = %p peer_type = %d cb_flags: 0x%x 
139,IIIIII,MGMT_TXRX_SENT_FROM_LOCAL: macidh8/tid8/ptype16:0x%08x, cbflags=0x%08x, peerflag=0x%x,addr=0x%08x 0x%04x cur_chan=%d 
140,II,MGMT_TX_WMI_FROM_HOST register %d %d 
140,II,MGMT_TX_WMI_FROM_HOST register %d %d 
141,III,WMI TX comp hold,idx:%d, desc id=%d,comp=%d 
142,II,MGMT_TX_WMI_FROM_HOST_COMP desc_id=0x%x tx_status=0x%x 
143,,MGMT_TX_WMI_TXCOMP_SEND_EVT PKT NULL 
142,II,MGMT_TX_WMI_FROM_HOST_COMP desc_id=0x%x tx_status=0x%x 
144,,OFFCHAN_DATA_TX_WMI_TXCOMP_SEND_EVT PKT NULL 
145,III,WMI TX comp send bundle, num:%d, desc id=%d comp=%d 
146,I,WMI TX comp send bundle: bundle_evt_size:0x%x 
147,II,MGMT_TX_WMI_FROM_HOST: tx_param_valid=%d ppdu_info=0x%x 
148,IIII,MGMT_TX_WMI_FROM_HOST is_home_8/is_curr_8=0x%x mode_8/submode_8=0x%x pmac->mac_id=%d e_mac_id=%d 
149,II,MGMT_TX_WMI_FROM_HOST: check tag =%d, tx_params_valid:%x 
150,IIII,MGMT_TX_WMI_FROM_HOST subtype=0x%02x addr=0x%04x%08x chanfreq=0x%x 
151,IIII,MGMT_TX_WMI_FROM_HOST: dword0=0x%x dword1=0x%x, subtype:%x, ppdu_info:0x%x 
152,I,WMI_SEND_EVENT_WRONG_TLV CmdId/EventId = 0x%x 
152,I,WMI_SEND_EVENT_WRONG_TLV CmdId/EventId = 0x%x 
153,III,_wlan_mgmt_rx_frame_handler Droping frame from non associated Peer type=0x%x subtype=0x%x bNull=%d 
154,II,OFLD wmi evt flush evt_id=%d, evt_len=%d 
155,,ofld wmi evt store failure - no memory 
156,II,OFLD wmi evt store evt_id=%d, evt_len=%d 
157,I,evt store:%x 
158,II,OFLD pend wmi evt, id=%d, len:%d 
159,II,OFLD drop wmi evt, id=%d, len:%d 
160,II,offldmgr_non_data_handler: status = 0x%x frametype = 0x%x 
161,IIII,_offldmgr_non_data_handler: status= 0x%x, sub_status = 0x%x offld_id 0x%x frametype = 0x%x 
162,III,_offldmgr_non_data_handler: peer = 0x%x addr1 0x%x addr2 = 0x%x 
163,II,OFLD proto data hdlr ret_Status=%d curr_wow=%d 
164,III,OFLD enhanced data hdlr ofld id=%d status=%d, wow data state:%d 
165,IIII,OFLD remote data hdlr pktlen=%d, dataT=%d addrT=%d vdevId=%d 
166,II,OFLD remote data hdlr nonds, id:%x, mode:%x 
167,II,OFLD remote data hdlr ds2ds, id:%x, mode:%x 
168,,drop data in wow awake 
169,IIII,OFLD status hdlr ofld id=%d status=%d, route_type=%d, status_buf_flags:0x%x 
170,IIII,OFLD status hdlr pktlen=%d, dataT=%d addrT=%d vdevId=%d 
171,,OFLD status hdlr: unable to handle this in status buf! HIF CPY 
172,I,OFLD status hdlr invalid eth type,l2 present:%x 
173,II,OFLD status hdlr nonds, id:%x, mode:%x 
174,II,OFLD status hdlr ds2ds, id:%x, mode:%x 
175,III,OFLD data parse rx_mode:%d, L3 offset=%d, L2 ethType=%x 
176,IIIIII,OFLD data parse DA %x %x %x %x %x %x 
177,I,Unknown RX Decap mode %d 
178,II,OFLD dereg htt name=%d ref_cnt=%d 
179,II,OFLD dereg wmi name=%d ref_cnt=%d 
180,III,OFLD dereg data name=%d vdev id=%d, vdev mask 
181,II,OFLD dereg nondata name=%d ref_cnt=%d 
182,II,OFLD reg HTT name=0x%x, refcnt:0x%x 
183,II,OFLD reg wmi name=0x%x, refcnt:0x%x 
184,II,OFLD reg data vdev id=%d, max_len =%d 
185,III,OFLD reg data name=0x%x, vdevid:0x%x, vdev_bitmap:0x%x 
186,II,OFLD reg nondata name=0x%x, refcnt:0x%x 
198,III,CHAN_MGR_PAUSE_COMPLETE: curr_chan = %d link = 0x%x link_flgs = 0x%x 
197,,chan mgr pause complete timeout 
196,II,CHAN_MANAGER_SM_EVENT: %d < %d
 
195,III,CHAN_MANAGER_SM_EVENT_DATA: chan = 0x%x sec_chan = 0x%x sw_time = 0x%x 
194,II,CHAN_MGR_CTS2S_TX_COMP: status = 0x%x ch_handle = 0x%x 
193,II,CHAN_MGR_PAUSE_CMPL_CB: status = 0x%x curr_time = 0x%x 
192,IIIII,CHAN_MGR_VDEV_PAUSE: chan = %d link = 0x%x flg = 0x%x max_sw_time = %d curr_time = 0x%x 
191,IIIIII,CHAN_MGR_TRIGGER_CHANNEL_CHANGE: pri_ch = %d, chan_change_dur = %d,is_chm_valid = 0x%x tx_chm = 0x%x, rx_chm = 0x%x, selfgen_chm = 0x%x 
190,IIIIII,CHAN_MGR_TRIGGER_CHANNEL_CHANGE: sec_ch = %d, chan_change_dur = %d,is_chm_valid = 0x%x tx_chm = 0x%x, rx_chm = 0x%x, selfgen_chm = 0x%x 
189,IIIII,CHAN_MGR_TRIGGER_HW_MODE_CHANGE: Cur_HW_Mode = %d, Next_HW_Mode = %d,pri_ch = %d, sec_ch = %d, HW_Mode_Switch_Dur = %d 
188,IIII,RESMGR_DELIVER_EVT: type = 0x%x, old_hw_mode = 0x%x, new_hw_mode = 0x%x, band_to_mac = 0x%x 
187,III,CHAN_MGR_VDEV_UNPAUSE:chan =%d link =0x%x curr_time = 0x%x 
199,III,RESMGR_CHMGR_SEND_CTS2SELF: cur_vc = 0x%x link = 0x%x status = 0x%x 
195,III,CHAN_MANAGER_SM_EVENT_DATA: chan = 0x%x sec_chan = 0x%x sw_time = 0x%x 
196,II,CHAN_MANAGER_SM_EVENT: %d < %d
 
200,II,CHAN_MANAGER_SM: %d => %d 
201,II,RESMGR_DEREG_EVT_HDLR:  handler = 0x%x arg = 0x%x deregistered 
202,II,RESMGR_DEREG_EVT_HDLR:  handler = 0x%x arg = 0x%x not found!!! 
203,II,RESMGR_REG_EVT_HDLR:  handler = 0x%x arg = 0x%x registered 
204,II,RESMGR_REG_EVT_HDLR: handler = 0x%x arg = 0x%x no memory!!! 
205,II,RESMGR_REG_EVT_HDLR:  handler = 0x%x arg = 0x%x exists!!! 
206,III,RESMGR_OCS_REQ_QUOTA_STATS  arg = 0x%x chan_mhz = 0x%x req_chan_time/latency = 0x%x 
206,III,RESMGR_OCS_REQ_QUOTA_STATS  arg = 0x%x chan_mhz = 0x%x req_chan_time/latency = 0x%x 
206,III,RESMGR_OCS_REQ_QUOTA_STATS  arg = 0x%x chan_mhz = 0x%x req_chan_time/latency = 0x%x 
210,I,RESMGR_OCS_ALLOCRAM_SIZE  size_in_bytes = %d 
209,I,OCM_Migrate: migrate_mode = 0x%x 
208,II,OCM_Resume: ocs_cfg = 0x%x, Pause_OCS = 0x%x 
207,II,OCM_Suspend: Pause_Pending = 0x%x, Pause_OCS = 0x%x 
217,IIII,RESMGR_DYN_SCH_CH_SX_STATS  chan_mhz = %d accu_tx_rx_dur_us = 0x%x accu_free_dur_us = 0x%x accu_sampling_dur_us = 0x%x 
218,IIII,RESMGR_DYN_SCH_HOME_CH_QUOTA  chan0_mhz = %d ch0_new_quota = %d chan1_mhz = %d ch1_new_quota = %d 
217,IIII,RESMGR_DYN_SCH_CH_SX_STATS  chan_mhz = %d accu_tx_rx_dur_us = 0x%x accu_free_dur_us = 0x%x accu_sampling_dur_us = 0x%x 
216,IIII,RESMGR_DYN_SCH_TOT_UTIL_PER  chan0_mhz = %d chan0_util_percentage = %d chan1_mhz = %d chan1_util_percentage = %d 
215,IIIII,RESMGR_DYN_SCH_CH_STATS_END  chan_mhz = %d rx_clear_cnt = %d tx_frame_cnt = %d rx_frame_cnt_us = %d sampling_dur_us = %d 
214,IIIII,RESMGR_DYN_SCH_CH_STATS_START  chan_mhz = %d start_rx_clear_cnt = %d start_tx_frame_cnt = %d start_rx_frame_cnt_us = %d start_time_us = %d 
213,I,RESMGR_DYN_SCH_ALLOCRAM_SIZE  size = %d 
212,II,RESMGR_DYN_SCH_ENABLE  enable = 0x%x fw_disable_bmap = 0x%x 
211,I,RESMGR_DYN_SCH_ACTIVE  is_active = %d 
270,IIIII,RESMGR_OCS_CHREQ_CREATE: req_id = 0x%x chan_req_addr = 0x%x chan_mhz = %d, sec_chan_mhz = %d prioirty = %d  
269,IIIIII,RESMGR_OCS_CHREQ_CREATE: start_tsf = 0x%x duration_usec = %d interval = %d dtim_start_tsf = 0x%x dtim_period = %d end_tsf = 0x%x 
268,IIIII,RESMGR_OCS_CHREQ_DELETE: req_id = 0x%x chan_req_addr = 0x%x chan_mhz = %d sec_chan_mhz = %d state = %d 
267,IIIIII,RESMGR_OCS_CHREQ_START: req_id = 0x%x chan_req_addr = 0x%x chan_mhz = %d sec_chan_mhz = %d band_center_freq2 = %d prioirty = %d  
266,IIIIII,RESMGR_OCS_CHREQ_START: start_tsf = 0x%x duration_usec = %d interval = %d dtim_start_tsf = 0x%x dtim_period=%d end_tsf = 0x%x 
265,IIIII,RESMGR_OCS_CHREQ_STOP: req_id = 0x%x chan_req_addr = 0x%x chan_mhz = %d sec_chan_mhz = %d state = %d 
264,I,RESMGR_OCS_CHREQ_UPDATE: start_tsf/req_id = 0x%x 
263,IIIII,RESMGR_OCS_CHREQ_UPDATE: req_id = 0x%x chan_req_addr = 0x%x chan_mhz = %d sec_chan_mhz = %d prioirty = %d  
262,IIIIII,RESMGR_OCS_CHREQ_UPDATE: start_tsf = 0x%x duration_usec = 0x%x interval = %d dtim_start_tsf = 0x%x dtim_period=%d end_tsf = 0x%x 
210,I,RESMGR_OCS_ALLOCRAM_SIZE  size_in_bytes = %d 
261,I,RESMGR_OCS_WIN_CAT_DUR  duration = %d 
260,IIIII,RESMGR_OCS_CHREQ_UPDATE  start_tsf = 0x%x duration_usec = 0x%x interval=%d prioirty = 0x%x chan_req_addr = 0x%x 
259,IIII,RESMGR_OCS_CHREQ_RESTART  start_tsf = 0x%x stop_tsf = 0x%x dtim_start_tsf = 0x%x dtim_period = %d 
258,IIIII,RESMGR_OCS_CHREQ_UPDATE req_id = 0x%x dtim_start_tsf = 0x%x dtim_period=%d purge_flag = 0x%x end_tsf = 0x%x 
257,II,RESMGR_OCS_CHREQ_UPDATE chan_mhz = %d sec_chan_mhz = %d 
256,,RESMGR_OCS_CH_SWITCH_REQ 
255,II,RESMGR_OCS_LATENCY_STRICT_TIME_SLOT  slot1_start_tsf = 0x%x slot2_start_tsf = 0x%x 
252,I,RESMGR_OCS_LATENCY_CASE_NO  arg = 0x%x 
254,I,RESMGR_OCS_CURR_TSF  current_tsf = 0x%x 
253,II,RESMGR_OCS_QUOTA_REM  cat1_quota_remain = 0x%x cat2_quota_remain = 0x%x 
252,I,RESMGR_OCS_LATENCY_CASE_NO  arg = 0x%x 
252,I,RESMGR_OCS_LATENCY_CASE_NO  arg = 0x%x 
252,I,RESMGR_OCS_LATENCY_CASE_NO  arg = 0x%x 
252,I,RESMGR_OCS_LATENCY_CASE_NO  arg = 0x%x 
252,I,RESMGR_OCS_LATENCY_CASE_NO  arg = 0x%x 
252,I,RESMGR_OCS_LATENCY_CASE_NO  arg = 0x%x 
252,I,RESMGR_OCS_LATENCY_CASE_NO  arg = 0x%x 
251,I,RESMGR_OCS_CLEANUP_CH_ALLOCATORS  cur_ch_alloc_addr = 0x%x 
250,I,RESMGR_OCS_CH_ALLOCATOR_FREE  cur_ch_alloc_addr = 0x%x 
249,I,RESMGR_OCS_CLEANUP_STALE_REQS  cur_ch_alloc_addr = 0x%x 
242,II,RESMGR_OCS_CHREQ_COMPLETE  curr_time = 0x%x ch_req_addr = 0x%x 
242,II,RESMGR_OCS_CHREQ_COMPLETE  curr_time = 0x%x ch_req_addr = 0x%x 
248,III,RESMGR_OCS_CONSTRUCT_CAT_WIN  chan_alloc_addr=0x%x chan_mhz=%d sec_ch_mhz=%d 
247,II,RESMGR_OCS_NEW_CAT_WINDOW_REQ  ch_req_addr = 0x%x state = %d 
246,II,RESMGR_OCS_NEW_CAT_WINDOW_TIMESLOT  start_tsf = 0x%x stop_tsf = 0x%x 
245,IIIII,RESMGR_OCS_RESOURCES  req_id = 0x%x ch_req_addr = 0x%x ch_alloc_addr = 0x%x state = 0x%x priority = 0x%x 
244,III,RESMGR_OCS_RESOURCES chan_mhz = %d sec_chan_mhz = %d, band_center_freq2 = %d 
243,II,RESMGR_OCS_CHREQ_GRANT  curr_time = 0x%x ch_req_addr = 0x%x 
242,II,RESMGR_OCS_CHREQ_COMPLETE  curr_time = 0x%x ch_req_addr = 0x%x 
241,I,RESMGR_OCS_CHANNEL_SWITCHED  status = %d 
240,II,RESMGR_OCS_MISS_TOLERANCE  miss_tolerance_cnt_timeslot1 = 0x%x miss_tolerance_cnt_timeslot2 = 0x%x 
239,I,RESMGR_OCS_NEXT_SCH_INTERVAL = %d 
238,II,RESMGR_OCS_PURGE_CHREQ  cur_ch_alloc_addr = 0x%x chan_mhz = %d 
237,I,RESMGR_OCS_PURGE_CHREQ  cur_ch_req_addr = 0x%x 
236,II,RESMGR_OCS_RECAL_QUOTAS  num_home_chans = %d tracking_interval = %d 
235,II,RESMGR_OCS_RECAL_QUOTAS  chan_mhz = %d latency = %d 
234,III,RESMGR_OCS_ALLOCATED_QUOTA_STATS  chan_mhz = %d req_chan_time_percentage = %d chan_time_quota = %d 
233,I,RESMGR_OCS_RECOMPUTE_SCHEDULE: ocs_ins = %d 
232,I,RESMGR_OCS %d has been paused 
231,,RESMGR_OCS_CURR_CAT_WINDOW 
230,III,RESMGR_OCS_CURR_CAT_WINDOW_REQ  req_id = 0x%x ch_req_addr = 0x%x state = %d 
229,II,RESMGR_OCS_CURR_CAT_WINDOW_TIMESLOT  start_tsf = 0x%x stop_tsf = 0x%x 
228,I,RESMGR_OCS_CURR_CAT_WINDOW: Channel change pending, flags = 0x%x 
227,III,RESMGR_OCS_CUR_CH_ALLOC  curr_chan_alloc_addr = 0x%x chan_mhz = %d sec_ch_mhz = %d 
226,III,RESMGR_OCS_WINNING_CH_ALLOC  curr_chan_alloc_addr = 0x%x chan_mhz = %d sec_ch_mhz = %d 
225,III,RESMGR_OCS_INVOKED: ocs_ins = %d last_ocs_entry_time = 0x%x current_time = 0x%x 
224,III,RESMGR_OCS_INVOKED: Cur_Ch_Alloc = 0x%x Flags = 0x%x Resched_Req = 0x%x 
223,I,RESMGR_OCS_SCHED_CH_CHANGE: ocs_ins = %d 
222,I,RESMGR_OCS_NEXT_TSFTIME  next_tsf_time = 0x%x 
221,III,RESMGR_OCS_TSF_TIMEOUT_US wake up latency = %d, wlan_chan_num = %d, wlan_cb_num = %d 
220,I,RESMGR_OCS_TSF_TIMEOUT_US  timeout_us = %d 
219,III,RESMGR_OCS_INVOKED: ocs_ins = %d ocs_entry_time = 0x%x ocs_exit_time = 0x%x 
273,IIIIII,RESMGR_LINK_CREATE link_pointer = 0x%x link_flags = 0x%x ch_mhz = %d phy_mode = %d band_center_freq1 = %d band_center_freq2 = %d 
272,I,RESMGR_LINK_DELETE  Link Pointer = 0x%x 
271,I,VCM_Init:  VC Pool Size = 0x%x 
287,III,RESMGR_VC_UPDATE_HOME_CHAN_INFO: mac_id = %d virtual_chan_count = 0x%x home_chan_count = 0x%x 
286,IIIIIIII,RESMGR_ADD_LINK ch_mhz = %d phy_mode = %d link_flags = 0x%x link_valid_attr = 0x%x no_160_link_cnt = %d 160_link_cnt = %d vc = 0x%x link = 0x%x 
285,IIIIII,RESMGR_VC_INIT_VIR_CHAN: chan_mhz = %d, mac_id = 0x%x, band = 0x%x, tx_chm = 0x%x, rx_chm = 0x%x, rx_nss = %d 
284,IIIIIII,RESMGR_VC_INIT_VIR_CHAN: nss1_tx_chm = 0x%x, nss2_tx_chm = 0x%x, selfgen_chm = 0x%x, nss_tx_11b_chainmask = 0x%x, selfgen_11b_chainmask = 0x%x, nss_tx_ofdm_chainmask = 0x%x, selfgen_ofdm_chainmask = 0x%x 
283,I,RESMGR_VC_INIT_HOME_CHAN: chan_mhz = %d 
282,II,RESMGR_OCS_REQ_QUOTA_STATS chan_mhz = %d req_chan_time/latency = 0x%x 
281,II,RESMGR_OCS_REQ_QUOTA_STATS  arg = 0x%x req_chan_time/latency = 0x%x 
280,IIII,RESMGR_VC_REGISTER_LINK: chan_mhz = %d link_count = %d ephemeral_link_count = %d is_home_chan = %d 
279,II,RESMGR_VC_ADD_LINK: link_flags = 0x%x link_valid_attr = 0x%x 
278,IIIIII,RESMGR_RMV_LINK ch_mhz = %d phy_mode = %d link_flags = 0x%x link_valid_attr = 0x%x no_160_link_cnt = %d 160_link_cnt = %d 
277,III,!cts2s_sent: 0x%x 0x%x 0x%x 
276,II,RESMGR_VC_FREE_VIR_CHAN: chan_mhz = %d is_home_chan = %d 
275,IIII,RESMGR_VC_UNREGISTER_LINK: chan_mhz = %d link_count = %d ephemeral_link_count = %d is_home_chan = %d 
274,I,RESMGR_VC_UPDATE_CUR_VC  chan_mhz = %d 
295,III,wlan_virtual_chan_apply_chan_num  rx = %d tx = %d org = %d 
294,III,RESMGR_VC_ARBITRATE_ATTRIBUTES  link_count = %d chain_number = %d per_link_chain_num = %d 
293,II,RESMGR_VC_ARBITRATE_ATTRIBUTES  chan_mhz = %d phy_mode/vc_prog_latency = %d 
292,III,RESMGR_VC_ARBITRATE_ATTRIBUTES  chan_mhz = %d per link tx_chainmask = %d, rx_chainmask = %d 
292,III,RESMGR_VC_ARBITRATE_ATTRIBUTES  chan_mhz = %d per link tx_chainmask = %d, rx_chainmask = %d 
291,IIII,RESMGR_VC_ARBITRATE_ATTRIBUTES current_chan_mhz = %d vc chan_mhz = %d, per link tx_chainmask = %d, rx_chainmask = %d 
290,III,RESMGR_VC_ARBITRATE_ATTRIBUTES  num = %d, tx_mask = %x rx_mask = %x 
289,IIIII,RESMGR_VC_ARBITRATE_ATTRIBUTES  chan_mhz = %d phy_mode/vc_prog_latency = %d band_center_freq = %d virtual_chan_ctxt = 0x%x virtual_chan = 0x%x 
288,III,VC_ARB_SMPS: mhz = %d, smps_supp = %d, dyn_smps = %d 
322,IIII,DBSMGR: Notify HW Mode, fake_hw_mode_change = %d, HW_Mode_Pending_Bitmask = 0x%x, Cur_HW_Mode = %d, cur_dbs_cfg = %d 
321,II,DBSMGR: Notify fake HW Mode, reason = %d, handler = 0x%p 
320,II,DBSMGR: Notify HW Mode, requestor = %d, cb = 0x%p 
319,,DBSMGR_UPDATE_ALLOWED_SCAN_POLICY: Scan Disallowed due to CAC in Progress 
318,,DBS_MGR_ASM: Handling 5G AS Grant 
317,,DBS_MGR_ASM: Recvd unexpected 5G AS Grant 
316,,DBS_MGR_ASM: Handling 5G AS status update 
315,IIII,DBS_MGR_ASM: cur_chm=0x%x, cur_dur=%d, new_chm=0x%x, new_dur=%d 
314,I,DBS_MGR_ASM: Recvd unhandled 5G AS event, evt=0x%x 
313,I,DBSMGR_CHM_NOTIF: event_type = 0x%x 
312,II,DBSMGR_SM_EVENT: %d < %d 
311,IIIII,DBSMGR: dbsmgr_set_hw_mode requestor = %d, hw_mode_switch_aborted = %d,fake_hw_mode_change_ongoing = %d, set_hw_mode_pending_bitmask = 0x%x, handler=0x%p 
310,IIII,DBSMGR: dbsmgr_set_hw_mode final_hw_mode = %d, cur_hw_mode = %d cur_dbs_cfg = %d next_hw_mode = %d 
309,I,DBSMGR: cancel fake hw mode change, reason = %d 
308,II,DBSMGR_Change_Scan_State: Cur_Scan_State = %d, New_Scan_State = %d 
307,II,DBSMGR: LFR Set HW Mode, Cur_HW_Mode = 0x%x, New_HW_Mode Requested = 0x%x 
306,IIIII,DBSMGR_RECOMPUTE_SCAN_POLICY: policy_priority_bitmap = 0x%x, unwanted_policy_bitmap = 0x%x, vdev_index = %d, chan_index = %d, is_reliable_scan = %d 
305,II,DBS_MGR_UNREG_SCAN_POLICY_HDL: handler = 0x%x arg = 0x%x not found 
304,II,DBS_MGR_UNREG_SCAN_POLICY_HDL handler = 0x%x arg = 0x%x 
303,II,DBS_MGR_REG_SCAN_POLICY_HDL: handler = 0x%x arg = 0x%x Exists!! 
302,I,DBS_MGR_REG_SCAN_POLICY_HDL: Pool Empty!! 
301,II,DBS_MGR_REG_SCAN_POLICY_HDL:  handler = 0x%x arg = 0x%x 
300,II,DBSMGR: connection_in_progress=%d, conn_in_progress_bitmap=0x%x 
299,I,DBSMGR: set fake hw mode, reason = %d 
298,,DBSMGR: set fake hw mode fail, no buffer 
297,III,DBSMGR: Policy Mgr Set HW Mode, Cur_HW_Mode = 0x%x, New_HW_Mode Requested = 0x%x, roam_in_progress = %d 
296,IIII,DBSMGR_UPDATE_MAC_CFG: conc_scan_cfg = 0x%x, fw_mode_cfg = 0x%x, hw_mode_pending = 0x%x, cur_hw_mode = %d 
323,III,DBSMGR_HW_Mode_Switch_Complete: Prev_HW_Mode = %d, Cur_HW_Mode = %d, HW_Mode_Switch_Dur = %d 
324,IIII,DBSMGR HW Mode change after Calibration: cur_hw_mode = %d, mac0_channel_mhz = %d, mac1_channel_mhz = %d, Loopback_Calibration_Dur = %d 
325,II,DBSMGR Loopback Calibration Fake HW mode change complete: cur_hw_mode = %d, Loopback_Calibration_Dur = %d 
326,II,DBSMGR: start calibration, cur_hw_mode = %d, home_chan_mhz=0x%x 
327,I,DBSMGR: start timer to wait noa start, timeout=%d 
328,II,DBSMGR_SM:  %d => %d 
329,IIIII,DBSMGR_HW_MODE_CHANGE_REQ: dbs_enable = %d, cur_hw_mode = %d, next_hw_mode = %d, hw_mode_pending = 0x%x, fake_hw_mode_change = %d 
188,IIII,RESMGR_DELIVER_EVT: type = 0x%x, old_hw_mode = 0x%x, new_hw_mode = 0x%x, band_to_mac = 0x%x 
312,II,DBSMGR_SM_EVENT: %d < %d 
365,IIIII,RESMGR_CHMMGR_CALC_PERVC_T1_CHM: chan_mhz = %d, tx_chainmask = 0x%x, rx_chainmask = 0x%x, hw_chm_changed = %d, chm_change_state = %d 
364,IIIII,RESMGR_CHMMGR_CALC_PERVC_T2_CHM: chan_mhz = %d, nss1_chainmask = 0x%x, nss1_chainmask = 0x%x, selfgen_chainmask = 0x%x, tx_chm_changed = %d 
363,IIII,RESMGR_CHMMGR_CALC_ABG_CHM: 11b_nss_tx = 0x%x, ofdm_nss_tx = 0x%x, 11b_selfgen = 0x%x, ofdm_selfgen = 0x%x 
362,IIII,RESMGR_CHMMGR_SMPS_CB: mac_id = %d, vc_mhz = %d, smps_pending_bitmask = 0x%x, smps_status = %d 
361,III,RESMGR_CHMMGR_CHAINMASK_CHANGE_REQ: cli_type = 0x%x, client_id = 0x%x, req_id = 0x%x 
360,I,RESMGR_CHMMGR_TICKLE: cli_type = 0x%x 
359,IIII,RESMGR_CHMMGR_RESOLVE_BANDWIDTH: band = %d, mac = %d, max_bw_supported = 0x%x, hw_mode = %d 
358,I,RESMGR_CHMMGR_INIT_DBSMGR_REQ: cli_type = %d 
357,IIII,RESMGR_CHMMGR_DB_UPDATE: mac = %d, band = %d, tx_chm = 0x%x, rx_chm = 0x%x 
356,III,RESMGR_CHMMGR_DB_UPDATE: nss1_tx_chm = 0x%x, nss2_tx_chm = 0x%x, selfgen_chm = 0x%x 
355,II,RESMGR_CHMMGR_INITIATE_VC_OPS: state = 0x%x, chm_ctx->hw_mode_change_pending = %d 
354,II,RESMGR_CHMMGR_INITIATE_VC_OPS: mac_id = %d, cur_vc_mhz = %d 
353,IIII,RESMGR_CHMMGR_NOTIF_SMPS: vc_mhz = %d, new_chainmask = 0x%x, bandwidth = 0x%x, finish_timeout_ms = %d 
352,I,SMPS operation failed. status = 0x%x 
351,IIII,RESMGR_CHMMGR_WAL_OPS: mac_id = %d, cur_mhz = %d,hw_chm_changed = %d, tx_chm_changed = %d 
350,IIIII,RESMGR_CHMMGR_WAL_OPS: tx_chainmask = 0x%x, rx_chainmask = 0x%xnss1_tx_chm = 0x%x, nss2_tx_chm = 0x%x, selfgen_chainmask = 0x%x 
349,IIII,RESMGR_CHMMGR_WAL_OPS: 11b_nss_tx = 0x%x, ofdm_nss_tx = 0x%x, 11b_selfgen = 0x%x, ofdm_selfgen = 0x%x 
348,II,RESMGR_CHMMGR_NOTIFY_ALL_T1_CLIENTS: Client_ID = %d, Resp_ID = %d  
347,II,RESMGR_CHMMGR_NOTIFY_T1_REQESTER: cli_id = %d, req_id = %d 
346,II,RESMGR_CHMMGR_NOTIFY_ALL_T2_CLIENTS: Client_ID = %d, Resp_ID = %d 
345,II,RESMGR_CHMMGR_NOTIFY_T2_REQESTER: cli_id = %d, req_id = %d 
344,,RESMGR_CHMMGR_NOTIFY_INIT_CHM 
343,IIIII,RESMGR_CHMMGR_NOTIF_VDEV_UP: chan_mhz = 0x%x, hw_rx_chm = 0x%x, rx_nss = %d, new_rx_chm = 0x%x, bandwidth = 0x%x 
342,I,RESMGR_CHMMGR_POST_PROCESS: error_code = %d 
341,IIIII,RESMGR_CHMMGR_DB_UPDATE: mac = %d, band = %d, tx_chm = 0x%x, rx_chm = 0x%x RX_NSS = %d 
340,IIII,RESMGR_CHMMGR_DB_UPDATE: nss1_tx_chm = 0x%x, nss2_tx_chm = 0x%x, selfgen_chm = 0x%x, bandwidth = 0x%x 
339,I,RESMGR_CHMMGR_PROCESS_CHM_CHANGE_REQ: chm_state = 0x%x 
338,II,RESMGR_CHMMGR_PROTO_CHANGES_COMP: chm_ctx_state = 0x%x, hw_mode_pending = %d 
337,III,RESMGR_CHMMGR_REGISTER: client_id = %d, cli_type = %d, client_idx = %d 
336,III,RESMGR_CHMMGR_RESOLVE_BANDWIDTH: band = %d, mac = %d, max_bandwidth = 0x%x 
335,IIIIIII,RESMGR_CHMMGR_RESOLVE_T1: mac_id = %d, band = %d, t1_cli_id = %d, tx_chainmask = 0x%x, rx_chainmask = 0x%x, res_rx_nss = %d, disable_ul_mu = 0x%x 
334,IIIII,RESMGR_CHMMGR_RESOLVE_T2: band = %d, mac = %d, nss1_tx_chainmask = 0x%x, nss2_tx_chainmask = 0x%x, selfgen_chainmask = 0x%x 
333,I,RESMGR_CHMMGR_SCHEDULE: chm_state = 0x%x 
332,I,RESMGR_CHMMGR_SEND_HW_MODE_PRE_NOTIF: event.resp_id = %d 
331,I,RESMGR_CHMMGR_SMPS_OP_COMPLETE_TIMEOUT: smps_pending_bitmask = %d 
330,III,RESMGR_CHMMGR_UNREGISTER: client_id = %d, cli_type = %d, client_idx = %d 
374,II,RESMGR_CONCURRENCY_DEREG_EVT_HDLR:  handler = 0x%x arg = 0x%x deregistered 
373,III,_resmgr_concurrency_mgr_is_low_freq_vdev_chreq_apply:  active_sta_vdev_num = 0x%x, active_vdev_num = 0x%x, resmgr_nan_discovery_enable = 0x%x 
370,II,_resmgr_concurrency_mgr_is_low_freq_vdev_chreq_apply:  handler = 0x%x enable = 0x%x 
370,II,_resmgr_concurrency_mgr_is_low_freq_vdev_chreq_apply:  handler = 0x%x enable = 0x%x 
370,II,_resmgr_concurrency_mgr_is_low_freq_vdev_chreq_apply:  handler = 0x%x enable = 0x%x 
370,II,_resmgr_concurrency_mgr_is_low_freq_vdev_chreq_apply:  handler = 0x%x enable = 0x%x 
372,II,_resmgr_concurrency_mgr_is_low_freq_vdev_chreq_apply:  nan_freq_2g = 0x%x nan_freq_5g = 0x%x 
371,II,_resmgr_concurrency_mgr_is_low_freq_vdev_chreq_apply:  num_home_chans = 0x%x chan = 0x%x 
371,II,_resmgr_concurrency_mgr_is_low_freq_vdev_chreq_apply:  num_home_chans = 0x%x chan = 0x%x 
370,II,_resmgr_concurrency_mgr_is_low_freq_vdev_chreq_apply:  handler = 0x%x enable = 0x%x 
370,II,_resmgr_concurrency_mgr_is_low_freq_vdev_chreq_apply:  handler = 0x%x enable = 0x%x 
369,I,resmgr_concurrency_mgr_notify:  module = 0x%x 
368,II,RESMGR_CONCURRENCY_REG_EVT_HDLR:  handler = 0x%x arg = 0x%x exists!!! 
367,II,RESMGR_CONCURRENCY_REG_EVT_HDLR: handler = 0x%x arg = 0x%x no memory!!! 
366,II,RESMGR_CONCURRENCY_REG_EVT_HDLR:  handler = 0x%x arg = 0x%x registered 
375,IIII,SCAN_ENG_SPOOFED_MAC_ADDR full_mac_addr = %08x%04x partial_mac_addr = %08x%04x 
376,IIIIII,SCAN_ENG_PARAM_2 idle_time = %d msec repeat_probe_time = %d msec probe_spacing_time = %d msec probe_delay = %d msec burst_duration = %d msec max_num_probes = %d 
377,IIIII,SCAN_ENG_PARAM_1 dwell_time_active = %d msec dwell_time_passive = %d msec min_rest_time = %d msec max_rest_time = %d msec max_scan_time = %d msec 
378,IIIIIIII,SCAN_ENG_START scan_id = 0x%x scan_req_type = %d num_chans_[request(3)|granted_2g(3)|granted_5g(3)] = %09d num_[ssid(3)|bssid(3)] = %06d flags = 0x%x vdev_freq = %d cur_chan_index_2g|5g = %d %d 
379,III,SCAN_ENG_START_DBS num_5g_active = %d, num_5g_passive = %d double_passive_chan_scan = %d 
380,II,AUTO_CHAN_EVT_HDNLR CURR_FREQ_ERROR scan_id = %d evt_mac_id = %d 
381,IIII,AUTO_CHAN_EVT_HDNLR CURR_CHAN_STATS_ERROR scan_id = %d evt_mac_id = %d type = 0x%x freq = 0x%x 
382,III,SCAN_BCN_RECVD mhz=%d at %08x send_probe_req_on_DFS_ch=%d ignored 
383,III,SCAN_BCN_RECVD mhz=%d at %08x is_scan_in_progress=%d ignored 
384,III,SCAN_BCN_RECVD mhz=%d at %08x is_passive_dwell_enabled=%d will handle bcn_rcvd. return 
385,IIIII,SCAN_SET_CHAN_LIST idx = %d, mhz = %d, is_passive = %d ch_info = 0x%x reg_info_1 = 0x%x 
386,II,SCAN_SET_CHANLIST_FAILED support_chan %d num_scan_chans %d 
387,IIIIII,SCAN_ENG_CANCEL scanhandler_id = %d scan_id = 0x%x requestor= 0x%x stop_mode = %d scan_in_progress = %d cancel_in_progress = %d 
388,I,SCAN_SM_START_COMMAND_FAILED current_scan = NULL handle = 0x%x 
389,IIII,SCAN_ENG_START_IN_PROGRESS = 1 scan_id = 0x%x requestor = 0x%x req_sub_id = 0x%x priority = %d -> return EBUSY 
390,III,SCAN_ADJUST_PARAM active=%d passive=%d rest=%d 
391,I,SCAN_ENG_MAX_SCAN_TIMEOUT scan_id = 0x%x 
392,IIIIIII,CHANNEL_CONGESTION_PRINTS cycle_cnt = %10d, busy = %10d, tx = %10d, rx = %10d, mr_rx = %10d, chan_freq= %d send_stats:%d 
393,I,SCAN_SCH_START_NEW_REQ_FAILED error_code=%d 
394,II,SCAN_SCH_SUSPENDED suspend_bitmap_63_32 = 0x%x, suspend_bitmap_31_0 = 0x%x 
395,II,SCAN_SCH_SUSPEND_SCAN requestor_id = 0x%x scan_id = 0x%x 
396,,SCAN_SCH_CANCEL no match found 
397,,SCAN_SCH_CANCEL already in progress 
398,IIII,SCAN_SCH_CANCEL scan_id = 0x%x requestor_id = 0x%x vdev_id = %d req_type = %d 
399,IIIII,SCAN_SCH_START_INFO monitoring_interval = %d ie_len = %d ie_chunk_bitmap = 0x%x opmode = %d subopmode = %d 
400,III,SCAN_SCH_START_BUF_CHUNK_COPY_FAILED param_len = %d opmode = %d subopmode = %d 
401,IIIII,SCAN_SCH_START scan_id = 0x%x requestor_id = 0x%x req_sub_id = 0x%x requested_priority = %d absolute_priority = %d 
402,III,SCAN_SCH_START_ALLOC_FAIL scan_id=0x%d requestor_id = 0x%x req_sub_id = 0x%x 
403,,SCAN_SCH_START VDEV is not valid 
404,IIIII,SCAN_SCH_START_PARAM_INVALID scan_id=0x%d requestor_id = 0x%x req_sub_id = 0x%x requested_priority = %d ie_len=%d 
405,II,SCAN_SCH_START_PARAM_INVALID scan_id=0x%d param=0x%x 
406,II,SCAN_SCH_ENGINE_STOP_DUE_TO_TIMEOUT  evt_scan_id = 0x%x evt_reason = 0x%x 
407,I,SCAN_SCH_STOP_COMMAND_FAILED status = 0x%x 
408,I,SCAN_EVENT_SEND_FAILED 0x%x 
409,I,SCAN_START_COMMAND_FAILED status = 0x%x 
410,II,SCAN_SCH_WMI_START_SCAN TRIM num_bssid from %d to %d 
411,II,SCAN_SCH_WMI_START_SCAN TRIM num_ssid from %d to %d 
412,IIIII,SCAN_EVENT_UNKNOWN scan_id = 0x%x vdev_id = %d ch_freq = %d req_sub_id = 0x%x  send_to_host(bit8)|reason = 0x%03x 
413,IIIII,SCAN_EVENT_FOREIGN_CHANNEL_EXIT scan_id = 0x%x vdev_id = %d ch_freq = %d req_sub_id = 0x%x  send_to_host(bit8)|reason = 0x%03x 
414,IIIII,SCAN_EVENT_RESTARTED scan_id = 0x%x vdev_id = %d ch_freq = %d req_sub_id = 0x%x send_to_host = %d 
415,IIIII,SCAN_EVENT_START_FAILED scan_id = 0x%x vdev_id = %d req_sub_id = 0x%x reason = %d send_to_host = %d 
416,IIII,SCAN_EVENT_SUSPENDED scan_id = 0x%x  ch_freq = %d reason = %d send_to_host = %d 
417,IIIII,SCAN_EVENT_PREEMPTED scan_id = 0x%x  ch_freq = %d preempted_by (scan_id) = 0x%x reason = %d send_to_host = %d 
418,IIIII,SCAN_EVENT_DEQUEUED scan_id = 0x%x vdev_id = %d ch_freq = %d req_sub_id = 0x%x  send_to_host(bit8)|reason = 0x%03x 
419,IIIIII,SCAN_EVENT_FOREIGN_CHANNEL scan_id = 0x%x  ch_freq = %d bss_ch_freq = %d req_sub_id = 0x%x send_to_host = %d passive/active = %d 
420,IIIII,SCAN_EVENT_BSS_CHANNEL scan_id = 0x%x vdev_id = %d ch_freq = %d req_sub_id = 0x%x send_to_host = %d 
421,IIIII,SCAN_EVENT_COMPLETED scan_id = 0x%x vdev_id = %d ch_freq = %d reason = %d send_to_host = %d 
422,IIIII,SCAN_EVENT_STARTED scan_id = 0x%x vdev_id = %d ch_freq = %d req_sub_id = 0x%x send_to_host = %d 
423,III,SCAN_SCH_RESUME requestor_id = 0x%x suspend_bitmap_63_32 = 0x%x, suspend_bitmap_31_0 = 0x%x 
424,III,SCAN_SCH_SUSPEND requestor_id = 0x%x suspend_bitmap_63_32 = 0x%x, suspend_bitmap_31_0 = 0x%x 
425,I,SCAN_SCH_CSA_FAILED status = 0x%x 
426,I,SCAN_SCH_NEXT_SCAN_FAILED error_code=%d 
427,IIIII,SCAN_EVENT_SEND_FAILED scan_id = 0x%x vdev_id = %d ch_freq = %d req_sub_id = 0x%x reason = %d 
428,I,wlan_scan_process_scan_results: Clear OCE bit for channel-%d 
429,I,wlan_scan_process_scan_results: Set OCE bit for channel-%d 
430,I,SCAN_EVENT_COMPLETED really cancelled scan_id %d 
431,IIIIIII,SCAN_SCH_SUPPRESS_MATCH scan_id = 0x%x, requestor = 0x%x, vdev_id = 0x%x, suppress_vdev_id_bitmap = 0x%x suppress_mod_bitmap[0:2] 0x%x 0x%x 0x%x 
432,III,SCAN_SCH_SUPPRESS_REQ sch_class = 0x%x id = 0x%x is_disable_scan = %d 
433,IIII,SCAN_SCH_SUPPRESS_REQ_ERROR req_mod_id=%d sch_class = 0x%x id = 0x%x is_disable_scan = %d 
434,IIIIIIIII,SCAN_SEND_PROBE_REQ_2G scan_id = 0x%x mac_id = %d freq = %d cur_index = %d max_num_probe = %d probe_timer_count = %d chainmask = %d ppdu_info = 0x%x max_tx_power=%d 
435,IIIIIIIII,SCAN_SEND_PROBE_REQ_5G scan_id = 0x%x mac_id = %d freq = %d cur_index = %d max_num_probe = %d probe_timer_count = %d chainmask = %d ppdu_info = 0x%x max_tx_power=%d 
436,I,SCAN_SM_PROBE_REQ_FRAME_GEN_FAILED scanhandler_id = %d 
435,IIIIIIIII,SCAN_SEND_PROBE_REQ_5G scan_id = 0x%x mac_id = %d freq = %d cur_index = %d max_num_probe = %d probe_timer_count = %d chainmask = %d ppdu_info = 0x%x max_tx_power=%d 
434,IIIIIIIII,SCAN_SEND_PROBE_REQ_2G scan_id = 0x%x mac_id = %d freq = %d cur_index = %d max_num_probe = %d probe_timer_count = %d chainmask = %d ppdu_info = 0x%x max_tx_power=%d 
436,I,SCAN_SM_PROBE_REQ_FRAME_GEN_FAILED scanhandler_id = %d 
437,IIIIII,SCAN_SEND_PROBE_REQ_INFO scan_id = 0x%x band_2G_info = 0x%x band_5G_info = 0x%x probe_time = %d last_ssid_idx = %d last_bssid_idx = %d 
438,IIII,SCAN_SEND_PROBE_REQ_5G_RET scan_id = 0x%x freq = %d cur_index = %d flags = 0x%02x 
439,IIII,SCAN_SEND_PROBE_REQ_2G_RET scan_id = 0x%x freq = %d cur_index = %d flags = 0x%02x 
440,I,SCAN_SEND_PROBE_REQ_RET_PASSIVE scan_id = 0x%x 
441,I,SCAN_SEND_PROBE_REQ_RET_VDEV scan_id = 0x%x 
442,II,cur time is %x, start time is %x 
443,IIIIIIII,SCAN_SM_REQ_NEXT_CHAN_AGILE_DFS_5G scanhandler_id = %d 2g_cur_idx = %d 2g_total = %d 5g_cur_idx = %d 5g_total = %d dwell = %d msec duration = %d usec freq = %d 
444,I,return is true, start time is %d 
445,,enter quite function 
446,II,SCAN_NOA_DWELL_TIME_OFFSET_AGILE_DFS_5G round_up_offset = %d scan_pre_foreign_chan_exit_time = %d 
447,IIIIIIII,SCAN_SM_REQ_NEXT_CHAN_AGILE_DFS_2G scanhandler_id = %d 2g_cur_idx = %d 2g_total = %d 5g_cur_idx = %d 5g_total = %d dwell = %d msec duration = %d usec freq = %d 
448,II,SCAN_NOA_DWELL_TIME_OFFSET_AGILE_DFS_2G round_up_offset = %d scan_pre_foreign_chan_exit_time = %d 
449,II,SCAN_NOA_DWELL_TIME_OFFSET_ASYNC_DBS round_up_offset = %d scan_pre_foreign_chan_exit_time = %d 
450,IIIIIIIII,SCAN_SM_REQ_NEXT_CHAN_ASYNC_DBS scanhandler_id = %d 2g_cur_idx = %d 2g_total = %d 5g_cur_idx = %d 5g_total = %d dwell = %d msec duration = %d usec pri_freq = %d sec_freq = %d 
451,,SCAN_NEXT_CH_ERROR n_chan is not assigned 
452,I,SCAN_SM_REQ_NEXT_CHAN_ASYNC_CMPLT scanhandler_id = 0x%x 
453,II,SCAN_NOA_DWELL_TIME_OFFSET_SYNC_DBS round_up_offset = %d scan_pre_foreign_chan_exit_time = %d 
454,IIIIIIIII,SCAN_SM_REQ_NEXT_CHAN_SYNC_DBS scanhandler_id = %d 2g_cur_idx = %d 2g_total = %d 5g_cur_idx = %d 5g_total = %d dwell = %d msec duration = %d usec 2g_freq = %d 5g_freq = %d 
455,IIIIIIIII,SCAN_SM_REQ_NEXT_CHAN_AGILE scanhandler_id = %d 2g_cur_idx = %d 2g_total = %d 5g_cur_idx = %d 5g_total = %d dwell = %d msec duration = %d usec 2g_freq = %d 5g_freq = %d 
456,II,SCAN_NOA_DWELL_TIME_OFFSET_AGILE round_up_offset = %d scan_pre_foreign_chan_exit_time = %d 
457,II,SCAN_NOA_DWELL_TIME_OFFSET_LEGACY round_up_offset = %d scan_pre_foreign_chan_exit_time = %d 
451,,SCAN_NEXT_CH_ERROR n_chan is not assigned 
458,IIIIIIII,SCAN_SM_REQ_NEXT_CHAN_LEGACY 2g_cur_idx = %d 2g_total = %d 5g_cur_idx = %d 5g_total = %d dwell = %d msec duration = %d usec pri_freq = %d sec_freq = %d 
459,I,SCAN_SM_REQ_NEXT_CHAN !error! not implemented scan policy: %d 
460,III,SCAN_SM_TRANSITIONS_MAC_%d %d => %d 
461,III,SCAN_SM_DISPATCH_MAC_%d %d < %d 
462,II,SCAN_SM_CANCEL scan_stop = 0x%x scan_timeout = %d 
463,IIII,SCAN_SM_OCS_TIMEOUT scan_id 0x%x, requestor = %d, curr_index = %d, curr_policy = %d 
464,IIIII,SCAN_MGR_CHECK_BAND_CHANNELS params->num_chan=%d params->chan_list[0]=%d has_2g_chan=%d has_5g_chan_active=%d has_5g_chan_passive=%d 
465,IIIII,SCAN_MGR_EVENT_COMPLETED scan_id = 0x%x num_ssid = %d num_bssid = %d num_chan = %d is_drop = %d 
466,III,SCAN_MGR_EVENT_ASYNC_COMPLETE scan_handler_id = 0x%x scan_handle->band_5g_cur_chan_index = 0x%x scan_handle->band_2g_cur_chan_index = 0x%x 
467,IIII,SCAN_MGR_EVENT_SUSPENDED scan_id = 0x%x cur_chan_index = 0x%x reason = 0x%x cur_scan_policy = %d 
468,IIIIIIIII,SCAN_MGR_EVENT_PREEMPTED scan_id = 0x%x cur_chan_index = 0x%x  mac_id = %d 2g_idx = %d 2g_curr = %d 5g_idx = %d 5g_curr = %dreason = 0x%x cur_scan_policy = %d 
469,II,wlan_scan_mgr_preprocess_event: Invalid input - scan_handler_id = %d, current_scan_sch_req = %p 
470,IIII,SCAN_MGR_RESUME_EVENT 2g cur_chan = %d, 2g next_chan = %d, 5g cur_chan = %d, 5g next_chan = %d 
471,III,SCAN_MGR_DBS_SCAN_DUTY_CYCLE_PARAM module_id = %d max_num_dbs_scans = %d max_num_legacy = %d  
472,,SCAN_MGR_DBS_SCAN_DUTY_CYCLE_PARAM scanhandle is NULL 
473,,SCAN_MGR_DBS_SCAN_DUTY_CYCLE_PARAM num_clients is 0 
474,I, SCAN_MGR_CLIENT_POLICY_SCAN_SELECTION scan_selection = %d 
475,,SCAN_MGR_CLIENT_POLICY_INVALID scanhandle is NULL 
476,IIIII,wlan_scan_mgr_compute_client_scan_policy_by_duty_cycle  module_id = %d cur_num_dbs = %d cur_num_legacy = %dmax_num_dbs=%d max_num_legacy = %d 
477,I,SCAN_MGR_SCAN_POLICY_RECOMPUTE_UNSUPPORT policy = %d 
478,I,SCAN_MGR_SCAN_POLICY_RECOMPUTE_END suppress mode bitmap = %d 
479,IIII,SCAN_MGR_SCAN_POLICY_RECOMPUTE vdev_index = %d, chan_index = %d, new_scan_policy = %d, scan_mgr_handle->cur_scan_policy = %d 
480,I,SCAN_MGR_CLIENT_SCAN_POLICY policy= %d 
481,IIII,SCAN_MGR_SCAN_POLICY_RECOMPUTE invalid chan index vdev_index=%d has_2g_chan=%d passive_5g=%d has_5g_chan_active=%d 
482,I,SCAN_MGR_SCAN_POLICY_RECOMPUTE_START suppress mode bitmap = %d 
483,,SCAN_MGR_CH_MODE_CHANGE scan cancelled 
484,III,SCAN_MGR_DS_PARAM mac_id = %d, chan = %d len = %d 
485,III,SCAN_MGR_BCN_RECV_WRONG_CH mac_id = %d cur_freq (%d != %d) 
486,III,SCAN_MGR_BCN_RECV_WRONG_CH mac_id = %d freq (%d != %d) 
487,I,SCAN_MGR_BCN_RECV_NO_CURRENT_SCAN mac_id = %d 
488,I,SCAN_MGR_BCN_RECV_FAILED mac_id = %d 
489,I,SCAN_SCH_NEXT_SCAN_FAILED after setting new channel lists, error_code=%d 
490,II,SCAN_MGR_CANCEL comp_pending=0x%x cancel_pending=0x%x 
491,IIII,SCAN_MGR_CANCEL scan_id = 0x%x requstor = 0x%x stop_mode = %d scan_eng_start_pending = %d 
492,III,SCAN_MGR_SCAN_START scan_id = 0x%x  cur_scan_policy = %d scan_cfg_state = %d 
493,IIII,SCAN_MGR_PDEV_SUSPEND_RESUNE_CHANGE_EVT pdev_id = %d requestor = %d, reason %d state = %d 
494,I,end of scan_policy_allowed_event_hdlr, suppress mode bitmap = %d 
495,I,begin of scan_policy_allowed_event_hdlr, suppress mode bitmap = %d 
496,III,SCAN_POLICY_EVENT current allowed policy = 0x%x, new allowed policy = 0x%x,current scan is %x
 
497,IIIII,SCAN_MGR_STATE_CHANGE scan_id = 0x%x num_ssid = %d num_bssid = %d num_chan = %d new_scan_state = %d (completed 0/legacy 1/DBS 2/async DBS 3/agile DBS 4) 
498,IIIII,SCAN_ADAPTIVE_DWELL_NEXT_SLOT_CHECK dwell_mode = %d band = %d next_index = %d next_period = %d (0 = end of slot) cur_tsf = %10d 
499,IIIII,SCAN_ADAPTIVE_DWELL_CH_CONGESTION_CHECK is_bcnprb_rcvd = %d ch_congest_avg = %d congest_threshold = %d cur_index = %d move_to_next %d (0 = slot, 1 = channel) 
500,IIII,SCAN_ADAPTIVE_DWELL_PASSIVE_STARTED dwell_mode = %d (0:con,1:mod,2:agg,3:dis,4:def) band = %d is_enabled = %d def_mode = %d 
501,IIII,SCAN_ADAPTIVE_DWELL_ALL_PROBE_SENT dwell_mode = %d band = %d index = %d period = %d (0 = end of slot) 
502,IIII,SCAN_ADAPTIVE_DWELL_ACTIVE_STARTED dwell_mode = %d (0:con,1:mod,2:agg,3:dis,4:def) band = %d is_enabled = %d def_mode=%d 
503,II,SCAN_ADAPTIVE_DWELL_CH_ACTIVITY_CALC  ch_congestion_cur/avg = %d, %d 
504,IIIIII,SCAN_ADAPTIVE_DWELL_CH_ACTIVITY_DIFF  cycle_cnt = %10d, busy = %10d, tx = %10d, rx = %10d, mr_rx = %10d, bcnprb = %10d 
505,IIIIIII,SCAN_ADAPTIVE_DWELL_CH_ACTIVITY_END mac_id: %d cycle_cnt = %10d, busy = %10d, tx = %10d, rx = %10d, my_rx = %10d, cur_tsf = %10d 
506,,SCAN_ADAPTIVE_DWELL_COLLECT_CH_ACTIVITY_NOT_STARTED 
507,,SCAN_ADAPTIVE_DWELL_CH_ACTIVITY_START_ALREADY 
508,IIIIIII,SCAN_ADAPTIVE_DWELL_CH_ACTIVITY_START mac_id: %d cycle_cnt = %10d, busy = %10d, tx = %10d, rx = %10d, my_rx = %10d, cur_tsf = %10d 
509,IIIII,SCAN_ADPATIVE_DWELL_CONFIG lpf_wt = %d, passive_monitor_interval = %d, wifi_activity_threshold = %d default_mode_wmi/internal = %d/%d 
510,II,SCAN_ADPATIVE_DWELL_ENABLED enabled = %d, tlv_present %d 
511,III,SCAN_ADPATIVE_DWELL_TABLE_ENTRY index %d {%d, %d} 
512,I,SCAN_ADPATIVE_DWELL_TABLE_5G_AGG num_entry = %d 
513,I,SCAN_ADPATIVE_DWELL_TABLE_2G_AGG num_entry = %d 
514,I,SCAN_ADPATIVE_DWELL_TABLE_5G_MOD num_entry = %d 
515,I,SCAN_ADPATIVE_DWELL_TABLE_2G_MOD num_entry = %d 
516,I,SCAN_ADPATIVE_DWELL_TABLE_5G_CON num_entry = %d 
517,I,SCAN_ADPATIVE_DWELL_TABLE_2G_CON num_entry = %d 
518,,CH_PREDICTION_FOREIGN_CH_END chan_freq not found in scanning chan list 
519,II,CH_PREDICTION_CALCULATE_RESULT value = %d stationary = %d 
520,IIII,CH_PREDICTION_CALCULATE_SAMPLE bssid = 0x%x%x prev_rssi = 0x%x curr_rssi = 0x%x (dbm above nf) 
521,II,CH_PREDICTION_CALCULATE top_k_freq = %d total_bss_found = %d 
522,,CH_PREDICTION_FOUND_BSS no buffer 
523,IIIII,CH_PREDICTION_FOUND_BSS SA = 0x%x%x subtype = 0x%x seq = %d, rssi = 0x%x (dbm above nf) 
524,IIIII,CH_PREDICTION_FOUND_BSS receive frames not-on-curr channel. SA = 0x%x%x subtype = 0x%x seq = %d chan = 0x%x 
525,IIII,CH_PREDICTION_FOUND_BSS received frames not to us. DA = 0x%x%x subtype = 0x%x seq = %d 
526,II,CH_PREDICTION_SCAN_START scan_type = %d (0 full scan/1 top_k scan/2 remaining scan) social_chan_scan = %d 
527,,CH_PREDICTION_SCAN_START_ERROR 
528,II,CH_PREDICTION_SCAN_START_PARAM_ERROR requestor=%d not equal module_id=%d 
529,III,CH_PREDICTION_SCAN_START_PARAM_ERROR scanhandle=0x%x,params=0x%x,scan_id=0x%x 
530,,SCAN_CH_PREDICT_STOP 
531,IIII,CH_PREDICTION_START module_id = %d top_k_num = %d stationary_thres = %d full_scan_period_ms = %d 
532,,CH_PREDICTION_SCAN_START scan_type = 2 (0 full scan/1 top_k scan/2 remaining scan) 
537,I,SCAN_NUM_SUPP_CHAN_LIST %d 
536,IIIIII,SCAN_SUPP_CHAN_INFO_1 mhz (%d) ch %d, band_center_freq1 (%d), band_center_freq2 (%d), phy_mode (%d), max_tx_power (%d) 
535,IIIIIII,SCAN_SUPP_CHAN_INFO_2 is_passive (%d), is_ht_allowed (%d), is_vht_allowed (%d), is_dfs_ch (%d), is_bcn_found (%d), is_radar_detected (%d), csa_recv_timestamp (%d) 
534,III,SCAN_SUSPEND_RESUME_UNIT_TEST vdev_id = %d num_args = %d, req = %d 
533,IIII,SCAN_SUPPRESS_UNIT_TEST sch_class = %d id = %d is_disable = %d num_args = %d 
538,II,clear radio stats, i %d, wal_pdev 0x%x 
539,,_wlan_iface_link_stats_process: wal_vdev is NULL 
540,,_wlan_iface_link_stats_process: vdev is NULL 
541,,wlan_clear_vdev_stats_BEThread: Fail to allocate clearLLStatsMsg buffer 
542,I,PS_STA_AVG_CHANNEL_CONGESTION(ERROR): chan_activity(%u) > 100 
543,II,PS_STA_AVG_CHANNEL_CONGESTION(ERROR):diff_all(%u) < diff_tx(%u) 
544,II,wlan_stats_processor: peer_stats->peer_tx_rate = %d rx_rate = %d 
545,II, PS_STA_AVG_CHANNEL_CONGESTION BusyChanRunningAvg = %d %d 
546,IIIIIII,TRAFFIC_STA_CONN_STATE vdev_id = %d, mac_id = %d, state = %d is_associated = %d  is_running = %d is_enabled = %d vdev_bitmap = 0x%x 
547,I,TRAFFIC_STA_CONN_STATE_FAILED state = %d 
548,IIIIIII,TRAFFIC_DATA_RESET_2 total_rx_bytes = %d actual_rx_bytes = %d rx_throughput = %d total_tx_bytes = %d actual_tx_bytes = %d tx_throughput = %d is_running = %d 
549,III,TRAFFIC_DATA_RESET_1 mac_id = %d, vdev_id = %d, vdev_bitmap = 0x%x 
550,II,TRAFFIC_DATA_RESET_ERROR vdev_id = %d, mac_id = %d 
551,II,TRAFFIC_VDEV_INIT_FAILED mac_id = %d, vdev_id = %d 
552,II,TRAFFIC_RELEASE traffic_mon = 0x%x num_req = %d 
553,III,TRAFFIC_MON_POST_VDEV_MIGRATE vdev_id = %d, macid = %d, vdev_bitmap = 0x%x 
554,III,TRAFFIC_MON_PRE_VDEV_MIGRATE vdev_id = %d, macid = %d, vdev_bitmap = 0x%x 
555,IIII,TRAFFIC_UNREG_SUCCESS vdev_id = %d req_id = %d num_req = %d is_running = %d 
556,II,TRAFFIC_NO_ENTRY_EXIST vdev_id = %d req_id = %d 
557,IIIII,TRAFFIC_UNREG_INVALID_INFO vdev_id = %d, req_id = %d, total_num_req = %d, is_enabled = 0x%x traffic_mon = 0x%x 
558,II,TRAFFIC_REG_REQ_INFO_2 mac_id = %d, vdev_bitmap = 0x%x 
559,IIIIIIIII,TRAFFIC_REG_REQ_INFO_1 is_running = %d, is_associated = %d, vdev_id = %d, req_id = %d, rx_thresh = %d, rx_status = %d, tx_thresh = %d, tx_status = %d total_req = %d 
560,II,TRAFFIC_MEMORY_ALLOC_FAILED vdev_id = %d req_id = %d 
561,II,TRAFFIC_ALREADY_REG vdev_id = %d req_id = %d 
562,II,TRAFFIC_DISABLED  vdev_id = %d req_id = %d 
563,IIIII,TRAFFIC_REG_INVALID_INFO  vdev_id = %d req_id = %d rx_thresh  %d tx_thresh = %d vtraffic_mon = 0x%x 
564,IIIIII,TRAFFIC_BYTES_START_CALC actual_rx_bytes = %d total_rx_bytes = %d rx_throughput = %d actual_tx_bytes = %d total_tx_bytes = %d tx_throughput = %d 
565,IIII,TRAFFIC_BYTES_CALC_FAILED is_associated = %d,is_enabled = %d, wlan_peer = 0x%x wal_peer = 0x%x 
566,,TRAFFIC_BYTES_CALC_FAILED traffic_mon is null 
567,IIII,TRAFFIC_MON_POST_PWR_CHNG vdev_id = %d, macid = %d, is_suspend = %d, mon_time = %d 
568,IIII,TRAFFIC_MON_PRE_PWR_CHNG vdev_id = %d, macid = %d, is_suspend = %d, mon_time = %d 
569,I,TRAFFIC_MEMORY_CORRUPTED 0x%x 
570,IIIIIIII,TRAFFIC_INFORM_CLIENT vdev_id = %d req_id = %d rx_status_chng = %d rx_thrsh = %d rx_throughput = %d, tx_status_chng = %d tx_thrsh = %d tx_throughput = %d 
577,II,wlan_est_linkspeed_vdev_en_dis vdev_id = %d 0x%x 
576,IIII,wlan_est_linkspeed_chan_time_end chan_mhz 0x%x chan_dur_us 0x%x busy_time_us 0x%x accu_idle_dur_us 0x%x 
575,II,wlan_est_linkspeed_indicate_home_chan_update chan_mhz 0x%x home_chan_added 0x%x 
574,II,wlan_est_linkspeed_vdev_evt_handler vdev_id = 0x%x, evt = 0x%x 
573,III,wlan_est_linkspeed_wal_pdev_evt_handler event 0x%x, new_power_state 0x%x, cur_power_state 0x%x 
573,III,wlan_est_linkspeed_wal_pdev_evt_handler event 0x%x, new_power_state 0x%x, cur_power_state 0x%x 
572,IIIIII,wlan_peer_calc_est_linkspeed vdev_id %d, est_link_speed_kbps 0x%x, idle_time 0x%x, sample_time 0x%x, tx_bytes 0x%x, tx_time 0x%x 
571,III,wlan_peer_calc_est_linkspeed2 goodput 0x%x, inst_linkspeed 0x%x, inst_linkspeed_kbps 0x%x 
597,II,RSSI_MONITOR_ARBITER: vdevid=%d, current_rssi=%u 
596,IIIIIII,RSSI_MONITOR_ARBITER: vdevid=%d, client=%u, rssi_threshold_type=%u, low_rssi_threshold=%u, high_rssi_threshold=%u, configure_low_rssi_thresh=%u, configure_high_rssi_thresh=%u 
595,IIIIII,RSSI_MONITOR_ARBITER_CONFIG_HW: vdevid=%d, configure_low_rssi_thresh=%u, final_low_rssi_thresh=%u, configure_high_rssi_thresh=%u, final_high_rssi_thresh=%u, rssi_weight=%u 
594,II,RSSI_MONITOR_CHECK_AND_DELIVER_EVENT: vdevid=%d, current_rssi=%u 
593,IIII,rssi_cmb_offset_correction, ch_idx:%d cmb_rssi:%d ch_rssi:%d, avg_dlt:%d 
592,,rssi_cmb_offset_correction, high delta! 
591,IIII,RSSI_MONITOR_DELIVER_EVENT: vdevid=%d, client=%u, evt_type=%u, cb_fn=%#x 
590,III,RSSI_MONITOR_DISABLE_THRESHOLDS_CLIENT_REQ: vdevid=%d, client=%u, rssi_threshold_type=%u 
589,II,RSSI_MONITOR_DISABLE_THRESHOLDS_CLIENT_REQ_ERR(!vdev_rssi_monitor): vdevid=%d, client=%u 
588,IIIII,RSSI_MONITOR_ENABLE_THRESHOLDS_CLIENT_REQ: vdevid=%d, client=%u, rssi_threshold_type=%u, low_rssi_threshold=%u, high_rssi_threshold=%u 
587,II,RSSI_MONITOR_ENABLE_THRESHOLDS_CLIENT_REQ_ERR(!vdev_rssi_monitor): vdevid=%d, client=%u 
586,II,RSSI_MONITOR_ENABLE_THRESHOLDS_CLIENT_REQ_ERR(!client_data): vdevid=%d, client=%u 
585,III,RSSI_MONITOR_GET_BEACON_RSSI_AVG: vdevid=%d, rssi_avg=%d, mac_id=%d 
584,II,RSSI_MONITOR_HW_EVENT: vdevid=%d, event_type=%u 
583,I,RSSI_MONITOR_HW_EVENT(!low_rssi_threshold_configured): vdevid=%d 
582,I,RSSI_MONITOR_HW_EVENT(!high_rssi_threshold_configured): vdevid=%d 
581,IIIIII,RSSI_MONITOR_UPDATE_BEACON_RSSI: vdevid=%d, mac_id=%u, rssi_last=%u, rssi_avg_last=%d rssi_new=%d rssi_avg_new=%d 
581,IIIIII,RSSI_MONITOR_UPDATE_BEACON_RSSI: vdevid=%d, mac_id=%u, rssi_last=%u, rssi_avg_last=%d rssi_new=%d rssi_avg_new=%d 
580,II,RSSI_MONITOR_VDEV_EVENT: vdevid=%d, notif=%u 
579,I,RSSI_MONITOR_VDEV_FREE: vdevid=%d 
578,I,RSSI_MONITOR_VDEV_INIT: vdevid=%d 
598,III,TBD: NULL pointer passed. wal_peer: 0x%x wlan_peer: 0x%x wlan_vdev: 0x%x 
599,I,THERMAL_MGR_THRESH_CROSSED %d 
600,I,THERMAL_MGR_NEW_THRESH %d 
601,I,THERMAL_MGR_THRESH_READ  %d 
602,, SET GTX PARAM from WMI is not supported  
603,III,LIMIT_OFFCHAN_ARBITER_RESULT flag=0x%x max_offchan_time=%d rest_time=%d 
604,IIII,LIMIT_OFFCHAN_ARBITER client=%d flag=0x%x max_offchan_time=%d rest_time=%d 
605,III,vdev_set_mandatory_ie_by_band: ie_id=%d, band=%d, id_len=%d 
606,II,VDEV_OCE_FLAGS vdev_id %d flags 0x%x 
607,II,wlan_vdev_migrate vdev_id[31-16]/from_mac[15-8]/to_mac[7-0] 0x%x, is_up[23-16]/mode[15-8]/submode[7-0] 0x%x 
608,II,wlan_vdev_unit_test: vdev_id = %d, cmd = WMI_VDEV_PARAM_ABG_MODE_TX_CHAIN_NUM, value = 0x%x 
609,I,LIMIT_OFFCHAN_ERROR vdev_id=%d 
610,I,LIMIT_OFFCHAN_ERROR client_id=%d 
611,IIII,WMI RSSI breach config: vdev %d enabled_bitmap 0x%x high_rssi %ddBm low_rssi %ddBm 
612,III,WMI RSSI threshold met: vdev %d evt_type 0x%x cur_rssi %d 
613,I,VDEV_DISPATCH_DISA_FRAME_TX failed status=%d 
614,I,WMI_VDEV_ENCRYPT_DECRYPT_DATA_REQ_CMDID invalid data_len %d 
615,I,WMI_VDEV_ENCRYPT_DECRYPT_DATA_REQ_CMDID invalid vdev_id %d 
616,I,DISA event sent to HOST: frame_len=%d 
617,,Failed to allocate memory for DISA event!!! 
618,III,vdev_set_scan_default_ie status = 0x%x vdev_id=%d prunned_ie_len=%d 
619,IIII,dispatch_set_ie_cmd: ie_id = 0x%x, id_len = %d, source=%d, band=%d 
620,II,vdev_extract_mandatory_ies: id=%d, len=%d 
621,II,vdev_extract_optional_vendor_ies: oui=0x%x, len=%d 
622,I,vdev_set_mandatory_ie: not handled ie_id=%d 
623,II,vdev_set_mandatory_ie: ie_id=%d, id_len=%d 
624,I,dispatch_request_stats_ext_cmd vdev id =%d 
625,I,dispatch_request_stats_ext_cmd invalid vdev id =%d 
626,,dispatch_wmm_delts_cmd: end 
627,II,dispatch_wmm_delts_cmd: ac = %d vdev id = %d 
628,I,WMI_VDEV_GET_ARP_STAT_CMDID: vdev_id = %d event alloc failed 
629,I,WMI_VDEV_GET_KEEPALIVE_CMDID: vdev_id = %d event alloc failed 
630,II,wlan_vdev_tsf_tstamp_action: vdev_id = %d, vdev_ifUp = %d 
631,II,wlan_vdev_tsf_tstamp_action:vdev_id = %d, action = 0x%x 
632,IIIII,wlan_vdev_tsf_report: vdev_id = %d, tsf_low = 0x%x, tsf_high = 0x%x, qtimer_low=0x%x, qtimer_high=0x%x 
633,III,WMI_CMD_PARAMS AC = %d Med-Time usec = %d DwnGrd_Type = %d 
634,II,WAL_DBGID_SET_M4_SENT_MANUALLY  VDEV ID = %d, peer = 0x%x 
635,IIII,VDEV_INSTALL_KEY_FAIL vdev_id %d mac_addr %04x:%08x status %d 
636,III,11w PMF vdevId=%d key_ix=%d cipher=%d 
637,IIII,WMI_VDEV_SET_WMM_PARAMS_CMDID ac[31-16]/acm[15-0] = 0x%x cw_min = 0x%x cw_max = 0x%x txop_limit[31-16]/aifs[15-0] = 0x%x 
638,I,Invalid WAL VDEV in WMI_VDEV_SET_WMM_PARAMS_CMDID, VDEV ID = %d 
639,I,Invalid VDEV in WMI_VDEV_SET_WMM_PARAMS_CMDID, VDEV ID = %d 
640,II,WMI_CMD_PARAMS VdevId/AC/Arg1 = %d Cmd/Med-Time/Action/Arg2 = %d 
641,II,VDEV_STOP_ABORT_TX after_abort, hwq=0x%x, swq=0x%x 
642,II,VDEV_STOP_ABORT_TX abort_succeeds, hwq=0x%x, swq=0x%x 
643,II,VDEV_STOP_ABORT_TX abort_fails, hwq=0x%x, swq=0x%x 
644,II,VDEV_STOP_ABORT_TX try_to_abort, hwq=0x%x, swq=0x%x 
645,III,WAL Peer event Vdev ID = %d HW Q depth= %d, SW Q depth = %d 
646,III,WAL Peer event vdevp %d is_free %d, is_vdev_stopping %d 
647,III,VDEV free error, peer addr:0x%x, mac:0x8x 0x8x 
648,II,VDEV_MGR_STA_PS_EVENT: vdev_id=%d, event_type=%d 
649,III,WMI_VDEV_PARAM_ABG_MODE_TX_CHAIN_NUM: vdev_id = %d, tx_chains_num_11b = %d, tx_chains_num_11ag = %d 
650,II,WMI_VDEV_PARAM_SMPS_INTOLERANT: vdev_id:%d, param:%d 
651,III,WMI_VDEV_PARAM_DISABLE_NOA_P2P_GO ic_mode:%d ic_subopmode:%d param:%d  
652,III,WLAN_VDEV_SET_PARAM_FAIL3 paramid:%d vdevp:0x%x vdevp->bss:0x%x 
640,II,WMI_CMD_PARAMS VdevId/AC/Arg1 = %d Cmd/Med-Time/Action/Arg2 = %d 
653,II,VDEV_DOWN_ASSERT curr_tsf_63_32=0x%x,curr_tsf_31_0=0x%x 
654,IIII,VDEV_DOWN_ASSERT del_req_tsf_63_32=0x%x,del_req_tsf_31_0=0x%x,del_conf_tsf_63_32=0x%x,del_conf_tsf_31_0=0x%x 
655,IIII,VDEV_DOWN_ASSERT create_by=%d,delete_by=%d,create_tsf_63_32=0x%x,create_tsf_31_0=0x%x 
656,II,VDEV EVT: vdev down id=%d, mode=%d 
657,I,VDEV RESMGR_LINK_ATTR_SMPS_VALID VHT mode:%d 
658,I,VDEV RESMGR_LINK_ATTR_SMPS_VALID Peer_flags:%d 
659,II,VDEV_MGR_VDEV_UP id=%d, mode=%d 
660,IIII,VDEV_MGR_VDEV_START  vdev_id = 0x%x chan_mhz = %d mode = 0x%x sub_mode = 0x%x 
661,III,VDEV_MGR_HP_START_TIME  vdev_id = 0x%x chan_mhz = %d start_tsf = 0x%x 
662,IIIIII,VDEV_START: vdev_id[31-24]/mode[23-16]/mode[15-8]/mac_id[7-0] = 0x%x chan_mhz = %d  phy_mode=%d band_center_freq1=%d band_center_freq2=%d ldpc_rx_enabled=%d 
663,,Disable NAN on deleting the last non-NAN vdev 
664,II,VDEV EVT: vdev delete id=%d, mode=%d 
665,I,NAN vdev(id = %d) Delete indication OK to send 
666,III,VDEV EVT: WMI_VDEV_DELETE_RESP_EVENTID vdevId=%d vdev_type: %d vdev_subtype: %d 
667,IIIII,VDEV EVT peer not cleared idx=%d vdev_id = %d mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x usage_count = %d 
668,II,VDEV EVT:RT thread handle vdev_stop_down_del cmd:%d, vdev_id:%d 
669,III,VDEV EVT:BE thread handle vdev_stop_down_del msg cmd = %d, vdev_id = %d, vdev_mode = %d 
670,III,VDEV EVT: vdev create id=%d, mode=%d submode=%d 
671,III,VDEV_MGR loopback cal  vdev_id = 0x%x cal_time = %d do_noa = %d 
672,II,VDEV_MGR loopback cal  vdev_id = 0x%x cur_policy_mgr_hw_mode = %d 
673,III,set_restore_mac_addr status = %d, freq = %d, evh = 0x%x 
674,I,allow during connecting, subtype:%x 
675,,vdev connecting client is registered in non wow mode 
676,,WLAN_VDEV_NOTIF_ROGUE_AP_IE2_DETECTED  
677,,WLAN_VDEV_NOTIF_ROGUE_AP_IE1_DETECTED 
678,IIIIII,VENDOR SPECIFIC IE :%u, %u, %02x, %02x, %02x, %02x 
679,I,oui_action_matched %x 
680,II,Capability mismatch %x != (%x) 
681,III,%d byte fail to match for mac address.                                actual_mac = %d, Configured mac = %d 
682,III,%d byte fail to match for data.                                        actual_data %d, configured data %d 
683,III,action bitmask of %dth OUI is %x and oui matched is %x 
684,I,FILS_DISCOVERY Stopped on vdev_id = %d 
685,I,FILS_DISCOVERY Started on vdev_id = %d 
686,I,wlan_vdev_get_migrate_active_vdev_list  vdev_id_list=0x%x 
687,II,wlan_vdev_fill_vdev_mac_entry: vdev_id=%d, pdev_id=%d 
688,II,Received IBSS Beacon peer = 0x%x send_to_host =  
689,IIIIIII,VDEV_MGR_MY_BEACON_RECEIVED: vdev_id = %d curr_time = 0x%x  curr_vdev_tsf = 0x%x seq = 0x%x rssi = 0x%x bss_ch = %d recv_ch = %d 
690,III,VDEV_MGR_MY_BEACON_BAD_IE id=%d,len=%d,status=0x%x 
691,III,VDEV_MGR_MY_BEACON_PARSED malformed id = %d len=%d remain_len=%d 
692,II,VDEV_HDL_OWN_BEACON neighbor report not offloaded yet %d %d 
693,I,VDEV_HDL_OWN_BEACON  0x%x 
691,III,VDEV_MGR_MY_BEACON_PARSED malformed id = %d len=%d remain_len=%d 
690,III,VDEV_MGR_MY_BEACON_BAD_IE id=%d,len=%d,status=0x%x 
691,III,VDEV_MGR_MY_BEACON_PARSED malformed id = %d len=%d remain_len=%d 
694,I,number_of_configured_oui = %d 
695,I,VDEV_MGR_BCN_IN_SYNC: vdev_id = %d  
696,I,VDEV_MGR_FINAL_BMISS_DETECTED: vdev_id = %d 
697,I,VDEV_MGR_FIRST_BMISS_DETECTED: vdev_id = %d 
698,IIIII,VDEV_MGR_AP_KEEPALIVE_INACTIVE  vdev_id = %d cur_txrx_ref_time = 0x%x last_txrx_time = 0x%x last_tx_time = 0x%x last_rx_time = 0x%x 
699,,[NDI Keep Alive] send NDP END event to HOST 
700,,[NDI Keep Alive] send activity probe frame 
701,III,[NDI Keep Alive] last_txrx_time = 0x%x now = 0x%x inactivity_gen = %d 
702,III,IBSS Keep Alive  rx_last_activity = 0x%x ibss_max_bcn_lost_uses = 0x%x current time = 0x%x 
703,IIII,VDEV_MGR_AP_KEEPALIVE_UNRESPONSIVE  vdev_id = %d assoc_id = 0x%x inact_gen = 0x%x n_buffered_mpdu = 0x%x 
704,IIII,VDEV_MGR_AP_KEEPALIVE_INACTIVE  vdev_id = 0x%x assoc_id = 0x%x inact_gen = 0x%x n_buffered_mpdu = 0x%x 
705,IIII,VDEV_MGR_AP_KEEPALIVE_IDLE  vdev_id = %d assoc_id = 0x%x inact_gen = 0x%x n_buffered_mpdu = 0x%x 
706,,vdev_bmiss_crit_ch_req_cb: ch_req completed without receiving beacon 
707,,vdev_bmiss_crit_ch_req_cb: ch_req granted 
708,III,VDEV_MGR_HP_START_TIME: vdev_id = %d, chan_mhz = 0x%x, start_tsf = 0x%x 
709,III,VDEV_MGR_OFF_CHAN_GO_CH_REQ_SETUP: tbtt_pre_slop = 0x%x, tbtt_post_slop = 0x%x, go_quota_remain = 0x%x 
710,II,VDEV_MGR_OFF_CHAN_GO_CH_REQ_SETUP: tbtt_diff1 = 0x%x, tbtt_diff1 = 0x%x 
711,IIII,VDEV_MGR_OFF_CHAN_GO_CH_REQ_SETUP: curr_tsf = 0x%x, next_tbtt = 0x%x, go_time_to_tbtt = 0x%x, sta1_time_to_tbtt = 0x%x 
712,II,VDEV_MGR_OFF_CHAN_GO_CH_REQ_SETUP: vdev_id = %d, go_chan_quota_per_bi = 0x%x 
713,IIIII,VDEV_MGR_AP_TBTT_CONFIG: vdev_id =%d, chan_mhz = 0x%x, tbtt_link_type = 0x%x, ni_intval = 0x%x, tbtt_offset = 0x%x 
714,III,Corr_sta_tbtt_drift: vdev_id = %d, chan_mhz = 0x%x, start_tsf = 0x%x 
715,III,wlan_vdev_sta_concurrency_event_handler: vdev_id = %d, next_state  = 0x%x, cur_state = 0x%x 
716,IIII,VDEV_MGR AP Connection protection critical channel request: vdev_id = %d, chan_mhz = 0x%x, start_tsf = 0x%x, duration = %d 
717,,VDEV_MGR_FIRST_BMISS_DETECTED: Post Critical ch_req 
718,III,VDEV_MGR_OCS_HP_LP_REQ_POSTED: vdev_id = %d, hp_ch_req = 0x%x, lp_ch_req = 0x%x 
719,II,VDEV_MGR_LOWPOWER_LP_CHREQ_ENABLED: vdev_id = %d, factor = 0x%x 
719,II,VDEV_MGR_LOWPOWER_LP_CHREQ_ENABLED: vdev_id = %d, factor = 0x%x 
720,III,VDEV_MGR_HP_START_TIME: vdev_id = %d, chan_mhz  = 0x%x, start_tsf = 0x%x 
721,II,VDEV_MGR_LOWPOWER_HP_CHREQ_ENABLED: vdev_id = %d, chan_mhz  = 0x%x 
722,I,wlan_vdev_up_ch_req_setup noA_disableEnable_P2pgo:%d  
723,I,WLAN_VDEV_DPD_CAL_START vdev_id:%d 
724,I,VDEV_MGR_VDEV_START_OCS_HP_REQ_STOP: vdev_id = %d 
725,I,VDEV_MGR_PEER_AUTHORIZED: vdev_id = %d 
726,I,VDEV_MGR_FIRST_BCN_RECEIVED: vdev_id = %d 
724,I,VDEV_MGR_VDEV_START_OCS_HP_REQ_STOP: vdev_id = %d 
727,I,VDEV_MGR_VDEV_START_OCS_HP_REQ_COMPLETE: vdev_id = %d 
728,II,VDEV_MGR_VDEV_START_OCS_HP_REQ_COMPLETE without VDEV UP: vdev_id = %d, ch_req_flag = 0x%x 
729,II,WMI_EVENT_SEND: vdev_id = %d, opmode = %d, event = WMI_VDEV_START_RESP_EVENTID 
730,II,WMI_EVENT_ALLOC_FAILURE: vdev_id = %d, opmode = %d, evt_id = WMI_VDEV_START_RESP_EVENTID 
731,II,WLAN_VDEV_DPD_CAL_DONE vdev_id:%d ch:%d 
732,IIIII,VDEV_MGR_AP_TBTT_CONFIG: vdev_id = %d, chan_mhz = 0x%x, tbtt_link_type = 0x%x, ap_tbtt_offset = 0x%x 
733,I,no_null_to_ap_for_roaming=%d 
734,I,enable_null_leaky_ap_pause=0x%x 
735,II,Disable leaky AP CTS2S: vdev_id = %d pause_delay_us = %d  
736,,VDEV_MGR_VDEV_PAUSE csa_roaming_ongoing and no host unpause 
737,,VDEV_MGR_VDEV_PAUSE unpause non_protocol_unpaused 
738,I,VDEV_UNPAUSE_FAIL: ifPaused not set with pause_bitmap = 0x%x in _wlan_vdev_unpause 
739,IIII,VDEV_MGR_VDEV_PAUSE: enable_null_leaky_ap_pause=0x%x no_null_to_ap_for_roaming=%d leakyAp_cts2s_enable=%d pause_delay_us=%d 
740,,VDEV_PAUSE_FAIL ifPaused set with pause_bitmap = 0 in _wlan_vdev_pause 
741,I,vdev->bcn_tx_paused_wlan_vdev_pause_1=0x%x 
742,II,VDEV Unpause Failure: VDEV ID = %d pause_bitmap = 0x%x in Unpause complete 
743,IIII,VDEV_MGR_VDEV_PAUSE_DELAY_UPDATE: vdev_id = %d avg_data_null_tx_delay = %d avg_rx_leak_window = %d pause_delay_us = %d 
744,IIIII,VDEV_MGR_VDEV_PAUSE_COMP: vdev_id = %d pause_status = SUCCESS data_null_tx_delay = %d avg_data_null_tx_delay = %d actual_leak_window = %d avg_rx_leak_window = %d 
745,IIIII,VDEV_MGR_VDEV_PAUSE_COMP: vdev_id = %d pause_status = FAILURE data_null_tx_delay = %d avg_data_null_tx_delay = %d actual_leak_window = %d avg_rx_leak_window = %d 
746,IIII,VDEV_MGR_VDEV_PAUSE_COMP: vdev_id = %d pause_status = LEAKY AP DETECTED data_null_tx_delay = %d actual_leak_window = %d pause_delay_us = %d 
747,III,COEX_MWS_OTHER: [SAR] WMI callback - error in parsing cmd(0x%x) buffer(0x%x) len(%d) 
748,IIIII,WLAN_MODULE_COEX: [SAR] band_id=0x%x, chain_id=0x%x, mod_id=0x%x, limit_value=0x%x validity_bitmap=0x%x 
749,III,COEX_MWS_OTHER: [SAR] sar_enable=0x%x, num_limit_rows=0x%x commit_limits=0x%x 
750,II,WLAN_COEX_SLEEP: Received WOW Entered/Exit event from OffloadMgr %d,                                                        pCOEX->is_wow_entered = %d 
751,II,COEX_GENERIC_ERROR: Set TDM Guard Period to %d, Error (0x%x) 
752,II,COEX_BT_ACTIVITY: prof_bitmap(0x%x), scan_bitmap(0x%x) 
753,,COEX_MWS_ANT_DIVERSITY: CHMMGR_HW_MODE_CHANGE_PRE_NOTIFY 
754,,COEX_MWS_ANT_DIVERSITY: CHMMGR_TX_CHM_CHANGED 
755,II,COEX_MWS_ANT_DIVERSITY: [Warr] chnmsk completed but ReqId:%d not matched with RespId:%d 
756,IIII,COEX_MWS_ANT_DIVERSITY: chnmsk completed Rx:0x%x, Tx:0x%x, Cal:%d, ReqId:%d 
757,IIIIIII,COEX_MWS_ANT_DIVERSITY: Chainmask Req Fail(%d):Rx:0x%x, Tx:0x%x, RxNSS:0x%x, SMPS_Diff:%d, ReqId:%d, Cal:%d 
758,IIIIII,COEX_MWS_ANT_DIVERSITY: Chainmask Req:Rx:0x%x, Tx:0x%x, RxNSS:0x%x, SMPS_Diff:%d, ReqId:%d, Cal:%d 
759,,COEX_GENERIC_ERROR: COEX_ERROR_VDEV_MGR_REGISTER_FAIL 
760,I,WLAN_COEX_VDEV: wlan_swbmiss_bcn_evt_register failed with rc=0x%x 
761,I,WLAN_COEX_MCS_RATE: wal_vdev_t is NULL, min allowed mcs: %u 
762,I,COEX_MWS_OTHER: Limit_MCS_RATE:%u 
763,I,WLAN_COEX_SET_SWBMISS: wlan_vdev_t is NULL, enable: %u 
764,II,COEX_GENERIC_ERROR: ERROR: VDEV couldn't be found for the COEX PDEV to Enable/Disable NULL for Leaky AP Pause !                                                                             vdev_id = %d, pCOEX->pdev = 0x%08x 
765,II,COEX_GENERIC_ERROR: Enable/Disable NULL for Leaky AP Pause Request sent to VDEV/OCS_MGR !                                                                             vdev_id = %d, enable_null_pause = %d 
766,,COEX_GENERIC_ERROR: Disable NULL for Leaky AP Pause due to Scan Stop ! 
767,,COEX_GENERIC_ERROR: Enable NULL for Leaky AP Pause due to Scan Start during A2DP ! 
768,I,COEX_GENERIC_ERROR: COEX_ERROR_UNKNOWN_NULLPTR Status(%u) 
769,IIIIIIIII,WLAN_COEX_SLEEP: status(%u) enable(%u) mac(%u) reason(%u) dup(%u) coex_on(%u) mws_fwk_enable(%u) btc_fwk_reason(%u) psp_allow_sleep(%u) 
770,III,WLAN_COEX_VDEV_PAUSE: wlan_vdev_t is NULL, max_time: %u, Pause: %u, SoftAPCtrl: %u 
771,,COEX_MWS_OTHER: [SAR] deprecated SAR limit command was triggered 
772,IIIII,COEX_GENERIC_ERROR: frameType 0x%x vdev %d txSt 0x%x flush %d consFlshCnt %d 
773,,COEX_GENERIC_ERROR: [SAR][Error] cannot get correct number of SAR limits from FW to send to host 
774,,COEX_GENERIC_ERROR: [SAR][Error] cannot get SAR limits from FW to send to host 
775,,COEX_REPORT_BT_INFO_ALLOCATION_FAILED:  WMI EVT CLASS LOW Allocation faliure  
776,II,WLAN_COEX_CTS2S_TIMEOUT: Now : %u, WbPrepare: %u 
793,,WLAN_MODULE_COEX: [GNSS COEX] Critical demod ENTRY msg received 
792,,WLAN_MODULE_COEX: [GNSS COEX] Critical demod EXIT msg received 
791,,WLAN_MODULE_COEX: [GNSS COEX] Critical demod INVALID msg received 
790,IIIII,COEX_PSP_STAT_1: Resp0(%u) Resp1(%u) Resp2(%u) Resp3(%u) Resp4(%u) 
789,IIIII,COEX_PSP_STAT_2: DP(%u) Max(%u) RespIdx(%u) ValidDps(%u) PsPAvg(%u) 
788,I,COEX_PSP_ERROR: COEX_PSP_ERROR_VDEV_NULL Stimulus(%u) 
787,II,COEX_PSP_ERROR: COEX_PSP_ERROR_COEX_PSP_ENTRY Stimulus(%u) State(0x%x) 
786,,COEX_PSP_ERROR: COEX_PSP_ERROR_COEX_PSP_EXIT 
785,,COEX_PSP_ERROR: COEX_PSP_ERROR_READY_DISABLED 
784,IIIII,COEX_PSP_RX_STATUS_STATE_1: ExpTS(%d) ActTS(%d) IsOverRun(%u) RespOverUnderRunTime(%d) ApResponseRxDuration(%u) 
780,,COEX_PSP_SEND_PSPOLL: 0 
783,IIII,COEX_PSP_NONWLAN_INTERVAL: BaseIntrvl(%u) NonWlanIdleTime(%u) PsPollSpecInterval(%u) ApResponseTimeout(%u) 
782,II,COEX_PSP_SEND_PSPOLL: State(0x%x) PSPNum(%u) 
780,,COEX_PSP_SEND_PSPOLL: 0 
781,IIIII,COEX_PSP_READY_STATE: T2NonWlan(%u) EndTS(%d) MoreData(%u) ExpTS(%d) NonWlanIdleTime(%u) 
780,,COEX_PSP_SEND_PSPOLL: 0 
779,IIIIII,COEX_PSP_SPEC_POLL: En(%u) Count(%u) TS(%u) AllowSpecPsPollTx(%u) Delta(%u) Intrvl(%u) 
778,III,COEX_PSP_SEND_PSPOLL: status(0x%x) PsPollState(0x%x) PsPollNum(%u) 
777,,COEX_MWS_ANT_DIVERSITY: 0x4001 
804,,COEX_GENERIC_ERROR: Defer the Disable NULL for Leaky AP Pause due to A2DP Stop during Scan to SCAN_COMPLETE ! 
803,,COEX_GENERIC_ERROR: Enable NULL for Leaky AP Pause due to A2DP Start during Scan ! 
802,IIIIII,WLAN_COEX_OCS_MGR: Stimulus(%u) Status(%u) State(0x%x) ExpBtStartTime(%d) now(%u) delta(%d) 
801,IIIIIII,WLAN_COEX_OCS_RECOMP: State(0x%x) A2dpCrit(%u), ExpBtStartTime(%u), ExpBtStartTimeUT(%u), now (%u) delta(%d) delta_ut(%d) 
800,I,WLAN_OCS_REQ: OCS Update: VDEV Restart OCS Requests sent to VDEV/OCS_MGR for vdev_id = %d 
799,I,WLAN_OCS_REQ: ERROR - OCS Update: PDEV couldn't be found for the COEX VDEV id %d ! 
798,,WLAN_OCS_REQ: OCS Start: No mac operating in 2G 
797,III,WLAN_OCS_REQ: OCS Start: COEX_OCS_START_ERROR (0x%x), ocs_req_state(0x%x) bt_req(0x%x) 
797,III,WLAN_OCS_REQ: OCS Start: COEX_OCS_START_ERROR (0x%x), ocs_req_state(0x%x) bt_req(0x%x) 
796,,WLAN_OCS_REQ: OCS Update: No mac operating in 2G 
795,III,WLAN_OCS_REQ: OCS Update: COEX_OCS_UPDATE_ERROR (0x%x), ocs_req_state(0x%x) bt_req(0x%x) 
794,II,WLAN_MODULE_COEX: COEX_GENERIC_ERROR  0x%x 0x%x 
805,,BTM_OFLD solicited deinit 
806,,BTM_OFLD deinit 
807,II,BTM_OFLD Solicited btm enable: timeout=%d max_attemp_cnt=%d 
808,,BTM_OFLD Solicited btm disable 
809,III,BTM_RESPONDED_SUCCESS vdev_id = %d status_code = 0x%x dialog_token = %d 
810,III,BTM_MEMORY_FAILED vdev_id = %d, status_code = %d dialog_token = %d 
811,III,BTM_MEMORY_FAILED vdev_id = %d, status_code = %d, dialog_token = %d 
812,,BTM_VDEV_FAILED_TO_SEND_RESPONSE_AFTER_DELAY 
813,,BTM_OFLD_ENABLE_ROAM 
814,I,BTM_OFLD_STICKY_TS vdev_conn=%d 
815,II,BTM_OFLD Rx BTM Request: seq_no = %d, dialog token = %d 
816,II,BTM_OFLD Dont handle new Req: prev Req processing is in progress. prev_DT = %d, cur_DT = %d) 
817,II,BTM_OFLD enable: flags=0x%x sticky_time=%d 
818,II,BTM_OFLD BTM_Query Completion Status: %d, Dialog Token: %d 
819,II,BTM_OFLD_INVOKE_ROAM_CB status=%d sticky_sec=%d 
820,IIIIIII,BTM_REQUEST_INFO_1 roam_status = 0x%x, is_btm_cnd_match_roam_cache = %d, scan_action = 0x%x, roam_scan_type = 0x%x status_code = %d num_bssid = %d match_cnd_cnt = %d 
821,IIIII,BTM_CANDIDATE_INFO chan = %d bssid = %08x%04x pref = %d cnd_cnt = %d 
822,IIIIIIII,BTM_REQUEST_INFO vdev_id = %d, opmode = %d, flags = 0x%x num_cnd = %d, max_pref = %d, mode = 0x%x home_bssid = %08x%04x 
823,III,BTM_OFLD_QUERY_TS ind_code=%d,curr_attempt_cnt=%d,max_attempt=%d 
808,,BTM_OFLD Solicited btm disable 
824,,BTM_OFLD Solictied BTM in progress 
825,,BTM_OFLD Solictied BTM disable 
826,,BTM_OFLD not init 
827,III,BTM_CND_LIST %08x%04x pref %d 
828,II,BTM_SEND_RESPONSE_DELAY vdev_id = %d, status_code = 0x%x  
829,,BTM_VDEV_FAILED_TO_SEND_RESPONSE 
830,II,BTM_OFLD BTM_Response Completion Status: %d, Dialog Token: %d 
831,II,MLME_PROCESS_DEAUTH roam_state=%d, mlme_state=%d 
832,II,MLME_PROCESS_DISASSOC roam_state=%d, mlme_state=%d 
833,,WLAN_MLME_SYNC_TIMEOUT 
834,,WMI_ROAM_SYNCH_FRAME_EVENTID evt2 alloc failed 
835,,WMI_ROAM_SYNCH_FRAME_EVENTID evt1 alloc failed 
836,IIII,MLME_SYNC_REPLAY_COUNT_U32 0x%02x%02x%02x%02x 
837,IIII,MLME_SYNC_REPLAY_COUNT_L32 0x%02x%02x%02x%02x 
838,I,MLME_SUBNET_CHANGE_STATUS %d 
839,I,mlme_sync_alloc_fail %d 
840,IIIII,mlme_sync vdev_id=%d, old_hw_mode=%d new_hw_mode=%d auth_status=%d size = %x 
836,IIII,MLME_SYNC_REPLAY_COUNT_U32 0x%02x%02x%02x%02x 
837,IIII,MLME_SYNC_REPLAY_COUNT_L32 0x%02x%02x%02x%02x 
838,I,MLME_SUBNET_CHANGE_STATUS %d 
839,I,mlme_sync_alloc_fail %d 
841,IIIIII,mlme_sync vdev_id=%d, old_hw_mode=%d new_hw_mode=%d auth_status=%d size = %x, req_hw_mode=%d 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
843,I,MLME_DEBUG_CMN  0x%x 
843,I,MLME_DEBUG_CMN  0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
844,I,add_bcn_prb: bcn_prb_len 0x%x 
845,II,add_reassoc_req: reassoc_req_len 0x%x reassoq_frame 0x%x 
846,II,MLME_WMI_SEQ_UPDATE_SESSION_COMP: ret=0x%x last_index=0x%x 
847,I,MLME_WMI_EVENT_FILTER: ret=0x%x  
848,II,MLME_WMI_SEQ_DELETE_SESSION_COMP: ret=0x%x last_index=0x%x 
849,I,MLME_INSTALL_KEY key_type=%d 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
850,I,MLME_WMI_SEQ_UPDATE_SESSION: seq_id=0x%x 
851,I,MLME_WMI_SEQ_DEL_SESSION: seq_id=0x%x 
852,I,MLME_WMI_SEQ_ABORT: seq_id=0x%x 
853,IIIII,MLME_UPDATE_FREQ_PHYMODE_CH_WIDTH mhz=%d freq1=%d freq2=%d phymode=%d ch_width=%d 
854,IIII,MLME_UPDATE_FREQ_PHYMODE_CH_WIDTH phymode==MODE_UNKNOWN mhz=%d freq1=%d freq2=%d phymode=%d 
855,IIIIIII,MLME_DEBUG_CMN  0x%x 0x%x 0x%x 0x%x 0x%x 0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
856,I,MLME_WMI_CMD_RPOXY cmdid=0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
857,,mlme_del_session: in delete 
858,,wlan_mlme_install_key session not found 
859,,wlan_mlme_install_key invalid param 
860,IIII,MLME_GTK_OFFLOAD_DEL_IN_PROGRESS peer_addr %08x04x vdev_id %d enable %d 
861,IIII,MLME_GTK_OFFLOAD_KEY_NOT_FOUND peer_addr %08x04x vdev_id %d enable %d 
862,IIII,MLME_GTK_OFFLOAD_INVALID_SESSION peer_addr %08x04x vdev_id %d enable %d 
863,III,MLME_GTK_OFFLOAD_INVALID peer_addr 0x%x vdev 0x%x enable %d 
864,III,MLME_UPDATE_RIC_ADD index = %d ts_info = 0x%x rde_ie = %d 
865,III,MLME_UPDATE_RIC_TRY_SLOT small_up_index = %d, user_priority = %d < %d 
866,I,MLME_UPDATE_RIC_FIND_SLOT index = %d 
867,I,MLME_UPDATE_RIC_REPLACE index = %d 
868,I,MLME_UPDATE_RIC_DELETE index = %d 
869,IIIII,MLME_UPDATE_RIC_CFG ts_info = 0x%x user_priority = 0x%x tsid = 0x%x direction = 0x%x is_add = %d 
870,III,MLME_SET_ROAM_STATUS prev_state=%d cur_state=%d is_eap1x_recv=%d 
871,III,MLME_DEBUG_CMN  0x%x 0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
872,I,min_ext_caps %d 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
857,,mlme_del_session: in delete 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
873,,mlme_update_session: in update 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
874,II,mlme_ft_add_ss curr_op_cls=%d smps=%d 
875,I,MLME_FT_ADD_SESSION  buf_len:0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
871,III,MLME_DEBUG_CMN  0x%x 0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
876,III,MLME_INIT_CFG cap=0x%x,11r=%d,cckm=%d 
877,,MLME_INIT_CFG offld_param null 
878,,MLME_INIT_CFG param null 
871,III,MLME_DEBUG_CMN  0x%x 0x%x 0x%x 
871,III,MLME_DEBUG_CMN  0x%x 0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
879,IIIII,MLME_REASSOC_1x1 freq=%d ht_caps=%d,%d vht_caps=%d,%d 
871,III,MLME_DEBUG_CMN  0x%x 0x%x 0x%x 
880,III,MLME_DEBUG_CMN  0x%x 0x%x 
881,,wlan_mlme_reassoc_process_rsp  FILS: AEAD decryption of reassoc rsp failed 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
882,II,MLME_REASSOC_SEND ppdu_info=0x%x mac=%d 
883,,MLME_REASSOC_SEND tx fail 
884,,MLME_REASSOC_SEND no abf 
885,I,MLME_REASSOC_SEND invalid vdev=%d 
886,,MLME_REASSOC_SEND invalid vdev 
888,IIII,MLME_PREAUTH_SEND_HNDL  comp_status=0x%x, mlme_session_ctxt=0x%x(0=invalid), session_valid=%d(255=invalid), mlme_state=%d(255=invalid) 
887,IIII,MLME_REASSOC_SEND_HNDL  comp_status=0x%x, mlme_session_ctxt=0x%x(0=invalid), session_valid=%d(255=invalid), mlme_state=%d(255=invalid) 
889,II,wlan_pdev_update_pmk_cache  num_cache = %d op_flag = 0x%x 
890,IIII,Current IP address %d %d %d %d 
891,,no hlp_pkt_param 
892,,hlp_buf_len 0  
893,II,mlme_cfg_ctx->fils_ap_conn_profile.buf_len %x pkt_type %d 
894,,hlp_pkt_len is > 512 
895,,wlan_pdev_update_fils_hlp mlme_cfg_ctx is null 
896,I,wlan_pdev_update_fils_hlp vdev is null for vdev_id = %d 
842,II,MLME_DEBUG_CMN  0x%x 0x%x 
897,,FILS: PMK cache not found 
898,I,FILS: rmsk len - %d 
899,I,FILS_PMKID_MATCH pmkid_match %d 
900,,FRMPARSE_FILS_PMKID_MISMATCH 
901,II,FRMPARSE_FILS_RSN_PMKID_INVALID pmk 0x%x or num_pmkid %d 
902,I,FILS_WPA_RSN_IE_PARSE ie_status %d 
903,I,FILS_RSN_IE_PARSE ie_status %d 
904,,MLME_SUPPL_DISCONN 
905,II,MLME_SUPPL_DISCONN_INVALID 0x%x 0x%x 
906,,MLME_SUPPL_CONN 
907,II,MLME_SUPPL_CONN_INVALID 0x%x 0x%x 
843,I,MLME_DEBUG_CMN  0x%x 
871,III,MLME_DEBUG_CMN  0x%x 0x%x 0x%x 
908,III,_wlan_mlme_intersect_key_mgmt_type ap_key_mgmt=0x%x user_key_mgmt=0x%x key_mgmt=0x%x 
935,IIIII,MLME_PREPARE_PEER_ASSOC vdev_id=%d phy_mode=%d mhz=%d ch_width=%d flags=0x%08x 
934,II,MLME_PREPARE_PEER_ASSOC legatcy_rate[%d]=%d 
933,I,MLME_PREPARE_PEER_ASSOC_HT num_ht_rate=%d 
932,II,MLME_PREPARE_PEER_ASSOC_HT rates[%d]=%d 
931,IIII,MLME_PREPARE_PEER_ASSOC_VHT_PEER tx_hi=%d, rx_hi=%d, tx_mcs=0x%x rx_mcs=0x%x 
930,IIII,MLME_PREPARE_PEER_ASSOC_VHT_SELF tx_hi=%d, rx_hi=%d, tx_mcs=0x%x rx_mcs=0x%x 
929,IIIII,MLME_PREPARE_PEER_ASSOC_VHT_INTERSECT tx_max=%d, rx_max=%d, tx_mcs=0x%x rx_mcs=0x%x,nss=%d 
928,I,MLME_PREPARE_PEER_ASSOC num_legacy_rate=%d 
927,IIIIIII,MLME_PREPARE_WMM_PARAM ac=%d cwmin=%d cwmax=%d aifs=%d txoplimit=%d no_ack=%d acm=%d 
926,IIII,MLME_PREPARE_VDEV_START: chan_mhz = %d, band = %d, vht_cap_ldpc_rx = %d, ht_cap_ldpc_rx = %d 
925,III,MLME_VDEV_PREPARE_START rx_nss=%d,tx_nss=%d,rx_streams=%d 
924,IIII,MLME_GTK_OFFLOAD_CMD vdev_id=%d enable=%d reply_counter = 0x%x 0x%x 
923,IIIII,MLME_VDEV_INSTALL_KEY_CMD vdev_id=%d key_id=%d key_type=%d key_cipher=%d rsc_counter_l=%d 
922,IIII,MLME_PEER_ASSOC_CMD vdev_id=%d ht_caps=0x%08x peer_vht_caps=0x%08x phy_mode=%d 
921,IIII,MLME_PEER_ASSOC_CNF_EVT vdev_id=%d mac_addr=%08x%04x -> ret %d 
920,IIII,MLME_PEER_DELETE_RESP_EVT vdev_id=%d mac_addr=%08x%04x -> ret %d 
919,IIIII,MLME_VDEV_START_RESP_EVT vdev_id=%d, status=0x%x chain_mask=%d smps_mode=%d -> ret %d 
918,III,MLME_VDEV_STOPPED_EVT evt->vdev_id=%d vdev->id=%d ret %d 
917,III,MLME_PEER_CREATE_CMD vdev_id=%d mac_addr=%08x%04x 
916,III,MLME_PEER_DELETE_CMD vdev_id=%d mac_addr=%08x%04x 
915,I,MLME_VDEV_DOWN_CMD vdev_id=%d 
914,IIII,MLME_PEER_FLUSH_CMD vdev_id=%d mac_addr=%08x%04x peer_tid_bitmap=0x%x 
913,IIIIIIII,MLME_VDEV_START_REQ_CMD vdev_id=%d mhz=%d freq1=%d freq2=%d info=0x%x reg_info 0x%x 0x%x phy_mode=%d 
912,I,MLME_VDEV_STOP_CMD vdev_id=%d 
911,IIII,MLME_VDEV_SET_PARAM_CMD vdev_id=%d param_id=0x%x value=0x%x thread_id=0x%x 
910,II,MLME_SET_WMM_PARAM_CMD vdev_id=%d enabled=%d 
909,IIII,MLME_VDEV_UP_CMD vdev_id=%d assoc_id=%d mac_addr=%08x%04x 
937,I,wlan_mlme_rt_thread_comm_msg_handler: null vdev id=%d 
936,II,wlan_mlme_rt_thread_comm_msg_handler: vdev=%d,msg_id=%d 
938,,wlan_11k_offload_register  
939,I,11K_INVOKE_NEIGHBOR_REP_REQ ssid_len %d  
940,IIIIII,11K_offload_VDEV_PARAM_CONFIG bmiss_count_trigger: %d low_rssi_offset: %d neighbor_report_req_cap: %d neighbor_rep_cache_timeout: %d per_threshold_offset: %d time_offset: %d 
941,,deconfiguring  11k 
942,II,11K_offload_VDEV_PARAM_CONFIG vdev_id:%d %d 
943,I,wlan_11k_offload_per_notify_handler region: %d 
944,,11K_offload_COMP_CONFIG  
945,,11K_offload_de_config  
946,I,wlan_11k_offload_vdev_notify_handler notiftype: %d 
947,I,11K_offload_SWBMISS_EVT_HDLR evt_type:%d 
948,II,11K_offload_SETUP_RSSI_THRESHOLDS low_rssi_threshold:%d high_rssi_threshold:%d 
949,,11K_offload_SETUP_RSSI_THRESHOLDS threshold not set 
950,II,11K_offload_IS_CHANMAP_AVAIL: radio_measurement_enabled: %d num_candidates %d 
951,II,11K_offload_IS_CHANMAP_AVAIL: radio_measurement_enabled: %d neighbor_report_offloaded %d 
952,I,11K_offload_RSSI_EVT_HDLR: Threshold met evt_type %d 
953,,11K_offload_neighbor_report_req_timeout wlan_11k_vdev_handle->vdev is NULL 
954,,11K_offload_neighbor_report_req_timeout wlan_11k_vdev_handle is NULL 
955,,11K_offload_SEND_NEIGHBOR_REP_REQ failed 
956,,11K_offload_SEND_NEIGHBOR_REP_REQ failed- management buffers exhausted 
957,I,11K_offload_SEND_NEIGHBOR_REP_REQ peer is not authenticated %x 
958,I,11K_offload_SEND_NEIGHBOR_REP_REQ current_capping %d 
959,I,11K_offload_SEND_NEIGHBOR_REP_REQ radio_measurement_enabled: %d 
960,I,11K_offload_ACTION_FRAME_HDLR OFFLOAD_STATUS_DROP frm_len 0, dialog token %d 
961,II,11K_offload_ACTION_FRAME_HDLR OFFLOAD_STATUS_NONE as this is not a radio measurement frame category:%d action:%d 
962,,11K_offload_ACTION_FRAME_HDLR OFFLOAD_STATUS_NONE as frm_len is less than action hdr  
963,,11K_offload_PROC_NEIGH_REPO_RESP OFFLOAD_STATUS_NONE 
964,I,BUILD_11K_CHANMAP chan_num=%d 
965,II,NEIGHBOR_REPORT_REQ_COMPLETION Status: %d, Dialog Token: %d 
966,,11w PMF: PN Replay attack detected 
967,,11w PMF: PN validation successful 
968,,11w PMF reg service bit ENABLE  
969,I,11w PMF send SA query state=%d 
970,II,11w PMF deauth/disassoc reason_code %x frmType=%d 
971,,11w PMF SA query rsp with valid transId rcvd 
972,II,11w PMF current transId=%d startTransId=%d 
973,IIII,11w PMF action frm %x %x %x %x 
974,,11w PMF drop unenryp robust action category 
975,,11w PMF BIP check failed  
976,I,11w PMF MGMT RECEIVED from unknown AP vdev_id=%d 
977,IIIII,11w PMF mgmt hdlr subtype=%d len=%d wal_peer: %p vdev: %p wlan_peer:%p 
978,IIII,11W PMF: Send SA query vdevId=%d, transId=%d query_type=%d tx_status=%d 
979,I,11w PMF MMIE check failed vdevId=%d 
980,I,11w PMF Invalid key idx = %d 
981,,11w PMF: MMIE valid 
982,,11w PMF: BC/MC GMAC MGMT frame MMIE MIC check Failed 
983,,11w PMF: BC/MC CMAC MGMT frame MMIE MIC check Failed 
984,,11w PMF: Memory allocation failed 
985,,11w PMF: BC/MC MGMT IPN check Failed 
986,,11w PMF: IE is not Mgmt MIC IE or Invalid length 
987,II,11w PMF: can not handle frame size: %d, max:%d 
988,II,igtk: Same key reinstalled,vdev_id:%d, keyLen:%d
 
989,III,11W PMF: Update iGTK vdevId=%d, keyIdx=%d, KeyLen=%d 
990,I,11W PMF: Update iGTK key_cipher=0x%x 
991,III,11W PMF Offload CMD hdlr: WMI_PMF_OFFLOAD_SET_SA_QUERY_CMDID vdevId=%d, interval=%d, retry_count=%d 
992,,11W PMF: SA query timed out. Send STA kickout event to Host 
993,II,11W PMF: SA query timeout hdlr cur retry cnt=%d, max retry cnt=%d  
994,II,11W PMF: SA query timeout hdlr vdevId=%d, query_state=%d  
995,,11W PMF Offload vdev init 
996,I,11W PMF: vdevID=%d down. clear PMF INFO 
997,III,ROAM_DISABLE_FAIL client_id = 0x%x cur_state = %d, cur_disable_bitmap = 0x%x 
998,III,ROAM_DISABLE client_id = 0x%x curr_state = %d cur_disable_bitmap = 0x%x 
999,II,ROAM_ENABLE client_id = 0x%x cur_disable_bitmap = 0x%x 
1000,IIIIIII,ROAM_INVOKE_PARAM_CHECK invoke_roam_scan_mode = %d ap_sel_mode = %d roam_delay = %d num_chan = %d num_bssid = %d num_buf = %d p_cmd->flags=0x%x 
1001,I,ROAM_INVOKE_STATE_CHECK roam_offload = %d in_use = %d scan_mode = %d ap ssid_len = %d 
1002,IIIIII,ROAM_INVOKE_STATE_CHECK roam_offload = %d in_use = %d scan_mode = %d ap ssid_len = %d roam_sm_state=%d vdev_id=%d 
1003,I,ROAM_INVOKE_START_FAILURE error code = 0x%x 
1004,II,ROAM_INVOKE_SCAN_FAILED invoke_roam = %d, invoke_bmt = %d 
1005,II,ROAM_FW_INVOKE_BSSID BSSID = 0x%08x%04x 
1006,II,ROAM_HOST_INVOKE_BSSID BSSID = 0x%08x%04x 
1007,I,ROAM_INVOKE_PARAM_CHAN channel = %d 
1008,III,ROAM_PER_CLIENT_UNREG_SUCCESS vdev_id = %d req_id = %d num_req = %d 
1009,II,ROAM_PER_CLIENT_NO_ENTRY_EXIST vdev_id = %d req_id = %d 
1010,III,ROAM_PER_CLIENT_UNREG_INVALID_INFO vdev_id = %d, req_id = %d num_requestor = %d 
1011,II,ROAM_PER_CLIENT_UNREG_INVALID_INFO vdev_id = %d, req_id = %d 
1012,IIIIIII,ROAM_PER_CLIENT_REG_REQ_INFO vdev_id = %d, req_id = %d, rx_slots = %d, tx_slots = %d, rx_percentage = %d, tx_percentage = %d, total_req = %d 
1013,II,ROAM_PER_CLIENT_MEMORY_ALLOC_FAILED vdev_id = %d req_id = %d 
1014,IIIII,ROAM_PER_CLIENT_REG_INVALID_INFO_PER_OFFSET_SIZE_GREATER vdev_id = %d req_id = %d percentage_offset = %d curr_rx_thresh_percnt = %d curr_tx_thresh_percnt = %d 
1015,IIIII,ROAM_PER_CLIENT_REG_INVALID_INFO_SLOT_SIZE_GREATER vdev_id = %d req_id = %d slots_offset = %d curr_rx_slot_size = %d curr_tx_slot_size = %d 
1016,II,ROAM_PER_CLIENT_ALREADY_REG vdev_id = %d req_id = %d 
1017,II,ROAM_PER_CLIENT_REG_INVALID_INFO_NOT_INITIALIZED  vdev_id = %d req_id = %d 
1018,,ROAM_PER_CLIENT_REG_INVALID_INFO vdev_roam NULL 
1019,II,ROAM_PER_CLIENT_REG_INVALID_INFO  vdev_id = %d req_id = %d 
1020,IIII,ROAM_ENABLE_DISABLE_TRIGGER client_id=%d enable=%d reason=%d disable_trigger_mask=0x%x 
1021,II,ROAM_UPDATE_EXT_CAP len=%d cap=0x%x 
1022,I,ROAM_ENABLE_DISABLE_ERROR client_id = 0x%x 
1023,IIII,ROAM_STA_QBSS_INFO aac = %d, chan_util = %d, sta_cnt = %d, pcnt = %d 
1024,IIIIII,ROAM_STA_KICKOUT_RECV in_use = %d, running = %d, scan_status = %d, roaming = %d, cur_rssi = -%d dBm send_to_host = %d 
1025,,ROAM_STA_KICKOUT_RECV error 
1026,IIIIII,ROAM_INVOKE_START_SUCCESS roam_scan_type = %d num_buf = %d flags=0x%x report_failure=%d is_allow_home_bssid=%d burst_scan=%d 
1003,I,ROAM_INVOKE_START_FAILURE error code = 0x%x 
1027,III,ROAM_BTM_INVOKE_FAILED status = 0x%x, invoke_roam = %d, invoke_bmt = %d 
1028,III,ROAM_BTM_INVOKE_FAILED roam_status = 0x%x, num_bssid|chan = %d %d 
1029,II,ROAM_GET_CACHE_LIST_BSSID req_num_bssid = %d num_cache_bssid = %d 
1030,I,ROAM_GET_CACHE_LIST_BSSID_FAILURE error code = 0x%x 
1031,,ROAM_GET_CACHE_LIST_BSSID_FAILURE invaild para 
1032,IIIII,WLAN_ROAM_FILS_PARAM next_seq = %d username_len = %d realm_len = %d rik_len = %d rrk_len = %d 
1033,IIIIII,ROAM_CND_SELECTION_OCE_WAN_PARAM weightage_pcnt = %d, num_slot = %d, score = 0x%x 0x%x 0x%x 0x%x 
1034,IIIIII,ROAM_CND_SELECTION_ESP_QBSS_PARAM weightage_pcnt = %d, num_slot = %d, score = 0x%x 0x%x 0x%x 0x%x 
1035,IIIII,ROAM_CND_SELECTION_NSS_PARAM nss_total_pcnt %d, nss_score_|4x4|3x3|2x2|1x1 pcnt %d %d %d %d 
1036,III,ROAM_CND_SELECTION_BAND_PARAM band_total_pcnt %d, band_score_|2G|5G| pcnt %d %d 
1037,IIIII,ROAM_CND_SELECTION_BW_PARAM bw_total_pcnt %d, bw_score_|160|80|40|20 pcnt %d %d %d %d 
1038,IIIIIIII,ROAM_CND_SELECTION_RSSI_PARAM best|good|bad|5g_pref_rssi_threshold %d %d %d %d, pcnt_coeff %d %d, bucket_size = %d %d 
1039,IIIIII,ROAM_CND_SELECTION_WEIGTAGE_PCNT rssi|ht|vht|he|beamforming|pcl %d, %d, %d %d %d %d 
1040,,ROAM_CND_SELECTION_ALGO_INVALID_PARAM ignore 
1041,,ROAM_CND_SELECTION_ALGO_DISABLE 
1042,IIII,ROAM_BG_SCAN_CONFIG bad_rssi_thresh_2g = %d bad_rssi_thresh_5g = %d client_bitmap = 0x%x flags=0x%x 
1043,III,ROAM_BG_SCAN_CONFIG_INVALID_RSSI_OFFSET_2G use default value=0bad_rssi_thresh=%d,bad_rssi_thresh_offset_2g=%d,flags=0x%x 
1044,III,ROAM_BG_SCAN_CONFIG_INVALID_RSSI disable bg scan,bad_rssi_thresh=%d,bad_rssi_thresh_offset_2g=%d,flags=0x%x 
1045,IIIII,wmi_rssi_reject_data index = %d, bssid = %08x%04x retry_delay = %d msec, rssi = %d dbm 
1046,II,wlan_vdev_roam_set_rssi_rejected_ap_param enable = %d buf = 0x%x 
1047,IIIII,ROAM_DENSE_CONFIG rssi_thres_offset = %d traffic_thres = %d dense_min_aps = %d initial_dense_status = %d, fw_dense_status = %d 
1048,III,ROAM_CONFIG_EARLYSTOP thres_max = -%d dBm, thres_min = -%d dBm, enable = %d 
1049,II,ROAM_PREFERRED_FACTOR factor[%d] = %d 
1050,III,ROAM_PREFERRED_BSSID bssid[%d] = %08x%04x 
1051,IIIII,ROAM_WHITELIST ssid[12-15][16-19][20-23][24-27][28-31] = 0x%08x %08x %08x %08x %08x 
1052,IIIII,ROAM_WHITELIST SSID[%d] ssid_len = %d, ssid[0-3][4-7][8-11] = 0x%08x %08x %08x 
1052,IIIII,ROAM_WHITELIST SSID[%d] ssid_len = %d, ssid[0-3][4-7][8-11] = 0x%08x %08x %08x 
1053,III,ROAM_BLACKLIST_BSSID bssid[%d] = %08x%04x 
1054,IIIIII,ROAM_CONFIG_ROAM_FILTER flag = 0x%x op_bitmap = 0x%x num_whitelist = %d num_blacklist = %d num_preferred_bssid = %d rssi_rejected_ap = %d 
1055,IIIIIIII,ROAM_CONFIG_AP_PROFILE ssid_len = %d rssi_margin = %d dBm rsn_authmode = 0x%x rsn_mipher = 0x%x rsn_ucipher = 0x%x flags = 0x%x abs_threh = %d bg_rssi_margin = %d 
1056,IIIII,penal_algo = %d penal_threshold = -%d dBm penal_factor = %d max_penal = %d, param2 = %d 
1057,IIIII,boost_algo = %d boost_threshold = -%d dBm boost_factor = %d max_boost = %d, param1 = %d 
1058,IIIII,ROAM_SCAN_HIRSSI_THRESHOLD hirssi_scan_delta = %d hirssi_scan_max_count = %d hirssi_upper_bound = -%d dBm hirssi_threshold = -%d dBm ref_rssi = -%d dBm 
1059,IIII,ROAM_CONFIG_RSSI_THRESH rssi_threshold1 = -%d dBm rssi_threshold2 = -%d dBm rssi_threshold2_2g = -%d dBm rssi_threshold2_5g = -%d dBm 
1060,,ROAM_CONFIG_RSSI_INVALID_THRESH_OFFSET_5G use default value=0 
1061,,ROAM_CONFIG_RSSI_INVALID_THRESH_OFFSET use default value=0 
1062,I,ROAM_CONFIG_RSSI_INVALID_THRESH use default value=%d dBm 
1063,III,ROAM_CONFIG_RSSI_THRESH roam_scan_rssi_thresh = -%d dBm roam_rssi_thresh_diff = %d dBm rssi_thresh_offset_5g = %d 
1064,III,roam_scan_period = %d roam_scan_age = %d roam_ctrl.running = %d 
1065,III,ROAM_CONFIG_RSSI_CHANGE  change_val = %d dBm bcn_rssi_weight = %d hi_rssi_timer_interval = %d msec 
1066,II,ROAM_CONFIG_RSSI_CHANGE  change_val = %d rssi_threshold1 = %d -> cap it to rssi_threshold1 
1067,IIII,ROAM_SET_CHAN_LIST type=%d num_chans=%d chan0_freq=%d chan1_freq=%d 
1068,I,ROAM_CHANMAP_UPDATE_FROM_CHNL_LIST chan_num=%d 
1069,IIIII,ROAM_SCAN_PARAMS idle_time:%d max_scan_time:%d probe_delay:%d scan_ctrl_flags:%d n_probes:%d 
1070,IIIIII,ROAM_SCAN_PARAMS dtime_act:%d dtime_pass:%d burst_dur:%d min_rest:%d max_rest:%d repeat_prob:%d 
1071,,ROAM_SCAN_PARAMS fw_offload_enable = 0. ignored 
1072,IIIIII,ROAM_SET_SCAN_MODE curr_scan_mode=%x new_scan_mode=%x running=%d roam_state=%d scan_delay_time=%d msec trigger_reason_bitmask=0x%x 
1073,III,ROAM_SCAN_CMD_FROM_HOST arg=0x%x running=%d scan_status=%d 
1074,III,ROAM_FW_OFFLOAD_ENABLE flags=0x%x fw_offload_enable=%d bmiss_final_scan=%d 
1075,I,ROAM_FW_OFFLOAD_ENABLE flags=0x%x when it is running. ignored 
1076,,ROAM_FREE_NOT_IN_USE 
1077,III,ROAM_EARLYSTOP_SCAN (freq %d) earlystop_rssi = -%d dBm, best_candidate_rssi = -%d dBm 
1078,II,ROAM_EARLYSTOP_SCAN (freq %d) stop earlystop because earlystop_rssi(<<10) = -%d dBm below threshold2 
1079,II, ROAM_BETTER_AP_EVENT  candidate_found = %d send_beacon_to_host = %d 
1080,II,ROAM_SUITABLE_AP_EVENT  candidate_found = %d send_beacon_to_host = %d 
1081,IIIII,ROAM_SCAN_CANCELLED  scan_id = 0x%x type = 0x%x reason = 0x%x scan_queue_status = 0x%x sta_kickout = %d 
1082,II,ROAM_BETTER_AP_EVENT  candidate_found = %d send_beacon_to_host = %d 
1080,II,ROAM_SUITABLE_AP_EVENT  candidate_found = %d send_beacon_to_host = %d 
1083,IIII,ROAM_SCAN_COMPLETE_1  reason(SUCC 0/CANCEL 1/PREEMPTED 2/TIMEOUT 3/INTERNAL FAIL 4) = %d evt_scan_id = 0x%x sta_kickout=0x%x invoke_roaming|btm = 0x%x 
1084,IIIII,ROAM_SCAN_COMPLETE candidate_found = 0x%x scan_info.scan_id = 0x%x roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d final_scan = %d send_bcn_to_host = %d 
1085,IIIIIII,ROAM_CND_BSS_SCORE total_score = %d, ht = %d vht = %d he = %d phy_mode = %d, chan = %d prorated_pcnt = %d 
1086,II,ROAM_CND_BSS_SCORE not find peer addr=%08x%04x 
1082,II,ROAM_BETTER_AP_EVENT  candidate_found = %d send_beacon_to_host = %d 
1082,II,ROAM_BETTER_AP_EVENT  candidate_found = %d send_beacon_to_host = %d 
1087,II,ROAM_SCAN_EXTSCAN_CHECK cur_rssi = %d good_rssi_threshold = %d 
1088,II,ROAM_DENSE_CHANGED is_dense = %d normal_rssi_threshold = -%d dBm 
1089,I,ROAM_DENSE_TRAFFIC_UNREGISTERED vdev_id = %d 
1090,II,ROAM_DENSE_CHANGED is_dense = %d dense_rssi_threshold = -%d dBm 
1091,IIII,ROAM_DENSE_TRAFFIC_REGISTERED vdev_id = %d rx_thrughput_thres = %d bytes/sec tx_thrughput_thres = %d bytes/sec status = %d 
1092,IIIIIII,ROAM_DENSE_CLIENT_SCAN_COMPLETED requestor = %d num_ch = %d roamable_ap_cnt = %d min_dense_ap = %d cur_is_dense = %d cur_rssi_thresh = -%d dBm cur_rssi_avg = -%d dBm 
1093,IIII,ROAM_DENSE_CLIENT_SCAN_START roamable_ap_cnt = %d requestor = %d is_restart = %d is_ol_reg = %d 
1094,II,ROAM_EARLYSTOP_SCAN best_candidate_rssi = -%d dBm earlystop_rssi = -%d dBm 
1095,IIIIIII,ROAM_BETTER_CANDIDATE_FOUND valid_cnd:%d chan_num = %d candidate_rssi_last = -%d dBm curr_rssi_avg = -%d dBm bcn_rssi_last = -%d dBm rssi_margin = %d dBm bg_rssi_margin = %d 
1096,,ROAM_CHECK_LCA:max_disallowed_aps is NULL 
1097,II,ROAM_CANDIDATE_FILTER_MATCH %d match (bssid blacklist 0/ssid whitelist 1) index = %d  
1098,,REALM_MATCH_FAIL 
1099,II,ROAM_CANDIDATE_FILTER_MATCH %d match (bssid blacklist 0/ssid whitelist 1) index = %d 
1100,IIIII,ROAM_INVOKE_BSSID_CHECK Recv BSSID %08x%04x num_bssid=%d index=%d DROP = %d 
1101,II,ROAM_CONFIG_BG_RSSI_THRESH bad_rssi_thresh = -%d dBm flags = 0x%x 
1102,II,ROAM_CONFIG_RSSI_THRESH_CONFIG rssi_threshold1 = -%d dBm rssi_threshold2 = -%d dBm 
1103,I,ROAM_PARAM_SET scan_mode 0x%x 
1104,,wlan_vdev_roam_param_set fw_offload is disabled 
1105,IIII,ROAM_FINAL_BMISS_SCAN scan_policy=0x%x,skip_dfs=%d,active_dwell=%d birst_dur=%d 
1106,III,ROAM_EARLYSTOP_SCAN supp_num_chan=%d num_chan=%d, earlystop_rssi=-%d dBm 
1107,IIIII,ROAM_SCAN_REQUESTED  send_beacon_to_host = %d scan_type(FULL 0/CHANLIST 1/CHANMAP 2/FORCED 3/5G_ONLY 4) = %d roam_scan_state (IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d final_scan = %d num_chan = %d 
1108,I,use_11k_chan_map %d 
1109,II,ROAM_SCAN_REJECTED ho_disabled_scan %d trigger_reason %d 
1110,IIIIII,ROAM_SCAN_REJECTED diff %d (last %d cur %d) < %d trigger_bitmap = 0x%x trigger_reason %d 
1111,IIII,ROAM_SCAN_REJECTED scan_status %d roam_state %d final_bmiss %d trigger_reason %d 
1112,II,ROAM_CANCEL_LOW_PRIO_SCAN  send_beacon_to_host = %d roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d  
1113,III,ROAM_SCAN_REJECTED scan_status %d send_beacon_to_host %d trigger_reason %d 
1114,II,ROAM_SCAN_REJECTED disabled_trigger_mask = 0x%x trigger_reason=%d 
1115,II,ROAM_SCAN_REJECTED scan_mode %d trigger_reason %d 
1116,I,ROAM_BTM_CALLBACK status=%d 
1117,,ROAM_TRY_BTM_QUERY not capable 
1118,IIIII,ROAM_TRY_BTM_QUERY roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2)=%d pending_scan_type=%d pending_trigger_reason=%d scan_type=%d trigger_reason=%d 
1119,IIIII,ROAM_RSSI_ACTIVE_SCAN  tmr_running = %d roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d start_scan = 0x%x prev_state = 0x%x final_scan = %d 
1120,IIIII,ROAM_RSSI_ACTIVE_ROAM  tmr_running = %d roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d start_scan = 0x%x prev_state = 0x%x final_scan = %d 
1121,IIII,ROAM_LOW_RSSI_INTERRUPT  bcn_rssi_avg =  -%d dBm bcn_rssi_last = -%d dBm hi_thresh = -%d dBm lo_thresh = -%d dBm 
1122,IIIII, ROAM_RSSI_GOOD bcn_rssi_avg = -%d dBm bcn_rssi_last = -%d dBm roam_scan_mode(PERIODIC 1/RSSI_CHANGE 2/BOTH 3/HO 4) = 0x%x prev_state = 0x%x tmr_running(bit1)/final_scan(bit0) = 0x%02x 
1123,IIIII,ROAM_RSSI_ROAM_STATE tmr_running = %d roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d start_scan = 0x%x prev_state = 0x%x final_scan = %d 
1124,IIIII,ROAM_SCAN_HIRSSI_CHECK curr_high_rssi_thresh = -%d dBm hirssi_threshold = -%d dBm hirssiscan_upperbound = -%d dBm curr_hiscan_count = %d, hirssiscan_maxcount = %d 
1125,II,ROAM_GET_VENDOR_AND_SCORE id = %d len=%d remain_len=%d 
1126,III,ROAM_CND_SCORE_PARSED malformed id = %d len=%d remain_len=%d 
1127,III,ROAM_WLM_NOTIF_HDLR policy=%d flags=0x%x level=%d 
1128,IIII,ROAM_SCAN_CANCELLED  scan_id = 0x%x type = 0x%x reason = 0x%x sta_kickout = %d 
1129,IIIIIII,ROAM_SCAN_STARTED evt_type 0x%x scan_id = 0x%x roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d is_lazy = %d is_bg_roam = %d cur_rssi = -%d dBm bad_rssi_thres = -%d dBm 
1130,IIII,cur|good|roamableAP|threshold_diff %d %d %d %d 
1131,II,PER_REJECT_5G_TO_2G cur %d cnd %d 
1132,,ROAM_DISCARD_CANDIDATE found in LCA 
1133,IIIII,ROAM_CANDIDATE_RSSI_ADJUST rssi = -%d dBm boost_threshold = -%d dBm boost_factor = %d penalty_threshold = -%d dBm penalty_factor = %d 
1134,IIIIII,ROAM_CANDIDATE_SECURITY_MATCH  rsRssi = -%d dBm curr_rssi = -%d dBm final_bmiss_received = %d rssi_margin = %d dBm send_beacon_to_host = %d bg_rssi_margin = %d 
1135,I,ROAM_CHANMAP_UPDATE chan_num=%d 
1136,,ROAM_MBO_ASSOCIATION_DISALLOWED 
1137,II,ROAM_CANDIDATE_BSSID_CHECK same mac as sta peer, bssid = %08x%04x, drop it 
1138,III,ROAM_CANDIDATE_BSSID_CHECK_SAME bssid = %08x%04x match vdev_id = %d bssid, drop it 
1139,III,ROAM_CANDIDATE_BSSID_CHECK bssid = %08x%04x match vdev_id = %d myaddr, drop it 
1140,,ROAM_RSN_PARAM_MISMATCH 
1141,I,ROAM_CANDIDATE_FILTER_PCL %d 
1142,IIII,ROAM_WPA_MISMATCH parse_status = %d wpa_ucipher = 0x%08x wpa_mipher = 0x%08x wpa_authmode = 0x%08x (16 bit cur/16 bit candidate) 
1143,IIIII,ROAM_RSN_MISMATCH parse_status = %d rsn_ucipher = 0x%08x rsn_mipher = 0x%08x rsn_authmode = 0x%08x (16 bit cur/16 bit candidate) mfp_enable (bit2)/ap_cap(bit1)/ap_req(bit0) = 0x%01x 
1144,I,ROAM_VDEV_EVT_NOT_INUSE type=%d 
1145,IIII,ROAM_SCAN_TIMER_EXPIRE id = %d (periodic 1/hirssi 2/first bmiss 3) interval = %d(msec) roam_ctrl.running = %d roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d 
1145,IIII,ROAM_SCAN_TIMER_EXPIRE id = %d (periodic 1/hirssi 2/first bmiss 3) interval = %d(msec) roam_ctrl.running = %d roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d 
1146,IIII,ROAM_SCAN_PERIODIC_TIMER stop cur_low_rssi = -%d dBm >= %d dBm (rssi_thresh_2 -%d diff %d) 
1147,IIII,ROAM_SCAN_PERIODIC_TIMER ignored cur_rssi = -%d dBm >= %d dBm (rssi_thresh_2 -%d diff %d) 
1148,II,ROAM_SCAN_TIMER_EXPIRE curr_low=-%d dBm curr_high=-%d dBm 
1149,IIIII,ROAM_SCAN_TIMER_EXPIRE id = %d (periodic 1/hirssi 2/first bmiss 3) interval = %d(msec) roam_ctrl.running = %d roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d curr_rssi=-%d dBm 
1150,II,ROAM_DEV_STOP: vdev_id = %d running = 0x%x 
1151,,ROAM_STOP_FAIL_NOT_INUSE 
1152,IIII,ROAM_DENSE_TRAFFIC_REGISTERED vdev_id %d, rx_thrughput_thres = %d bytes/sec, tx_thrughput_thres = %d bytes/sec, status = %d 
1153,II,ROAM_DENSE_START is_dense = %d ap|dense_ssid_len = 0x%x 
1068,I,ROAM_CHANMAP_UPDATE_FROM_CHNL_LIST chan_num=%d 
1154,II,ROAM_CHANMAP[%d] 0x%x 
1155,,ROAM_CHANMAP_VDEV_START keep chanmap due to same ssid 
1156,,ROAM_CHANMAP_VDEV_START reset chanmap due to different ssid 
1157,I,ROAM_CND_CACHE_BUF cache_size = %d 
1158,IIIII,ROAM_CHANMAP_CMP_SSID: vdev_id = %d, prev AP 1st_4B=%lu len=%d, new AP 1st_4B=%lu, len=%d 
1159,II,ROAM_DEV_START: vdev_id = %d runnning: 0x%x 
1160,II,ROAM_DEV_START_NOT_ENABLED: vdev_id = %d disable_bitmap=0x%x 
1161,,ROAM_START_FAIL_NOT_INUSE 
1162,IIIIII,ROAM_MAWC_CONFIG vdev_id = %d enable = %d traffic_load = %dkBps, best_ap_threshold = -%ddBm, high_adjust = %d dBm, low_adjust = %d dBm 
1163,I,ROAM_MAWC_CONFIG_INVALID vdev_id = %d 
1164,IIII,ROAM_MAWC_ADJUST_THRESH threshold low_thresh -%d dBm to -%d dBm, hi_thresh -%d dBm to -%d dBm 
1165,III,ROAM_MAWC_RSSI_TRAFFIC_CHECK cur_rssi = -%d dBm best_ap_thresh = -%d dBm, traffic_load = %d 
1166,II,ROAM_MAWC_RSSI_ALREADY_ADJUSTED high_adjust = %d low_adjust = %d 
1164,IIII,ROAM_MAWC_ADJUST_THRESH threshold low_thresh -%d dBm to -%d dBm, hi_thresh -%d dBm to -%d dBm 
1167,III,ROAM_MAWC_MOTION_NOTIFY vdev_id = %d, cur_motion_state = %d new_motion_state = %d (0:unknown,1:stationary,2:walk,3:transit) 
1168,II,ROAM_HO_FILTER_DISALLOW: before cnt=%d, after cnt=%d 
1169,,ROAM_HO_FILTER_DISALLOW no disallow chan in pcl 
1170,III,ROAM_EVENT_TO_HOST reason=%d, notif=%d, ret=%d 
1171,IIIIII,ROAM_FINAL_BMISS_RECVD  curr_rssi_avg = -%d dBm bcn_rssi_last = -%d dBm roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d scan_param.mode(5-7)/fina_scan(0-4) = 0x%02x scan_status(bit3)/candidate_found(bit2)/send_beacon_to_host(bit1)/final_bmiss_recvd(bit0) = 0x%02x is_qnull_fbmiss = %d 
1172,III,ROAM_SWBMISS_BCN_RECV_THRE2 bcn_rssi_last = -%d dBm rssi_threshold2 = %d hit_rssi_thresh_cnt = %d 
1173,IIII,ROAM_SWBMISS_BCN_RECV_VAL bcn_rssi_last = -%d dBm evt->bcn_rssi_avg = -%d dBm change = %d rssi_change_val = %d 
1174,II,ROAM_SCAN_TIMER_START  id = %d (periodic 1/hirssi 2/first bmiss 3/rssi_config 4/per rest 5/final bmiss 6) interval = %d(msec) 
1175,II,ROAM_SCAN_TIMER_STOP  id = %d (periodic 1/hirssi 2/first bmiss 3/rssi_config 4/per rest 5/final bmiss 6) interval = %d(msec) 
1176,II,ROAM_DENSE_BSSID bssid = %08x%04x 
1177,IIIII,ROAM_DENSE_ADJUST_THRESH is_dense = %d old_low_thresh = -%d dBm, new_low_thresh = -%d dBm, new_hi_thres = -%d, offset=%d 
1178,IIIIIIII,ROAM_TRAFFIC_EVENT_RECV_INFO vdev_id|req_id|thresh_status = 0x%x, recv_rx_thrghput = %d bytes/sec, recv_tx_thrghput = %d bytes/sec req_rx_thrghput = %d bytes/sec req_tx_thrghput = %d bytes/sec last_traffic_thres_breach = %d dense_scan_skipped = %d scan_status = %d 
1179,IIIII,ROAM_TRAFFIC_EVENT_RECV_INVALID  vdev_id = %d, req_id = %d, status = %d, recv_rx_thrghput = %d bytes/sec recv_tx_thrghput = %d bytes/sec 
1180,IIIII,ROAM_SCAN_TIMER_EXPIRE id = %d (periodic 1/hirssi 2/first bmiss 3/config rssi 4) interval = %d(msec) roam_ctrl.running = %d roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d scan_status = %d 
1181,IIIII,ROAM_UPDATED_THRESH hirssi_thresh = -%ddBm, rssi_thresh1 = -%ddBm curr_rssi = -%ddBm, low_rssi_thresh = -%ddBm, high_rssi_thresh = -%ddBm 
1182,IIIII,ROAM_RSSI_REJECTED_AP_ALLOW_UPDATE new_list = %d, bssid %08x%04x exp_delay = %d msec, exp_rssi = -%ddBm 
1183,IIIIIIIII,ROAM_AP_SCORE bssid = %08x%04x chan = %d curr_score = %d, ap_score = %d rssi = -%d dBm ht|vht|he_bits = 0x%01x STA|AP_BF = 0x%01x prorated_pcnt = %d 
1184,IIIIIII,ROAM_RSSI_SCORE pcnt = %d, score = %d, num_slot = %d, slot_size = %d, rssi = %d, rssi_diff = %d, slot_index = %d 
1185,II,ROAM_RSSI_SCORE_INVALID good|bad_bucket_size %d %d 
1186,III,ROAM_QBSS_ESP_SCORE pcnt = %d score = %d chan_cong_pcnt = %d(default = 255) 
1187,II,ROAM_QBSS_ESP_SCORE_INVALID_SLOT num_slot = %d, chan_cong_pcnt = %d 
1188,II,ROAM_QBSS_ESP_SCORE_INVALID num_slot = %d, chan_cong_pcnt = %d 
1189,IIII,ROAM_PCL_SCORE chan_val = %d, wt_pcnt = %d, max|curr|_score = %d %d 
1190,IIII,ROAM_NSS_SCORE nss = %d, tot|curr|_score = %d %d index = %d 
1191,II,ROAM_BW_SCORE bw = %d, score = %d 
1192,I,ROAM_HO_SYNC_COMPLETE error = 0x%x (HOST_ISSUE 0xfffffff) 
1193,,wlan_roam_state_sync_exit 
1194,I,ROAM_HO_SYNC_START prev_roam_state = %d 
1195,I,ROAM_HO_DBS_WAKE:sta_sap_mcc=%d 
1196,,ROAM_CONNECTED no delete old session but reset roam params 
1197,I,ROAM_CONNECTED pctrl->curr_cnd->is_home_bssid=%d 
1198,I,ROAM_SEND_NOTIF_TO_HOST send NOTIF_ROAM_REASSOC vdev_id=%d 
1199,II,ROAM_UNIT_TEST_OVERRIDE_REASSOC_RSP_RSSI_REJECT retry_time = %d min_rssi_delta = %d 
1200,I,ROAM_UNIT_TEST_OVERRIDE_REASSOC_RSP unit test command enabled to override reassoc rsp %d 
1201,II,ROAM_HO_MGMT_RX subtype = %d status_code = %d 
1202,,ROAM_UNIT_TEST_SKIP_SEND_REASSOC_REQ unit test skip sending reassoc req 
1203,I,ROAM_UNIT_TEST_OVERRIDE_AUTH_RSP unit test command enabled to override auth rsp %d 
1201,II,ROAM_HO_MGMT_RX subtype = %d status_code = %d 
1204,,ROAM_SKIP_PREAUTH 
1205,III,ROAM_HO_TEMP_PEER_ALLOC_FAILED mac_id = %d, bssid = %0x04%x 
1206,IIIIII,ROAM_HO_ENTER_CH  roaming attempt to bssid = %08x%04x, mhz=%d (cur bssid = %08x%04x, mhz=%d)  
1207,I,ROAM_HO_DELAY_PREAUTH %d msecs 
1208,,ROAM_SM_DEL_HOMEBSSID fail to create tmp peer 
1207,I,ROAM_HO_DELAY_PREAUTH %d msecs 
1209,I,ROAM_HO_ANT_REQUEST status=0x%x 
1210,III,ROAM_SEND_NOTIF_TO_HOST send NOTIF_ROAM_START vdev_id=%d, state=%d, roam_start_sent=%d 
1211,I,ROAM_HO_STOP: 0x%x 
1212,IIII,ROAM_HO_CACHE_CANDIDATE_INFO phymode==MODE_UNKNOWN mhz=%d freq1=%d freq2=%d phymode=%d 
1213,IIIIII,ROAM_FRMPARSE_OCE_ESP_CAP esp_pcnt = %d, ac_index = %d, ac_bitmap = 0x%x acc_cat = %d,airtime = %d, cap = %d 
1214,IIIIII,ROAM_SM_QBSS_INFO cap = %d, qbss_|cnt = %d utilz = %d, aac = %d pcnt = %d esp_pcnt = %d 
1215,II,ROAM_HO_ABORT_RETRY %d -> delay %d msec 
1216,I,ROAM_HO: recover hw mode to %d 
1217,IIII,ROAM_HO_ABORT is_set_spoof_mac=%d,supp_init=%d,runing=%d,error_code=%d 
1218,IIII,ROAM_HO_ABORT del_in_prog=%d,upt_in_prog=%d,home_bss_del=%d,old_hw_mode=%d 
1219,III,ROAM_HO_ABORT cur_state=%d is_sync=%d disconn_from_host=%d 
1220,IIIIIII,ROAM_HO_DELAY_PAUSE vdev_is_paused %d qdepth %d/%d/%d (hw/sw/last) pause_delay %d/%d msecs (cnt %d) 
1221,,htt_holder_evt_hdr buf_full! 
1222,II,htt_holder_evt_hdr cur_state=%d,evt=%d 
1223,II,subnet_detection_status_hdr cur_state=%d,status=%d 
1224,II,ROAM_HO_OCS_CH_CB  rcvd event = %d @ cur_state = %d (GRANTED 0/COMPLETED 1/STOPPED 2/PREEMPTED 3/END 4) 
1225,II,ROAM_HO_SORT_CANDIDATE_CUR  cur_index = %d position = %d 
1226,III,ROAM_HO_SORT_CANDIDATE  total_candidate = %d best_urssi = %d sel_5g_margin = %d 
1227,III,ROAM_HO_SORT_CANDIDATE find forced bssid index1=%d index2=%d position=%d 
1228,II,ROAM_HO_SORT_CANDIDATE  total_candidate = %d forced_bssid_num=%d 
1229,IIIIII,ROAM_HO_SAVE_CANDIDATE  idx = %d bssid = %08x%04x rssi = -%d dBm prefer = %d is_home_bssid=%d 
1230,II,ROAM_OUI_ACTION bitmask 0x%x mhz = %d 
1231,,ROAM_HO_SAVE_CANDIDATE_NO_CACHE_FOUND 
1232,III,ROAM_HO_SAVE_CANDIDATE_NO_CACHE_FOUND bssid = %08x%04x rssi = -%d dBm 
1233,IIII,ROAM_HO_SAVE_CANDIDATE_DUP  duplicate candidate AP, bssid = %08x%04x new_score = %d old_score= %d 
1234,,ROAM_HO_SAVE_CANDIDATE_PARAM_ERROR 
1235,III,ROAM_OUI_ACTION_FORCE stored %d curr %d expected_chain_num %d  
1236,IIIIIIII,ROAM_HO_SWITCH_CH  bssid = %08x%04x mac_id=%d (rssi = -%d dBm mhz = %d phy_mode = 0x%x band_center_freq1 = %d band_center_freq2 = %d) 
1237,,ROAM_HO_SWITCH_HW_MODE Pending 
1238,IIIII,ROAM_HO_SWITCH_HW_MODE bssid = %08x%04x, from %d to %d, status=%d 
1239,IIIII,ROAM_HO_GET_CANDIDATE  blacklisted(bit31)_is_bcn(bit30)_total_cnd(hi_14)_cnd_idx(lo_16) = 0x%08x  bssid = %08x%04x rssi = -%d dBm mhz = %d 
1240,IIIIIIII,ROAM_HO_CACHE_ADD curr_cookie = %d bssid = %08x%04x score=%d cache_count = %d min_cookie = %d min_cookie_index = %d new_entry/update = %d 
1241,I,ROAM_HO_SAVE_CANDIDATE_MALFORMED mandatory=%d 
1242,III,ROAM_HO_SAVE_CANDIDATE malformed id = %d len=%d remain_len=%d 
1243,IIIII,ROAM_CND_CACHE_IGNORE bssid = %08x%04x cur_cookie = %d new_score = %d old_score = %d 
1244,IIII,ROAM_CND_CACHE_IGNORE bssid = %08x%04x score = %d min_score = %d 
1245,IIIII,ROAM_CND_CACHE_GET_ENTRY bssid = %08x%04x index %d count %d found %d 
1246,I,ROAM_CND_CACHE_GET_ENTRY cache->cache_count=%d 
1247,II,ROAM_CND_CACHE_GET_ENTRY roam_cnd_addr=0x%x cache=0x%x 
1248,III,ROAM_HO_IES_PARSE_ERROR id=%d,len=%d,status=0x%x 
1249,IIIII,ROAM_HO_IES id = %d oui: 0x%x oui_type=%d oui_subtype=%d len=%d 
1250,,ROAM_HO_WAKE:start_notif_sent=1 before sending abort 
1251,III,ROAM_SEND_NOTIF_TO_HOST send NOTIF_ROAM_ABORT vdev_id=%d, state=%d, roam_start_sent=%d 
1252,III,ROAM_OUI_ACTION_RESTORE stored %d curr %d expected_chain_num %d  
1253,I,ROAM_HO_FAIL cur_state = %d 
1250,,ROAM_HO_WAKE:start_notif_sent=1 before sending abort 
1251,III,ROAM_SEND_NOTIF_TO_HOST send NOTIF_ROAM_ABORT vdev_id=%d, state=%d, roam_start_sent=%d 
1254,IIII,ROAM_VDEV_RESTART_FROM_HOST@state=%d in_use=%d,running=%d,ho_flags=0x%x 
1255,IIII,ROAM_VDEV_STOP_FROM_HOST@state=%d in_use=%d,running=%d,ho_flags=0x%x 
1210,III,ROAM_SEND_NOTIF_TO_HOST send NOTIF_ROAM_START vdev_id=%d, state=%d, roam_start_sent=%d 
1256,II,ROAM_HO_UPDATE_STATUS  rcvd status = %d@cur_state = %d 
1257,II,ROAM_HO_START_DEFERRED vdev_roam not NULL cnt %d -> delay %d msec 
1258,,ROAM_HO_START_FAIL no candidate 
1259,IIIII,ROAM_HO_START cnd(idx/total) %d/%d roam_state %d, f_bmiss_rcvd %d, bcn_to_host %d 
1260,II,ROAM_HO_START_DEFERRED is_sync_in_progress cnt %d -> delay %d msec 
1261,II,ROAM_HO_START_IGNORED flags %x running %d 
1262,II,ROAM_HO_OFFLOAD_SET_PARAM  result(0/1/2/3) = %d rsn_authmode = 0x%x 
1263,II,ROAM_HO_OFFLOAD_SET_PARAM assoc_ie status=%d,len=%d 
1264,IIIII,ROAM_HO_OFFLOAD_SET_PARAM  result(0/1/2/3) = %d flags = 0x%x rssi_cat_gap = %d, sel_5g_margin = %d, ho_delay_for_rx = %d 
1265,II,ROAM_HO_OFFLOAD_SET_PARAM roam_scan_mode = 0x%x offload_param NULL HO_ENABLED_CHK %d 
1266,II,ROAM_HO_OFFLOAD_SET_PARAM  result(0/1/2/3) = %d roam_scan_mode = 0x%x 
1267,,ROAM_HO_OFFLOAD_SET_PARAM no param 
1268,I,ROAM_HO_OFFLOAD_SET_PARAM  result(0/1/2/3) = %d 
1269,I,ROAM_HO_ENA_DIS_SCAN enable:%d 
1270,,ROAM_HO_STOP 
1271,,ROAM_HO_STOP 0xffffffff 
1272,,ROAM_HO_START 
1273,II,ROAM_HO_START_FAIL running=%d scan_mode=0x%x 
1274,,ROAM_UPDATE_LCA:pctrl is NULL or max_disallowed_aps is NULL 
1275,III,ROAM_HO_ANT_CB %d %d %d 
1276,II,EXTENDED_ID %d > MAX_EXT_PARAMS %d 
1277,IIII,lca_disallow_params disallow_duration = %d rssi_channel_penalization = %d num_disallowed_aps = %d disallow_lca_enable_source_bitmap = %x 
1278,,Missing lca_disallow_params 
1279,IIII,ROAM_HO_HTT_SAVED_POOL_UNMAP: ep=%d flow_type=%d,flow_id=%d,flow_pool_id=%d 
1280,IIII,ROAM_HO_HTT_CONSUME: msg_type=0x%x,flow_type=%d,flow_id=%d,flow_pool_id=%d 
1281,IIII,ROAM_HO_HTT_SAVED_POOL_MAP: ep=%d flow_type=%d,flow_id=%d,flow_pool_id=%d 
1282,IIII,ROAM_HO_HTT_MISMATCH: msg_type=0x%x,flow_type=%d,flow_id=%d,flow_pool_id=%d 
1283,III,ROAM_HO_HTT_SAVED_SEC_IND ep=%d,peer_id=%d,sec_type=%d 
1284,III,HTT_T2H_MSG_TYPE_RX_ADDBA ep=%d peer_id=%d,tid=%d 
1285,III,ROAM_HO_HTT_SAVED_RX_DELBA: ep=%d,peer_id=%d,tid=%d 
1286,III,ROAM_HO_HTT_CONSUME: msg_type=0x%x,peer_id=%d,tid=%d 
1287,III,ROAM_HO_HTT_SAVED_PEER_UNMAP: ep=%d vdev_id=%d,peer_id=0x%x 
1288,III,ROAM_HO_HTT_CONSUME: msg_type=0x%x,vdev_id=%d,peer_id=0x%x 
1289,III,ROAM_HO_HTT_MISMATCH: msg_type=0x%x,vdev_id=%d,peer_id=0x%x 
1290,III,ROAM_HO_HTT_SAVED_PEER_MAP: ep=%d vdev_id=%d,peer_id=0x%x 
1289,III,ROAM_HO_HTT_MISMATCH: msg_type=0x%x,vdev_id=%d,peer_id=0x%x 
1291,I,ROAM_HO_HTT_UNREGISTER holder->registed_cnt = %d 
1292,I,ROAM_HO_HTT_REGISTER holder->registed_cnt = %d 
1293,II,ROAM_HO_HTT_FORWARD  forward_cnts = %d forward_bytes = %d 
1294,I,ROAM_HO_HTT_FORWARD ALLOC_FAIL msg_bytes=%d 
1295,,ROAM_HO_WAKE: sending htt_data_msg 
1296,III,ROAM_HO_HTT_FORWARD msg_type=0x%x forward_cnts = %d forward_bytes = %d 
1297,III,ROAM_HO_HTT_FORWARD ALLOC_FAIL msg_type=0x%x msg_bytes=%d 
1298,IIII,ROAM_HO_HTT_DISPATCH full=%d dl_unicast_count=%d dl_count=%d evt_sent=0x%x 
1299,IIIIII,ROAM_HO_HTT_DATA_STORE: ep=%d msg_type=0x%x msg_bytes=0x%x peer_id(bit31)|tid=0x%x buffered_count=0x%x buffer_remaing_size=0x%x 
1300,I,ROAM_HO_HTT_DATA_STORE: unexpected_msg_type=0x%x 
1301,I,ROAM_HO_HTT_EVT_VDEV_NOT_FOUND vdev_id=%d 
1302,II,ROAM_HO_HTT_EVT: type=0x%x vdev_id=%d 
1303,II,ROAM_SUBNET_DETECT_COMPLETE vdev_id=%d status=%d
 
1304,,ROAM_SUBNET_DETECT_COMP_NOT_STARTED 
1305,I,ROAM_SUBNET_DETECT_TIMER_IGNORE ipv4 neither ipv6 is enabled or have valid own ip address. flags=0x%x 
1306,II,ROAM_SUBNET_DETECT_SEND_NS count=%d/%d
 
1307,II,ROAM_SUBNET_DETECT_SEND_ARP count=%d/%d
 
1308,,ROAM_SUBNET_DETECT_TIMER_EXPIRE not started. ignored 
1309,,ROAM_SUBNET_DETECT_TIMER_EXPIRE invalid vdev 
1310,IIII,ROAM_SUBNET_DETECT_IPV6_INFO gw_ipv6_addr 31_0 = %08x 63_32 = %08x 95_64 = %08x 127_96 = %08x 
1311,IIII,ROAM_SUBNET_DETECT_IPV6_INFO my_ipv6_addr 31_0 = %08x 63_32 = %08x 95_64 = %08x 127_96 = %08x 
1312,,ROAM_SUBNET_DETECT_INVALID_MY_IPV6_ADDR 
1313,II,ROAM_SUBNET_DETECT_INVALID_GW_MAC gw_mac_addr = %08x:%04x 
1314,I,ROAM_SUBNET_DETECT_IPV6_NOT_ENABLED flag=0x%x 
1315,IIII,ROAM_SUBNET_DETECT_IPV4_INFO my_ipv4_addr = 0x%x gw_ipv4_addr=0x%x, gw_mac_addr = %08x:%04x 
1316,,ROAM_SUBNET_DETECT_INVALID_MY_IPV4_ADDR 
1313,II,ROAM_SUBNET_DETECT_INVALID_GW_MAC gw_mac_addr = %08x:%04x 
1317,I,ROAM_SUBNET_DETECT_IPV4_NOT_ENABLED flag=0x%x 
1318,I,ROAM_SUBNET_DETECT_START vdev_id=%d
 
1319,II,ROAM_SUBNET_DETECT_INVALID_CONFIG max_retries = %d timeout = %d 
1320,,ROAM_SUBNET_DETECT_START_FILS ignored 
1321,I,ROAM_SUBNET_DETECT_START_INVALID vdevp NULL (given vdev_id=%d) 
1322,,ROAM_SUBNET_DETECT_STARTED_MAX_RETRIES zero 
1323,,ROAM_SUBNET_DETECT_START_NON_WOW ignored 
1324,,ROAM_SUBNET_DETECT_ALREADY_STARTED or NULL 
1325,IIII,SUBNET_DETECT_INVALID_VDEV vdev_id=%d vdevp=0x%08x is_free=%d is_up=%d
 
1326,,SUBNET_DETECT_INVALID_INST NULL
 
1327,IIII,ROAM_SUBNET_DETECT_DATA_RX gw_mac=%08x:%04x recv:%08x:%04x 
1328,,ROAM_SUBNET_DETECT_DATA_RX_INVALID_VDEV ignore frame 
1329,IIIII,ROAM_SUBNET_DETECT_CONFIG_1 gw_ipv6_addr 31_0 = %08x 63_32 = %08x 95_64 = %08x 127_96 = %08x flag=0x%x 
1330,IIIII,ROAM_SUBNET_DETECT_CONFIG   gw_mac_addr = %08x:%04x ip_v4_addr = 0x%x timeout = %d max_retries = %d 
1331,II,ROAM_SUBNET_DETECT_CONFIG_INVALID flag = 0x%x vdev_id=%d -> disabled 
1332,I,ROAM_SUBNET_DETECT_CONFIG_INVALID vdev_id=%d -> disabled  
1333,I,ROAM_SUBNET_DETECT_UNREGISTER cur_registred_cnt = %d 
1334,II,ROAM_SUBNET_DETECT_REGISTER sd->registred_cnt = %d, thread_id = %d 
1335,I,ROAM_SUBNET_DETECT_ROAM_EVT_ERR not configured for vdev_id=%d 
1336,II,ROAM_SUBNET_DETECT_ROAM_EVT type=0x%x vdev_id=%d 
1337,III,ROAM_SUBNET_DETECT_ARP_NA_PROC_IGNORE vdev_id=%d i=%d started=%d 
 
1338,,ROAM_SUBNET_DETECT_NA_PROC wlan_na_proc_frame return STATUS_NONE
 
1339,II,ROAM_SUBNET_DETECT_ARP_NA_PROC_ERR vdev_id=%d i=%d
 
1340,IIIII,ROAM_SUBNET_DETECT_ARP_NA_PROC_ERR(status: %d) arp_opcode: 0x%x vdev_id=%d i=%d started=%d 
 
1341,,ROAM_SUBNET_DETECT_ARP_PROC wlan_arp_resp_proc_frame return STATUS_NONE
 
1339,II,ROAM_SUBNET_DETECT_ARP_NA_PROC_ERR vdev_id=%d i=%d
 
1346,IIII,wlan_roam_dispatch_notify_inter_thread:thread=%d,msg_size=%d,cb=0x%x,cb_ctxt=0x%x 
1345,II,_wlan_roam_htt_dispatch_event_inter_thread:vdev_id=%d,event=0x%x 
1344,II,_wlan_roam_subnet_detection_indicate_status:vdev_id=%d,status=0x%x 
1343,III,wlan_roam_execute_notify:msg_size=%d,cb=0x%x,cb_ctxt=0x%x 
1342,III,ROAM_HO_THREAD_MSG: vdev_id=%d, msg_id=0x%x, event=0x%x 
1362,II,ROAM_UNIT_TEST_2: final_bmiss %d roam_state %d 
1361,I,ROAM_INVOKE_PARAM_CHAN start flag=0x%x 
1360,IIII,ROAM_INVOKE_PARAM_CHAN setting idx=%d, ch=0x%x, mac=%08x%04x 
1359,I,ROAM_INVOKE_PARAM_CHAN invoke count=%d 
1358,I,ROAM_INVOKE_PARAM_CHAN error max supp=%d 
1357,IIIII,ROAM_DEBUG_Q_DEPTH vdev_id = %d (0xFF invalid) bss_peer = 0x%x (0 if invalid) wal_peer = 0x%x (0 if invalid), hw_q = %d sw_q = %d 
1356,II,ROAM_ADJUST_DELAY_UNIT_TEST vdev_id = %d mandatory [id] is missing 
1355,III,ROAM_ADJUST_DELAY_UNIT_TEST vdev_id = %d unkown id = %d num_args = %d 
1354,III,ROAM_ADJUST_DELAY_UNIT_TEST vdev_id = %d id = %d default to delay = %d 
1353,III,ROAM_ADJUST_DELAY_UNIT_TEST vdev_id = %d id = %d delay = %d 
1352,II,BTM_CANDIDATE_INFO bssid = %08x%04x 
1351,III,BMT_UNIT_TEST num_args = %d bmt_flags %d num_bssid = %d 
1350,IIIIIII,ROAM_MAWC_CONFIG_UNIT_TEST vdev_id = %d enable = %d traffic_load_thresh = %d best_ap_rssi_thresh = %d rssi_high/low_adjust = %d %d num_args = %d 
1349,IIIIIII,ROAM_PER_CONFIG_UNIT_TEST vdev_id = %d enable = %d rest_time = %d pcnt = %d rate_high/low_adjust = %d %d num_args = %d 
1348,I,ROAM_SCORE_CONFIG_UNIT_TEST disable = 0x%x 
1347,IIIIII,ROAM_CND_SELECTION_WEIGTAGE_PCNT rssi|ht|vht|he|beamforming|pcl %d %d %d %d %d %d 
1038,IIIIIIII,ROAM_CND_SELECTION_RSSI_PARAM best|good|bad|5g_pref_rssi_threshold %d %d %d %d, pcnt_coeff %d %d, bucket_size = %d %d 
1037,IIIII,ROAM_CND_SELECTION_BW_PARAM bw_total_pcnt %d, bw_score_|160|80|40|20 pcnt %d %d %d %d 
1036,III,ROAM_CND_SELECTION_BAND_PARAM band_total_pcnt %d, band_score_|2G|5G| pcnt %d %d 
1035,IIIII,ROAM_CND_SELECTION_NSS_PARAM nss_total_pcnt %d, nss_score_|4x4|3x3|2x2|1x1 pcnt %d %d %d %d 
1398,IIIIIII,ROAM_PER_MON_CALC type = %d(1:rx, 2:tx), tpkt = %d, lowpkt = %d recv_pkt = %d, recv_lopkt = %d, slot_num = %d, pcnt = %d 
1397,II,PER_MON_INIT_FAILED status = %d type = %d 
1396,IIIII,ROAM_PER_MON_INIT type = %d, ofdm_low|high = 0x%x 0x%x, cck_low|high = 0x%x 0x%x 
1395,II,ROAM_PER_MON_UPDATE ignore vdev_roam=0x%x or evt=%d 
1394,III,ROAM_PER_EVT_ACTION evt = %d region_tx|rx  %d %d 
1393,,ROAM_PER_FAILED_EVENT 
1392,IIIIIII,ROAM_PKT_FILT_MCS max_nss_bw = %d max_mcs_index = %d max_pkt = %d, hi_per_mcs = %d, allow = %d, low_per_pkt = %d, tot_per_pkt = %d 
1391,IIIII,ROAM_PKT_FILT_OFDM  max_index = %d, max_pkt = %d, allow = %d, lpkt = %d, tot_per_pkt = %d 
1390,IIIIII,ROAM_PKT_FILT_CCK  max_index = %d, max_pkt = %d, allow = %d, hirate_pkt = %d, lpkt = %d, tot_per_pkt = %d 
1389,,ROAM_PER_EVNT_DLVR_FAILED vdev_roam NULL 
1388,IIIIIII,ROAM_PER_EVNT_DLVR_FAILED vdev_id = %d, mac = %d, op = %d, vdev_flag = 0x%x, enable = %d, state = %d, type = %d 
1387,IIII,ROAM_PER_EVNT_DLVR state = %d(0:none, 1:init, 2:active, 3:suspend), type = %d(1:rx, 2:tx, 3:both) time_|last_run = %dmsec, mon_start = %dmsec 
1386,I,ROAM_PER_INIT_SUCCESS vdev_id %d 
1385,II,ROAM_PER_MON_UPDATE vdev_roam=0x%x or mon_type=%d 
1384,IIIIIIII,ROAM_PER_MON_UPDATE suspend = %d, state = %d, type = %d, rx|tx_bitmap = 0x%x, 0x%x tmr = %d rx|tx_region = %d %d 
1383,I,PER_MON_FAILED status = %d 
1382,,PER_MON_FAILED peer NULL 
1381,IIIIIII,PER_MON_RESET reason = %d, type = %d(1:rx, 2:tx) pcnt = %d slot = %d tpkt = %d lo_pkt = %d missed_slot = %d 
1379,II,ROAM_PER_PDEV_UNREG_FAILED status = %d, vdev_id = %d 
1380,IIIIIIII,ROAM_PER_VDEV_EVT type = %d, is_pdev_evt_reg = %d, rx_state = %d, tx_state = %d vdev_id = %d, raom_vdev_id = %d peer = 0x%x, 0x%x 
1373,II,ROAM_PER_PDEV_REG_FAILED status = %d vdev_id = %d 
1379,II,ROAM_PER_PDEV_UNREG_FAILED status = %d, vdev_id = %d 
1373,II,ROAM_PER_PDEV_REG_FAILED status = %d vdev_id = %d 
1378,III,ROAM_PER_WAL_PDEV_HDR ignore wal_pdev=0x%x event_arg=0x%x event=0x%x 
1377,I,ROAM_PER_PARAM_TLV NULL cmd = 0x%x 
1376,I,ROAM_PER_CONFIG_INVALID vdev_id = %d 
1375,IIIIIIIII,ROAM_PER_CONFIG vdev_id = %d enable = 0x%x hirate_thres = 0x%x, lowrate_thresh = 0x%x, pcnt = 0x%x, rest_time = %d fw_offload = %d, running  = %d per_mon_time = 0x%x 
1374,IIIIIIIII,ROAM_PER_CONFIG_2 TX|hirate = %d lowrate = %d pcnt = %d, slot_size = %d RX|hirate = %d lowrate = %d pcnt = %d slot_size = %d, min_rssi = -%d 
1373,II,ROAM_PER_PDEV_REG_FAILED status = %d vdev_id = %d 
1372,IIIIIIIII,ROAM_PER_TXRX_HIGH_INDEX type = %d index(%d %d %d %d %d %d %d %d) 
1371,IIII,ROAM_PER_MCS_TXRX_DATA mcs(6-9):- %d %d %d %d 
1370,IIIIIIII,ROAM_PER_OFDM_TXRX_DATA (0-7)%d %d %d %d %d %d %d %d 
1369,IIIIIII,ROAM_PER_CCK_TXRX_DATA (0-6) %d %d %d %d %d %d %d 
1368,IIIIIIII,ROAM_PER_TXRX_LOW_INDEX %d %d %d %d %d %d %d %d 
1367,IIIIIIII,ROAM_PER_MCS_TXRX_DATA nss = %d, bw = %d, mcs(0-5):- %d %d %d %d %d %d 
1366,IIIIII,ROAM_PER_REST_TMR_EXP id = %d intval = %d(msec) roam_ctrl.running = %d roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d scan_status = %d, curr_rssi = -%d dBm 
1365,II,PER_CLIENT_NOTIFIER_PER_MON_NULL per_mon:0x%x vdev_roam:0x%0x 
1364,,PER_CLIENT_NOTIFIER_PER_CLIENT_INFO_NULL 
1363,IIIIII,ROAM_PER_CLIENT_NOTIFY_CHECK evt = %d, evt_allow = %d tx
x_slots = 0x%x tx
x_pcnt = 0x%x curr_tx
x_slots = 0x%x per_tx
x_pcnt = 0x%x  
1428,II,add_ccx_ie: ccx_cap=%d,ese_conn=%d 
1427,,add_ccx_ie: null 
1426,I,FILS_DEBUG HLP IEs len %d 
1425,I,wlan_frmgen_add_rsn_wpa_akm_suite akm=%d 
1424,IIII,MLME_DEBUG_CMN  0x%x 0x%x 0x%x 0x%x 0x%x 
1416,IIII,MLME_DEBUG_CMN  0x%x 0x%x 0x%x 0x%x 
1423,II,MLME_FRMGEN wmm_tspec_ie_len=%d is_11r=%d 
1422,I,WLAN_FRMGEN_GET_ACTION_BA wrong type:%d 
1421,I,WLAN_FRMGEN_GET_ACTION_SMPS incorrect sm_power_control:0x%x 
1420,IIIIIIII,WLAN_FRMGEN_GET_ACTION_TM lci_ie_len:%d lci_ie:0x%x civ_ie_len:%d civ_ie:0x%x ftm_ie_len:%d ftm_ie:0x%x vendor_ie_len:%d vendor_ie:0x%x 
1419,IIIIIIII,WLAN_FRMGEN_GET_ACTION_TMR lci_ie_len:%d lci_ie:0x%x civ_ie_len:%d civ_ie:0x%x ftm_ie_len:%d ftm_ie:0x%x vendor_ie_len:%d vendor_ie:0x%x 
1418,III,frmgen_get_default_ie vdev_id=%d fc_type=0x%x length=%d 
1417,III,WLAN_FRMGEN_GET_NULLFUNC_WITH_HTCTRL FAIL! peer:0x%x addr1:0x%x addr3:0x%x 
1416,IIII,MLME_DEBUG_CMN  0x%x 0x%x 0x%x 0x%x 
1414,I,frmgen_reassoc_req: missing ie=%d 
1414,I,frmgen_reassoc_req: missing ie=%d 
1415,II,MLME_REASSOC_ADD_VENDOR_IE %d %d 
1414,I,frmgen_reassoc_req: missing ie=%d 
1413,II,WLAN_FRMGEN_GET_TDLS_ACTION_CH_SWITCH_REQ FAIL! vdev:0x%x peer:0x%x 
1412,II,WLAN_FRMGEN_GET_TDLS_ACTION_CH_SWITCH_RESP FAIL! vdev:0x%x peer:0x%x 
1411,III,WLAN_FRMGEN_GET_TDLS_ACTION_PTI FAIL! vdev:0x%x peer:0x%x bss:0x%x 
1410,III,WLAN_FRMGEN_GET_TDLS_ACTION_PTR FAIL! vdev:0x%x peer:0x%x bss:0x%x 
1409,IIII,frmgen_insert_default_ie vdev_id=%d frm_type=0x%x sub_type=0x%x ies_len=%d 
1408,I,MLME_FRMGEN_RIC_IE ric_ie_length too long:%d 
1407,IIII,MLME_FRMGEN_RIC_IE ric_idx %d ric_ie_len %d tspec.ts_info.tsid = 0x%x .user_priority = 0x%x 
1406,IIII,frmgen_set_default_ie: vdev=0x%x,frm_type=0x%x,buf=0x%x,len=%d 
1405,IIIII,frmgen_set_default_ie vdev_id=%d frm_type=0x%x ies_len=%d status=%d i=%d 
1404,I,build_nan_element_container_attr: pbuff: %p 
1403,I,nan_element_container_attr(After filling rate): pbuff: %p 
1402,I,nan_element_container_attr(After filling ex_rate): pbuff: %p 
1401,I,nan_element_container_attr(After filling HT CAP): pbuff: %p 
1400,I,nan_element_container_attr(After filling VHT CAP): pbuff: %p 
1399,I,nan_element_container_len: %d 
1552,II,MLME_FRMPARSE_ERROR_AUTH frm_len %d (< %d) 
1551,I,MLME_FRMPARSE_AUTH status_code %d 
1550,II,MLME_FRMPARSE_ERROR_BEACON_PROBE_RSP frm_len %d (< %d) 
1549,IIIIII,MLME_FRMPARSE_BEACON_PROBE_RSP is_bcn %d ie_count %d id 0x%02x len %d ie_status 0x%x remaining_len %d 
1548,II,MLME_FRMPARSE_WARN_BEACON_PROBE_RSP is_bcn %d remaing_len %d incomplete 
1547,II,MLME_FRMPARSE_ERROR_BEACON_PROBE_RSP is_bcn %d mandatory IE %d missing 
1546,I,MLME_FRMPARSE_ERROR_CISCO_VENDOR invalid_len=%d 
1545,I,MLME_FRMPARSE_CISCO_VENDOR version ie ver = %d 
1544,II,MLME_FRMPARSE_WARN_DS_PARAMS ie->ie_len %d (exp %d). trying to interpret 
1543,III,MLME_FRMPARSE_WARN_DS_PARAMS ie->ie_len %d remaining_len %d (exp %d). ignore this IE 
1542,II,MLME_FRMPARSE_WARN_EDCA_PARAM ie->ie_len %d (exp %d). ignore this IE 
1541,II,MLME_FRMPARSE_WARN_EDCA_PARAM ie->ie_len %d remaining_len %d. ignore this IE 
1540,II,MLME_FRMPARSE_WARN_ERP ie->ie_len %d (exp %d) 
1539,III,MLME_FRMPARSE_WARN_ERP ie->ie_len %d remaining_len %d (exp %d). ignore this IE 
1538,II,MLME_FRMPARSE_WARN_ESP_CAP ie->ie_len %d (exp %d) ignore this IE 
1537,II,MLME_FRMPARSE_WARN_ESP_CAP remaining_len %d (exp %d) ignore this IE 
1536,II,MLME_FRMPARSE_WARN_EXT_CAP ie->ie_len %d (remaining %d) ignore this IE 
1535,I,MLME_FRMPARSE_WARN_EXT_CAP ie->ie_len %d ignore this IE 
1534,II,MLME_FRMPARSE_WARN_EXT_SUPP_RATE ie->ie_len %d remaining_len %d. ignore this IE 
1533,III,MLME_FRMPARSE_WARN_EXT_SUPP_RATE rate_index %d (> %d)-> trimmed to %d 
1532,I,MLME_FRMPARSE_WARN_EXT_SUPP_RATE skipped unknown rate 0x%x 
1531,,MLME_FRMPARSE_WARN_EXT_SUPP_RATE no known rate value 
1530,I,FILS_DEBUG Parsing HLP Container - %d 
1529,,FILS_DEBUG not a DHCP ACK 
1528,IIIIIIII,FILS_DEBUG own_ip_addr %d.%d.%d.%d recvd ip addr %d.%d.%d.%d 
1527,II,BTM_OFLD_PARSE_BTM_REQ_GET_PREFERENCE_ERROR remaining len(%d) < ie_hdr_len(%d) 
1526,II,BTM_OFLD_PARSE_BTM_REQ_GET_PREFERENCE Sub IE ID = %d, Length = %d 
1525,II,BTM_OFLD_PARSE_BTM_REQ_GET_PREFERENCE_ERROR remaining length(%d) < ie_len(%d) 
1524,,BTM_OFLD_PARSE_BTM_REQ_GET_PREFERENCE IE not present 
1523,II,MLME_FRMPARSE_WARN_HT_CAP ie->ie_len %d (exp %d) ignore this IE 
1522,II,MLME_FRMPARSE_WARN_HT_CAP remaining_len %d (exp %d) ignore this IE 
1521,II,MLME_FRMPARSE_WARN_HT_OPER ie->ie_len %d (exp %d) ignore this IE 
1520,II,MLME_FRMPARSE_WARN_HT_OPER remaining_len %d (exp %d) ignore this IE 
1519,,wlan_frmparse_is_dhcp_ack: dest addr doesnt match self addr 
1518,,wlan_frmparse_is_dhcp_ack: src addr doesnt match peer addr 
1517,,wlan_frmparse_is_dhcp_ack: ipv4 hdrlen is not as expected 
1516,,wlan_frmparse_is_dhcp_ack: not a udp packet 
1515,IIII,wlan_frmparse_is_dhcp_ack: src & dst port does not match dst:%d src:%d expected dst:%d expected src:%d 
1514,,wlan_frmparse_is_dhcp_ack: dhcp magic bytes did not match 
1513,,wlan_frmparse_is_dhcp_ack: dhcp options doesnt specify as DHCP ACK 
1512,,wlan_frmparse_is_dhcp_ack: doesnt match xid sent 
1511,I,MLME_FRMPARSE_ERROR_MS_VENDOR invalid_len=%d 
1510,II,MLME_FRMPARSE_WARN_MDIE ie->ie_len %d (exp %d). ignore this IE 
1509,II,MLME_FRMPARSE_WARN_MDIE remaining_len %d (exp %d). ignore this IE 
1508,II,FRMPARSE_WARN_MU_EDCA_PARAM ie->ie_len %d (exp %d). ignore this IE 
1507,II,FRMPARSE_WARN_MU_EDCA_PARAM ie->ie_len %d remaining_len %d. ignore this IE 
1506,I,Parsing nan_element_container_attr failed due to unexpected len: %d 
1505,IIIII,Parsing nan_element_container_attr ie_count %d id 0x%02x len %d ie_status 0x%x remaining_len %d 
1504,III,Parsing nan_element_container_attr failed id 0x%02x len %d ie_status 0x%x 
1503,I,Parsing nan_element_container_attr remaing_len %d incomplete 
1502,I,Parsing nan_element_container_attr mandatory IE %d missing 
1501,,11K_offload_PARSE_NEIGH_REP_RSP_ERROR frm_body is NULL 
1500,II,11K_offload_PARSE_NEIGH_REP_RSP_ERROR remaining_length(%d) < fixed_length(%d) 
1499,I,wlan_frmparse_neighbor_report_response remaining_length %d 
1498,II,11K_offload_PARSE_NEIGH_REP_RSP_ERROR remaining_length(%d) < ie_hdr_len(%d) 
1497,II,11K_offload_PARSE_NEIGH_REP_RSP_ERROR remaining_length(%d) < ie_len(%d) 
1496,II,11K_offload_PARSE_NEIGH_REP_RSP_ERROR Unknown IE found. ID = %d, Len = %d 
1495,II,MLME_FRMPARSE_WARN_QBSS ie->ie_len %d remaining_len %d. ignore this IE 
1494,II,MLME_FRMPARSE_WARN_QBSS ie->ie_len %d (!= %d) 
1493,II,MLME_FRMPARSE_WARN_QOS_CAP ie->ie_len %d (exp %d). ignore this IE 
1492,II,MLME_FRMPARSE_WARN_QOS_CAP remaining ie_len %d (exp > %d). ignore this IE 
1491,II,MLME_FRMPARSE_ERROR_REASSOC_RSP frm_len %d (< %d) 
1490,I,MLME_FRMPARSE_ERROR_REASSOC_RSP status_code=%d 
1489,II,Parsing extension IE in re-assoc rsp with eid %d len %d 
1488,II,Unknown extended element id: %d  len: %d in reassoc rsp 
1487,IIIII,MLME_FRMPARSE_REASSOC_RSP ie_count %d id 0x%02x len %d ie_status 0x%x remaining_len %d 
1486,III,MLME_FRMPARSE_ERROR_REASSOC_RSP missing mandatory IE 
1485,II,MLME_FRMPARSE_WARN_RIC_DATA ie->ie_len %d (exp %d). ignore this IE 
1484,II,MLME_FRMPARSE_WARN_RIC_DATA remaining_len %d (exp %d). ignore this IE 
1483,II,MLME_FRMPARSE_WARN_RIC_DESCRIPTOR ie->ie_len %d (< %d). ignore this IE 
1482,II,MLME_FRMPARSE_WARN_RIC_DESCRIPTOR remaining_len %d (< %d). ignore this IE 
1481,II,MLME_FRMPARSE_WARN_SSID ie->ie_len %d (> %d) 
1480,II,MLME_FRMPARSE_WARN_SSID ie->ie_len %d remaining_len %d. ignore this IE 
1479,II,MLME_FRMPARSE_WARN_SUPP_RATE ie->len %d (> %d)-> ignore this IE 
1478,II,MLME_FRMPARSE_WARN_SUPP_RATE ie->ie_len %d remaining_len %d. ignore this IE 
1477,I,MLME_FRMPARSE_WARN_SUPP_RATE skipped unknown rate 0x%x 
1476,,MLME_FRMPARSE_WARN_SUPP_RATE no known rate value 
1475,II,MLME_FRMPARSE_WARN_TSPEC ie->ie_len %d (exp %d). ignore this IE 
1474,II,MLME_FRMPARSE_WARN_TSPEC remaining_len %d (exp %d). ignore this IE 
1473,III,MLME_FRMPARSE_WARN_VENDOR invalid ie_len=%d remaining_len=%d (<%d) 
1472,II,MLME_FRMPARSE_WARN_VENDOR ie->ie_len %d remaining_len %d. ignore this IE 
1471,I,MLME_FRMPARSE_VENDOR_VHT unknown type %d 
1470,I,MLME_FRMPARSE_VENDOR_VHT unknown subtype %d 
1469,II,MLME_FRMPARSE_WARN_VENDOR_VHT remaining_len %d (exp %d) ignore this IE 
1468,I,MLME_FRMPARSE_WARN_VENDOR_VHT ERROR vht_caps. status %x
 
1467,I,MLME_FRMPARSE_WARN_VENDOR_VHT ERROR vht_oper. status %x
 
1466,II,MLME_FRMPARSE_WARN_VHT_CAP ie->ie_len %d (exp %d) ignore this IE 
1465,II,MLME_FRMPARSE_WARN_VHT_CAP remaining_len %d (exp %d) ignore this IE 
1464,II,MLME_FRMPARSE_WARN_VHT_OPER ie->ie_len %d (exp %d) ignore this IE 
1463,II,MLME_FRMPARSE_WARN_VHT_OPER remaining_len %d (exp %d) ignore this IE 
1462,II,MLME_FRMPARSE_WARN_WMM_AC ie_len %d (< %d). ignore this IE 
1461,I,MLME_FRMPARSE_ERROR_WMM_AC undefined ac %d 
1460,II,MLME_FRMPARSE_WARN_WMM_IE ie_len %d (< %d). ignore this IE 
1459,,BTM_OFLD_PARSE_BTM_REQ_ERROR frm_body is NULL 
1458,II,BTM_OFLD_PARSE_BTM_REQ_ERROR remaining_length(%d) < fixed_length(%d) 
1457,II,BTM_OFLD_PARSE_BTM_REQ_ERROR remaining_length(%d) < BSS_Termination_Duration_Length(%d) 
1456,I,BTM_OFLD_PARSE_BTM_REQ_ERROR remaining_length(%d) < session_info_length_field(1) 
1455,II,BTM_OFLD_PARSE_BTM_REQ_ERROR remaining_length(%d) < session_info_length(%d) 
1454,II,BTM_OFLD_PARSE_BTM_REQ_ERROR remaining_length(%d) < ie_hdr_len(%d) 
1453,II,BTM_OFLD_PARSE_BTM_REQ_ERROR remaining_length(%d) < ie_len(%d) 
1452,IIIIIIII,BTM_OFLD_PARSE_BTM_REQ Candidate_Info BSSID: %02x:%02x:%02x:%02x:%02x:%02x, Channel:%d, Preference: %d 
1451,II,BTM_OFLD_PARSE_BTM_REQ Unknown IE found. ID = %d, Len = %d 
1450,I,MLME_FRMPARSE_WPA_IE skip parsing as rsn_ie_len (%d) is present 
1449,IIII,MLME_FRMPARSE_WPA_RSN_CIPHER index %d unknown vendor oui 0x%08x 0x%08x 0x%08x 
1448,I,MLME_FRMPARSE_WPA_RSN_CIPHER_ERR can't use_group for suite type 0x%x 
1447,III,MLME_FRMPARSE_WPA_RSN_CIPHER index %d unknown suite type 0x%08x cipher_suite_type = %d 
1446,IIIII,MLME_FRMPARSE_WPA_RSN_CIPHER cipher_suite_count %d is_rsn %d suite_type %d (0=group,1=pair) cipher_type 0x%08x ie_status 0x%x 
1445,I,MLME_FRMPARSE_ERROR_WPA_RSN missing version field. remaining_len %d 
1444,II,MLME_FRMPARSE_ERROR_WPA_RSN version (%d) is not 1. remaining ie_len %d 
1443,I,MLME_FRMPARSE_WARN_WPA_RSN incomplete group cipher suite. remaining_len = %d (< 4) 
1442,I,MLME_FRMPARSE_WARN_WPA_RSN pairwise suite count remaining_len %d (< 2) 
1441,II,MLME_FRMPARSE_WARN_WPA_RSN incomplete pairwise cipher suite. remaining_len = %d (< %d) 
1440,I,MLME_FRMPARSE_WARN_WPA_RSN incomplete akm suite count remaining_len %d (< 2) 
1439,II,MLME_FRMPARSE_WARN_WPA_RSN incomplete akm suite. remaining_len = %d (< %d) 
1438,I,MLME_FRMPARSE_WARN_WPA_RSN incomplete rsn caps. remaining_len = %d (< 2) 
1437,I,MLME_FRMPARSE_WARN_WPA_RSN rsn_caps.pre_auth set in WPA. 
1436,I,MLME_FRMPARSE_WARN_WPA_RSN pmkid. remaining_len = %d (< 2) 
1435,II,MLME_FRMPARSE_WARN_WPA_RSN pmkid. remaining_len = %d (< %d) 
1434,I,MLME_FRMPARSE_WARN_WPA_RSN incomplete group mgmt cipher suite. remaining_len = %d (< 4) 
1433,IIII,MLME_FRMPARSE_WPA_RSN_AKM index %d unknown vendor oui 0x%08x 0x%08x 0x%08x 
1432,II,MLME_FRMPARSE_WPA_RSN_AKM index %d unknown suite type 0x%08x
 
1431,IIIII,MLME_FRMPARSE_WPA_RSN_AKM akm_suite_count %d is_rsn %d proto 0x%08x key_mgmt 0x%08x ie_status 0x%x 
1430,II,wlan_get_rx_nss nss=%d,%d 
1429,I,wlan_get_tx_nss nss=%d 
1553,I,KEYMGMT_CLR_KEY_ENTRY id=%d 
1554,IIIIII,KEYMGMT_INSTALL_KEY_ENTRY id=%d idx=%d key_flags_bitmap=0x%x len=%d peer_addr=0x04%x08%x 
1555,II,KEYMGMT_ADD_KEY_ENTRY_NO_MEM id=%d key_idx=%d 
1556,III,KEYMGMT_ADD_KEY_ENTRY_EXISTING key_idx=%d flags=0x%x len=%d 
1557,IIII,KEYMGMT_ADD_KEY_ENTRY id=%d key_idx=%d flags=0x%x len=%d 
1558,III,KEYMGMT_RESET_KEY id=%d peer_addr=%08x%04x 
1553,I,KEYMGMT_CLR_KEY_ENTRY id=%d 
1559,I,KEYMGMT_ADD_GROUP_KEY ERROR key_ciper:%d 
1560,I,KEYMGMT_ADD_GROUP_KEY WEP ERROR key_len:%d 
1561,,KEYMGMT_ADD_GROUP_KEY ERROR! wal_peer is NULL 
1562,I,KEYMGMT_ADD_PEER_ENTRY ERROR key_ciper:%d 
1563,I,KEYMGMT_ADD_PEER_ENTRY WEP ERROR key_len:%d 
1564,III,KEYMGMT_ADD_KEY_ENTRY_REINSTALLATION ERROR id=%d flags=0x%x len=%d 
1565,,KEYMGMT_ADD_PEER_ENTRY ERROR! wal_peer is NULL 
1566,I,BEACON_RESYNC_ARBITER_VDEV_DEINIT: vdev_id=%d 
1567,I,BEACON_RESYNC_ARBITER_VDEV_INIT: vdev_id=%d 
1568,III,BEACON_RESYNC_ARBITER_RESOLVE: vdev_id=%d, is_vdev_holding=%d, SLIST_EMPTY(hold_list)=%d 
1569,II,BEACON_RESYNC_ARBITER_REMOVE_CLIENT: vdev_id=%d, client_id=%d 
1570,II,BEACON_RESYNC_ARBITER_ADD_CLIENT: vdev_id=%d, client_id=%d 
1571,I,BEACON_RESYNC_ARBITER_CANCEL_ALL_REQUESTS: vdev_id=%d 
1572,II,BEACON_RESYNC_ARBITER_CANCEL_REQUEST: vdev_id=%d, client_id=%d 
1573,II,BEACON_RESYNC_ARBITER_REQUEST: vdev_id=%d, client_id=%d 
1574,,WLAN_BEACON_DTIMSYNC_CB ERROR! dev is NULL 
1575,II,nextdtim: 0x%08x%08x 
1576,,ni_dtimperiod is ZERO 
1577,III,_wlan_tsfoor_handler: vdev_id = %d : 0x%x tesf = 0x%x 
1578,II,WLAN_BEACON_CANCEL_RESYNC: vdev_id=%d, resyncBeacon=%d 
1579,II,WLAN_BEACON_RESYNC: vdev_id=%d, resyncBeacon=%d 
1580,IIII,WLAN_BEACON_TBTTOFFSET_UPDATE_HANDLER vdev_map mismatch i:%d vdev_map:0x%x vdev_id_map:0x%x max_diff:0x%x 
1581,,WLAN_BEACON_TBTTOFFSET_UPDATE_HANDLER ERROR! pmac is NULL 
1582,,WLAN_BEACON_WAL_TBTTOFFSET_UPDATE_HANDLER ERROR! pmac is NULL 
1583,IIII,QUIET IE STA: period=%d dur=%d, offset=%d, tbtt cnt=%d 
1584,II,tsf_beacon: 0x%08x%08x 
1585,,WLAN_BEACON_UPDATE_AGGR_CW register txdone notif fail! 
1588,II,phyerr event err: buf_len:%d>%d 
1587,,phyerr event: alloc event failure 
1586,IIIII,phyerr event, lo:%d, now_mac:%d, now_os:%d, phy0:%d, phy1:%d 
1589,III,wlan_dfs_phyerr_offload_unit_test input: vdevId=%d testId=%d num_args=%d 
1590,II,TXBFEE_DBGID_HOST_CONFIG_CMDID  ID=0x%x Value=0x%x 
1591,III,TXBFEE_DBGID_GID_RECEIVED vdev_id = %d gid=0x%x userpos=0x%x 
1592,I,Gid=%d
 
1593,II,i=%d, membership=0x%x
 
1594,,Non-directed GID frame
 
1595,II,TXBFEE_DBGID_BRPOLL_RECEIVED vdev_id = %d fbSegBmap=0x%x 
1596,IIII, TXBFEE_DBGID_NDPA_RECEIVED  vdev_id = %d sInfo0=0x%x sInfo1=0x%x Token=0x%x 
1597,, VDEV Registration Failed 
1598,IIIII,TXBF: SUBFee=0x%x MUBFee=0x%x SUBFer=0x%x MUBFer=0x%x chan->phy_mode=%d 
1599,II,wlan_txbf_cbf_recv:su_cv_expiry_cnt = %x cv_expiry_time =%x 
 
1600,IIIIII,nr=%x bw=%x nc=%x st=%x ng=%x cb=%x
 
1601,III,mimo_ctrl->fb_type=%x cv_idx=%d nc=%d
 
1602,I,wlan_txbf_cbf_recv:Sizeof cbf = %x
 
1603,II,UNIT_TEST_GEN  0x%x 0x%x 
1604,IIIII,UNIT_TEST_GEN  0x%x 0x%x 0x%x 0x%x, 0x%x 
1603,II,UNIT_TEST_GEN  0x%x 0x%x 
1605,,wlan_vdev is NULL 
1606,III,REGDB set init country command pdev_id=%d, cc_type=%d, cc_value=%x 
1607,II,REGDB set current country command pdev_id=%d cc=%x 
1608,,REGDB send WMI_REG_CHAN_LIST_CC_EVENTID 
1609,IIII,REGDB ruleIdx=%d freq info=%x bw_pwr=%x flag=%x 
1610,,REGDB wmi buf alloc fail 
1611,IIII,REGDB max_rules=%d 2g_rules=%d 5g_rules=%d, evt_len=%d 
1612,II,REGDB read reg rules alpha2 %c %c 
1613,IIIIII,REGDB dfs_reg=%x, phybitmap=%x minbw2g=%d maxbw2g=%d minbw5g=%d maxbw5g=%d 
1614,IIIIII,REGDB send def reg rules phy_id=%d status_code=%d, ctry_id=%d dom_code=%d, num_2g_rules=%d, num_5g_rules=%d 
1615,II,REGDB send default reg rules for alpha2: %c %c 
1616,I,REGDB send reg rules failed - status=%d 
1613,IIIIII,REGDB dfs_reg=%x, phybitmap=%x minbw2g=%d maxbw2g=%d minbw5g=%d maxbw5g=%d 
1617,IIIIII,REGDB phy_id=%d status_code=%d, ctry_id=%d dom_code=%d, num_2g_rules=%d, num_5g_rules=%d 
1618,II,REGDB send reg rules for alpha2: %c %c 
1616,I,REGDB send reg rules failed - status=%d 
1619,,REGDB fail - invalid get type 
1620,,REGDB fail - invalid country code input 
1621,IIII,REGDB send reg rules for mac_id=%d get_type=%d cc_type=%d cc_value=%x 
1622,, register - WMI_SERVICE_REGULATORY_DB  
1623,II,REGDB test command num_args=%d testId=%d value1=%x 
1624,,11d scan start scan not allowed, non-sta is up 
1625,I,11d: scan_vdev_stop_handler, vdev_id=%d 
1626,II,11d: scan_vdev_start_handler vdev id=%d, period=%d 
1627,I,11d: STOP_COMMAND_FAILED, %d 
1628,I,11d: SCAN_START_COMMAND_FAILED, %d 
1629,,11d: Length shorter than expected ieee80211_country_ie. 
1630,,11d: No CTRY IE  
1631,III,11d: frames_handler, subtype:%d, length:%d,vdevid:%d 
1632,III,11d: idx=%d, votes=%d, curr_cc_cnt=%d 
1633,,11d: invalid country code. ignore 
1634,,11d: wake evt not set, ignore scan 
1635,IIII,11d: new cc code = %c %c cur cc code = %c %c 
1636,III,11d: US_bcn=%d, cc_cnt=%d, fcc=%d 
1637,IIII,11d: bcn max_votes=%d idx=%d, cc=%c %c 
1638,I,11d: scan_evt_handler evt->type = %d 
1639,I,11d: SCAN_SCH_START_ALLOC_FAIL, %d 
1640,II,11d: scan evt_handler notif->type = %d,vdev->id=%d 
1641,I,11d: send new cc evt_id=%d 
1642,II,11d: test command num_args=%d testId=%d 
1643,,WMI_NDP_END_REQ_CMDID 
1644,,WMI_NDP_RESPONDER_REQ_CMDID 
1645,,WMI_NDP_INITIATOR_REQ_CMDID 
1646,,WMI_NDI_GET_CAP_REQ_CMDID 
1647,II,NAN_WmiCmdHdlr cmd:%x nan discovery state (%d) 
1648,,NAN-NAN_DBGID_SPARE_80: 0xBBBB 
1649,,NAN-NAN_DBGID_SPARE_80: 0xAAAA 
1650,,NAN_DBGID_NULL_PTR 
1651,,wmi_packet_prepared to be sent 
1652,,WMI_buffer_cleared 
1653,II,wmi_buffer pointers sent:0x%X received:0x%X 
1654,,Null Ptr error 
1655,,wmi_send_completion 
1657,,NANATTR_Init: pNan is Null returning A_EFAULT 
1656,,INVALID SERVICE NAME 
1658,I,NAN Service ID Attr has bad length %d 
1662,IIIIII,NAN-BEACON_RX: from %02x:%02x:%02x:%02x:%02x:%02x 
1661,IIIII,NAN-BEACON_RX: RSSI %u  valid %u  cluster 0x%04x  BI %u  statusFlags 0x%08x 
1660,I,Subscribe SID Attr: contains %d IDs 
1659,IIIIIIIII,NAN-SYNC_BEACON_DW_STATS: total rx %u  c1=(%u/%u/%u  %u) c2=(%u/%u/%u  %u) 
1663,,NAN: Beacon Tx is already in progress. Skipping new request to send 
1697,,NAN - 5G FAW Antenna granted 
1696,I,Invalid channel %u
 
1695,,EnableReqHdlr: Failed to Enable MAC 
1694,,EnableReqHdlr:NAN Basic mode started  
1693,,NAN-DISABLE 
1692,,nan_ctrl_disable: NAN_disable sleep 
1691,,NAN-ENABLE failed 
1690,,nan_ctrl_enable: NAN_ENABLE sleep 
1690,,nan_ctrl_enable: NAN_ENABLE sleep 
1689,,NAN-ENABLE 
1688,I,postpone NAN-ENABLE, cur_hw_mode = %d 
1687,I,NANCTRL_NANDisable_Internal()cmd_requestor: %d 
1686,,nan_ctrl_disable: NAN_ENABLE sleep 
1685,II,NANCTRL_NAN_Enable_timeout: do postponed nan enable, hw_mode=%d, enable_pending = %d 
1684,,NANCTRL_ResmgrEvtHdlr: start timer for postponed nan enable 
1679,,WMI_EVENT_BUFFER not available for NAN 
1683,,Disabled DiscMacAddressEvent 
1682,,Disabled disableDiscStartedClusterEvent 
1681,,Disabled disableDiscJoinedClusterEvent 
1680,,NANCTRL_SendFollowupInd 
1679,,WMI_EVENT_BUFFER not available for NAN 
1678,,NANCTRL_StatsReqHdlr: Received 
1677,,NANCTRL_StatsReqHdlr: Received Timing Sync Req 
1676,I,nan_config: Discovery beacon interval length error tlv.length: %d 
1675,I,nan_config: Discovery beacon interval:%d 
1671,,NAN Enable/Config: DW_EARLY_TERMINATION_LENGTH ERROR 
1674,I,RANGING_ENABLED %d 
 
1673,II,Discovery_Ind %x %d
 
1672,I,NAN-ENABLE mac addr randomization interval = %d 
1671,,NAN Enable/Config: DW_EARLY_TERMINATION_LENGTH ERROR 
1670,I,NAN_TLV_TYPE_DW_EARLY_TERMINATION %d 
 
1669,,NAN Enable/Config: NAN_TX_RX_CHAINS_TLV_LENGTH_ERROR 
1668,I,NAN_TLV_TYPE_TX_RX_CHAINS %d 
 
1667,I,NANCTRL_TransmitFollowupReqHdlr trId - %d 
1666,I,NANCTRL_TransmitFollowupReqHdlr trId : %d 
1665,II,NANCTRL_TransmitFollowupRespIndHdlr msgId - %d trId - %d 
1664,I,NANCTRL_UpdateScanPolicy: NAN disableAsyncScanFlag %d 
1734,,nan_de_if:Dummy frame Wake 
1733,,nan_de_if: Dummy frame sleep 
1732,I,wlan_nan_de_if_tx_completion_bcn: completion status: %d 
1731,,nan_sched: Disc beacon completion sleep 
1730,,Error processing Tx completion for Beacon 
1729,III,Ignoring processing Tx completion for SDF/NMF nan_ctxt:%x nan_ctxt->vdevp:%x abf:%x 
1728,,Error processing Tx completion for SDF 
1727,IIII,NAN-TX_COMPLETE - frame_type:%d DWCM_RETRY:%d status:%u followup_queued:%d 
1726,IIII,NAN-TX_COMPLETE - frame_type:%d DWCM_RETRY:%d status:%u abf->flag=0x%x 
1725,I,NAN-TX_COMPLETE frame_type:%d 
1724,,NAN-TX_COMPLETE - power state awake setting back-off-params 
1723,,nan_ctrl_pm_arb_req: NULL pointer ctxt 
1722,,nan_ctrl_pm_arb_req: NULL pointer Vdev 
1721,I,nan_ctrl_pm_arb_req: awake_status %d 
1720,II,wlan_nan_de_if_FollowupInd transactionId  : %d Status : %d 
1719,I,wlan_nan_de_if_bcn_send frame_hdr is NULL or len %x 
1718,,nan_de_if_delete: Sleep 
1717,II,Followup_tx_complete retry_count : count:%d completion_status : %d  
1716,II,Followup_tx_complete - Done : retry_count:%d completion_status:%d  
1715,,nan_de_if: tx_completion_sdf awake 
1714,,nan_de_if: tx_completion_sdf sleep 
1713,I,wlan_nan_de_if_sdf_send SDF/NMF frame_hdr is NULL or len %x 
1712,,local send failed 
1711,IIII,NAN_DBGID_DWCM SDF/NMF QUEUE_ sdf_queued:%d, nmf_queued:%d, followup_queued:%d retry_count:%d 
1710,I,wlan_nan_de_if_sdf_send SDF/NMF-%d Queued 
1709,IIIII,wlan_nan_de_if_sdf_send frame_type=%d seq_num=%d abf->flag=0x%x in_dw_only:%d in_dw:0x%x 
1708,,wlan_nan_de_if_sdf_send: Skipping frame transmission as outside dw 
1707,II,NAN_DBGID_DWCM Trsp timer = %d %d 
1706,,Too close to DW hence skipping attempt to send SDF01 
1705,I,NAN_DBGID_DWCM dw time left = %d 
1704,I,NAN_DE_IF: Too close to DW on retry hence skipping attempt to send SDF %d 
1703,,NAN_DBGID_DWCM dw unknown 
1702,I,NAN_DE_IF: Send secure frame len = %d 
1701,,Tx completion received with NULL abf frame 
1700,II,Tx completion received with %d  and not %d 
1699,,Setting Dtim period to true 
1698,,Setting CRITICAL priority 
1738,IIIII,NAN -> API_MSG_HEADER: msgId %u  msgVersion %u  msgLen %u  handle %u  transId %u 
1737,IIIII,NAN ->     MSG_DATA: %02X %02X %02X %02X %02X 
1736,II,NAN -  OTA_PKT_HEADER:  isTx %u  frameLength %u 
1735,IIIII,NAN ->      PKT_DATA: %02X %02X %02X %02X 
1772,II,Config Changed: nss %d -> %d 
1771,II,Config Changed: committed dw 5g %d -> %d 
1771,II,Config Changed: committed dw 5g %d -> %d 
1770,II,Config Changed: discMacaddrRandInterval %u -> %u 
1769,,DW frame buffer allocation failed ERR ERR 
1765,II,NAN_FOLLOWUP : NANMAC_BuildFollowupFrame VSA short of len so exiting : %u : %u 
1768,II,NAN_SDF : NANMAC_BuildDwServiceDiscoveryFrame short of len so exiting : %u : %u 
1768,II,NAN_SDF : NANMAC_BuildDwServiceDiscoveryFrame short of len so exiting : %u : %u 
1767,,NAN_FOLLOWUP : Frame allocation failed 
1766,II,NAN_FOLLOWUP : NANMAC_BuildFollowupFrame short of len so exiting : %u : %u 
1765,II,NAN_FOLLOWUP : NANMAC_BuildFollowupFrame VSA short of len so exiting : %u : %u 
1764,II,NANMAC_ConfigCommittedDW #1 %d:%d 
1763,II,NANMAC_ConfigCommittedDW #2 %d:%d 
1760,,wlan_nan_mac: wakeup for nan_enable 
1762,I,Register MAC address for AP vdev, vdev_id=%d 
1761,I,Unregister MAC address for NDI, vdev_id=%d 
1760,,wlan_nan_mac: wakeup for nan_enable 
1759,I,Unregister MAC address for AP vdev, vdev_id=%d 
1758,I,discMacRandomTimeout = %u 
1757,I,PrepareForDw : Free dwTxSdfBuf Len:%d 
1756,,NAN <==================================] DW_STOP 
1755,II,NAN [==================================> DW_START (pri=%u  5g=%u) 
1754,II,DWStart TxOp %x %x 
1753,,NAN_DBGID_SDF_SEND 
1752,III,NAN_MAC: SDF framelen = %d attrId = 0x%x attrlen = 0x%x 
1751,,wlan_nan_mac: Match not found, de-allocating cache 
1750,II,NAN_MAC: Received ouitype%x Secured frame framelen = %d 
1749,II,NAN_MAC: Received ouitype%x non Secured  frame framelen = %d 
1748,II,NANMAC_SdfTxComplete : Building Followup Frame followupBuilt:%d Len:%d 
1747,,NANMAC_SdfTxComplete : Calling NANMAC_TransmitDwFollowupFrame 
1746,II,role 0x%x, debuggingflags 0x%x 
1745,I,debuggingflags 0x%x 
1744,,NANMAC_TransmitDwFollowupFrame : FollowupBuf NULL 
1743,,NANMAC_TransmitDwFollowupFrame : Failed to TX SDF 
1742,,NANMAC_TransmitDwFollowupFrame : DW FollowupFrame queued for transmit 
1741,,TransmitDwServiceDiscoveryFrame : Faild to TX 
1740,,TransmitDwServiceDiscoveryFrame : DW SDF queued for transmit 
1739,III,Current TW params: twSize=%d n=%d twIndex=%d
 
1798,,NANPUB_Init: pNan is Null returning A_EFAULT 
1797,II,NAN-PUBSUB_PREPARED: handle %u  flags 0x%X 
1796,IIII,NAN-SUBSCRIBE_MATCH_LOG: handle %u  match handle %u  match timestamp %u  timestamp %u 
1795,IIIIIIII,NAN-PUBSUB_FOLLOWUP_RECEIVED: handle %u  matchHandle 0x%04X  macAddr %02X:%02X:%02X:%02X:%02X:%02X 
1794,IIII,NAN-PUBSUB_FOLLOWUP_RECEIVED: handle %u  matchHandle 0x%04X inId %u  reqId %u 
1793,I,NAN-PUB : isServiceUpdateId : %d 
1792,IIIIIII,NAN-PUBSUB_MATCHED: handle %u  svcId %02X:%02X:%02X:%02X:%02X:%02X  
1791,IIII,NAN-PUBSUB_MATCHED: inId %u  reqId %u  svcCtrl 0x%02x  len %u 
1790,I,NAN-PUBSUB_REMOVE_DEFERRED: handle %u 
1789,I,NAN-PUBSUB_REMOVE_PENDING: handle %u 
1788,I,NAN-PUBSUB_REMOVED: handle %u 
1787,I,txType = %d 
1786,I,PMK Set, len %d 
1785,I,PASSPHRASE Set, len %d 
1784,I,Cancel Range Request with id: %d 
1783,I,NAN_DBGID_INVALID_MSG_PARAM, tlv.length: 0x%x 
1782,I,NAN-PUBSUB_UPDATED: handle %u 
1781,III,SDEA Control Received in Publish Value security_required %d ranging_required %d range_report_required %d 
1780,I,NAN PUBLISH SDEA UPDATATE INDI : %d 
1779,III,NAN-PUBSUB_PROCESSED: handle %u	status %u  value %u 
1679,,WMI_EVENT_BUFFER not available for NAN 
1778,,NANPUB_UpdatePublishFA 
1777,I,NAN_PrepareFAAttr_ForSDF fa_attr_offset_len: %d 
1776,,SDEA Control Received in Publish 
1775,,PMK Set, building PMKID 
1774,I,NAN_PrepareFAAttr_ForSDF pPublish->txAttr.len %d 
1773,I,SDEA Control Received in Publish Value new value%d 
1805,,INVALID SDF: ieee80211_frame not found 
1804,I,_wlan_nan_if_internal_rx_sdf_handler drop this frame seq_no:%d 
1803,,INVALID SDF: ieee80211_action_nan not found 
1802,,nan_rx_offload_register: Wake 
1801,,nan_rx_offload_register: NAN_ENABLE sleep 
1800,,nan_rx_filter: Wake 
1799,,nan_rx_filter: Sleep 
1820,III,NAN20_StartScanPeriodicULW: Enabled(%d) ScanCnt(%d) ScanSchedIdx(%d) 
1819,III,NAN20_StartScanPeriodicULW start_time internal %x external %x curr_time %x 
1818,,NAN20_StartScanPeriodicULW: Start ULW failed as ulw allocation failed 
1817,IIII,NAN20_StopScanPeriodicULW: Enabled(%d) ScanCnt(%d) ScanSchedIdx(%d) force(%d) 
1816,I,NAN20_StopScanPeriodicULW curr_time %x 
1815,,NAN20_StopScanPeriodicULW: Stop ULW failed as ulw update failed 
1814,II,CHANNEL_TYPE:%d channel_Freq %d 
1813,,NANScan_Event: p2p scan starts, disable NAN 
1812,IIIII,NANScan_Event: scanid=%d, event=0x%x, rsn=0x%x, ch=%d nanScanType:%d 
1811,IIIII,NANScan_Event: STARTED, %d %d 0x%x %d %d 
1810,III,NANScan_Event: START FAILED, %d %d 0x%x 
1809,III,NANScan_Event: COMPLETED, %d %d 0x%x 
1808,III,NANScan_Event: DEQUEUED, %d %d 0x%x 
1807,IIII,NANScan_Event: CH_SWITCH, %d %d 0x%x 0x%x 
1806,IIII,NANScan_Event: UNHANDLED EVENT, 0x%x %d %d 0x%x 
1894,III,NAN-CHREQ_GRANT: freq %u  type %u  tsfLo 0x%08x 
1893,III,NAN-CHREQ_END: freq %u  type %u  tsfLo 0x%08x 
1892,III,NAN-CHREQ_ERROR: freq %u  type %u  tsfLo 0x%08x 
1891,IIII,NAN_DBGID_TSF_DUMP: #1 curr_tsf_upper 0x%X, curr_tsf_lower 0x%X, nextDwTsf_upper 0x%X, nextDwTsf_lower 0x%X 
1890,I,NAN_SCHED: ULW distance to the next DW %x 
1889,,nan_sched: Disc channel Wake 
1888,I,NAN_DBGID_BEACON_TX_SEND DB Bcn Tbd= %d 
1838,,NAN_SCHED_DO_CHANNEL_REQ: Read config error 
1887,II,NAN_DBGID_DW_SKIP:0x%X, curr_tsf_lower:0x%X 
1886,II,NAN_DBGID_DW_SKIP:0x%X, next_tsf_lower:0x%X 
1885,II,NAN_DBGID_DW_SKIP:0x%X, offset:0x%X 
1884,II,NAN_DBGID_DW_SKIP:0x%X, start_time:0x%X 
1883,,wlan_nan_sched: Wakeup not permitted in 5G 
1882,II,nan_sched: offset_tbtt %d sta_Channel %d 
1881,II,nan_sched: no time for one more DB diff:%d interval:%d 
1880,III,nan_sched: offset %d pSync->nextDwTsf %d curr_tsf %d  
1879,,nan_sched: DW Channel end Wake 
1878,,nan_sched:DW Channel end sleep 
1877,,Start DB Request 
1833,,Stop DB Request 
1876,,nan_sched: DW Channel grant: Wake 
1875,,nan_sched: DW Channel grant error: sleep 
1874,III,NAN_DBGID_SPARE_80: type 0x%X  freq %p  curr_tsf 0x%08x 
1873,IIII,NAN_DBGID_TSF_DUMP: curr_tsf_upper 0x%X, curr_tsf_lower 0x%X, nextDwTsf_upper 0x%X, nextDwTsf_lower 0x%X 
1872,III,NAN_DBGID_DW_SKIP:0x%X, curr_tsf_lower:0x%X, diff: 0x%X 
1871,III,NAN_DBGID_DW_SKIP:0x%X, curr_tsf_lower:0x%X, diff: 0x%x 
1870,III,NAN_DBGID_DW_SKIP:0x%X, curr_tsf_lower:0x%X, diff: %p 
1869,,NAN_DBGID_SPARE_80:0xFFF5 
1868,I,NAN_DBGID_SPARE_80:0xFFF4, timer: 0x%X 
1867,II,NAN_ENABLE_DBG_STATS: enabled:%d period:%d 
1866,III,NANSCHED_FaScheduler: Triggering FA index:%d FA type:%d Active:%d 
1865,,NAN_SCHED: FawChannelGrant 
1864,,# UN-Pause NDP vdev 
1863,I,NAN_SCHED: Un-Pause NDP vdev : %d 
1862,I,NAN_SCHED: Pause NDP vdev : %d 
1861,,NAN_SCHED: FawChannelEnd 
1860,,nan_sched faw_grant_end sleep 
1859,,nan_faw_channel_grant: Wake 
1858,III,NANSCHED_GetCurrNanSlot: Tsf:0x%x(U) 0x%x(L) dwOffset:%d 
1857,III,NANSCHED_GetCurrNanSlot: dw0SlotNum:%d slotNum:%d slotOffset:%d 
1856,,NANSCHED_GetNANDwEnd_Tsf() pSync NULL !!! 
1855,IIII,NAN-Dw End Tsf: offset %x start_time %x currSlot %x slotOffset %x 
1854,,NANSCHED_HandleDwEnd 
1853,,NANSCHED_HandleDwEnd Primary DW 
1852,IIII,NAN_DBGID_TSF_DUMP: #2 curr_tsf_upper 0x%X, curr_tsf_lower 0x%X, nextDwTsf_upper 0x%X, nextDwTsf_lower 0x%X 
1851,II,NAN_DBGID_BEACON_TX_SEND Dw Sync Bcn Tbd= %d, DWtype = %d 
1850,,NAN-NAN_DBGID_SPARE_80: 0xFFFA 
1849,IIII,NAN_SCHED: Flushing pending frames SDF(%d)/FOLLOWUP(%d)/NMF(%d)/Total(%d) in SW queue at Pre DW 
1848,IIII,NANSCHED_NanTimeoutSlotStart: dw0SlotNum:%d slotNum:%d slotOffset:%d timerDuration:%d 
1847,III,NANSCHED_NanTimeoutSlotStart: Forcing to end FA %d early %d 0x%x 
1846,IIII,NANSCHED_NanTimeoutSlotStart: idx:%d slotActive:%d SlotBitmap:0x%x AvailabilityMap:0x%x 
1845,III,NAN_PRINT_DBG_STATS: Printing debug stats(periodInDw:%u, dwCount:%u, dwSkippedCount:%u) 
1844,IIII,NAN_PRINT_DBG_STATS: faInLateTime:%u faOutInBetweenTime:%u faOutEarlyTime:%u faUlwTime:%u 
1843,II,NAN_PRINT_DBG_STATS: FAType:%d chan:%d 
1842,IIII,NAN_PRINT_DBG_STATS: faTotalTime:%u faActiveTime:%u(Percentage:%d) faSkippedCount:%d 
1841,,NAN_RESET_DBG_STATS: Resetting debug stats 
1840,IIIII,NAN-RX_CALLBACK: type 0x%X  lenth %u  currTsf 0x%08x  rssi %u  freq %u 
1840,IIIII,NAN-RX_CALLBACK: type 0x%X  lenth %u  currTsf 0x%08x  rssi %u  freq %u 
1839,,NAN - 5G Enabled failed  
1838,,NAN_SCHED_DO_CHANNEL_REQ: Read config error 
1838,,NAN_SCHED_DO_CHANNEL_REQ: Read config error 
1837,II,5G DW Start: %d status_error:%d 
1836,I,5G DW Start status: %d 
1835,IIII,NANSCHED_StartDw_5g() status: %d fa_entry: %p dw_secondary_started: %d nanSecFreq: %d 
1834,I,NAN-NAN_DBGID_SPARE_80: NANSCHED_StartFaw: channel %d 
1833,,Stop DB Request 
1832,IIII,NANSCHED_StopDw_5g() status: %d fa_entry: %p dw_secondary_started: %d dw_secondary_active: %d 
1831,,nan_sched:wal_tsf_dw_timer: wake 
1830,II,NAN-TSF_TIMEOUT: currTsf 0x%08x  usecs %u 
1829,,NANSCHED_TsfTimeoutDWTbtt:wake 
1828,,NAN-NAN_DBGID_SPARE_80: 0xFFF9 
1827,IIIII,NAN-TX_COMPLETE: type 0x%X  handle %p  buf %p  status %u  currTsf 0x%08x 
1826,,nan_sched_resmgr_link: NAN Ctxt NULL 
1825,,nan_sched_resmgr_link: NAN VDEV is NULL - NAN is not enabled 
1824,,nan_sched_resmgr_link: Channel->mhz zero or channel is NULL 
1822,I,nan_sched_resmgr_link nss: %d 
1824,,nan_sched_resmgr_link: Channel->mhz zero or channel is NULL 
1823,II,nan_sched_resmgr_link: create new link channel:%d flags: 0x%x 
1822,I,nan_sched_resmgr_link nss: %d 
1821,I,5G DW freq:%d 
1788,I,NAN-PUBSUB_REMOVED: handle %u 
1909,,NANSUB_Init: pNan is Null returning A_EFAULT 
1796,IIII,NAN-SUBSCRIBE_MATCH_LOG: handle %u  match handle %u  match timestamp %u  timestamp %u 
1795,IIIIIIII,NAN-PUBSUB_FOLLOWUP_RECEIVED: handle %u  matchHandle 0x%04X  macAddr %02X:%02X:%02X:%02X:%02X:%02X 
1794,IIII,NAN-PUBSUB_FOLLOWUP_RECEIVED: handle %u  matchHandle 0x%04X inId %u  reqId %u 
1908,III,NAN-SUBSCRIBE_MATCH_NEW: handle %u  match handle %u	timestamp %u 
1907,III,NAN-SUBSCRIBE_MATCH_REPEAT: handle %u  match handle %u  timestamp %u 
1906,I,NAN-SUB : isServiceUpdateId : %d 
1905,III,NAN-SUBSCRIBE %d, %d, %d 
1904,IIIIIII,NAN-PUBSUB_MATCHED_SKIPPED_SSI: handle %u  svcId %02X:%02X:%02X:%02X:%02X:%02X  
1791,IIII,NAN-PUBSUB_MATCHED: inId %u  reqId %u  svcCtrl 0x%02x  len %u 
1792,IIIIIII,NAN-PUBSUB_MATCHED: handle %u  svcId %02X:%02X:%02X:%02X:%02X:%02X  
1791,IIII,NAN-PUBSUB_MATCHED: inId %u  reqId %u  svcCtrl 0x%02x  len %u 
1790,I,NAN-PUBSUB_REMOVE_DEFERRED: handle %u 
1789,I,NAN-PUBSUB_REMOVE_PENDING: handle %u 
1788,I,NAN-PUBSUB_REMOVED: handle %u 
1785,I,PASSPHRASE Set, len %d 
1903,I,Ranging config indication event %d 
1902,II,Ranging config ingress distance:%d egress distance:%d  
1782,I,NAN-PUBSUB_UPDATED: handle %u 
1901,I,NAN SUBSCRIBE SDEA UPDATATE INDI : %d 
1900,,NAN SUBSCRIBE SDEA Ranging Disabled: Delete ranging instance 
1779,III,NAN-PUBSUB_PROCESSED: handle %u	status %u  value %u 
1899,I,Initiate service based ranging with range_id %d 
1898,,Match not found Range initiation failed 
1897,,Cancel ranging 
1896,,Cancel Ranging failed 
1895,I,NANSUB_SubscribeUpdateLocalMatchFilter : %d 
1925,II,NANSYNC_EnableDisableDiscMacRandomization(): %d RandomTimeout: %d 
1924,II,NAN20_Sync stats ndp freq1:%d freq2:%d 
1923,,NAN MAC randomization timer expired 
1922,IIIIII,old mac: %02x:%02x:%02x:%02x:%02x:%02x 
1921,IIIIII,new mac: %02x:%02x:%02x:%02x:%02x:%02x 
1920,IIII,NAN-BEACON_TX_SEND: type 0x%X  tsfLo 0x%08x  rval %u  hc %u 
1919,I,NAN-BEACON_TX_CANCEL: tsfLo 0x%08x 
1918,III,NAN-BEACON_TX (prepare): buf %p  len %u  rval %u 
1917,,nan_sync Set ClusterID: Wake 
1916,I,NANSYNC_SetClusterId: %d 
1915,,nan_sync Set ClusterID: Sleep 
1914,III,NAN-ROLE_CHANGE: %d -> %d (isFORCED=%d) 
1913,IIII,NAN-NEW_ANCHORMASTER: rank=0x%08x_%08x (mp=%d  rf=%d) 
1912,III,NAN-ANCHORMASTER_RECORD_UPDATE_LAST:  rank=0x%08x_%08x BTT=0x%08x 
1911,IIII,NAN-ANCHORMASTER_RECORD_UPDATE: rank=0x%08x_%08x HC=%d BTT=0x%08x 
1910,IIII,NAN-NEW_MASTERRANK: rank=0x%08x_%08x (mp=%d  rf=%d) 
1943,II,NAN-REQUESTOR_ID: code 0x%X  requestorId 0x%X 
1942,I,NAN_SD_ATTR_INSTANCE_ID_DONT_CARE: code 0x%X 
1942,I,NAN_SD_ATTR_INSTANCE_ID_DONT_CARE: code 0x%X 
1943,II,NAN-REQUESTOR_ID: code 0x%X  requestorId 0x%X 
1942,I,NAN_SD_ATTR_INSTANCE_ID_DONT_CARE: code 0x%X 
1942,I,NAN_SD_ATTR_INSTANCE_ID_DONT_CARE: code 0x%X 
1942,I,NAN_SD_ATTR_INSTANCE_ID_DONT_CARE: code 0x%X 
1941,,NANMATCH_Init: pNan is Null returning A_EFAULT 
1940,IIII,NAN : SUBSCRIBE_MATCH_EXPIRED serviceHandle:0x%x handle:%d timestamp1:%d timestamp2:%d 
1939,II,NAN : MATCH_EXPIRED delta:%d unmatchTimeout:%d 
1679,,WMI_EVENT_BUFFER not available for NAN 
1938,II,NANMATCH_SendRangeResult ranging_indication_event 0x%x range_measurement %d 
1937,,NANMATCH_SendRangeResult: Failed to get Range Result 
1936,II,NANMATCH_SendRangeResult:Inner_threshold %d Outer_threshold %d 
1935,,NANMATCH_SendRangeResult: Notify if the devices enters subsequently 
1934,,NANMATCH_SendRangeResult:Only_inner threshold set 
1933,,NANMATCH_SendRangeResult: Ingress met no action needed 
1932,,NANMATCH_SendRangeResult: Ingress met 
1931,,NANMATCH_SendRangeResult: Notify if the devices exits subsequently 
1930,,NANMATCH_SendRangeResult: Egress met no action needed 
1929,,NANMATCH_SendRangeResult: Egress met 
1928,,NANMATCH_SendRangeResult: Continuous range result 
1927,II,NAN : SUBSCRIBE_MATCH_EXPIRED serviceHandle:0x%x handle:%d 
1926,I,nan_match_delete_ranging_instances: range_id %d 
1990,I,NAN20_UTILS: Received NMF Secured frame framelen = %d 
1989,I,NAN_20_ReceiveNMF_Parse_And_Validate failed: status: %d 
1981,,NAN20_UTILS: NMF RANGING TERMINATE RECEIVED 
1980,,NAN20_UTILS: NMF NAN_SCHEDULE_REQUEST RECEIVED 
1979,,NAN20_UTILS: NMF NAN_SCHEDULE_RESPONSE RECEIVED 
1978,,NAN20_UTILS: NMF NAN_SCHEDULE_CONFIRM RECEIVED 
1977,,NAN20_UTILS: NMF NAN_RANGING_REPORT RECEIVED 
1976,,NAN20_UTILS: NMF NAN UPDATE NOTIFICATION RECEIVED 
1988,II,NAN_20_ReceiveNMF_Parse_And_Validate: Received NMF with oui_subtype: %d framelen:%d 
1969,,NAN20_utils: 1st avail attribute decode failed 
1987,,NAN20_UTILS: Max ULW entries reached, Ignoring received ULW attr 
1986,,NAN20_UTILS: Invalid ULW attr 
1985,,NAN20_UTILS: Invalid attribute params 
1984,,NAN20_UTILS: element container not found: Reject NDP 
1983,,NAN_20_ReceiveNMF_Parse_And_Validate: Confirm receieved without NDP attribute 
1982,,NAN_20_ReceiveNMF_Parse_And_Validate: RSUA was not accepted 
1981,,NAN20_UTILS: NMF RANGING TERMINATE RECEIVED 
1980,,NAN20_UTILS: NMF NAN_SCHEDULE_REQUEST RECEIVED 
1979,,NAN20_UTILS: NMF NAN_SCHEDULE_RESPONSE RECEIVED 
1978,,NAN20_UTILS: NMF NAN_SCHEDULE_CONFIRM RECEIVED 
1977,,NAN20_UTILS: NMF NAN_RANGING_REPORT RECEIVED 
1976,,NAN20_UTILS: NMF NAN UPDATE NOTIFICATION RECEIVED 
1975,II,NAN20_UTILS: NMF attrId%x attrLen %x  
1974,IIII, %x %x %x %x  
1973,I, %x  
1972,I,NAN20_utils: element container len: %d 
1971,I,parsing nan_element_container_attr failed status: %d 
1967,,NAN20_utils: 2nd avail attribute decode failed 
1970,,NAN20_utils: 2nd avail attribute received 
1969,,NAN20_utils: 1st avail attribute decode failed 
1968,,NAN20_utils: 1st avail attribute received 
1967,,NAN20_utils: 2nd avail attribute decode failed 
1966,III,p_dev_cache: %p NMF frame FA seqIdx: %d cache seqdIdx: %d 
1965,III,Failed to transmit NMF status: %d, index %d flags %d
 
1964,II,NAN20_UTILS: NMF Tx Completion; Couldn't find peer discovery mac addr from ndi mac addr(ost:%d, sent:%d) 
1963,II,NAN20_UTILS: NMF Tx Completion with oui_subtype: %d sentFlag:%d 
1962,I,NAN_20_Utils_BuildDwNANManagementFrame ERR: Already a frame built for this queue_type:%d 
1961,,Failed to alloc NMF buffer 
1960,II,NAN20_UTILS:1 FA time_bit_map1-%x, time_bit_map2-%x 
1959,II,NAN20_UTILS:2 NDC/IMMU time_bit_map1-%x, time_bit_map2-%x 
1958,I,NAN20_UTILS: NMF Sched update notify tx com len %x 
1958,I,NAN20_UTILS: NMF Sched update notify tx com len %x 
1957,I,NAN20_utils_process_sched_update_notify_tx_comp:data len: %x 
1956,,NAN20_UTILS: wlan_nan20_validate_attr invalid NDC attr 
1955,,NAN20_UTILS: wlan_nan20_validate_attr invalid NDL attr 
1954,,NAN20_UTILS: wlan_nan20_validate_attr invalid FA attr 
1953,,NAN20_UTILS: wlan_nan20_validate_fa_attr - ** Invalid FA attr 
1952,,NAN20_UTILS: wlan_nan20_validate_fa_attr - Valid FA attr 
1951,,NAN20_UTILS: wlan_nan20_validate_ndc_attr - ** Invalid NDC 
1950,,NAN20_UTILS: wlan_nan20_validate_ndc_attr - Valid NDC 
1949,,NAN20_UTILS: wlan_nan20_validate_ndl_attr - ** Invalid immutable 
1948,,NAN20_UTILS: wlan_nan20_validate_ndl_attr - Valid immutable 
1947,IIII,wlan_nan_get_default_fa_channel =%d, Band=%d, BandConfigured=%d, ndp_channel_cfg=%d 
1946,,wlan_nan_get_default_fa_channel: ERR: 5G channel can't be forced because of self/peer capabilities 
1945,II,wlan_nan_get_default_fa_channel ====2.4G==== channel:%d phy_mode:%d 
1944,II,wlan_nan_get_default_fa_channel ====5G==== channel:%d phy_mode:%d 
2038,,NAN20_RANGING - ERROR_FA: is zero bytes #4 
2037,II,NAN20_RANGING: valid_bit_map: %d flags: %d 
2036,,NAN20_RANGING:RANGE REPORT FLAG SET 
2035,I,NAN20_RANGING: RSUA Decode with token_id:%d 
2034,I,NAN20_RANGING: Publish ranging failed %d 
2033,II,NAN20_RANGING: type_state_field %d RangeControl:data: 0x%x 
2032,I,NAN20_RANGING: Allocated RSUA (cnt:%d) 
2031,,NAN20_RANGING ERROR: Alloc RSUA failed 
2030,II,NAN20_RANGING ERROR: Build RSUA Invalid arguments pBuf:0x%x buf_len:%d 
2002,,NAN20_RANGING: Ranging not supported 
2029,,NAN20_RANGING: Building RSUA with status as REJECTED 
2028,,NAN20_RANGING: Ranging required bit set 
2027,IIII,NAN20_RANGING: Built RSUA token_id:%d status:%d valid_bit_map:%d reason_code:%d 
2026,I,NAN20_RANGING: Deallocated RSUA (cnt:%d) 
2025,,NAN20_RANGING: Dealloc RSUA failed 
2024,IIIIII,NAN20_RANGING - Send ranging report for peer: 0x%x:0x%x:0x%x:0x%x:0x%x:0x%x 
2023,IIIIII,NAN20_RANGING - Create Ranging instance for peer 0x%x:0x%x:0x%x:0x%x:0x%x:0x%x 
2022,III,NAN20_RANGING - Ranging instance created(idx : %d) with req_id : %x token_id : %d 
2021,,NAN20_RANGING - Ranging instance create failed - No free slots 
2020,IIIIII,NAN20_RANGING - Delete ranging instance for peer 0x%x:0x%x:0x%x:0x%x:0x%x:0x%x 
2019,III,NAN20_RANGING - Ranging instance deleted (idx : %d) with req_id : %x token_id : %d 
2015,II,NAN20_RANGING - Ranging instance not found - No match for req_id : %x token_id : %d 
2017,IIIIII,NAN20_RANGING - Get Ranging instance for peer 0x%x:0x%x:0x%x:0x%x:0x%x:0x%x 
2018,II,NAN20_RANGING - Ranging instance match found (idx : %d) with req_id : %x 
2017,IIIIII,NAN20_RANGING - Get Ranging instance for peer 0x%x:0x%x:0x%x:0x%x:0x%x:0x%x 
2016,III,NAN20_RANGING - Ranging instance match found (idx : %d) with req_id : %x token_id : %d 
2015,II,NAN20_RANGING - Ranging instance not found - No match for req_id : %x token_id : %d 
2014,IIIIII,NAN20_RANGING - Ranging session is NULL, peer mac: 0x%x:0x%x:0x%x:0x%x:0x%x:0x%x 
2013,IIIIII,NAN20_RANGING - Ranging session is active 0x%x:0x%x:0x%x:0x%x:0x%x:0x%x 
2012,I,NAN20_RANGING: Ranging Role 
2002,,NAN20_RANGING: Ranging not supported 
2011,I,NAN20_RANGING: Ranging request handler client_id:%d 
2010,,NAN20_RANGING: Ranging instance creation failure 
2009,,NAN20_NDP - ERROR_FA: is zero bytes #5 
2008,I,NAN20_RANGING: Continuous slots %d 
2007,I,NAN20_RANGING: Availability slots from RSUA_RESP - %d 
2006,III,NAN20_RANGING: Calling Ranging status notification handler with status:%d rep_ss_period:%d client_id:%d
 
2005,II,NAN20_RANGING - Ranging Instance complete: req_id: %d distance: %d 
2004,II,NAN20_RANGING - process range result client_id: %d RangeControl: 0x%x 
2003,,NAN20_RANGING - Ranging_report bit set by the peer 
2002,,NAN20_RANGING: Ranging not supported 
2002,,NAN20_RANGING: Ranging not supported 
2001,,NAN20_RANGING - Intiating range request failed: Session active 
2000,,NAN20_RANGING- Obataining peer channel failed 
1999,III,NAN20_RANGING- Obataining peer channel success: mhz: %d, CF1: %d phymode: %d 
1998,IIIIII,NAN20_RANGING - Initiate ranging with MAC: 0x%x:0x%x:0x%x:0x%x:0x%x:0x%x 
1997,,NAN20_RANGING: responder instance not found 
1996,,NAN20_RANGING: Entering build range report function 
1995,,NAN20_RANGING: Invalid attribute buffer
 
1994,,NAN20_RANGING: Instance not found, cancel failed 
1993,I,wlan_nan20_sm_ranging terminatd failed: status %d 
1992,,NAN20_RANGING - Get Ranging instance failed 
1991,II,NAN20_RANGING: Built Range Report token_id:%d ranging_report_length:%d 
2117,IIII,GetDefaultPrimaryChannelInfo_ForOperClass: %d, %x, %x, %d 
2116,,NAN_20_Build_Avail_Attribute: ERROR_FA: Build availability basic sanity fails: No FA generated 
2115,,NAN_20_Set_Committed_Slot_Changed: Update SDF with FA_ATTR_Control 
2114,I,NAN_20_Update_FA_AttributeControl: update_sdf: %d  
2113,,NAN_20_Update_FA_AttributeControl: update_sdf: TRUE  
2112,,NAN_20_Update_FA_AttributeControl: Update SDF with FA_ATTR_Control 
2111,I,ResolveFa: returning error %d 
2110,I,ResolveFa: peer cache null and channel null for OuiSubtype %d 
2109,II,ResolveFa: peer cache null and channel %d for OuiSubtype %d 
2108,III,ResolveFa: OuiSubtype%d mhz%x phymode%d 
2107,,wlan_get_nan_active_fa_channels: FA Error no FA session 
2106,,wlan_get_nan_fa_channel_info: FA Error no FA session 
2105,I,wlan_nan20_build_nan_availability_attr_nmf: ERROR_FA: calling incorrect function for ouitype %d 
2104,,wlan_nan20_build_nan_availability_attr_nmf: ERROR_FA: Channel forced but no channel info provided 
2103,,wlan_nan20_build_nan_availability_attr_nmf: ERROR_FA: Channel forced to 2G when device is in 5G only 
2102,,wlan_nan20_build_nan_availability_attr_nmf: ERROR_FA: Channel forced to 5G when device is in 2G only 
2101,I,wlan_nan20_build_nan_availability_attr_nmf: ERROR_FA: Unable to create FA Session for outsubtype %d 
2100,,wlan_nan20_build_nan_availability_attr_nmf: ERROR_FA: NDP or Ranging Instance is NULL cannot build FA/NA 
2098,I,wlan_nan20_build_nan_availability_attr_nmf: pnan_fa_session_for_peer %u 
2099,,wlan_nan20_build_nan_availability_attr_nmf: FA session already present, do save fa 
2098,I,wlan_nan20_build_nan_availability_attr_nmf: pnan_fa_session_for_peer %u 
2097,,Filling pavail_per_attr_entry 
2096,I,wlan_nan20_convert_band_only_info_to_channel_info: channel not null %x 
2095,I,wlan_nan20_convert_band_only_info_to_channel_info: Phymode=%d 
2094,III,wlan_nan20_fill_fa_nan_avail_attr: map_id:%d p_fa_session:0x%x band_config:%d  
2093,,wlan_nan20_fill_fa_nan_avail_attr: Maximum entry list count reached 
2092,I,wlan_nan20_fill_fa_nan_avail_attr: Ignoring the fa entry[%d]; not same as fa session entry 
2091,I,wlan_nan20_fill_fa_nan_avail_attr: Ignoring the fa entry[%d] 
2090,I,wlan_nan20_fill_fa_nan_avail_attr: avail not a subset ignore and continue slotbitmap 0x%x 
2089,I,wlan_nan20_fill_fa_nan_avail_attr: subset check slotbitmap 0x%x 
2088,,wlan_nan20_fill_fa_nan_avail_attr: schedule updated 
2087,II,wlan_nan20_fill_fa_nan_avail_attr: index2: 0x%x; entry_list_cnt: 0x%x 
2086,II,wlan_nan20_fill_fa_nan_avail_attr: Filling entry list of type %d; time_bit_map 0x%x 
2085,I,wlan_nan20_fill_fa_nan_avail_attr: Final timebitmap 0x%x  
2084,I,wlan_nan20_fill_fa_nan_avail_attr: entry_list_cnt:%d  
2083,,wlan_nan20_fill_pavail_per_attr: pfa_session is NULL 
2082,I,wlan_nan20_fill_pavail_per_attr: Filling pavail_per_attr with %x 
2081,,wlan_nan20_fill_pavail_per_attr: Returning with a single avail per attr 
2080,II,wlan_nan20_fa_session_index: Counter band %d stored FA %d 
2079,II,wlan_nan20_fa_sessioni_index: Counter channel %d stored FA %d 
2078,I,wlan_nan20_fa_session_index: FA Counter channel %d 
2077,I,wlan_nan20_fa_session_index: FA session count %d 
2076,II,wlan_nan20_get_cf1_from_center_freq: found cf1 ch %d for center ch%d 
2075,,Peer proposed NDC is not present in data response so rejecting 
2074,I,wlan_nan20_pick_best_peer_fa: Process and save FA failed %d 
2073,I,wlan_nan20_pick_best_peer_fa slotsAvailableMap:0x%x 
2072,I,wlan_nan20_pick_best_peer_fa PeerMaxChannelSwitch:0x%d 
2071,,wlan_nan20_pick_best_peer_fa ERR: NDC/NDL immutable can't be served returning 
2070,IIII,wlan_nan20_pick_best_peer_fa: OuiSubtype:%d map_id:%d ndc_slot_bitmap:0x%x ndl_immutable_slot_bitmap:0x%x 
2069,I,wlan_nan20_pick_best_peer_fa: Ignoring potential entry ost:%d 
2068,IIII,wlan_nan20_pick_best_peer_fa: chan Type(%d), AvailabilityType(%d), UsagePref(%d), TimeBitMapPresent(%d) 
2067,II,wlan_nan20_pick_best_peer_fa 1: pDeviceCap->band_config:%d peer_dev_cap->supported_band:%d 
2066,,wlan_nan20_pick_best_peer_fa: skipping 5G entry as local or remote end is 2G only #1 
2065,II,wlan_nan20_pick_best_peer_fa 2: pDeviceCap->band_config:%d peer_dev_cap->supported_band:%d 
2064,,wlan_nan20_pick_best_peer_fa: skipping 5G entry as local or remote end is 2G only #2 
2063,I,wlan_nan20_pick_best_peer_fa: ChanBitMap 5G %x 
2062,,Invalid channel or DFS channel 
2061,,wlan_nan20_process_and_save_individual_fa_session: channel is given and this is non-matching band so skipping saving entry 
2060,II,wlan_nan20_pick_best_peer_fa: ERR Given immutable slots can't be served Given:0x%x overlapping:0x%x 
2059,II,wlan_nan20_pick_best_peer_fa: ERR Given NDC slots can't be served Given:0x%x overlapping:0x%x 
2058,,No more time slots ignore 
2056,I,wlan_nan20_process_and_save_individual_fa_session: FA session count %d 
2057,,wlan_nan20_process_and_save_individual_fa_session ERR: Maximum FA sessions reached 
2056,I,wlan_nan20_process_and_save_individual_fa_session: FA session count %d 
2055,II,wlan_nan20_process_and_save_individual_fa_session: availabilitytype%x %d 
2054,II,wlan_nan20_received_nan_fa: Received OperClass %d ChanBitMap:0x%x 
2053,IIIII,wlan_nan20_save_fa_information: Saving FA information ost:%d freq:%d center_freq:%d OperClass:%d slot_bitmap:0x%x 
2052,III,wlan_nan20_save_fa_information: Failed to Save FA information ost:%d mode:%d channel:%d 
2051,,wlan_nan20_set_fa_session_active: FA Error no FA session 
2050,,wlan_nan20_set_fa_session_active: ULW Notify set to TRUE 
2049,I,NAN20_FA: wlan_nan20_set_fa_session_active vdev_id:%d 
2048,,wlan_nan20_set_fa_session_active: Res mgr link failure 
2047,I,NAN_20_FA: Schedule update for peer entry fa_session 0x%x 
2046,,NAN_20_FA: Schedule update for peer failed 
2045,,wlan_nan_fa_get_phymode: FA Error no FA session 
2044,I,wlan_nan_update_fa: p_fa_peer_availability->entry_list_cnt %d 
2043,I,wlan_nan_update_fa: p_fa_peer_availability->entry_list..chan_band_entry_count %d 
2042,II,wlan_nan_update_fa: self operating class%d time_bmap %x 
2041,II,wlan_nan_update_fa: peer operating class%d time_bmap %x 
2040,III,NAN_20_FA: Schedule updated for operating class%d entry%d updated bmap %x 
2039,I,wlan_nan20_set_fa_session_slot_bit_map_update: 0x%x 
2118,I,NAN20_SM: event=%d not handled 
2119,,NAN20_SM: wlan_nan20_sm_state_send_sched_conf_entry 
2118,I,NAN20_SM: event=%d not handled 
2120,,NAN20_SM: wlan_nan20_sm_state_send_sched_rsp_entry 
2118,I,NAN20_SM: event=%d not handled 
2121,,NAN20_SM: wlan_nan20_sm_state_send_security_install_entry 
2122,,NAN20_SM : wlan_nan20_sm_state_wait_for_peer_create_event terminating 
2123,,NAN20_SM : wlan_nan20_sm_state_wait_for_peer_create_event 
2124,I,NAN20_SM : wlan_nan20_sm_state_wait_for_responder_req_from_service_event : %d 
2125,,NAN20_SM : wlan_nan20_sm_state_send_initiator_req_entry 
2126,,NAN20_SM : wlan_nan20_sm_state_terminating_event 
2127,,NAN20_SM: Range report frame built 
2128,,NAN20_SM: Range report frame build failed 
2129,,wlan_nan20_sm_state_active_event: Transmit Data End 
2130,,wlan_nan20_sm_state_active_event: Build Data End 
2131,,NAN20_SM: Found NDP instance turn off disc beacon 
2132,I,NAN20_SM: wlan_nan20_sm_state_active_entry ndp_id : %d 
2133,I,NAN20_SM: wlan_nan20_sm_state_active_entry mode : %d 
2134,II,NAN20_SM: Current state:%d Event:%d 
2135,,NAN20_SM wlan_nan20_sm_state_idle_event STATE_SEND_RESPONDER_REQ 
2136,,NAN20_SM : wlan_nan20_sm_state_idle_event SEND_INITIATOR_REQ 
2137,,NAN20_SM : wlan_nan20_sm_state_idle_event BUILD_INITIATOR_REQ 
2138,IIII,NAN20_SM : wlan_nan20_sm_process_nmf TYPE : %d, dialog_token : %d ndp:%d/rtt:%d 
2139,I,NAN20_SM: nan20_sm_process_nmf Unknown frame %d 
2140,II,NAN20_SM : wlan_nan20_sm_process_nmf TYPE : %d, dialog_token : %d 
2139,I,NAN20_SM: nan20_sm_process_nmf Unknown frame %d 
2140,II,NAN20_SM : wlan_nan20_sm_process_nmf TYPE : %d, dialog_token : %d 
2141,II,NAN20_SM: wlan_nan20_sm_recvd_ack oui_subtype: %d event_type:%d 
2142,II,NAN20_SM: wlan_nan20_sm_recvd_ack Invalid state !! Expected-state:%d current-state:%d 
2143,,NAN20_SM: wlan_nan20_sm_recvd_ack Invalid SM Session 
2144,I,NAN20_SM: wlan_nan20_sm_recvd_ack received unknown OUI oui_subtype: %d 
2145,III,NAN20_SM: wlan_nan20_sm_recvd_ack oui_subtype: %d sent_flag:%d dialog_token:%d 
2146,,NAN20_SM: build_send_sched_req invalid NMF 
2147,,NAN20_SM: build_send_sched_req invalid sm session 
2148,,NAN20_SM: build_send_sched_rsp invalid NMF 
2149,,NAN20_SM: build_send_sched_rsp invalid sm session 
2150,,NAN20_SM: build_send_sched_conf invalid NMF 
2151,,NAN20_SM: build_send_sched_conf invalid sm session 
2152,,NAN20_SM : Range report build event 
2153,II,nan20_sm_recvd_ranging_terminate received_ota data_end_in_progress: %d state = %d 
2154,II,nan20_sm_data_end_received_ota data_end_in_progress: %d state = %d 
2155,,NAN20_SM : wlan_nan20_sm_recvd_data_end Clear NDP end while security enabled will drop here 
2156,,NAN20_SM : wlan_nan20_sm_recvd_data_end Null sm session 
2157,I,NAN20_SM : wlan_nan20_sm_recvd_data_end mode:%d 
2158,,nan20_sm_data_end_ack 
2159,,NAN20_SM: =====SENT SCHED NOTIFY====== 
2160,,NAN20_SM: =====Q'd SCHED NOTIFY====== 
2161,,NAN20_SM: SCHED_UPDATE_NOTIF invalid NMF 
2162,,NAN20_SM: send_sched_update_notif invalid state 
2163,I,wlan_nan20_sm_build_data_end: state %d 
2164,,NDP end is in progress return 
2165,,wlan_nan20_sm_build_data_end: get pm_session_failed 
2166,,NAN20_SM : wlan_nan20_sm_recvd_nmf_3rd_msg Invalid SM 
2167,III,NAN20_SM: wlan_nan20_sm_recvd_indication pub_id:%d status:%d ndp_control:%d 
2168,II,NAN20_SM: wlan_nan20_sm_recvd_indication duplicated, token: %d, ndp_id: %d 
2169,I,NAN20_SM : wlan_nan20_sm_send_responder_req state: %d 
2170,,NAN20_SM : wlan_nan20_sm_send_responder_req sm session not found 
2171,,NAN20_SM : received response with reject 
2172,,NAN20_SM : wlan_nan20_sm_recv_frame_pre_validation Clean up 
2173,,NAN20_SM : wlan_nan20_sm_send_initiator_req 
2174,I,NAN20_SM : wlan_nan20_sm_send_initiator_req state: %d 
2175,,NAN20_SM : wlan_nan20_sm_send_initiator_req sm session not found 
2176,,NAN20_SM : wlan_nan20_sm_build_initiator_req invalid sm_session 
2177,,NAN20_SM : wlan_nan20_sm_build_initiator_req 
2178,,NAN20_SM : wlan_nan20_sm_recvd_peer_create_event 
2179,,NAN20_SM : wlan_nan20_sm_recvd_responder_req_from_service 
2180,II,NAN20_SM: wlan_nan20_age_sm_session session_dw_count:%d state:%d 
2181,II,NAN20_SM: Age SM session timeout for mode:%d reason_code:%d 
2182,III,NAN20_SM: wlan_nan20_sm_free_need_again_buffer index:%d flags:0x%x buf 0x%x 
2183,,NAN20_SM: wlan_nan20_sm_free_need_again_buffer START 
2184,,NAN20_SM: wlan_nan20_delete_sm_session num active SM is 0 
2185,II,NAN20_SM: wlan_nan20_delete_sm_session ndp_id:%d dialog_token: %d 
2186,I,NAN20_SM: wlan_nan20_delete_sm_session found matching session=%d 
2187,III,NAN20_SM: wlan_nan20_delete_sm_session index:%d flag:0x%x buf 0x%x 
2188,I,wlan_nan20_sm_parse_buffer:  get dialog token 0, OUI sub type 0x%x 
2134,II,NAN20_SM: Current state:%d Event:%d 
2189,II,wlan_nan20_create_sm_session(): mode:%d dialog_token:%d 
2191,I,nan_unit_test GET_NAN_DW_END_TSF: end_dwTsf: 0x%x  
2190,III,nan_unit_test GET_2G_NDL_ACTIVE: ndp_channel_present: %d is_2Gndl_present: %d start_time: 0x%x 
2354,I,NAN20_set_htvht_capability_ie vdev opmode: %d 
2353,,set_htvht_capability_ie: sta vdev is NULL return 
2352,II,HT_CAPS: band: %d buf_len: %d 
2351,II,VHT_CAPS: band: %d buf_len: %d 
2350,III,wlan_nan20 data attr %d %d %d 
2349,,wlan_nan20_ndp_alloc_ndp call #3 
2336,,NAN20_NDP - ERROR_FA: is zero bytes #3 
2348,,wlan_nan20 ndp alloc ndp failed #5 
2347,,wlan_nan20 data end for initiator role 
2346,,wlan_nan20 data end for responder role 
2345,IIII,ndp_attr.dialog_token %d ndp_attr.type %d ndp_attr.ndp_id %d ndp_attr.ndp_control %d 
2344,,NAN20_NDP : wlan_nan20_build_ndp_responder_req 
2343,III,wlan_nan20_ndp_alloc_ndp call #2 %x %x %x 
2342,,NAN20_NDP: wlan_nan20_build_ndp_responder_req Invalid vdev 
2341,,Changing the committed DW to 5G 
2332,,NAN20_NDP - ERROR_FA: is zero bytes #2 
2340,,wlan_nan20_ndp_alloc_ndp call #4 
2339,,NAN20_NDP: wlan_nan20_build_sched_conf 
2338,,NAN20_NDP: get_ndp_instance failed in wlan_nan20_build_sched_conf 
2337,,NAN20_NDP: NMF alloc failed in wlan_nan20_build_sched_conf 
2336,,NAN20_NDP - ERROR_FA: is zero bytes #3 
2335,,NAN20_NDP: wlan_nan20_build_sched_rsp 
2334,,NAN20_NDP: get_ndp_instance failed in wlan_nan20_build_sched_rsp 
2333,,NAN20_NDP: NMF alloc failed in wlan_nan20_build_sched_rsp 
2332,,NAN20_NDP - ERROR_FA: is zero bytes #2 
2331,I,NAN20_NDP: wlan_nan20_build_ulw: No ULW present %d 
2330,II,NAN20_NDP: wlan_nan20_build_ulw %d 0x%x 
2329,,NAN20_NDP: get_ndp_instance failed in wlan_nan20_build_ulw 
2328,,NAN20_NDP: NMF alloc failed in wlan_nan20_build_ulw 
2327,,wlan_nan20_check_ndp_off_channel: no active ndp session 
2326,,wlan_nan20_check_ndp_off_channel: no active fa_sesion 
2325,,wlan_nan20_check_ndp_off_channel: ndp session inactive 
2324,,creating HT Capabilities in element container failed !!! 
2323,,creating VHT Capabilities in element container failed !!! 
2322,IIIII,create_nan_element_container: self channel: %d num_s_rate: %d num_ex_s_rate: %d is_HT: %d, is_VHT: %d 
2321,I,NAN20_NDP - wlan_nan20_create_ndp_instance ndp_ctxt_ndp_id=%d 
2320,IIIIII,NAN20_NDP - Create NDP instance Addr:0x%x 0x%x ndp_id:%d ndp_instance_id:%d role:%d dialog_token:%d 
2319,I,NAN20_NDP - p_vdev for vdev_id %d is NULL 
2318,I,NAN20_NDP - Register MAC address for NDI, vdev_id=%d 
2317,IIIIIIIII,NAN20_NDP - Delete NDP instance Addr:%2x:%2x:%2x:%2x:%2x:%2x ndp_id:%d ndp_instance_id:%d vdev_id:%d 
2316,IIIIII,NAN20_NDP - Delete NDP instance Self NDI Addr:%2x:%2x:%2x:%2x:%2x:%2x 
2315,IIIIIII,NAN20_NDP - Delete NDP instance Peer NDI Addr:%2x:%2x:%2x:%2x:%2x:%2x dialog_token:%d 
2314,I,NAN20_NDP - p_vdev is NULL for self_ndi_vdev_id: %d 
2313,I,NAN20_NDP - VDEV_DOWN call for ndp_vdev_id: %d 
2312,I,NAN20_NDP - Unregister MAC address for NDI vdev_id=%d 
2311,,NAN20_NDP: wlan_nan20_disable_ndp_instance 
2310,,NAN20_NDP: get_ndp_instance failed in wlan_nan20_disable_ndp_instance 
2309,I,NAN20_NDP: wlan_nan20_disable_ndp_instance ndp_instance_id:%d  
2308,I,NAN20_NDP_Enabling 5G : %d 
2307,I,NAN20_NDP_Disabling 5G %d 
2306,II,NDP channel:%d corresponding NSS:%d 
2305,I,wlan_nan20_get_ndc_schedule: %x 
2304,II,wlan_nan20_get_ndp_instance_by_ndp_id %d %d 
2303,II,wlan_nan20_get_ndp_instance_by_ndp_id %x %x 
2302,I,NAN20_NDP -wlan_nan20_get_num_active_ndi_ndp_instance:%d 
2301,I,NAN20_NDP -wlan_nan20_get_num_active_ndp_instance:%d 
2300,,NAN20_NDP NDP NOT allowed because of Different configuration(Open/Security) 
2299,,NAN20_NDP Passphrase Same 
2298,,NAN20_NDP Passphrase different 
2297,,NAN20_NDP PMK same 
2296,,NAN20_NDP PMK different 
2295,,NAN20_NDP NDP allowed on this NDI 
2294,IIIII,merge_nan_element_container: Peer channel: %d num_s_rate: %d num_ex_s_rate: %d is_HT: %d, is_VHT: %d 
2293,,Peer didn't advertize HT caps !!! 
2292,II,NO NDL SCHEDULE UPDATE %x %d 
2291,,NO NDP SESSION WITH PEER 
2062,,Invalid channel or DFS channel 
2290,II,NAN20_NDP This is first request towards the peer : Channel Validation Success peer_disc_mac : 0x%x 0x%x 
2289,II,NAN20_NDP Channel not forced : Channel Validation Success peer_disc_mac : 0x%x 0x%x 
2288,IIIII,NAN20_NDP Channel forced Channel Validation Failed peer_disc_mac : 0x%x 0x%x channel_mhz : %d Freq1 : %d Freq2 : %d 
2287,IIIII,NAN20_NDP Channel forced Channel Validation Success peer_disc_mac : 0x%x 0x%x channel_mhz : %d Freq1 : %d Freq2 : %d 
2286,,NAN20_NDP wlan_nan20_ndp_concurrency_validation Failed 
2285,,NAN20_NDP wlan_nan20_ndp_concurrency_validation Success 
2284,,NAN20_NDP: Suppressing NDP confirm event 
2283,,nan20_ndp_disabled: data_end_ind 
2282,I,NAN20_NDP: wlan_nan20_ndp_dispatch_peer_assoc ndp_id : %d 
2281,,NAN20_NDP - test bed mode Dual map, Not active 
2280,I,NAN20_NDP: wlan_nan20_ndp_dispatch_peer_assoc NULL instance : %d 
2279,,NAN20_NDP: wlan_nan20_ndp_dispatch_peer_assoc Invalid phy mode 
2278,,NAN20_NDP: wlan_nan20_ndp_dispatch_peer_assoc Invalid vdev 
2277,I,NAN20_NDP: Peer_Assoc wlan_nan20_set_fa_session_active => vdev_id : %d 
2276,,NAN20_NDP: Peer_Assoc - wlan_vdev_up 
2275,,NAN20_NDP: Peer_Assoc - res mgr link failed 
2274,,NAN20_NDP: Peer_Assoc - Build data end 
2273,,NAN20_NDP : wlan_nan20_ndp_end_indication_event_hdlr 
2272,III,NAN20_NDP: wlan_nan20_ndp_end_indication_event_hdlr Sent Event instance_id:%d vdev_id:%d reason_code:%d 
2271,,wlan_nan20_ndp_end_req_hdlr: NAN Discovery disabled #3 
2270,,wlan_nan20_ndp_instance not found 
2269,,wlan_nan20_ndp NMF pool alloc failed 
2268,,wlan_nan20_ndp Invalid Instance ID 
2267,IIIIIIIII,NAN20_NDP : wlan_nan20_ndp_end_req_hdlr NDP id : %d NDP_INST id : %d vdev_id:%dSelf Peer NDI Addr:%2x:%2x:%2x:%2x:%2x:%2x 
2266,IIIIII,NAN20_NDP : Peer Peer NDI Addr:%2x:%2x:%2x:%2x:%2x:%2x 
2265,I,wlan_nan20_sm_build_data_end() failed: status %d 
2264,II,NAN20_NDP: wlan_nan20_ndp_get_frequency %x %x 
2263,,NAN20_NDP RESPNDR Concurrency validation failed 
2262,,NAN20_NDP: Non Auto responder NDI not available 
2261,,NAN20_NDP: Auto responder NDI not available 
2260,,NAN20_NDP: wlan_nan20_create_ndp_instance return failure 
2259,,NAN20_NDP: Decided to reject so no need to Indicate 
2258,I,NAN20_NDP : wlan_nan20_ndp_indication_event_hdlr vdev_id : %d 
2257,I,NAN20_NDP : register wlan_nan20_ndp_register_for_vdev_notif ndp_id : %d  
2256,,NAN20_NDP : NULL Service id 
2255,,NAN20_NDP : PMK Entry NULL  
2221,,NAN20_NDP : PMK 
2220,I,0x%X 
2254,III,NAN20_NDP - NDP initiation Request Addr: 0x%x 0x%x dialog_token:%d 
2253,I,wlan_nan20_create_ndp_instance returend fail indicating reason_code=%x 
2252,,wlan_nan20_ndp_alloc_ndp call #1 
2251,III,NAN20_NDP - ndp_initiator_req : rsp_status: %d reason_code: %d nan20_log_index: %d 
2250,II,NAN20_NDP - wlan_nan20_ndp_initiator_rsp_event_hdlr - %d:%d 
2249,,NAN20_NDP - Get NDP channel failed 
2248,II,NAN20_NDP - Chosen channel_mhz:%d channel_freq1:%d 
2247,,NAN20_NDP INITIATOR Channel validation failed 
2246,,NAN20_NDP INITIATOR Peer validation failed 
2245,,NAN20_NDP INITIATOR Concurrency validation failed 
2244,IIIII,NAN20_NDP ndp_initiator_validation status %dNDI: 0x%x 0x%x peer_disc_mac : 0x%x 0x%x 
2243,II,NAN20_NDP This is first request towards the peer : Peer validation Success for peer_disc_mac : 0x%x 0x%x 
2242,II,NAN20_NDP Peer validation Failed for peer_disc_mac : 0x%x 0x%x 
2241,II,NAN20_NDP Peer validation Success for peer_disc_mac : 0x%x 0x%x 
2240,IIIIII,wlan_nan20_ndp_prepare_peer_assoc phymode: %d is_ht: %d is_vht: %d ni_flags: 0x%x num_supp_rate: %d num_ext_supp_rate: %d 
2239,I,wlan_nan20_ndp_prepare_peer_assoc num_legacy_rate=%d 
2238,II,wlan_nan20_ndp_prepare_peer_assoc legatcy_rate[%d]=%d 
2237,II,wlan_nan20_ndp_prepare_peer_assoc num_ht_rate=%d peer_nss: %d 
2236,II,wlan_nan20_ndp_prepare_peer_assoc rates[%d]=%d 
2235,IIII,wlan_nan20_ndp_prepare_peer_assoc peer tx_hi=%d, rx_hi=%d, tx_mcs=0x%x rx_mcs=0x%x 
2234,IIII,wlan_nan20_ndp_prepare_peer_assoc self tx_hi=%d, rx_hi=%d, tx_mcs=0x%x rx_mcs=0x%x 
2233,IIIII,wlan_nan20_ndp_prepare_peer_assoc VHT_INTERSECT tx_max=%d, rx_max=%d, tx_mcs=0x%x rx_mcs=0x%x,nss=%d 
2232,I,NAN20_NDP : wlan_nan20_ndp_register_for_vdev_notif %d 
2231,,nan20_ndp_responder_req_hdlr: wake 
2230,II,NAN20_NDP : wlan_nan20_ndp_responder_req_hdlr rsp_code:%d vdev_id:%d 
2229,II,NAN20_NDP : wlan_nan20_ndp_responder_req_hdlr: self_ndi_vdev_id:%dvdev_id :%d are differnt so replace 
2228,I,NAN20_NDP - responder_req_hdlr Register MAC address for NDI, vdev_id=%d 
2227,I,wlan_nan20_sm_recvd_responder_req_from_service call failed status: %d 
2226,III,NAN20_NDP - ndp_responder_req: rsp_status: %d reason_code: %d nan20_log_index: %d 
2225,I,NAN20_NDP responder_req_hdlr Invalid PMK length - %d 
2224,II,NAN20_NDP responder_req_hdlr Invalid Passphrase length - %d:%d 
2223,,NAN20_NDP : Responder NULL Service ID 
2222,,NAN20_NDP : Responder NULL PMK Entry 
2221,,NAN20_NDP : PMK 
2220,I,0x%X 
2219,,NAN20_NDP : wlan_nan20_ndp_responder_req_hdlr PMKID verification failed 
2218,II,NAN20_NDP - wlan_nan20_ndp_responder_rsp_event_hdlr %d:%d 
2217,,NAN20_NDP responder validation Failed 
2216,,NAN20_NDP responder validation Success 
2215,,NAN20_NDP : wlan_nan20_ndp_vdev_notif_cbhandler NULL 
2214,II,NAN20_NDP : wlan_nan20_ndp_vdev_notif_cbhandler Instance Null Peer mac address %x : %x 
2213,III,NAN20_NDP : wlan_nan20_ndp_vdev_notif_cbhandler type:%d self_ndi_vdev_id:%d ndp_id:%d 
2212,II,mac addr : %x : %x 
2211,,NAN20_NDP: wlan_nan20_sched_req_hdlr 
2210,,NAN20_NDP: get_ndp_instance failed in wlan_nan20_sched_req_hdlr 
2209,,NAN20_NDP: NMF alloc failed in wlan_nan20_sched_req_hdlr 
2205,,NAN20_NDP - ERROR_FA: is zero bytes 
2208,,NAN20_NDP: wlan_nan20_sched_update_notif_hdlr 
2207,,NAN20_NDP: get_ndp_instance failed in wlan_nan20_sched_update_notif_hdlr 
2206,,NAN20_NDP: NMF alloc failed in wlan_nan20_sched_update_notif_hdlr 
2205,,NAN20_NDP - ERROR_FA: is zero bytes 
2204,,NAN20_NDP select NDI:First instance 
2203,I,NAN20_NDP: wlan_nan20_ndp_indication_event_hdlr security:%d 
2202,I,NAN20_NDP select NDI:Configuration :%d 
2201,I,NAN20_NDP: Auto responder NDI not available, PMK not present: %d 
2200,,NAN20_NDP select NDI:Configuration matches Secure 
2199,,NAN20_NDP select NDI:Configuration matches Open 
2198,IIIIII,wlan_nan20_update_sta_vdev_ulw: staVdevUp:%d ndp_instance:0x%x check_ndp_offchanel:%d ndp_offchanel:%d duration:%d schedDuration:%d 
2197,,wlan_nan20_update_sta_vdev_ulw: Start STA ULW failed as ulw allocation failed 
2196,,wlan_nan20_update_sta_vdev_ulw: Update STA ULW failed 
2195,IIII,wlan_nan20_update_sta_vdev_ulw: Start ULW start_time internal %x external %x curr_time %x schedIdx:%d 
2194,I,wlan_nan20_update_sta_vdev_ulw: Stop STA ULW cur_time:%x 
2193,,wlan_nan20_update_sta_vdev_ulw: Stop STA ULW failed as ulw update failed 
2192,IIII,wlan_nan_fill_peer_flags: is_vht: %d peer_is_vht: %d, self_is_vht: %d flags: 0x%x 
2360,I,NAN_FASessionIsUlwNotifySent: ULW not sent for fa session %d 
2359,,NAN_FASessionIsUlwNotifySent: All ULW notifications successfully sent before actual ULW 
2358,I,NAN_FASessionSendUlwNotify: Send Unicast ulw_notify for fa session %d 
2357,I,NAN_FASessionUlwNotifySent: Found FA session sent:%d 
2356,,NAN_FASessionUlwNotifySent: Couldn't find FA session 
2355,I,NAN_FASessionUpdateUlwNotify: Setting ulw_notify for fa session %d 
2405,I,NANCHANSCHED_ChannelHandler: Invalid input handler type:%d 
2404,IIIII,NANCHANSCHED_ChannelHandler: Channel:%d status:%d currSlotDw0:%d, currSlot:%d slotOffset:%d 
2403,IIII,NANCHANSCHED_ChannelHandler: Channel_scheduled:%d Chan_hndlr_type_mask:0x%x Channel_fa_mask:0x%x update_fa_schedule:%d 
2402,,NANCHANSCHED_ChannelHandler: Nothing to handle 
2401,IIIII,NANCHANSCHED_ChannelHandler: ChannelType:%d status:%d ch_ctx_mask:0x%x startSlot:%d num_slots:%d 
2400,,NANCHANSCHED_ChannelScheduler: Not scheduling any channel as NAN might have stopped 
2399,III,NANCHANSCHED_ChannelScheduler: Entered curr_slot_dw0:%d curr_slot:%d slot_offset:%d 
2398,II,NANCHANSCHED_ChannelScheduler: Scheduling from slot_dw0:%d slot:%d  
2397,IIIII,NANCHANSCHED_ChannelScheduler: Entry[%d] valid:%d scheduled:%d slot_bitmap:0x%x fa_mask:0x%x 
2396,IIIII,NANCHANSCHED_ChannelScheduler: Entry[%d] start_time:%d duration:%d start_slot:%d num_slots:%d 
2395,IIII,NANCHANSCHED_ChannelScheduler: offset 0x%x  duration 0x%x new_offset 0x%x new_duration 0x%x 
2395,IIII,NANCHANSCHED_ChannelScheduler: offset 0x%x  duration 0x%x new_offset 0x%x new_duration 0x%x 
2394,I,NANCHANSCHED_ChannelScheduler: Entry[%d] Nearest schedule 
2393,III,NANCHANSCHED_ChannelScheduler: Schedule channel schedIdx:%d, chanHndlrType:%d chanHndlrTypeMask:%x 
2392,I,NANCHANSCHED_ChannelScheduler: DW schdule with crit_ocs_priority=%d 
2391,,NANCHANSCHED_ChannelScheduler ERR: Channel scheduling failed 
2390,II,NANCHANSCHED_ChannelScheduler ERR: Invalid schedIdx:%d and/or chanHndlr:0x%x 
2389,III,NANCHANSCHED_CombineChannelScheduleSlotMap: ERR Incorrect input params inChanSchedSlotMap1:0x%x inChanSchedSlotMap2:0x%x outChanSchedSlotMap:0x%x 
2388,II,NANCHANSCHED_FillNanAvailCommittedEntryList: Entry list is NULL(0x%x) or there is no enough space(%d) 
2387,II,NANCHANSCHED_FindMaximumContiguousSlotMap: cnt:%d slot_bitmap:0x%x  
2386,III,NANCHANSCHED_GenerateChannelScheduleSlotMap: ERR Incorrect input params slotBitmap:0x%x outChanSchedSlotMap:0x%x bitDuration:%d 
2385,I,NANCHANSCHED_Get2GNDLactive: ndp channel %x 
1838,,NAN_SCHED_DO_CHANNEL_REQ: Read config error 
2384,IIIII,NANCHANSCHED_UpdateChannelSchedule: Input fa_index[%d] schedule:%d slot_bitmap:0x%x fa_mask:0x%x freq:%d 
2383,IIIIII,NANCHANSCHED_UpdateChannelSchedule: Entry[%d] valid:%d chan_mhz:%d flags = 0x%x slot_bitmap:0x%x fa_mask:0x%x 
2382,,NANCHANSCHED_UpdateChannelSchedule: Found channel entry[%d] for given channel 
2381,,NANCHANSCHED_UpdateChannelSchedule: Found channel entry[%d] for given FA id 
2380,III,NANCHANSCHED_UpdateChannelSchedule: match_fa_idx:%d match_chan_idx:%d free_chan_idx:%d 
2379,IIIII,NANCHANSCHED_UpdateChannelSchedule: ch_freq:%d ch_phymode:%d selected_phymode:%d center_freq1:%d selected_center_freq1:%d 
2378,III,NANSCHED_UpdateChannelSchedule: FA entry[%d] not valid(%d)/schedule(%d) 
2377,III,NANSCHED_UpdateChannelSchedule: Can't generate channel schedule map #1 
2376,I,NANSCHED_UpdateChannelSchedule: fa_type_update nss %d 
2375,I,NANCHANSCHED_UpdateChannelSchedule:Remove link Channel:%d 
2374,IIII,NANCHANSCHED_UpdateChannelSchedule: match_fa_idx:%d schedule:%d fa_mask:0x%x slot_bitmap:0x%x 
2373,III,NANSCHED_UpdateChannelSchedule: Can't generate channel schedule map #2 
2372,I,NANSCHED_UpdateChannelSchedule: channel_link update nss %d 
2371,III,NANSCHED_UpdateChannelSchedule: Can't generate channel schedule map #3 
2370,I,NANSCHED_UpdateChannelSchedule: channel_link create nss %d 
2369,,NANCHANSCHED_UpdateChannelSchedule: create new link channel failed 
2368,IIII,NANCHANSCHED_UpdateChannelSchedule: match_chan_idx:%d free_chan_idx:%d fa_mask:0x%x slot_bitmap:0x%x 
2367,II,NANCHANSCHED_UpdateChannelSchedule: Invalid FA_index %d or FA_valid:%d 
2366,I,chan_type %d 
2366,I,chan_type %d 
2365,I,nanChan- hndlr_type_mask 0x%x 
2364,II,g_NanChanSchedCtx.hdlr_type_info[%d].chan_ctx_mask 0x%x 
2363,IIII,NANCHANSCHED_UpdateOcsReqPriority: Entry[%d] valid:%d chan_type_mask:0x%x is_priority_critical=%d 
2362,III,NANCHANSCHED_UpdateOcsReqPriority: Entry[%d] valid:%d chan_type_mask:0x%x 
2361,I,NANCHANSCHED_update_chan_link_param NSS %d 
2461,IIII,ULW single shot notif %x start_time internal %x external %x curr_time %x 
2460,I,---------Sort Entry[%d] ULW WORKING ON -------

 
2459,IIIII,---------Sort Entry[%d] Updating start time depending on count(current %d, actual %d) and period(%u) offset:%u

 
2458,III,---------Entry[%d] %x %x-------

 
2444,I,NAN20_ULW: ULW attribute count down %d 
2457,II,NAN_ULW: STARTING WITH FAW [%x %x]

 
2456,IIII,NAN_ULW: WORKING ON [0x%x, end 0x%x] FAW start [0x%x , end 0x%x] 

 
2455,,wlan_nan20_calculate_ulw_based_start_and_duration: FAW start is greater than the ULW start

 
2454,,wlan_nan20_calculate_ulw_based_start_and_duration: FAW start and end after ULW 
2453,,wlan_nan20_calculate_ulw_based_start_and_duration: FAW start and end after ULW

 
2452,IIII,#1 FAW SKIPPED by ULW0x%x, end 0x%x start 0x%x , end 0x%x 

 
2451,IIII,#2 FAW SKIPPED by ULW 0x%x, end 0x%x FAW start 0x%x , end 0x%x 

 
2450,IIII,OVERLAP ULW start 0x%x, end 0x%x FAW start 0x%x , end 0x%x 

 
2449,IIIIII,==== FINAL FAW[%d] duration %x offset %x %x %x %x
 
2448,II,wlan_nan20_find_cur_one_shot_ulw_end_time  offset 0x%x 0x%x 
2447,II,wlan_nan20_find_cur_one_shot_ulw_end_time  offset in past 0x%x 0x%x 
2446,II,wlan_nan20_find_cur_one_shot_ulw_end_time  0x%x 0x%x 
2445,,NAN20_ULW: Invalid ULW attribute 
2444,I,NAN20_ULW: ULW attribute count down %d 
2443,III,wlan_nan20_local_ulw_end_timeout: End Local ULW %d %x %x 
2442,IIII,wlan_nan20_local_ulw_end_timeout: curr_tsf:0x%x 0x%x duration:%u offset:%u 
2441,II,wlan_nan20_local_ulw_start_timeout: Start Local ULW for index %d %d 
2440,IIII,wlan_nan20_local_ulw_start_timeout: start_time:0x%x 0x%x period:%u duration:%u 
2439,II,wlan_nan20_local_ulw_start_timeout: curr_tsf:0x%x 0x%x 
2438,II,wlan_nan20_local_ulw_start_timeout: offset: %u count:%d 
2437,I,wlan_nan20_peer_ulw_delete: Invalid peer index %d 
2436,,wlan_nan20_peer_ulw_delete: Deleted peer 
2435,,wlan_nan20_peer_ulw_delete: Deleted peer ULW entry 
2434,I,wlan_nan20_peer_ulw_update: Peer entry found %d 
2433,I,wlan_nan20_peer_ulw_update: ULW schedule found %d 
2432,I,wlan_nan20_peer_ulw_update: Free Peer ULW entry %d 
2431,I,wlan_nan20_peer_ulw_update: Free Peer entry %d 
2430,IIII,wlan_nan20_peer_ulw_update: peer_idx:%d ulw_idx:%d free_peer_idx:%d free_ulw_idx:%d 
2429,II,wlan_nan20_peer_ulw_update: Fa session not active(0x%x) or ulw attr is NULL(0x%x) 
2428,,wlan_nan20_peer_ulw_update: Exiting count down 0 
2427,,wlan_nan20_peer_ulw_update: ERR No free Peer entry exiting 
2426,,wlan_nan20_peer_ulw_update: ERR No free Peer ULW entry exiting 
2425,II,wlan_nan20_peer_ulw_update: ULW is not updated from last time existing (sed_id:%d rcvd_seq_id:%d) 
2424,II,wlan_nan20_peer_ulw_update: Check ULW Seq is corrects (sed_id:%d rcvd_seq_id:%d) 
2423,II,wlan_nan20_peer_ulw_update: Pause ULW as update received(sed_id:%d rcvd_seq_id:%d) 
2422,I,wlan_nan20_peer_ulw_update: ERR Unhandled ULW ctrl type:%d 
2421,II,wlan_nan20_peer_ulw_update: band_id:%d channel_mhz:%d 
2420,II,wlan_nan20_peer_ulw_update: start_time:0x%x 0x%x 
2419,III,wlan_nan20_peer_ulw_update: curr_tsf:0x%x 0x%x diff:%d 
2418,II,wlan_nan20_ulw_config: Invalid input parameters p_ulw_info:0x%x sched_id:0x%x or NAN is disabled 
2417,,wlan_nan20_ulw_config: ULW allocated failed 
2416,II,wlan_nan20_ulw_config_update: Invalid input parameters p_ulw_info:0x%x sched_id:0x%x or NAN is disabled 
2415,IIII,wlan_nan20_ulw_config_update: Updated ULW sched_id:%d seq_id:%d map_id:%d diff:%u 
2414,II,wlan_nan20_ulw_end_timeout: End ULW peer_idx:%x, ulw_idx:%x 
2413,IIII,wlan_nan20_ulw_end_timeout: curr_tsf:0x%x 0x%x duration:%u offset:%u 
2412,IIII,wlan_nan20_ulw_start_timeout: start_time:0x%x 0x%x period:%u duration:%u 
2411,II,wlan_nan20_ulw_start_timeout: Start ULW peer_idx:%d, ulw_idx:%d 
2410,II,wlan_nan20_ulw_start_timeout: curr_tsf:0x%x 0x%x 
2409,II,wlan_nan20_ulw_start_timeout: offset: %u count:%d 
2408,II,wlan_nan20_update_peer_fa_ulw_status: Nothing to update peer_idx:%d ulw_idx:%d 
2407,II,wlan_nan20_update_ulw_mask: Nothing to update peer_idx:%d ulw_idx:%d 
2406,III,wlan_nan20_update_ulw_mask: Updated fa_mask:0x%x peer_idx:%d ulw_idx:%d 
2464,III,OFFLOAD HDLR UNIT TEST CMD: num_args=%d vdevId=%d testid=%d 
2463,I,OFFLOAD HDLR UNIT TEST: status = %d 
2462,III,Offload unit test input: vdevid:%d, group=%d, type=%d 
2465,III,VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
2465,III,VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
2465,III,VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
2465,III,VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
2465,III,VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
2465,III,VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
2465,III,VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
2465,III,VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
2465,III,VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
2465,III,VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
2466,II,VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 
2467,,the cur match is sending to host, drop this frame 
2465,III,VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
2468,III,VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x  
2469,IIII,VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 0x%x 
2465,III,VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
2469,IIII,VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 0x%x 
2469,IIII,VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 0x%x 
2469,IIII,VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 0x%x 
2466,II,VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 
2465,III,VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
2470,II,WOW_PROBE_RESP_TX offload flags = 0x%x enabled = %d 
2471,,WOW_PROBE_RESP_TX: wps ie recv, wakeup host 
2472,,WOW_PROBE_RESP_TX: send probe resp 
2473,I,WOW_PROBE_RESP_TX: tx done cb, compl status=%d 
2474,I,WOW_RECV_MGMT frame_type = 0x%x 
2475,IIII,BEACON TX ignored, vdev id:%x, mac_id:%x, bcn_tx_paused:%x, pdev_id:%x 
2476,III,WOW_BEACON_OFFLOAD_TX  completion_status = 0x%x bcn_pending_count = 0x%x bcn_buf_initialized = 0x%x 
2477,II,WOW_PROBE_RESP_TX: PRB TMPL CMDID, probe_resp_len=%d flags=%x 
2478,II,CSA_OFFLOAD_DEREGISTER_VDEV vdev_id = %d is_wmi_vdev_down=0x%x 
2479,II,CSA_OFFLOAD_REGISTER_VDEV vdev_id = %d vdev_mode=0x%x 
2480,II,csa vdev_start notif,csa ch:0x%x, prev csa ch:0x%x 
2481,IIII,_csa_vdev_notif_handler: enable:%x pause_until_beacon:%x, csa state:%x, notify:%x
 
2482,,pause disable 
2483,I,pause vdev, csa:%x 
2484,II,CSA_OFFLOAD_CSA_RECV_ERROR_IE  vdev_id = %d tbtt_cnt=0x%x 
2484,II,CSA_OFFLOAD_CSA_RECV_ERROR_IE  vdev_id = %d tbtt_cnt=0x%x 
2485,II,CSA_OFFLOAD_CSA_RECV_ERROR_IE vdev_id = %d tbtt_cnt=0x%x 
2486,IIII,CSA_OFFLOAD_BEACON_CSA_RECV, CSA_IE  vdev_id = %d tbtt_cnt=0x%x, csa ch:0x%x, prev csa ch:0x%x 
2487,IIII,CSA_OFFLOAD_BEACON_CSA_RECV, XCSA_IE  vdev_id = %d tbtt_cnt=0x%x, csa ch:0x%x, prev csa ch:0x%x 
2488,III,csa handle ie: enable:%x pause_until_beacon:%x, csa state:%x
 
2489,II,CSA_OFFLOAD_WMI_EVENT_ERROR  vdev_id = %d csa_proc=0x%x 
2490,III,CSA_OFFLOAD_WMI_EVENT_SENT vdev_id = %d : state: 0x%x, flag: 0x%x 
2491,III,CSA_OFFLOAD_CSA_TIMER_EXP  vdev_id = %d csa_proc=0x%x curr_tsf=0x%x 
2492,III,CSA_OFFLOAD_CSA_TIMER_ERROR vdev_id = %d csa_proc/bcn_tsf=0x%x curr_tsf=0x%x 
2493,II,CSA_OFFLOAD_CSA_TIMER_ERROR  vdev_id=0x%x state=0x%x 
2494,II,CSA_OFFLOAD_WMI_CHANSWITCH_RECV  cur_ch=0x%x new_ch=0x%x 
2497,,wlan_p2p_lo_start_test entry 
2496,,wlan_p2p_lo_stop_test entry 
2495,IIIIII,P2P LO unit test input: type=%d, args[1]=%d,args[2]=%d,args[3]=%d,args[4]=%d,args[5]=%d 
2498,I,_wlan_p2p_lo_frames_handler receive p2p action frame,wow_enable=%d 
2499,,_wlan_p2p_lo_frames_handler,drop2 
2500,,_wlan_p2p_lo_frames_handler,drop 1 
2501,IIII,_wlan_p2p_lo_frames_handler, subtype:%x, length:%d,vdevid:%d, state:%d 
2502,III,_wlan_p2p_lo_listen_interval_timeout p2p_lo_cfg_cnt = %d, p2p_lo_cur_cnt=%d,wow_enable=%d 
2503,I,_wlan_p2p_lo_scan_evt_handler evt->type = %d 
2504,I,_wlan_p2p_lo_vdev_init SCAN_SCH_START_ALLOC_FAIL, %d 
2505,I,_wlan_p2p_lo_vdev_stop_handler, vdev_id=%d 
2506,IIIIIII,_wlan_p2p_lo_vdev_start_handler vdev id=%d,channel=%d,period=%d,interval=%d,count=%d,device_types_len=%d,prob_resp_len=%d 
2507,II,_wlan_p2p_lo_vdev_start_handler lo_pdev->p2p_lo_vdev->vdev_id = %d, vdev id=%d 
2508,III,_wlan_p2p_lo_vdev_evt_handler notif->type = %d,vdev->id=%d,vdev->ic_opmode=%d 
2509,IIIIII,_wlan_p2p_lo_send_probreq_buf_complete src_mac:0x%x:0x%x:0x%x:0x%x:0x%x:0x%x 
2510,I,WPS: Skipped Requested Device Type attribute (max %u types) 
2511,I,WPS: Invalid Requested Device Type length %u 
2512,III,wlan_p2p_lo_wps_set_attr ERROR,type=%d,pos=0x%x, len=%d 
2513,II,wlan_p2p_lo_wps_parse_msg ERROR,ie_buf=0x%x,ie_len=%d 
2514,III,wlan_p2p_lo_parse_subelement ERROR.attr_type=%d,data=0x%x,attr_len=%d 
2515,II,wlan_p2p_lo_vendor_ie_parse ERROR pos=0x%x, pos[1] =%d 
2516,I,_wlan_p2p_lo_scan_stop P2P LO SCAN_STOP_COMMAND_FAILED, %d 
2517,II,_wlan_p2p_lo_scan_start p2p_lo_cfg_interval = %d,p2p_lo_state=%d 
2518,I,_wlan_p2p_lo_scan_start P2P LO SCAN_START_COMMAND_FAILED, %d 
2519,,_wlan_p2p_lo_vdev_probe_req_flush send probe request failure 
2520,,_wlan_p2p_lo_probe_req_store alloc probe req buffer failed,don't support larger size probe request 
2521,,_wlan_p2p_lo_probe_req_store no memory, delete oldest one 
2522,,_wlan_p2p_lo_probe_req_store alloc probe req buffer failed,delete oldest one and try it again 
2523,I,mgmt send failure:%d 
2524,,allocate mgmt failure 
2525,I,QUIET IE AP: test cfg success start_time=0x%x 
2526,,QUIET IE AP: test cfg fail 
2527,IIII,QUIET IE AP: test input num_args=%d vdevId=%d dur=%d cnt=%d 
2528,I,QUIET IE AP: test cb status=%d 
2529,III,QUIET IE AP: post migration,vdevId:%d, cac:%d, vdevPaused:%d 
2530,III,QUIET IE AP: quiet IE Start time=0x%x Curr_time=0x%x timeout=0x%x 
2531,,QUIET IE AP: cancel current quiet IE config 
2532,I,QUIET IE AP: start quiet IE: input duration out of range, duration_us = %d 
2533,IIII,QUIET IE AP: start quiet IE: module id=%d, vdev id=%d, dur=%d, beaconing_cnt=%d 
2534,IIII,QUIET IE AP: append quiet IE, tbtt cnt=%d dur=0x%x offset=0x%x len=%d 
2535,II,QUIET IE AP: not appending quiet IE. time_to_quite_period_start = 0x%x, time_to_bcn_tx = 0x%x 
2536,III,QUIET IE AP: bi_us=%d diff=%d curr_wal_time=0x%x 
2537,I,QUIET IE AP: quiet duration time-usec:0x%x 
2538,III,QUIET IE AP: timer cb-next evt:%d, cac:%d, paused:%d 
2539,I,QUIET IE AP: vdev init vdevId=%d 
2540,,QUIET IE STA: test cfg success 
2541,,QUIET IE STA: test cfg fail 
2542,,QUIET IE STA: test cfg, vdev not up or incorrect mode 
2543,IIII,QUIET IE STA: test input num_args=%d vdevId=%d dur=%d per=%d 
2544,II,QUIET IE STA: post migration,vdevId:%d, suspend:%d 
2545,II,QUIET IE STA: Quiet period starts in=0x%x, vdevId=%d 
2546,,QUIET IE STA: cancel current quiet IE config 
2547,IIIII,QUIET IE STA: vdevId=%d, next_start=%d, period=%d, duration=%d, quiet_enabled=%d 
2548,IIII,QUIET IE STA, time-usec:0x%x, vdevId=%d, evt:%d, suspend:%d 
2549,I,sap obss vdev notify fails: obss vdev not exist id:%d 
2550,I,sap obss vdev init fails: opmode not support:%d 
2561,I,sap obss detect: not support: vdev id:%d 
2560,IIII,sap obss detect: vdev id:%d, period:%d,mode:%d %d 
2559,IIIII,more mode:%d %d %d %d %d 
2558,III,event report fails in wow, vdev id:%d, reason:%d, match_mask:0x%x 
2557,IIIII,event report,vdev id:%d, reason:%d, match_mask:0x%x, addr:0x%04x 0x%02x 
2556,I,Beacon parser invoked, len wrong:%d 
2555,I,Length shorter than expected  erp_ie:%d 
2554,III,loop_vdev:%d, match_mask:0x%x, need_report:%d 
2553,II,Beacon parser error, type:%d, sub:%d 
2552,I,Length shorter than expected  ht_oper_ie:%d 
2551,III,timer is not started: vdev id:%d t:%d, c:%d 
2562,I,sap obss detect unit test: args0 
2564,I,WOW_RECV_MGMT  frame_type = 0x%x 
2565,III,WOW action frame received wh->i_fc[0] = %d, action_category = %d, action_sub_category_bitmap = %d 
2564,I,WOW_RECV_MGMT  frame_type = 0x%x 
2563,,Length less than frame_length + action_category + sub_category_bitmap. 
2566,I,set proc pattern err, unsupported len:%d 
2567,I,Invalid pattern id %d 
2568,III,OFLD send periodic ptrn vdev_id=%d ptrnId=%d ptrnLen=%d 
2569,I,WOW_NS_ARP_OFLD_DISABLE vdev_id = %d 
2570,II,HW CCE ns offload disabled, vdev id:%x, ns_cnt:%x 
2571,III,WOW enable cmd vdevId=%d ARP %d NS %d 
2572,II,WOW_ARP_OFLD_ENABLE vdev_id =%d  ip_addr = 0x%x 
2573,IIIII,WOW_NS_OFLD_ENABLE_1 vdev_id = %d ipv6_addr_31_0 = 0x%x ipv6_addr_63_32 = 0x%x ipv6_addr_95_64 = 0x%x ipv6_addr_127_96 = 0x%x 
2574,IIIII,WOW_NS_OFLD_ENABLE_0 vdev_id = %d ipv6_addr_31_0 = 0x%x ipv6_addr_63_32 = 0x%x ipv6_addr_95_64 = 0x%x ipv6_addr_127_96 = 0x%x 
2575,,WOW NS OFLD CCE del flt 
2576,II,WOW_NS_OFLD add flt CCE j=%d TGT IPv6 last 4 bytes ipv6_addr_127_96 = 0x%x 
2577,,WOW ARP OFLD CCE del flt 
2578,I,WOW ARP OFLD CCE add flt tgt ip = 0x%x  
2579,II,NA_PROC_FRAME Invalid Len %d version 0x%x
 
2580,IIIIII,NA_PROC_FRAME Invalid NA L2=%d 0x%x L3=%d 0x%x L4=%d 0x%d
 
2581,,NA_PROC_FRAME Invalid vdev 
2582,,ARP_NS_SUBNET_CHANGE_DATA_RX Not valid ARP/NS 
 
2583,II,NA_CHECKSUM_FAIL rec=0x%x exp=0x%x 
2584,,warning:ns invalid,drop 
2585,IIIII,OFLD NS REPLIED vdev_id = %d ipv6_addr_31_0 = 0x%x ipv6_addr_63_32 = 0x%x ipv6_addr_95_64 = 0x%x ipv6_addr_127_96 = 0x%x 
2586,,NS req frame dropped , NS reply frame allready in air 
2587,IIIII,OFLD NS RECEIVED vdev_id = %d TGT IP ipv6_addr_31_0 = 0x%x ipv6_addr_63_32 = 0x%x ipv6_addr_95_64 = 0x%x ipv6_addr_127_96 = 0x%x 
2588,II,OFLD ARP REPLIED vdev_id = %d ip_addr = 0x%x 
2589,,ARP req frame dropped ,arp reply frame allready in air 
2590,II,OFLD ARP RECEIVED vdevId=%d srcIp=0x%x 
2591,,Resetting NS frame in air parm 
2592,,Resetting ARP frame in air parm 
2593,,OFLD NS error,invalid option 
2594,III,OFLD NS validate checksum fail, expect checksum:%x checksum in frame:%x payload_len:%x
 
2595,III,WOW_RECV_DATA_PKT  tgt_ip = 0x%x src_ip = 0x%x ops = 0x%x 
2596,I,WOW_RECV_DATA_PKT  ARPPKT_REQUEST received :0x%x 
2597,I,bpf pdev is not initialized: %x
 
2598,IIII,dropped:v:%x f:%x c:%x d:%x
 
2599,I,not found vdev:%x
 
2600,II,unicast recv count = %d, unicast allow count = %d 
2601,I,Adaptive BPF next_timeout = %d 
2602,I,Adaptive BPF: (curr_time - bpf_last_sleep_timestamp) = %d 
2603,I,BPF PS AWAKE curr_time = %d 
2604,I,BPF PS SLEEP curr_time = %d 
2605,I,Disable Adaptive APF curr_time = %d 
2606,I,Enable Adaptive APF curr_time = %d 
2607,,Next state is APF 
2608,,Next state is non APF 
2609,II,evaluate next state curr_time = %d, uc_bitmap = %d 
2610,I,Active APF for unicast mode = %x is not supported 
2611,I,Active APF for MCBC mode = %x is not supported 
2612,II,Active APF command mcbc_mode = %x, uc_mode = %x 
2613,I,vdev not created:%x
 
2614,II,Active APF conf for unicast: uc APF mode = %x, data path conf = %x 
2615,II,Active APF conf for MCBC: MCBC APF mode = %x, data path conf = %x 
2616,III,WOW notify for active APF: uc mode = %x, mcbc mode = %x, data path config = %x 
2599,I,not found vdev:%x
 
2617,II,no mem for inst:v:%x, f:%x
 
2618,II,no filter available:v:%x, f:%x
 
2619,II,del pre filter:v:%x, f:%x
 
2613,I,vdev not created:%x
 
2620,II,invalid filter id, fw max:%x, host set:%x
 
2621,III,invalid, t:%x, c:%x, l:%x
 
2622,I, _wlan_bpf_offload_cmd_handle_get_vdev_stats: no buf %x
 
2599,I,not found vdev:%x
 
2623,I,_wlan_bpf_offload_cmd_handle_get_cap: no buf %x
 
2599,I,not found vdev:%x
 
2633,III,bpf dump vdev:%d, filter_id:%d, total_len:%d
 
2632,IIII,hex:%02x%02x%02x%02x 
2631,II,OFLD BPF unit test cmd: Route UC active vdevId=%d, enable=%d 
2630,,OFLD BPF unit test disable UC route in active mode 
2629,,OFLD BPF unit test enable UC route in active mode 
2628,,OFLD BPF unit test enable UC route in active mode fails as bpf not enabled 
2599,I,not found vdev:%x
 
2627,I,Allow Percentage is incorrect: %d
 
2626,I,minimum monitored value should be non zero: %d
 
2625,I,traffic threshold value should be non zero: %d
 
2624,III,Adaptive APF params: Allow percentage = %d, Min monitored packet = %d, Traffic threshold = %d
 
2634,II,WOW gtk_offload_dispatch_wmi_cmd: GTK_OFFLOAD_REQUEST_STATUS_OPCODE 0x%x%x
 
2635,,WOW gtk_offload_dispatch_wmi_cmd: GTK_OFFLOAD_DISABLE_OPCODE
 
2636,II,WOW gtk_offload_dispatch_wmi_cmd: GTK_OFFLOAD_ENABLE_OPCODE 0x%x%x
 
2637,I,WOW gtk_offload_dispatch_wmi_cmd: wrong kek_len = %d 
2638,IIIIIIII,FILS_DEBUG GTK OFFLOAD repay_counter %d %d %d %d %d %d %d %d 
2639,III,FILS_DEBUG GTK OFFLOAD command recvd vdev id %d flags %d kek_len %d 
2640,IIIIIIII,FILS_DEBUG GTK OFFLOAD extended repay_counter %d %d %d %d %d %d %d %d 
2641,III,FILS_DEBUG GTK OFFLOAD extended command recvd vdev id %d flags %d kek_len %d 
2642,,_gtk_offload_send_status: no buf 
2643,,WOW gtk_offload_can_deliver_rxdata_tohost: delay m2 packet. 
 
2644,,WOW gtk_offload_can_deliver_rxdata_tohost: no buffer for m2 packet. 
 
2645,,WOW gtk_offload_can_deliver_rxdata_tohost: gtk_error. 
 
2646,,WOW gtk_offload_can_deliver_rxdata_tohost: not eapol_key. 
 
2647,,WOW gtk_offload_process_rekey:Already sending
 
2648,,WOW gtk_offload_can_deliver_rxdata_tohost: no gtk_vdev_ctx. 
 
2649,,gtk offload ignore the frame. 
2650,,WOW gtk_offload_send_rekey_failure_event:Exit
 
2651,,_gtk_offload_send_rekey_failure_event: no evt 
2652,II,FILS_DEBUG gtk_offload_check_rekey: Buffer is not enough to contain keyData length %d keydata_length %d 
2653,I,FILS_DEBUG key_info %x 
2654,,gtk_offload_process_rekey:type is not AES/TKIP 
2655,,gtk_offload_process_rekey:mic fail 
2656,,gtk_offload_process_rekey:decrypt_key fail 
2657,I,gtk_offload_process_rekey: neither MIC or encrKeyData is present %d 
2658,II,_gtk_offload_process_rekey, replay:%x, cur:%x 
2659,III,_gtk_offload_process_rekey %d mic %d encrKeyData %d 
2660,I,_gtk_offload_decrypt_key: aes_siv_decrypt failed %d 
2661,,WOW gtk_offload_deferred_m2_callback:install key
 
2662,I,_gtk_offload_deferred_m2_callback, txrx status:%x 
2663,,_gtk_offload_deferred_m2_callback, allocate buffer failure 
2664,I,_gtk_offload_deferred_m2_callback, refresh cnt:%x 
2665,I,WOW gtk_offload_tx_completion_callback, tx_completion_status=%d
 
2666,,Delete NON ICMPv6 MC CCE filter 
2667,,Add NON ICMPv6 MC CCE filter 
2668,,Delete NON ARP BC CCE filter 
2669,,Add NON ARP BC CCE filter 
2670,IIIIII,OFFLOAD HDLR CCE UNIT TEST CMD: num_args=%d vdevId=%d args =%d %d %d %d  
2671,I,mcast filter command =%d  
2672,I,Enhanced mcast enable %d 
2673,,Null vdev for enhanced mcast 
2674,,Null command for enhanced mcast 
2675,IIII,WLAN_CHATTER_MC_FILTER_DEL_EX  vdev_id = 0x%x mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x status = 0x%x 
2676,II,OFLD MC_FLT_DEL_EX num_flt=%d vdev_id=%d 
2677,III,WLAN_CHATTER_MC_FILTER_DEL_EX  vdev_id = 0x%x mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x 
2678,III,WLAN_CHATTER_MC_FILTER_ADD_EX	vdev_id = 0x%x mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x 
2679,I,OFLD MC_FLT_ADD_EX Disable hash flt-- no slot avail,vdev_id=%d 
2680,I,OFLD MC_FLT_ADD_EX Enable hash flt, vdev_id=%d 
2681,I,OFLD MC_FILTER_ADD_EX hash flt idx=%d 
2682,I,OFLD MC_FILTER_ADD_EX num_flt=%d 
2683,IIII,WLAN_CHATTER_MC_FILTER_ADD_EX  vdev_id = 0x%x mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x status = 0x%x 
2684,II,WOW MC addr matched vdevId=%d reason=%d 
2685,IIII,WLAN_MC_FILTER mcbc_status = %d vdev_id = 0x%x mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x 
2686,,L2 not valid 
2687,III,Not for enhanced mcast %d %d %d 
2692,,wlan_mcast_flt_add_test entry 
2691,,wlan_mcast_flt_clear_test entry 
2690,,wlan_mcast_flt_del_test entry 
2689,,wlan_mcast_flt_set_test entry 
2688,IIIIII,MCAST FILT unit test input: type=%d, args[1]=%d,args[2]=%d,args[3]=%d,args[4]=%d,args[5]=%d 
2693,I,pkt filter command =%d  
2694,II,pkt filter vdevPtr count =%d filter id = %d 
2695,,pkt filter error: No filters set 
2696,I,data length out of bounds =%d  
2697,I,All pkt fltrs used =%d  
2698,I,num of sub-filters exceeds allowed =%d  
2699,,pkt filter registering  
2700,,vdev pktFltrInfo is NULL  
2701,,pkt fltr data handler: vdev is NULL  
2702,III,WOW add timer ptrn vdev_id=%d, ptrn_id=%d, timeout_ms=%d 
2703,II,WOW del ptrn vdev id=%d ptrn id=%d 
2704,IIII,WOW add ptrn vdev id=%d idx=%d ptrn id=%d ptrn len=%d 
2705,I,WOW_RECV_BITMAP_PATTERN  pattern_id = 0x%x 
2706,II,WOW Eapol check match vdevId=%d reason=%d 
2707,II,WOW Magic pkt rcvd vdevId=%d reason=%d 
2708,II,WOW RA filter match vdevId=%d reason=%d 
2709,I,WOW NA drop unsolicity na, vdev:%d 
2710,I,dispatch_ipsec_natkeepalive_filter_cmd: action = %d 
2711,,_wlan_natkeepalive_handler  OFFLOAD_STATUS_DROP 
2712,II,P2P_UPDATE_SCHEDULE_OPPS  0x%x 0x%x 
2712,II,P2P_UPDATE_SCHEDULE_OPPS  0x%x 0x%x 
2712,II,P2P_UPDATE_SCHEDULE_OPPS  0x%x 0x%x 
2712,II,P2P_UPDATE_SCHEDULE_OPPS  0x%x 0x%x 
2713,II,P2P_NOA_GO_PRESENT  0x%x 0x%x 
2714,II,P2P_NOA_GO_ABSENT  0x%x 0x%x 
2712,II,P2P_UPDATE_SCHEDULE_OPPS  0x%x 0x%x 
2715,III,P2P_SCHEDULE_TIMEOUT  0x%x 0x%x 0x%x 
2716,II,Current Priority=0x%x  Next Priority=0x%x 
2717,II,P2P_SCHEDULE_TIMEOUT  0x%x 0x%x 
2718,I,next tbtt wakeup %d  
2719,IIII,p2p_ps_set_noa: start_time=0x%x, duration=%u, interval=%u, type_count=%u 
2720,I,p2p_ps_set_noa: Host Periodic NOA Configuration FAILED, FW_Periodic_NOA_Map=0x%x 
2721,I,p2p_ps_set_noa: vdev_id = %d, Host NOA Disabled 
2722,III,p2p_ps_set_oppps: vdev_id = %d, oppps_enable = %d, ctwindow = %d 
2723,IIII,p2p_ps_set_oppps: Host OPPPS enable FAILED, FW_Periodic_NOA_Map=0x%x, Host_Periodic_NOA_Map = 0x%x, ctwin = %d, bcn_intval = %d 
2724,IIII,P2P_GO_BCN_TX_COMP: bcn_tx_status = 0x%x chan_mhz = 0x%x cur_wal_time = 0x%x cur_vdev_tsf = 0x%x 
2725,I,p2p_notify_sta_sleep: %d 
2726,,p2p_notify_sta_sleep: vdev is NULL 
2727,II,p2p_vdev_evt_handler  vdev_id = %d, evt = %d 
2728,I,p2p_client_recal_noa: vdev_id = %d  
2729,I,P2P_GO_GET_NOA_INFO  0x%x 
2729,I,P2P_GO_GET_NOA_INFO  0x%x 
2730,III,P2P_CALC_SCHEDULES_CALL_ALL_NEXT_EVENT_FROM_WHILE_LOOP  0x%x 0x%x 0x%x 
2731,IIIIII,P2P_GO_GET_NOA_IE  0x%x 0x%x 0x%x 0x%x 0x%x 0x%x 
2732,IIIII,wlan_p2p_add_noa: boa_idx=%u, start_time=0x%x, duration=%u, interval=%utype_count=%u 
2733,I,P2P_DEV_REGISTER  vdev_id = %d 
2734,IIIII,p2p_go_notify_periodic_noa: noa_idx=%u, start_time=0x%x, duration=%u, interval=%u, type_count=%u 
2735,,p2p_wal_pdev_event_handler: Recal P2P Client NOA schedules due to wakeup 
2736,,p2p_wal_pdev_event_handler: Clear P2P Client NOA schedules due to power collapse 
2737,I,P2P_GO_TBTT_OFFSET  0x%x 
2738,IIIII,P2P_GO_ADD_ONE_SHOT_NOA  0x%x 0x%x 0x%x 0x%x 0x%x 
2739,III,P2P_GO_ADD_ONE_SHOT_NOA  0x%x 0x%x 0x%x 
2729,I,P2P_GO_GET_NOA_INFO  0x%x 
2740,IIIIII,P2P_GO_GET_NOA_INFO  0x%x 0x%x 0x%x 0x%x 0x%x 0x%x 
2741,I,P2P_HANDLE_NOA: NoaPresent = %d 
2741,I,P2P_HANDLE_NOA: NoaPresent = %d 
2742,IIII,P2P_HANDLE_NOA: Reject Invalid NOA, duration=%d,interval=%d start_time=0x%x type_count=%d 
2770,I,P2P_CALC_SCHEDULES_ENTER  0x%x 
2769,IIII,P2P_CALC_SCHEDULES_FIRST_VALUE  0x%x 0x%x 0x%x 0x%x 
2768,III,P2P_CALC_SCHEDULES_EARLIEST_NEXT_EVENT  0x%x 0x%x 0x%x 
2767,II,P2P_CALC_SCHEDULES_CALL_ALL_NEXT_EVENT_FROM_WHILE_LOOP  0x%x 0x%x 
2766,I,P2P_CALC_SCHEDULES_TIMEOUT_1  0x%x 
2765,I,P2P_CALC_SCHEDULES_TIMEOUT_2  0x%x 
2764,I,P2P_FIND_ALL_NEXT_EVENTS_ENTER  0x%x 
2763,IIIII,P2P_FIND_ALL_NEXT_EVENTS_INDIVIDUAL_REQ_AFTER_CHANGE  0x%x 0x%x 0x%x 0x%x 0x%x 
2762,I,P2P_FIND_ALL_NEXT_EVENTS_REQ_EXPIRED  0x%x 
2761,I,P2P_FIND_ALL_NEXT_EVENTS_REQ_ACTIVE  0x%x 
2760,I,P2P_FIND_NEXT_EVENT_ENTER  0x%x 
2759,I,P2P_FIND_NEXT_EVENT_REQ_NOT_STARTED  0x%x 
2758,II,P2P_FIND_NEXT_EVENT_REQ_COMPLETE_NON_PERIODIC  0x%x 0x%x 
2757,II,P2P_FIND_NEXT_EVENT_IN_MID_OF_NOA  0x%x 0x%x 
2756,II,P2P_FIND_NEXT_EVENT_REQ_COMPLETE  0x%x 0x%x 
2755,I,P2P_SCHEDULE_TIMEOUT  0x%x 
2754,III,P2P_NOA_GO_PRESENT  0x%x 0x%x 0x%x 
2753,,P2P_NOA_GO_PRESENT(No_More_Events): Unpause BSS Peer 
2752,II,P2P_NOA_EXPIRY_DELTA: curr_time = 0x%x pkt_exp_time = 0x%x 
2713,II,P2P_NOA_GO_PRESENT  0x%x 0x%x 
2751,,P2P_NOA_GO_ABSENT: TDLS Link is Active so Pause BSS Peer only  
2750,,P2P_NOA_GO_PRESENT: Unpause BSS Peer 
2714,II,P2P_NOA_GO_ABSENT  0x%x 0x%x 
2749,I,P2P_PROCESS_SCHEDULE_ENTER  0x%x 
2748,IIII,P2P_PROCESS_SCHEDULE_AFTER_CALC  0x%x 0x%x 0x%x 0x%x 
2747,III,P2P_PROCESS_SCHEDULE_STARTED_TIMER  0x%x 0x%x 0x%x 
2746,II,P2P_SETUP_SCHEDULE_TIMER  0x%x 0x%x 
2745,IIIII,P2P_UPDATE_SCHEDULE_OPPS: duration = %u go_sched_type = %u interval = %u start_time = 0x%x type_count = %u 
2744,IIII, P2P_UPDATE_SCHEDULE: duration = %u interval = %u start_time = 0x%x type_count = %u 
2743,IIII,P2P_UPDATE_START_TIME: curr_go_tsf = 0x%x, noa_start_time_go_tsf = 0x%x, curr_wal_time = 0x%x, noa_start_wal_time = 0x%x 
2777,II,wlan_pm_arbiter_dump_wake_stats: mac_id=%d, ModuleID=%d 
2776,IIIIII,PS_STA_PM_ARB_REQUEST: vdev_id=%d, mac_id=%d, ModuleID=%d, Flags=0x%x, LastRequestTime=%d, Request=%d 
2775,II,PS_STA_PM_ARB_RESOLVE: macid=%d, power_state=%d 
2774,II,wake_monitor mac:%d win_len:%dms 
2773,IIIIII,wake_monitor mac:%d w_list mod:%d vdev:%d total_time:%dms total_cnt:%d max_time:%dms 
2772,IIIIII,wake_monitor mac:%d s_list mod:%d vdev:%d total_time:%dms total_cnt:%d max_time:%dms 
2771,III,wlan_pm_arbiter_vdev_migration: vdevid=%d, old_mac_id=%d, new_mac_id=%d 
2779,,PS_PRE_SEND: wlan peer is NULL 
2778,I,STA PS: VOWiFi: voip_notify_pdev: vo_call_start=%d 
2780,II,AP_PS_DBGID_HOST_TX_PAUSE vdev_map = %0x, pause: %d 
2781,I,AP_PS_DBGID_VDEV_DELETE: vdev_id = %d 
2782,I,AP_PS_DBGID_VDEV_CREATE: vdev_id = %d 
2783,,AP vdev not existing any more. But CABQ is running. 
2784,,PS_BUF_WAL_PEER_EVENT: wlan peer is NULL 
2785,I,AP_PS_DBGID_START_CAB vdev_id = %d 
2786,IIIII,AP_PS_DBGID_DELIVER_CAB vdev_id = %d Tid = %d NumMPDU = %d Flags = 0x%x RetryOther = %d 
2787,I,AP_PS_DBGID_CAB_FINISH vdev_id = %d 
2788,II,STA PS: wlan_ps_sta_health_monitor_timeout: vdev_id=%d sta_flags=0x%X 
2789,II,STA PS: VOWiFi: ps_poll_timer_start: interval_ms=%d, spec_pspoll_nodata_count=%d 
2790,I,STA PS: VOWiFi: ps_poll_timer_timeout: sta_flags=0x%X 
2791,II,STA PS: VOWiFi: voip_notify: vdev_id=%u, vo_call_start=%d 
2792,I,STA PS: VOWiFi: resync_appm: sta_flags=0x%X 
2793,I,PS_STA_GET_INACT_TIME: type of frame(%d) not recognized 
2794,IIIIII,PS_STA_PSPOLL_SEQ_DONE vdev_id = %d QueueTime = %d CompleteTime = %d ResponseTime = %d ResponseDuration = %d ResponseFrameCtrl/QosCtrl = 0x%x 
2795,II,PS_STA_WOW_MODE vdev_id = %d Enable = %d 
2796,II,PS_STA_COEX_MODE vdev_id = %d Enable = %d 
2797,IIIIII,PS_STA_UAPSD_AUTO_TRIG_PER_AC vdev_id = %d WMM_AC = %d UserPriority = %d SrvIntl = %d SuspIntl = %d DelayIntl = %d 
2798,II,PS_STA_UAPSD_AUTO_TRIG VdevID = %d NumAC = %d 
2799,III,PS_STA_SET_PARAM vdev_id = %d param = 0x%x value = 0x%x 
2800,III,PS_STA_DELIVER_EVENT vdev_id = %d EventType = %d Statue = %d 
2801,IIII,PS_STA_PSPOLL_ALLOW vdev_id = %d Allow = %d Flags = 0x%x Time = %d 
2802,I,wlan_ps_sta_unpause: vdev_id=%d 
2803,II,wlan_ps_sta_pause: vdev_id=%d, timeout_us=%u 
2804,IIIIII,PS_STA_QPOWER_RESYNC vdev_id = %d VDevUpCnt = %d IsBTConnected = 0x%x Flags = 0x%x VDevSubMode = 0x%x BitMap = 0x%x 
2805,,wlan_ps_sta_txrx_inactivity_check extend2 
2806,II,wlan_ps_sta_txrx_inactivity_check extend: override_ito_us=%d, inactive_time_us=%d 
2807,II,wlan_ps_sta_txrx_inactivity_check extend: num_of_no_rx_activity_with_tim=%d, inactive_time_us=%d 
2808,I,STA PS vdev_id = %d, No buffers available for null frames 
2809,,PS_STA_WAL_PEER_EVENT: wlan peer is NULL 
2810,,PS_STA_WAL_PEER_EVENT_PRE_SEND: wlan peer is NULL 
2819,II,wlan_ps_sta_state_pause_event: vdev id = %d, pause_stat_rx_frms_leaked = %d 
2818,III,SPEC_PSPOLL_TIMEOUT: vdevid=%d, spec=%d, timeout=%d 
2817,IIII,sleep_awake_event_rx: MD=%d, pspoll_count=%d, is_qos_null:%d, nodata_count=%d 
2816,IIII,sleep_awake_event_rx: is_qos_null:%d, wakeup_dur=%d, nodata_count=%d, max_count=%d 
2815,,STA PS: VOWiFi: data_complete:  
2814,,total_spec_pspoll_count reaches MAX: reset it 
2813,IIIII,wlan_ps_sta_tx_sent_send_nullfunc: vdevid=%d, force_ps=0X%x, sta_handle=%p, peer_type=%d, blocked_tids=0X%x 
2812,II,PS_STA_SPECPOLL_TIMER_STARTED vdev_id = %d SpecPsPollNoDataCnt = %d 
2811,I,PS_STA_SPECPOLL_TIMER_STOPPED: vdev_id = %d 
2826,IIIIIIII,wlan_qpower_check_traffic_history during voip: vdev_id = %d num_entries = 0x%x total_rx_bytes = 0x%0x first_entry_timestamp:%0x%0x current_time:%0x%0x spec_wakeup_needed:%0x 
2825,IIIIII,wlan_qpower_check_traffic_history: total_rx_bytes = 0x%0x total_tx_bytes = 0x%x last_exit_timestamp:%0x:%0x first_entry_timestamp:%0x%0x 
2824,IIIIIIII,wlan_qpower_check_traffic_history: vdev_id = %d num_entries = 0x%x num_wakeups_with_tx = 0x%x num_wakeups_with_rx:%0x total_duration:%0x rx_throughput:%0x tx_throughput:%0x spec_wakeup_needed:%0x 
2823,I,wlan_ps_sta_txrx_inactivity_check is_tim_war_enabled wal_vdev id : %d  
2822,IIIIIIII,wlan_qpower_is_spec_wakeup_needed: vdev_id = %d active_duration = 0x%x current_ito_us = 0x%x congestion:%0x thresh:%0x voip_in_progress:%0x specIto:%0x spec_wakeup:%0x 
2821,IIIII,wlan_qpower_record_end: current_index = %0x exit_timestamp:%0x:%0x entry_timestamp:%0x%0x 
2820,III,wlan_qpower_record_start: current_index = %0x entry_timestamp:%0x%0x 
2827,I,wlan_egap_sm_state_pwrsave_on_event  event_type = %d 
 
2828,,wlan_egap_sm_state_pwrsave_on_exit  
 
2829,IIII,EGAP bypass chainmask mgr Set number of Chains  :curr_tx_chainmask = 0x%x, curr_rx_chainmask = %d, new rx_chainmask = %d new tx_chainmask = %d 
 
2830,,wlan_egap_sm_state_pwrsave_on_entry  
 
2831,I,wlan_egap_sm_state_wait_event  event_type = %d 
 
2832,,wlan_egap_sm_state_wait_exit  
 
2833,,wlan_egap_sm_state_wait_entry  
 
2834,I,wlan_egap_sm_state_pwrsave_off_event : event_type = %d  
 
2835,,wlan_egap_sm_state_pwrsave_off_exit  
 
2836,,wlan_egap_sm_state_pwrsave_off_entry  
 
2837,II,AP_PS_DBGID_EGAP_CHANGE_SM_STATE: curr_state = %d state = %d 
2838,I,wlan_egap_sm_state_idle_event : event_type = %d  
 
2839,,wlan_egap_sm_state_idle_exit 
 
2840,,wlan_egap_sm_state_idle_entry 
 
2841,IIII,wlan_wmi_egap_param_cmd cmd->enable = %d cmd->inactivity_time = %d cmd->wait_time = %d cmd->flags = %d 
 
2842,,wlan_egap_delete_ap_vdev_instance unregistering wlan_egap_vdev_notif_handler AP 
 
2843,I,registering wlan_egap_vdev_notif_handler AP nResult = %d 
 
2844,I,wlan_egap_is_traffic_pending = %d  
2845,I,wlan_egap_set_event_handler error in deregistering WLAN_EGAP_REG_EV_HANDLER_RX_PHYERR event : Result = %d  
2846,I,wlan_egap_set_event_handler error in registering pdev event : Result = %d WLAN_EGAP_REG_EV_HANDLER_RX_PHYERR  
2847,I,wlan_egap_set_event_handlers: WLAN_EGAP_REG_EV_HANDLER_RX_PHYERR = %d 
2848,I,wlan_egap_set_event_handler error in deregistering pdev event : Result = %d WAL_PDEV_EVENT_SWBA 
2849,I,wlan_egap_set_event_handler error in registering pdev event : Result = %d WAL_PDEV_EVENT_SWBA  
2850,I,wlan_egap_set_event_handlers: new_mask = %d 
2851,I,wlan_egap_sm_unable_to_start  egap_handle->flags = 0x%x 
 
2852,,wlan_egap_sm_start  
 
2853,,wlan_egap_sm_unable_to_start not idle 
 
2854,,ERROR !!! EGAP hdl is NULL 
 
2855,I,wlan_egap_sm_unable_to_stop  egap_handle->flags = 0x%x 
 
2856,,wlan_egap_sm_stop  
 
2854,,ERROR !!! EGAP hdl is NULL 
 
2857,II,Already in single chain tx_chainmask:0x%x, rx_chainmask:0x%x
 
2858,,_wlan_egap_init 
2859,,_wlan_egap_wmi_dispatch_cmds !egap_handle 
 
2860,,_wlan_egap_wmi_dispatch_cmds 
 
2861,,WLAN_EGAP_PARAM_IS_PWRSAVE_BY_INACTIVITY_ENABLED  
 
2862,,wlan_egap_set_param_handler: pdev = NULL  
 
2863,,wlan_egap_set_param_handler: egap_handle = NULL  
 
2864,II,wlan_egap_set_param_handler:AP_PS_DBGID_EGAP_SET_PARAM paramid = %d , param_value = %d 
 
2865,,_wlan_egap_delete_vdev_instance unregistering wlan_egap_vdev_notif_handler non AP 
 
2866,I,registering wlan_egap_vdev_notif_handler Non AP nResult = %d 
 
2867,,_wlan_egap_wal_peer_event_handler :egap_handle = NULL  
 
2868,I,_wlan_egap_wal_peer_event_pre_send :sm_event.u.pre_send.frame_control = %d  
 
2869,,_wlan_egap_wal_peer_event_pre_send null egap_handle  
2870,,_wlan_egap_wal_peer_event_pre_send null pdev  
2871,,_wlan_egap_wal_peer_event_pre_send null wlan_vdev  
2872,,_wlan_egap_wal_peer_event_pre_send null peer  
2873,II,_wlan_egap_wal_pdev_event_handler sm_get_curstate(&(egap_handle->sm)) = %d event->event_type  = 0x%x  
 
2874,,_wlan_egap_wal_pdev_event_handler peer NULL 
2875,,_wlan_egap_wal_pdev_event_handler egap handle NULL 
2876,I,Not handled event in _wlan_egap_vdev_notif_handler notif->type = %d 
 
2877,,_wlan_egap_vdev_notif_handler peer == NULL 
 
2877,,_wlan_egap_vdev_notif_handler peer == NULL 
 
2878,,_wlan_egap_vdev_notif_handler : egap handle NULL  
 
2879,I,_wlan_egap_vdev_notif_handler notif->type = %d 
 
2880,IIII,AP_PS_DBGID_EGAP_NOTIF_STA_SLEEPING vdev->id = %d egap_handle->flags = %d ap_handle->num_clients = %d num_sleeping_sta = %d 
2881,,AP_PS_DBGID_EGAP_NOTIF_STA_SLEEPING parameters are null !! 
2882,II,wlan_egap_sendcomplete_event_handler frame_control type = %d frame subtype = %d  
 
2883,I,_wlan_egap_thread_comm_msg_handler error in unregistering pdev event : Result = %d WLAN_EGAP_REG_EV_HANDLER_RX_PHYERR  
2884,,WLAN_EGAP_THREAD_COMM_CMD_EVENT_PHYERR 
2885,,_wlan_egap_thread_comm_msg_handler :WLAN_EGAP_THREAD_COMM_CMD_EVENT_STA_POWERSAVE null peer  
2886,I,_wlan_egap_thread_comm_msg_handler cmd= %d 
2888,III,wlan_ps_buf_peer_create_instance() vdev_id = %d peer = %p slp_sta_handle =  %p 
2887,II,wlan_ps_buf_peer_delete_instance() vdev_id = %d peer = %d 
2889,II,STA_SMPS_DTIM_POWER_STATE_CHANGE : current_power_state = %d new_power_state = %d 
2890,II,SMPS action frame attempt mask %d smps_power_control %d 
2891,I,SMPS Action TX frame not sent, attemps:%d 
2892,IIII,STA_SMPS_VHT_OP_MODE_NOTIF_PEER_COMPLETE : vdevid = %d peerid = %d completion_status = %d peer_smps_frames_sent_mask = %d 
2893,I,STA_SMPS_VC_CTS2SELF_TX_COMPL : WLAN_SM_PWR_CTRL_STATIC vc_handle->last_frame_sm_pwr_ctrl %d 
2894,I,STA_SMPS_VC_CTS2SELF_TX_COMPL : WLAN_SM_PWR_CTRL_DYNAMIC vc_handle->last_frame_sm_pwr_ctrl %d 
2895,I,STA_SMPS_VC_CTS2SELF_TX_COMPL : WLAN_SM_PWR_CTRL_DISABLED vc_handle->last_frame_sm_pwr_ctrl %d 
2896,II,SMPS get Operation mode notification IE length %d %p 
2897,I,SMPS Build Operation mode notification IE: enable = %d 
2898,I,wlan_smps_prebmiss_delayed_handler: error %d 
2899,I,wlan_smps_prebmiss_delayed_handler: Enable RSSI monitoring for vdev_id %d 
2900,I,SMPS_CFG_CHANGE_NOTIFY: Invalid VC handle %p 
2901,IIIII,SMPS_CFG_CHANGE_NOTIFY:  mhz: 0x%x, ret = %d, prev_vc_rx_chain_mode: %d, next_vc_rx_chain_mode: %d, chain_mask_change_stage: %d 
2902,III,SMPS_CFG_CHANGE_NOTIFY: ONLY CFG PARAM CHANGE mhz: 0x%x, ret = %d, Notification mask = 0x%x 
2903,,SMPS_CFG_CHANGE_NOTIFY: rejected due to duplicate request 
2904,I,invalid smps cfg notification value new_cfg.channel_width = %d 
2905,II,wlan_smps_vc_cfg_notify queued cb = 0x%x, ret = %d 
2906,,wlan_smps_rejecting_queuing, something is already queued 
 
2907,III,wlan_smps_vc_cfg_notify vc_handle->cfg_change_stage=%d, new_cfg.update_cf=%d, new_cfg.vdev_map = %d 
2908,I,SMPS not supported on current channel 0x%x 
2909,III,wlan_smps_vc_cfg_notify : usr callback %d new_rx_chainmask = 0x%x new_channel_width = %d  
 
2910,I,vdev level notification is requested  = 0x%x 
2911,I,invalid smps cfg notification value channel_width = %d 
2912,IIII,invalid smps cfg notification ul_disablemu = %d, channel_width = %d rx_chainmask = 0x%x, tx_chainmask = 0x%x 
2913,IIIII,wlan_smps_chainmask_change_handle_done: status:%d, stage:%d->0,smps_cfg_notify_compl_args.ctxt=%d cur_chain_h16/next_chain=0x%x,smstate:%d 
2914,III,wlan_smps_cfg_notify_done: status:%d, stage:%d->0 smps_cfg_notify_compl_args.ctxt=%d  
2910,I,vdev level notification is requested  = 0x%x 
2915,,wlan_smps_cfg_change_timeout 
 
2916,I,wlan_smps_enable_static_smps:no need extra config for single chain mode 
2917,,wlan_smps_vc_cfg_notify queued cfg 
 
2918,I,STA_SMPS_DELETE_VIRTUAL_CHAN_INSTANCE : vc_handle = %d 
2919,I,STA_SMPS_CREATE_VIRTUAL_CHAN_INSTANCE : vc_handle = %d 
2920,II,STA_SMPS_DELETE_NON_STA_INSTANCE : vdevid = %d smps_handle = %d  
2921,II,STA_SMPS_CREATE_NON_STA_INSTANCE vdevid = %d smps_handle = %d 
2891,I,SMPS Action TX frame not sent, attemps:%d 
2922,,SMPS_AP Action frame could not send BW OMN notification connection is not VHT 
2923,III,STA_SMPS_SEND_VHT_OPMODE_NOTIF_FRAME_TO_PEER vdevid = %d peerid = %d ret_value = %d 
2924,I,STA_SMPS_DELETE_STA_INSTANCE : sta_handle = %d 
2925,I,STA_SMPS_CREATE_STA_INSTANCE : sta_handle = %d 
2926,I,wlan_smps_swbmiss_event_handler error %d 
2927,II,SMPS_BMISS event %d for vdev id %d 
2928,II,DTIM_UPDATE_CHAIN_ON_AWAKE: update chain in single chain, hwchain=%d, new=%d 
2929,III,STA_SMPS_DTIM_CHMASK_UPDATE_AWAKE : tx_chainmask = %d rx_chainmask = %d orig_rx_chainmask = %d 
2930,I,wlan_smps_pdev_update_dtim_chmask_on_sleep RSSI_INDICATION = %d 
2931,I,wlan_smps_virtual_chan_update_dtim_chmask WAL_PM_MAC_PARAM_RSSI_INDICATION = %d 
2932,II,SMPS_STA Action frame send power_control: %d ret_value:%d 
2933,,wlan_smps_sta_send_action_frame IEEE80211_NODE_HE 
2934,,SMPS_STA Action frame could not send BW OMN/OMI notification wrong tx NSS 
2935,,SMPS_STA Action frame could not send BW OMN/OMI notification wrong rx NSS 
2936,,SMPS_STA Action frame could not send BW OMN/OMI notification connection is not VHT 
2917,,wlan_smps_vc_cfg_notify queued cfg 
 
2937,I,STA_SMPS_VC_ACTION_FRAME_TX_COMPL : action_valid = %d 
 
2938,,STA_SMPS_VC_ACTION_FRAME_TX_COMPL : fallback on legacy SMPS configuration 
 
2939,,STA_SMPS_VC_ACTION_FRAME_TX_COMPL : incorrect state readjustment 
 
2940,II,STA_SMPS_VC_ACTION_FRAME_TX_COMPL Additional params: prev_forced_mode = %d channel mhz = 0x%x 
2941,IIIII,STA_SMPS_VC_ACTION_FRAME_TX_COMPL_OLD_DBG : power control = %d vc_handle->last_frame_sm_pwr_ctrl = %d completion status = %d current_state = %d vc_handle->cfg_change_stage = %d  
2942,II,wlan_smps_sta_update_rssi_values: invalid state %d %d 
2943,I,STA_SMPS_RSSI_THRESHOLD_CROSSED : rssi_lower_threshold = %d 
2944,I,STA_SMPS_RSSI_THRESHOLD_CROSSED : rssi_upper_threshold = %d 
2945,I,SMPS_VC_RSSI_SAMPLE_TIMEOUT: VC delete in progress = %d 
2946,I,SMPS_VC_RSSI_SAMPLE_TIMEOUT: No VC 
 
2947,,wlan_smps_virtual_chan_update : smps action frame sent  
2948,,wlan_smps_virtual_chan_update : smps restarted  
2949,IIIIII,wlan_smps_virtual_chan_update : vc_handle = %d, vc_handle->enabled = %d,vc_handle->cfg_notification_mode = %d, vc_handle->fw_forced_mode =%d , vc_handle->host_forced_mode = %d, smps_cur_state = %d   
2950,II,STA_SMPS_VIRTUAL_CHAN_SMPS_STOP : vc_handle = %d, vc_handle->enabled = %d  
2951,II,SMPSVC CHNL START : STA_SMPS_INVALID_SM_EVENT event = %d dynamicSMPSSupported = %d 
2952,II, STA_SMPS_VIRTUAL_CHAN_SMPS_START : vc_handle = %d, vc_handle->enabled = %d 
2953,II,SMPS_VC_SET_FW_FORCED_MODE : STA_SMPS_INVALID_SM_EVENT event = %d dynamicSMPSSupported = %d 
2954,I,STA_SMPS_FW_FORCED_MODE : event = %d  
2955,II,STA_SMPS_INVALID_SM_EVENT event = %d dynamicSMPSSupported = %d 
2956,I,STA_SMPS_HOST_FORCED_MODE : event = %d 
2957,II,SMPS_STATE_STATIC_EVENT: chain: %d, dropped ev:%d 
2972,IIII,wlan_smps_vc_cfg_notify,chainmask = %d channel_width = %d,timeout:%d, return :%d
 
2971,I,wlan_smps_vdev_set_fw_forced_mode,force_mode:%d
 
2970,IIII,END wlan_smps_unit_test_api_omi_omn_change_notify,chainmask = %d channel_width = %d,timeout:%d, return :%d
 
2969,II,END wlan_smps_unit_test_api_omi_omn_change_notify,ul_disablemu = %d txnss = %d 
 
2968,I,wlan_smps_unit_test_chainmask_change_notify_compl_cb smps status:%d
 
2967,I,wlan_smps_unit_test_chainmask_change_notify_queud_cb smps status:%d
 
2966,I,wlan_smps_unit_test_dtim1chain_test, num_args not enough 7 <low> <high> :%d
 
2965,IIIIIII,wlan_smps_unit_test_dtim1chain_test, chainmode=%d,currssi=%d,dtimchain=%d, low=%d, high=%d, newlow=%d, newhigh=%d 
2964,I,wlan_smps_unit_test_dtim1chain_test, num_args:%d
 
2963,IIIII,wlan_smps_unit_test_get_information, chainmode=%d,currssi=%d,dtimchain=%d, low=%d, high=%d 
2962,IIIII,wlan_smps_unit_test_get_information, enable=%d,sm=%d, host_forced_mode=%d, fw_forced_mode=%d, vc_inactive=%d 
2961,I,wlan_smps_unit_test_get_information,vdev_id=%d
 
2960,II,wlan_smps_unit_test_get_mac_reg, reg start:0x%08x, reg_count:0x%x 
2959,II,0x%08x:0x%08x 
2958,III,wlan_smps_unit_test_set_mac_reg, reg:0x%08x, new value:0x%08x, old value:0x%08x 
2973,I,WLAN_OPMODE_VDEV_FREE: vdev_id=%d 
2974,I,WLAN_OPMODE_VDEV_INIT: vdev_id=%d [!A_OK returned] 
2975,I,WLAN_OPMODE_VDEV_INIT: vdev_id=%d 
2976,II,WLAN_OPMODE_VDEV_EVT: vdev_id=%d, event=%d 
2977,II,WLAN_OPMODE_WAL_PDEV_EVT: pmac_id=%d, event=0x%x 
2978,IIII,WLAN_OPMODE_UPDATE_PMAC_LATENCY: mac_id=%d, final_latency=%d, power_state=%d, is_pmac_idle=%d 
2979,II,WLAN_OPMODE_SET_PMAC_LATENCY: mac_id=%d, opmode_latency=%d [!WAL_EOK returned] 
2980,II,WLAN_OPMODE_SET_PMAC_LATENCY: mac_id=%d, opmode_latency=%d 
2988,,EGAP UNIT TEST CONFIGURE EGAP AP NO AP VDEV !!
 
3002,II,EGAP UNIT TEST CONFIGURE EGAP AP vdev->ic_opmode = %d,vdev_id = %d 
 
3001,II,EGAP UNIT TEST ERROR: This is not in AP configuration vdev->ic_opmode = %d,vdev_id=%d 
 
3000,II,EGAP UNIT TEST ERROR: Too few arguments to configure EGAP vdev->ic_opmode = %d,vdev_id=%d 
 
2999,I,current config flags : egap_handle->flags = %d 
 
2998,IIII,UNIT TEST EGAP Current config info: egap is enabled=%d, phy error detection enabled =%d, power save enabled by inactivity =%d powersave by station ps state enabled =%d 
2997,IIII,UNIT TEST EGAP Current timer config info: egap is inactivity_time_us=%d, wait_time_us =%d, chm_req_grant_time_us =%d egap current state = %d 
2996,I,new config flags : egap_handle->flags = %d 
 
2995,IIII,UNIT TEST EGAP New config info: egap is enabled=%d, phy error detection enabled =%d, power save enabled by inactivity =%d powersave by station ps state enabled =%d 
2994,IIII,UNIT TEST EGAP New timer config info: egap is inactivity_time_us=%d, wait_time_us =%d, chm_req_grant_time_us =%d egap current state = %d 
2988,,EGAP UNIT TEST CONFIGURE EGAP AP NO AP VDEV !!
 
3002,II,EGAP UNIT TEST CONFIGURE EGAP AP vdev->ic_opmode = %d,vdev_id = %d 
 
3001,II,EGAP UNIT TEST ERROR: This is not in AP configuration vdev->ic_opmode = %d,vdev_id=%d 
 
3000,II,EGAP UNIT TEST ERROR: Too few arguments to configure EGAP vdev->ic_opmode = %d,vdev_id=%d 
 
2999,I,current config flags : egap_handle->flags = %d 
 
2998,IIII,UNIT TEST EGAP Current config info: egap is enabled=%d, phy error detection enabled =%d, power save enabled by inactivity =%d powersave by station ps state enabled =%d 
2997,IIII,UNIT TEST EGAP Current timer config info: egap is inactivity_time_us=%d, wait_time_us =%d, chm_req_grant_time_us =%d egap current state = %d 
2996,I,new config flags : egap_handle->flags = %d 
 
2995,IIII,UNIT TEST EGAP New config info: egap is enabled=%d, phy error detection enabled =%d, power save enabled by inactivity =%d powersave by station ps state enabled =%d 
2994,IIII,UNIT TEST EGAP New timer config info: egap is inactivity_time_us=%d, wait_time_us =%d, chm_req_grant_time_us =%d egap current state = %d 
2993,II,wlan_unit_test_find_ap_vdev: found AP vdev : ic_opmode = %d,vdev_id=%d
 
2992,,wlan_unit_test_get_egap_information : NULL VDEV !!
 
2991,II,EGAP UNIT TEST ERROR: This is not in AP configuration vdev->ic_opmode = %d,vdev_id=%d
 
2982,I,config flags : egap_handle->flags = %d 
 
2990,IIII,UNIT TEST EGAP config info: egap is enabled=%d, phy error detection enabled =%d, power save enabled by inactivity =%d powersave by station ps state enabled =%d 
2989,IIII,UNIT TEST EGAP timer config info: egap is inactivity_time_us=%d, wait_time_us =%d, chm_req_grant_time_us =%d egap current state = %d 
2988,,EGAP UNIT TEST CONFIGURE EGAP AP NO AP VDEV !!
 
2987,II,wlan_unit_test_get_egap_information new ap vdev->ic_opmode = %d,vdev_id=%d
 
2986,I,wlan_unit_test_keep_chainmask args[2] = %d
 
2985,,wlan_unit_test_keep_chainmask : NULL VDEV !!
 
2984,,EGAP UNIT TEST KEEP CHM AP NO AP VDEV !!
 
2983,II,wlan_unit_test_keep_chainmask: This is not in AP configuration vdev->ic_opmode = %d,vdev_id=%d
 
2982,I,config flags : egap_handle->flags = %d 
 
2981,IIII,UNIT TEST EGAP keep chm new config info: egap is inactivity_time_us=%d, wait_time_us =%d, chm_req_grant_time_us =%d egap keep chm = %d 
3013,I,PPS set membership gid error: mode not support:%d 
3012,I,PPS set membership gid error: peer is not bss 
3011,I,PPS set membership gid error: vpps is null 
3010,I,PPS set membership userpos error: mode not support:%d 
3009,I,PPS set membership userpos error: vpps is null 
3008,I,PPS set membership userpos error: peer is not bss 
3007,I,set ebt resync timeout to %u msec
 
3006,IIIII,pps vdev calc paid: paid:%d, ic_mode:%d, is_tx:%d, associd:%d, mac[5]:0x%x 
3005,I,PPS register bcon event handler error: rc=%d 
3004,I,PPS wmi_set_vdev_pkt_pwr_save: no entry 
3003,II,PPS wmi_set_vdev_pkt_pwr_save: old:0x%x, new:0x%x 
3034,II,pps arbiter: host:0x%x, fw:0x%x 
3033,II,pps arbiter: macid:%d, aribiter:%d 
3032,III,pps arbiter delimiter eof: feature:0x%x, old:%d, new:%d 
3031,I,pps arbiter ebt: mac is awake, power:%d 
3030,I,pps arbiter ebt: more than one mac 
3029,I,pps arbiter ebt: quit ie detected 
3028,I,pps arbiter ebt: dfs channel detected 
3027,III,pps arbiter ebt: feature:0x%x, host:0x%x, fw:0x%x 
3026,IIIII,pps arbiter ebt result: features:0x%x, ebt sub:0x%x, macid:%d, old:%d, new:%d 
3025,III,pps arbiter delimi crc: feature:0x%x, old:%d, new:%d 
3024,I,pps arbiter gid: more vdev enabled mu-mimo 
3023,IIII,pps arbiter gid result: feature:0x%x, macid:%d, old:%d, new:%d 
3022,IIII,pps arbiter gid: host:0x%x, fw:0x%x, gid:%d,userpos:%d 
3021,III,pps arbiter macmismatch: feature:0x%x, old:%d, new:%d 
3020,III,pps arbiter zero nsts: feature:0x%x,old:%d, new:%d 
3019,III,pps arbiter paid: host:0x%x, fw:0x%x, paid:0x%x 
3018,IIIII,pps arbiter PAID result: feature:0x%x, macid:%d, old:%d, new:%d, paid index:%d 
3017,III,pps arbiter rssi: feature:0x%x, old:%d, new:%d 
3016,II,pps ebt cac timeout cur:%d,vpps value:%d 
3015,I,pps ebt cac timeout result:%d 
3014,III,PPS swbmiss evt:%d, macid:%d, arbiter:0x%x 
3035,IIIII,RMC_BLACKLIST_PEER  mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x bl_ts = 0x%x bl_last_bcn_rssi = %d bl_avg_bcn_rssi = %d 
3036,III,RMC_PEER_BCN_INFO  mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x bcn_rssi = %d 
3037,,RMC_NO_LDR 
3038,IIII,RMC_LDR_SEL  mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x bcn_rssi = %d selected = %d 
3039,IIII,RMC_LDR_INF_SENT  peer/status = 0x%x mac_addr47to32 = 0x%x mac_addr31to0 = 0x%x cancellation = %d 
3040,I,RMC_LDR_INF_SENT  peer = 0x%x 
3041,I,RMC_DELETE_INSTANCE  rmc_hndl = 0x%x 
3042,I,RMC_CREATE_INSTANCE  pdev_hndl/vdev_ctxt_pool = 0x%x 
3043,II,RMC_CREATE_INSTANCE  pdev_hndl/vdev_ctxt_pool = 0x%x vdev = 0x%x 
3044,,RMC_CREATE_INSTANCE: wlan_vdev_register_notif_handle failed 
3045,I,RMC_WAL_EVENT_HANDLER  event_type = 0x%x 
3046,I,RMC_SET_ACTION_PERIOD  period_ms = %d 
3047,I,RMC_SET_MODE  enable_rmc = %d 
3048,II,RMC_PEER_ADD  peer = 0x%x idx = 0x%x 
3049,,RMC_CREATE_INSTANCE 
3050,,RMC_ACTION_FRAME_RX 5: 
3051,I,RMC_ACTION_FRAME_RX cancel = %d 
3052,,RMC_ACTION_FRAME_RX 4: 
3053,I,RMC_ACTION_FRAME_RX 2: subtype = %d 
3054,I,RMC_ACTION_FRAME_RX 1: len = %d 
3055,,RMC_ACTION_FRAME_RX (wal_peer is NULL) 
3056,IIIII,RMC_WHITELIST_PEER  mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x diff_us = %d curr_rssi = %d bl_rssi = %d 
3057,IIII,wlan_rmc_event_vdev_notif_handler: type = 0x%x peer = 0x%x addr0: 0x%x addr1: 0x%x  
3057,IIII,wlan_rmc_event_vdev_notif_handler: type = 0x%x peer = 0x%x addr0: 0x%x addr1: 0x%x  
3058,IIII,wlan_rtt_terminate_all_ftm_resp_context() idx: %d resp_ctxt = %p vdev = %p ftm_state = %d 
3059,,wlan_rtt_cancel_all_rtt_operation 
3060,I,wlan_rtt_start_burst_periodic_timer: timeout_ms:%dms 
3061,I,RTT_CALL_FLOW: WLAN_RTT_START_BURST_PERIODIC_TIMER ts = %u 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3064,I,RTT_CALL_FLOW: WLAN_RTT_SCHEDULE ts = %u 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3065,II,Received FTMR resp_tsf_h = 0x%x resp_tsf_l = 0x%x 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3066,,RTT_ERROR_REPORT :TM_SEQUENCE_RESTART 
3067,,RTT_ERROR_REPORT :TM_CFR_CAPTURE_ERROR 
3068,,RTT_ERROR_REPORT :TM_TOKEN_MISMATCH 
3069,I,RTT_CALL_FLOW: WLAN_RTT_START_PTSF_TIMER ts = %u 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3070,IIIII,RTT_FTM_PARAM_INFO  arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x arg5 = 0x%x 
3071,II,RTT TM FTM curr_tsf_delta = 0x%x new_tsf_delta = 0x%x 
3072,IIII,RTT TM FTM tsf_sync_info = 0x%x ftm_req_start_time = 0x%x ftm_req_complete_time = 0x%x current_time = 0x%x 
3073,IIII,state = %d tsf_sync_info = 0x%x resp_tsf = 0x%x Diff: %d 
3074,I,RTT_CALL_FLOW: WLAN_RTT_RECV_FTM1 ts = %u 
3075,I,RTT_TWOSIDED_RESP_CNT  number = %d 
3075,I,RTT_TWOSIDED_RESP_CNT  number = %d 
3076,,RTT_TWOSIDED_RESP_FINISH 
3077,,RTT_ERROR_REPORT :RTT_GET_TM_NOTWAIT_TM 
3077,,RTT_ERROR_REPORT :RTT_GET_TM_NOTWAIT_TM 
3078,I,RTT_CALL_FLOW: WLAN_RTT_TM_RX_HDL ts = %u 
3079,III,wlan_rtt_terminate_resp_context() state: %d busrt_exp: %d burst_count: %d 
3080,I,RTT_CALL_FLOW: WLAN_RTT_TMR_END_RX_HDL ts = %u 
3081,,RTT_ERROR_REPORT :RTT_GET_INVALID_TMR_STOP 
3081,,RTT_ERROR_REPORT :RTT_GET_INVALID_TMR_STOP 
3082,I,RTT_CALL_FLOW: WLAN_RTT_TMR_START_RX_HDL ts = %u 
3083,I,RTT_CALL_FLOW: WLAN_RTT_TMR_BUSY_REPLY ts = %u 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3075,I,RTT_TWOSIDED_RESP_CNT  number = %d 
3084,I,RTT_CALL_FLOW: WLAN_RTT_SEND_FTM1_COMPLETE ts = %u 
3085,I,RTT_CALL_FLOW: WLAN_RTT_START_FTM_DELTA_TIMER ts = %u 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3086,I,RTT_CALL_FLOW: WLAN_RTT_FTM1_EXCEED_MAX_RETRY ts = %u 
3087,I,RTT_CALL_FLOW: WLAN_RTT_SEND_FTM1_RETRY ts = %u 
3088,,RTT_ERROR_REPORT :RTT_WAL_FRAME_TX_DROP 
3089,,RTT_ERROR_REPORT :RTT_WAL_FRAME_TX_FAIL_XRETRY 
3090,,RTT_ERROR_REPORT :RTT_WAL_FRAME_TX_OK 
3091,I,RTT_CALL_FLOW: WLAN_RTT_TM_ACK_HDL ts = %u 
3092,,RTT_ERROR_REPORT :RTT_FRAME_TX_FAIL 
3093,III,wlan_rtt_send_tm_frame: abf: %p channel: %x pmac = %p 
3094,,RTT_ERROR_REPORT :ALLOCATE_FRAME_BUFFER_ERROR 
3095,I,RTT_CALL_FLOW: WLAN_RTT_SEND_FTM1 ts = %u 
3096,IIIII,RTT_SEND_TM_FRAME resp_ctxt: %p tkn = %d follow_tkn = %d tx_bw = %d resp_ctxt ftm state = %d 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3097,I,RTT_CALL_FLOW: WLAN_RTT_SEND_TM_FRAME ts = %u 
3098,I,RTT_CALL_FLOW: WLAN_RTT_RUN_NEXT_INIT ts = %u 
3099,I,Computed distance: %d 
3100,III,wlan_rtt_burst_instance_done: ftm1_done:%d num_meas:%d ftm_per_burst:%d  
3101,IIIII,wlan_rtt_burst_instance_done: num_burst_done:%d total_bursts:%d curr_state:%d burst_duration:%d, index:%d 
3102,I,RTT_CALL_FLOW: WLAN_RTT_INIT_BURST_INSTANCE_DONE ts = %u 
3103,III,Downgraded the BW: New bw: %d chnl_format: %u rate_info: %u 
3104,III,Channel Granted(Initiator): RTT 160MHz requested freq: 0x%x Grant came on freq: 0x%x phymode: %d 
3105,III,vdev mac id(%d) not same as pmac mac id(%d): change PM lock & set mac address: %d 
3106,IIII,Channel Granted(Responder): Responder operating freq = 0x%x pmac = %p Granted on freq: 0x%x phymode: %d 
3107,,Recieved a WMI event to sent to an invalid client 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3108,I,RTT_CALL_FLOW: WLAN_RTT_FTM1_RESP_TIMER_FIRED ts = %u 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3109,I,RTT_CALL_FLOW: WLAN_RTT_BURST_RESP_TIMER_FIRED ts = %u 
3110,I,RTT_CALL_FLOW: WLAN_RTT_DELTA_TIMER_FIRED ts = %u 
3111,I,RTT_CALL_FLOW: WLAN_RTT_DFS_TIMEOUT_HANDLER ts = %u 
3112,III,wlan_rtt_ftm_init_burst_periodic_timeout: ERR: Some other request is in progress; skip current burst %d for dest_mac:%x%x 
3113,IIIII,wlan_rtt_ftm_init_burst_periodic_timeout: Previous burst %d is not successful for dest_mac:%x%x curr_state:%d probe_rsp_pending:%d  
3114,IIIII,wlan_rtt_ftm_init_burst_periodic_timeout: Something is wrong with this request (buest %d) for dest_mac:%x%x curr_state:%d probe_rsp_pending:%d  
3115,III,wlan_rtt_ftm_init_burst_periodic_timeout: Starting burst %d for dest_mac:%x%x 
3116,IIII,wlan_rtt_ftm_init_burst_periodic_timeout: ERR: Burst periodic timeout when dest_mac:%x%x is not multiburst request(%d) or repetitive single shot request(%d)  
3117,IIII,wlan_rtt_ftm_init_burst_periodic_timeout: dest_mac:%x%x current_burst:%d total_bursts:%d 
3118,II,wlan_rtt_ftm_init_burst_periodic_timeout: single shot repetitive request for dest_mac:%x%x  
3119,IIII,wlan_rtt_ftm_init_burst_periodic_timeout: multiburst request for dest_mac:%x%x current_burst:%d total_bursts:%d  
3120,I,RTT_CALL_FLOW: WLAN_RTT_BURST_PERIODIC_INIT_TIMER_FIRED ts = %u 
3121,I,RTT_CALL_FLOW: WLAN_RTT_BURST_INIT_TIMER_FIRED ts = %u 
3122,II,Init PTSF fired resp_tsf_h = 0x%x resp_tsf_l = 0x%x 
3123,I,RTT_CALL_FLOW: WLAN_RTT_PTSF_TIMER_FIRED ts = %u 
3124,I,RTT_CALL_FLOW: WLAN_RTT_FTM1_INIT_TIMER_FIRED ts = %u 
3125,I,RTT_CALL_FLOW: WLAN_RTT_START_TMR_RETRY_TIMER ts = %u 
3126,,wlan_rtt_init_scheduler => All requests done nothing to schedule 
3127,IIII,wlan_rtt_init_scheduler => index:%d curr_index:%d schedule_timeout:%d next_mb_slot_index: %d 
3128,I,wlan_rtt_init_scheduler: Skipping initiator with index %d as it may creep into next multiburst start time 
3129,I,wlan_rtt_init_scheduler => next_mb_slot_index:%d  
3130,II,wlan_rtt_init_scheduler => diff1:%d diff2:%d 
3131,II,wlan_rtt_init_scheduler => curr_init:0x%x init_ctxt_usage_flags:0x%x 
3132,I,RTT_CALL_FLOW: WLAN_RTT_INIT_SCHEDULER_TIMEOUT_HANDLER ts = %u 
3133,I,RTT_CALL_FLOW: WLAN_RTT_TMR_RETRY_TIMER_FIRED ts = %u 
3134,I,RTT_CALL_FLOW: WLAN_RTT_SPS_TIMEOUT_HANDLER ts = %u 
3135,I,RTT_CALL_FLOW: WLAN_RTT_TIMEOUT_HANDLER ts = %u 
3136,I,RTT_CALL_FLOW: WLAN_RTT_FTM1_TIMER_STOP ts = %u 
3137,I,RTT_CALL_FLOW: WLAN_RTT_START_BURST_TIMER ts = %u 
3138,I,RTT_CALL_FLOW: WLAN_RTT_BURST_TIMER_STOP ts = %u 
3139,I,RTT_CALL_FLOW: WLAN_RTT_FTM_DELTA_TIMER_STOP ts = %u 
3137,I,RTT_CALL_FLOW: WLAN_RTT_START_BURST_TIMER ts = %u 
3140,I,RTT_CALL_FLOW: WLAN_RTT_START_FTM1_TIMER ts = %u 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3141,,RTT_ERROR_REPORT :0xff 
3142,,Event buffer allocation for wlan_rtt_cap_msg_req response failed 
3143,IIIIII,wlan_rtt_cap_msg_req_hdl: client_id: %d Req:%d Reqid:%d Major:%d Minor:%d Revision:%d 
3144,I,RTT_CALL_FLOW: WLAN_RTT_CAP_MSG_REQ_HDL ts = %u 
3145,II,wlan_wmi_oem_req: ERROR: TLV processing failed for sub_type:%d, req_id:%d 
3146,III,wlan_wmi_oem_req: INFO: OEM Req received with sub_type:%d, req_id:%d client: %d 
3147,II,_wlan_wmi_oem_req: Non TLV format msg received; tlv_head: %d 
3148,I,RTT_CALL_FLOW: WLAN_WMI_OEM_REQ ts = %u 
3149,,160 FTM channel format 
3150,,80p80 channel format 
3151,II, wlan_rtt_get_ftm_chnl_code bw:%d preamble:%d 
3152,IIII,wlan_rtt_meas_req_init: Unsupported vdev type %d for dest_mac %x%x with req_id %d 
3153,I,DFS channel quiet %d 
3154,IIIII,RTT_MEAS_REQ_BODY  control_inf = 0x%x meas_inf = 0x%x meas_params1 = 0x%x meas_params2 = 0x%x is_dest_qca: %d 
3155,IIIII,RTT_MEAS_REQ_BODY idx = %d dest_mac_0to31 = 0x%x dest_mac_32to47 = 0x%x sppof_bssid_0to31 = 0x%x spoof_bssid_32to47 = 0x%x 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3156,IIIIIIII,RTT_MEAS_REQ_HEAD ch_idx = %d, ch_mhz = %d, center_freq1 = %d ch_mode = %d sta_num:%d, max_reg_power: %d antenna_max: %d, max_tx_power: %d 
3157,IIII,RTT_MEAS_REQ_HEAD  req_id = %d num_chan = %d sps = %d client: %d 
3158,I,RTT_CALL_FLOW: WLAN_RTT_MEAS_REQ_INIT ts = %u 
3159,,Event buffer allocation for cancel measurement response failed 
3160,,wlan_rtt_tmr_handler() init_ctxt vdev is found to be NULL 
3161,I,RTT_CALL_FLOW: WLAN_RTT_TMR_HANDLER ts = %u 
3162,I,RTT_CALL_FLOW: WLAN_RTT_SET_VENDOR_IE_HT_VHT_ACK ts = %u 
3070,IIIII,RTT_FTM_PARAM_INFO  arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x arg5 = 0x%x 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3088,,RTT_ERROR_REPORT :RTT_WAL_FRAME_TX_DROP 
3089,,RTT_ERROR_REPORT :RTT_WAL_FRAME_TX_FAIL_XRETRY 
3163,,RTT_ERROR_REPORT :0xBABE 
3090,,RTT_ERROR_REPORT :RTT_WAL_FRAME_TX_OK 
3164,I,RTT_CALL_FLOW: WLAN_RTT_TMR_START_ACK_HDL ts = %u 
3165,,RTT_TIMER_STOP 
3166,II,wlan_rtt_send_tmr_frame: channel: %x pmac = %p 
3094,,RTT_ERROR_REPORT :ALLOCATE_FRAME_BUFFER_ERROR 
3167,II,Sending RTT Trigger frame resp_tsf_h = 0x%x resp_tsf_l = 0x%x 
3168,I,RTT_CALL_FLOW: WLAN_RTT_SEND_TMR_WITH_IE ts = %u 
3169,I,RTT_CALL_FLOW: WLAN_RTT_SEND_TMR_END ts = %u 
3170,I,RTT_CALL_FLOW: WLAN_RTT_SEND_TMR_START ts = %u 
3171,IIII,cancel_measurement_req(RTT_MEAS_CANCEL_ID: %d): cancel id: %d free_curr_init: %d, is_cancelled: %d 
3172,III,wlan_rtt_measurement_report: client_id: %d curr_init_ctxt:%p size: %d 
3173,I,RTT_CALL_FLOW: WLAN_RTT_MEASUREMENT_REPORT ts = %u 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3088,,RTT_ERROR_REPORT :RTT_WAL_FRAME_TX_DROP 
3089,,RTT_ERROR_REPORT :RTT_WAL_FRAME_TX_FAIL_XRETRY 
3163,,RTT_ERROR_REPORT :0xBABE 
3090,,RTT_ERROR_REPORT :RTT_WAL_FRAME_TX_OK 
3174,I,RTT_CALL_FLOW: WLAN_RTT_NULL_ACK_HDL ts = %u 
3092,,RTT_ERROR_REPORT :RTT_FRAME_TX_FAIL 
3175,II,wlan_rtt_send_null_frame: channel: %x pmac = %p 
3094,,RTT_ERROR_REPORT :ALLOCATE_FRAME_BUFFER_ERROR 
3176,I,RTT_CALL_FLOW: WLAN_RTT_SEND_NULL_FRAME ts = %u 
3177,I,RTT_CALL_FLOW: WLAN_RTT_INFORM_RANGING_STATUS_HDLR ts = %u 
3178,I,RTT_CALL_FLOW: WLAN_RTT_INFORM_RANGING_NEG_HDLR ts = %u 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3179,I,RTT_CALL_FLOW: WLAN_RTT_DELIVER_EVENT ts = %u 
3180,I,RTT_CALL_FLOW: WLAN_RTT_NULL_HANDLER ts = %u 
3181,III,Registered wlan_rtt_vdev_notify_handler() for init context : vdev = %p vdevid = %d status = 0x%x 
3182,,RTT request on a different vdev than the one set during channel change 
3183,IIIIIIII,wlan_rtt_init_handler: Starting initiator with mac_addr = %x%x  init_idx = %d init_ctxt_usage_flags = 0x%x pmac: %p mac_id: %d vdev: %p rate_info: 0x%x 
3184,I,RTT_CALL_FLOW: WLAN_RTT_INIT_HANDLER ts = %u 
3185,II,wlan_rtt_pm_arb_req(): mac_id: %d state: %d  
3186,,POST migrate event 
3187,,PRE migrate event 
3188,III,wlan_rtt_vdev_notify_handler() vdev = %p vdev_id = %d notification type = %d 
3189,I,RTT_CALL_FLOW: WLAN_RTT_TMR_RETRY_TIMER_STOP ts = %u 
3190,I,RTT_CALL_FLOW: WLAN_RTT_BURST_PERIODIC_TIMER_STOP ts = %u 
3191,I,RTT_CALL_FLOW: WLAN_RTT_PTSF_TIMER_STOP ts = %u 
3192,II,Unregistered wlan_rtt_vdev_notify_handler() for init context vdev = %p status = 0x%x 
3193,I,wlan_rtt_free_init_ctxt() usage flags = 0x%x 
3194,II,wlan_rtt_get_clear_stats ranging_dur: %x resp_dur: %x  
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3195,I,RTT_CALL_FLOW: WLAN_RTT_STA_RESPONDER_TIMER_FIRED ts = %u 
3196,I,RTT_CALL_FLOW: WLAN_RTT_SUCCESS_END_OF_FUNCTION ts = %u 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3196,I,RTT_CALL_FLOW: WLAN_RTT_SUCCESS_END_OF_FUNCTION ts = %u 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3197,I,RTT_CALL_FLOW: WLAN_RTT_CFG_RESPONDER_MODE_DISABLE ts = %u 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3198,I,RTT_CALL_FLOW: WLAN_RTT_CFG_RESPONDER_MODE_ENABLE ts = %u 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3196,I,RTT_CALL_FLOW: WLAN_RTT_SUCCESS_END_OF_FUNCTION ts = %u 
3199,I,RTT_CALL_FLOW: WLAN_RTT_GET_CHANNEL_INFO ts = %u 
3200,,RTT_ERROR_REPORT :0xFF 
3201,,Event buffer allocation for send_responder_cfg_info response failed 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3202,I,RTT_CALL_FLOW: WLAN_RTT_REGISTER_RANGING_NEG ts = %u 
3203,II,wlan_rtt_ranging_negotiation_status_notif_handler: StartTsf:%u curr_time%u 
3204,II,wlan_rtt_ranging_negotiation_status_notif_handlerr => burst_start_time_h:%u burst_start_time_l:%u 
3205,I,wlan_rtt_ranging_negotiation_status_notif_handler: Starting burst periodic timer with timeout:%u  
3206,I,RTT_CALL_FLOW: WLAN_RTT_RANGING_NEG_STATUS_NOTIF ts = %u 
3207,IIIII,WLAN_RTT_VOIP_NOTIFY voip_ctxt %p voip_state %d voip_ctxt.in_progress %d duration_ms %d duration_us %d 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3208,IIIIII,wlan_rtt_local_send()status: %d pmac_mac_id: %d vdev_mac_id: %d flags: 0x%x selfgen_chm: 0x%x abf: %p 
3209,,Selfgen chainmask granted is zero. return error 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3210,I,RTT_CALL_FLOW: WLAN_RTT_LOCAL_SEND ts = %u 
3211,IIII,RTT_CHANNEL_SWITCH_REQ  module_id %d duration = %d channel = %d priority = %d 
3212,II,VOIP in progress voip_ctxt:%p Limit duration to duration_us:%d 
3213,I,RTT_CALL_FLOW: WLAN_RTT_CHAN_SWITCH ts = %u 
3214,IIII,RTT_CHANNEL_SWITCH_GRANT  ev_id = %d p_chnl_switch_ctxt = 0x%x p_owner = 0x%x p_rtt_ctxt = 0x%x 
3215,I,RTT_CALL_FLOW: WLAN_RTT_CHAN_SWITCH_HDL ts = %u 
3216,III,wlan_rtt_resp_chan_switch_hdl()  ev_id = %d ftm_state:%d is_ftmr_pending:%d 
3217,IIIIIII,wlan_rtt_send_measurement_report_hdl: client_id: %d curr_init_ctxt: %p token_id:%d frag_idx:%d more_frag: %d buf:%p buf_len:%d 
3218,I,RTT_CALL_FLOW: WLAN_RTT_MEASUEMENT_REPORT2 ts = %u 
3219,,Event buffer allocation for send_rtt_error_report failed 
3220,IIII,RTT_ERROR_WMI_EVENT: ERROR: client_id: %d req_id:%d reason:%d init_ctxt: %p 
3221,I,wlan_pdev_register_limit_offchan_notif_handler failed: %d 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3222,I,rtt responder role is disabled in vdev mode: %d 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3223,I,RTT_CALL_FLOW: WLAN_RTT_RESP_INIT ts = %u 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3080,I,RTT_CALL_FLOW: WLAN_RTT_TMR_END_RX_HDL ts = %u 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3070,IIIII,RTT_FTM_PARAM_INFO  arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x arg5 = 0x%x 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3063,IIII,RTT_MAN_DEBUG arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x 
3224,III,Registered wlan_rtt_vdev_notify_handler() for resp context vdev: %p pmac: %p status: 0x%x 
3225,I,RTT_CALL_FLOW: WLAN_RTT_RECV_TMR_WITH_IE ts = %u 
3226,,RTT_ERROR_REPORT :RTT_RESP_BUSY 
3227,,RTT_ERROR_REPORT :RTT_RESP_REQ_ACCEPT 
3228,,RTT_ERROR_REPORT :RTT_RESP_CTXT_EXIST 
3229,I,wlan_oem_rtt_measreq_hdl: asm_req  status %d would be served from call back due to NACK 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3230,II,wlan_oem_rtt_measreq_hdl(): rtt_ctx_id: %d wdcvs_boost_enabled: %d 
3231,I,wlan_oem_rtt_measreq_hdl: Request with id %d won't be served because of an error 
3232,I,wlan_oem_rtt_measreq_hdl: Duplicate request id: %d; Dropping request 
3233,III,wlan_oem_rtt_measreq_hdl: client %d running. cannot new req from client: %d. So Dropping req_id: %d 
3234,I,RTT_CALL_FLOW: WLAN_OEM_RTT_MEASREQ_HDL ts = %u 
3235,I,RTT_CANCEL_MEASUREMENT_REQ: Req_id: %d 
3236,III,CHANNEL DUMP LOGGING: type %d enable %d g_rtt_min_delta: %d 
3237,I,RESPONDER IFFT enabled?  
3238,IIIIII,RTT_UNIT_TEST_DEST_MAC [0]= 0x%x [1]= 0x%x [2]= 0x%x [3]= 0x%x [4]= 0x%x [5]= 0x%x 
3239,IIIIII,Channel mhz:0x%x cfreq1:0x%x cfreq2:0x%x info:0x%x reginf1:0x%x reginf2:0x%x 
3240,IIIIII,RTT_UNIT_TEST_CMD numFrms= %d ChnlFrmt= %d frmType= %d reportType= %d burstDr= %d asap_mode= %d 
3241,,Channel not configured 
3242,,MAC address not configured 
3243,III,RTT_UNIT_TEST_CMD 1  num_args = %d arg0 = %d vdev_id = %d 
3244,III,RTT_CHANNEL_DFS_SWITCH_HDL  ev = %d sw_ctxt->arg = %p sw_ctxt->cb_fn %p 
3245,II,wlan_rtt_dfs_chan_init_handler rtt_ctxt->chnl_switch_ctxt.cb_fn %d rtt_ctxt->chnl_switch_ctxt.owner%d  
3246,,wlan_rtt_dfs_chnl_switch_cb_fn(): init_ctxt->pdev_rtt_ctxt is NULL. Return 
3247,I,RTT_CALL_FLOW: WLAN_RTT_BEACON_RX ts = %u 
3248,I,RTT_CALL_FLOW: WLAN_RTT_DFS_EXIT ts = %u 
3249,II,Unregistered wlan_rtt_vdev_notify_handler() for resp context vdev = %p status = 0x%x 
3250,I,RTT_CALL_FLOW: WLAN_RTT_RESP_EXIT_CLEAN ts = %u 
3251,I,wlan_rtt_exit_clean() rtt_chm_state: %d is not expected 
3252,IIIII,wlan_rtt_exit_clean(): rtt_ctx_id: %d wdcvs_boost_enabled: %d set_vdev_mac_addr: %d rtt_vdev: %p pmac: %p 
3253,I,RTT_CALL_FLOW: WLAN_RTT_EXIT_CLEAN ts = %u 
3254,,wlan_rtt_terminate_repetitive_ss_request: Freeing init_ctxt 
3255,,wlan_rtt_terminate_repetitive_ss_request: CUrrently running this init_ctxt; Marking it as non repetitive 
3256,II,wlan_rtt_terminate_repetitive_ss_request: dest_mac :%x %x 
3257,II,wlan_rtt_terminate_repetitive_ss_request: red_id:%d init_ctxt_usage_flags:0x%x 
3258,I,RTT_CALL_FLOW: WLAN_RTT_SCHED_RELEASE ts = %u 
3259,I,RTT_CALL_FLOW: WLAN_RTT_SCHED_DEL ts = %u 
3260,I,RTT_CALL_FLOW: WLAN_RTT_SCHED_REQ ts = %u 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3064,I,RTT_CALL_FLOW: WLAN_RTT_SCHEDULE ts = %u 
3062,IIII,RTT_REPORT  arg1 = 0x%x arg2 = 0x%x arg3 = x%x arg4 = 0x%x 
3261,I,RTT unknown rtt_chm_state: %d 
3262,,RTT CHAIN MASK GRANTED 
3263,III,wlan_rtt_chainmask_notif_handler(): ev type: %d rtt_chm_state: %d resp_id: %d 
3264,IIII,wlan_rtt_chainmask_change_req() chm_req.t2_req.req_id: %d num_selfgen_chains: %d rtt_chm_state: %d ret: 0x%x 
3265,IIIIII,wlan_rtt_get_nss_tx_chain_mask_config: mac_id: %d band: %d BW: %d nss1_tx_chm: 0x%x selfgen: 0x%x is_2txnsschains_granted: %d 
3291,IIII,RTTTLV_CHECK_AND_PAD_TLVS  is_req = %d buf_ptr = 0x%x buf_len = %d sub_type = %d 
3290,I,RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Maximum inner loops reached for sub_type:%d 
3289,I,RTTTLV_CHECK_AND_PAD_TLVS: WARN: ERROR Need to handle this tag ID %d for variable length
 
3288,II,RTTTLV_CHECK_AND_PAD_TLVS: WARN: TLV truncated. tlv_size_diff=%d, curr_tlv_len=%d
 
3287,I,RTTTLV_CHECK_AND_PAD_TLVS: WARN: TLV needs padding. tlv_size_diff=-%d
 
3286,II,RTTTLV_CHECK_AND_PAD_TLVS: Some loop(cnt = %d) didn't ended properly for sub_type:%d 
3285,I,RTTTLV_CHECK_AND_PAD_TLVS: Successfully processed TLVs for sub_type:%d
 
3284,I,RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Couldn't get expected number of TLVs for sub_type=%d
 
3283,IIIIII,RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Invalid TLV length for sub_type=%d Tag_order=%d buf_idx=%d Tag:%d Len:%d TotalLen:%d
 
3282,II,RTTTLV_CHECK_AND_PAD_TLVS: ERROR: No TLV attributes found for sub_type=%d Tag_order=%d
 
3281,III,RTTTLV_CHECK_AND_PAD_TLVS: VERBOSE: [tlv %d]: tag=%d, len=%d
 
3280,III,RTTTLV_CHECK_AND_PAD_TLVS: VERBOSE: Tag ID expecting is Loop end(%d) for loop started at index %d but received tag %d 
3279,II,RTTTLV_CHECK_AND_PAD_TLVS: VERBOSE: Get the first TLV Tag ID (tlv_index:%d) for last entered loop start (cnt=%d) 
3278,III,RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Can't get  the first TLV Tag ID (tlv_index:%d) for last entered loop start (cnt=%d) for sub_type=%d
 
3277,IIII,RTTTLV_CHECK_AND_PAD_TLVS: WARN: First TLV Tag ID (%d) for last entered loop start (index=%d) doesn't match; skipping this tlv with tag:%d for sub_type=%d 
3276,IIIII,RTTTLV_CHECK_AND_PAD_TLVS: VERBOSE: First TLV Tag ID (tlv_index:%d) for last entered loop start (total_active_loops=%d) matched (looping loop_cnt:%d) with tag:%d for sub_type=%d 
3275,III,RTTTLV_CHECK_AND_PAD_TLVS: ERROR: TLV has wrong tag in order for sub_type=%d. Given=%d, Expected=%d.
 
3275,III,RTTTLV_CHECK_AND_PAD_TLVS: ERROR: TLV has wrong tag in order for sub_type=%d. Given=%d, Expected=%d.
 
3274,II,RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Wrong TLV length %d for loop end for sub_type:%d 
3273,I,RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Loop start and End mismatch for sub_type:%d 
3272,IIII,RTTTLV_CHECK_AND_PAD_TLVS: VERBOSE: Processing of loop %d done for sub_type:%d; left out loop instances:%d TLVs per loop:%d 
3271,III,RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Exceeded given max loop count %d, for sub_type:%d tlv_index:%d 
3270,II,RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Wrong TLV length %d for loop start for sub_type:%d 
3269,IIII,%s: WMI TLV attribute definitions for %s:0x%x found; num_of_tlvs:%d
 
3268,III,%s: ERROR: Didn't found WMI TLV attribute definitions for %s:0x%x
 
3267,IIIII,%s: ERROR: TLV order %d greater than num_of_tlvs:%d for %s:0x%x
 
3266,IIIII,%s: WMI TLV attributes for %s:0x%x tlv[%d]:0x%x
 
3314,IIIII,EXTSCAN_ADD_ENTRY  compressed mac addr = 0x%x%x scan frame channel = 0x%x scan frame rssi = %d channel match = %u 
3306,II,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x 
3306,II,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x 
3297,I,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3295,III,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3313,I,SCAN_EVENT_SEND_FAILED: 0x%x 
3306,II,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x 
3295,III,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3295,III,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x 
3295,III,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x 
3312,IIII,EXTSCAN_CREATE_ENTRY_SUCCESS  compressed mac address 0x%x first free bssid entry addr 0x%x ssid len %u no. of free bssid entries left %u 
3311,I,EXTSCAN_CREATE_ENTRY_ERROR  arg1 = 0x%x 
3310,I,EXTSCAN_FIND_BSSID_BY_REFERENCE_ERROR  bssid reference value (hash value + position) = 0x%x 
3309,I,EXTSCAN_SEARCH_SCAN_ENTRY_KEY_FOUND  scan entry reference value = 0x%x 
3308,I,EXTSCAN_SEARCH_SCAN_ENTRY_KEY_NOT_FOUND  compressed mac addr = 0x%x 
3295,III,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x 
3307,IIII,EXTSCAN_FOUND_RSSI_ENTRY  compressed mac address = 0x%x rssi table entry idx = %u current entries in temp cache = %u rssi val = %u 
3306,II,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x 
3305,III,EXTSCAN_GET_FREE_ENTRY_SUCCESS  address of first free bssid entry = 0x%x bssid table free entry count = %u bssid addr 0x%x 
3304,II,EXTSCAN_GET_FREE_ENTRY_INCONSISTENT  bssid table free entry count = %u address of first free bssid entry 0x%x 
3303,I,EXTSCAN_GET_FREE_ENTRY_NO_MORE_ENTRIES  address of first free bssid entry = 0x%x 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3295,III,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3301,IIII,EXTSCAN_BSSID_FOUND_RSSI_SAMPLE  compressed mac addr = 0x%x current idx in rssi table = %u rx frame rssi value %u current idx rssi value 0x%x 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3295,III,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x 
3300,IIII,EXTSCAN_BSSID_ADDED_RSSI_SAMPLE  compressed mac addr = 0x%x no of entries in temp cache = %u max entries in temp cache = %u rx frame rssi = -%u 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3298,IIII,EXTSCAN_BSSID_REPLACED_RSSI_SAMPLE  compressed mac addr = 0x%x current idx in rssi table = %u rx frame rssi = %u current idx rssi %u 
3297,I,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x 
3296,IIIIII,EXTSCAN_SEARCH_SCAN_ENTRY_QUEUE  rx frame addr 3 = 0x%x 0x%x 0x%x 0x%x 0x%x 0x%x 
3295,III,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x 
3294,II,EXTSCAN_SEARCH_SCAN_ENTRY_KEY_FOUND  scan entry reference value = 0x%x compressed mac addr = 0x%x 
3293,I,EXTSCAN_SEARCH_SCAN_ENTRY_KEY_FOUND compressed mac addr = 0x%x 
3292,IIIII,EXTSCAN_BSSID_TRANSFER_CURRENT_SAMPLES current scan entries = %u rssi table entry count = %u rssi table free entry count = %u bssid table entry count %u bssid table free entry count %u 
3335,IIIIII,EXTSCAN_CONFIGURE_MAWC vdev_id = %d enable = %d supp_ratio = %d (current running = %d is_enabled = %d motion_state = %d) 
3334,I,EXTSCAN_CONFIGURE_MAWC_INVALID vdev_id = %d 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3333,IIIII,EXTSCAN_BUCKET_START_OPERATION  request id = %u no of buckets = %u no of channels = %u scan priority = %u is extscan running = %u 
3332,IIIII,SCAN_ENGINE_STOP_DUE_TO_TIMEOUT  0x%x 0x%x 0x%x 0x%x 0x%x 
3331,III,EXTSCAN_START_INTERNAL_ERROR  Register event handler for bucket events to host request id = %u requestor id = %u status = %u 
3306,II,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x 
3330,II,EXTSCAN_BUCKET_STOP_CURRENT_SCANS  scheduled bucket mask = 0x%x is extscan running = %u 
3320,II,EXTSCAN_UNIT_TEST_TRACE arg1 = 0x%-8x arg2 = 0x%-8x 
3329,III,EXTSCAN_BUCKET_SCAN_STOP_REQUEST  loop i value = %u bucket id = %u  bucket scan id = %u 
3306,II,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x 
3328,IIIII,EXTSCAN_STOP  request_id = %u requestor_id = %u vdev_id = %u extscan_param.request_id = %u running = %u 
3297,I,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x 
3306,II,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x 
3327,IIIII,EXTSCAN_BUCKET_PERIODIC_TIMER  arg1 = 0x%x timer running = %u timer tick = %u base period %u scan cycle count = %u 
3297,I,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x 
3326,IIIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3325,IIIII,EXTSCAN_MAWC_SUPPRESSED_CHECK (bucket %d) motion_state = %d (0:unknown,1:stationary,2:walk,3:transit) suppress_ratio = %d suppressed_count = %d suppressed = %d 
3324,II,EXTSCAN_MAWC_MOTION_NOTIFY cur_motion_state = %d new_motion_state = %d (0:unknown,1:stationary,2:walk,3:transit) 
3323,IIIIIIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x arg6 = 0x%-8x arg7 = 0x%-8x arg8 = 0x%-8x arg9 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3322,IIII,EXTSCAN_BUCKET_PROCESS_SCAN_EVENT  scan cycle in progress = %u scan ID = %u scan event type = 0x%x requestor id = %u 
3321,IIIII,EXTSCAN_BUCKET_CANNOT_FIND_BUCKET  arg1 = 0x%x scan cycle in progress = %u scan ID = %u scan event type = 0x%x requestor id = %u 
3320,II,EXTSCAN_UNIT_TEST_TRACE arg1 = 0x%-8x arg2 = 0x%-8x 
3319,III,EXTSCAN_START_SCAN_REQUEST_FAILED  bucket index = %u bucket scan id = %u scan events to be notified for bucket = 0x%x 
3318,IIII,EXTSCAN_BUCKET_SEND_OPERATION_EVENT  arg1 = 0x%x event_type %u request id %u no of buckets %u 
3317,I,EXTSCAN_BUCKET_SEND_OPERATION_EVENT_FAILED  scan start failed event type = 0x%x 
3316,IIIII,EXTSCAN_BUCKET_START_SCAN_CYCLE  arg1 = 0x%x timer tick = %u scheduled_bucket_mask = 0x%x no of buckets = %u scan cycle count = %u 
3315,II,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x% 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3295,III,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3295,III,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x 
3340,III,EXTSCAN_UNIT_TEST_TRACE arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3295,III,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3295,III,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3295,III,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3339,II,EXTSCAN_NOTIFY_HOTLIST_MATCH  compressed mac addr = 0x%x flags = 0x%x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3338,I,EXTSCAN_EVENT_SEND_FAILED  0x%x 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3337,I,EXTSCAN_EVENT_SEND_FAILED arg1 = 0x%-8x 
3326,IIIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3336,IIIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x arg6 = 0x%-8x 
3344,I,EXTSCAN_MAIN_MALFORMED_FRAME  invalid ssid length = %u 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3295,III,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x 
3297,I,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3343,IIII,EXTSCAN_INVALID_PARAMETER: 0x%d cmdid = 0x%x error_type = 0x%x context = 0x%x  
3338,I,EXTSCAN_EVENT_SEND_FAILED  0x%x 
3342,IIII,EXTSCAN_SEND_START_STOP_EVENT  command id = %u extscan operation mode = 0x%x send event status = 0x%x request id = %u 
3338,I,EXTSCAN_EVENT_SEND_FAILED  0x%x 
3341,I,EXTSCAN_UNIT_TEST_TRACE arg1 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3346,IIIIIIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x arg6 = 0x%-8x arg7 = 0x%-8x arg8 = 0x%-8x 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3295,III,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3299,IIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3345,I,EXTSCAN_EVENT_SEND_FAILED: %d 
3295,III,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x 
3295,III,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x 
3323,IIIIIIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x arg6 = 0x%-8x arg7 = 0x%-8x arg8 = 0x%-8x arg9 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3306,II,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3302,IIIII,EXTSCAN_CLEAR_ENTRY_CONTENT arg1 = 0x%-8x arg2 = 0x%-8x arg3 = 0x%-8x arg4 = 0x%-8x arg5 = 0x%-8x 
3348,II,EXTSCAN_START_UNIT_TEST request_id = %d num_args = %d 
3347,II,EXTSCAN_STOP_UNIT_TEST request_id = %d num_args = %d 
3349,II,LPI: _wlan_wmi_lpi_scan_stop %d status:0x%x 
3350,I,LPI: _wlan_wmi_lpi_scan_stop %d 
3351,IIIIIII,LPI_SCAN_START idle_t:%d max_scn_time:%d prob_dly:%d n_chan:%d n_ssids:%d n_bssid:%d ie_len:%d 
3352,IIIIII,LPI_SCAN_START dw_act:%d dw_pas:%d min_rest:%d max_rest:%d r_prob:%d spc_prob:%d 
3353,IIIIII,LPI_SCAN_START scan_id:%d scan_req_id:%d vdev_id:%d priority:%d ctrl_flag:0x%x burst_durat:%d 
3354,II,LPI: _wlan_wmi_lpi_scan_start - WMI_LPI_STATUS_DROPPED_REQ %d ie_len:%d 
3355,II,LPI: _wlan_wmi_lpi_scan_start - WMI_LPI_STATUS_DROPPED_REQ %d num_bssid:%d 
3356,II,LPI: _wlan_wmi_lpi_scan_start - WMI_LPI_STATUS_DROPPED_REQ %d num_ssids:%d 
3357,II,,LPI: _wlan_wmi_lpi_scan_start - WMI_LPI_STATUS_ILLEGAL_CHAN_REQ %d num_chan:%d 
3358,II,LPI: _wlan_wmi_lpi_scan_start : %d Magic frequency:%d GHz Send from ADSP to check current firmware status(Is responsive)  
3359,,LPI: scan cancel as wlan vdev is free 
3360,II,LPI: _wlan_wmi_lpi_mgmt_snooping_config : %d enable:%d 
3361,II,LPI: ht nss:%d, mcs: %d 
3362,III,LPI: vht mcs_map:0x%x, rx_nss:%d, rx_mcs:%d 
3363,III,LPI: vht mcs_map:0x%x, tx_nss:%d, tx_mcs:%d 
3364,I,LPI: sec_mode: %d 
3365,I,LPI: ess: 0x%x 
3366,I,LPI: report_context_hub: %d 
3367,,LPI_EXTENTED_CAP_LCI_SUPPORTED 
3368,,LPI_EXTENTED_CAP_LOC_CIVIC_SUPPORTED 
3369,I,LPI: tx_rate: %d 
3370,II,LPI: _wlan_lpi_probe_rsp_beacon_handler : %d freq:%d 
3371,III,LPI: _wlan_lpi_probe_rsp_beacon_handler : %d ssid.ssid_len:%d, frame_len:%d 
3372,II,LPI: _wlan_lpi_probe_rsp_beacon_handler : %d is_probe:%d 
3373,II,_wlan_lpi_check_if_entry_present : mac: %x:%x 
3374,II,check error,ie_bitmap:%x: index:%x 
3375,II,LPI: wmi_lpi_complete : %d tx_cmpl_counter : %d 
3374,II,check error,ie_bitmap:%x: index:%x 
3376,I,_wlan_lpi_update_age_of_measurement : %d 
3377,I,LPI: _wlan_lpi_scan_cancel_by_vdev status:0x%x 
3378,I,LPI: _wlan_lpi_handoff_handler %d 
3379,III,LPI_PROBE_RESP_BCN_HANDLER data_buff_index:%d ie_len:%d len_of_chan_scanned:%d 
3380,III,LPI_PROBE_RESP_BCN_HANDLER ie_bitmap:0x%08x mac:0x%08x%04x 
3381,IIIIII,LPI: _wlan_lpi_send_handoff_event : %d ctxt-ssid_len:%d resp:ssid_len:%d freq:%d rssi:%d vdev_id:%d 
3382,I,LPI: _wlan_lpi_send_handoff_event : %d 
3383,II,_wlan_lpi_send_status_event : %d status:0x%x 
3384,III,_wlan_lpi_send_result : %d RESULT_DATA_SIZE:%d total:%d 
3385,III, _wlan_lpi_send_result - !! Never reach here: %d data_size:%d Event_size:%d 
3386,II,_wlan_lpi_send_result : %d num_chan_scaned:%d 
3387,IIII,_wlan_lpi_send_result : Sending Scan results to ADSP send_counter : %d data_len:%d len_of_chan_scaned: %d, total:%d 
3388,I,LPI: _wlan_lpi_send_result : %d Send In Progress not got wmi_lpi_complete cb yet !!! 
3389,I,LPI: _wlan_lpi_send_result : %d 
3390,III,_wlan_lpi_scan_evt_handler snoop scan : %d chan_freq:%d num_chan_scaned:%d 
3391,III,_wlan_lpi_scan_evt_handler Discovery scan : %d chan_freq:%d num_chan_scaned:%d 
3392,II,_wlan_lpi_scan_evt_handler : %d evt_type:0x%x 
3393,,obss scan start vdev null 
3394,,obss scan start fixed param null 
3395,,obss scan start param tlvs null 
3396,,obss scan stop vdev null 
3393,,obss scan start vdev null 
3397,,Channel not in 2.4 GHz sent 
3398,I,obss scan vdev pool alloc failed=%d 
3399,I,obss scan start vdev id =%d 
3396,,obss scan stop vdev null 
3400,,obss scan stop fixed param null 
3395,,obss scan start param tlvs null 
3401,II,obss send: num_of_scans:%x,send cnt:%x 
3402,,obss send: report is empty. Not sending OBSS report 
3403,,obss send 2040 per bss error 
3404,II,obss scan stop, refer cnt:%d, status 
3405,,obss scan stop successfully 
3406,,obss scan stop error 
3396,,obss scan stop vdev null 
3407,IIII,obss scan TE-A found_dup=%x, index:%d, op:%d,ch_id:%d 
3408,,obss scan TE-A rec null 
3409,II,obss scan TE-A type=%d, index:%d 
3410,II,obss scan HT cap present=%d, teb:0x%x 
3411,II,Beacon parser invoked, mac_id:%d, ch:%d 
3412,II,obss merge: num_of_scans:%x, idx:%x 
3413,,obss merge scan ptr error 
3414,II,obss scan send action sucess:vdev id:%x, status:%x 
3415,I,obss coex action frame buf null, vdev id:%x 
3416,,obss scan send action fail: no bss peer 
3417,II,obss scan send action:intolerent len:%x, frame len:%d 
3418,II,obss scan send action, add ch id:%x, op class:%d 
3419,II,obss scan send action:idx:%x, op class:%d 
3420,IIIIII,NLO_MAWC_CONFIG_UNIT_TEST vdev_id = %d enable = %d exp_backoff_ratio = %d init_scan_interval = %d max_scan_interval = %d num_args = %d 
3421,I,NLO_STOP_UNIT_TEST vdev_id %d 
3422,IIIIII,NLO_START_UNIT_TEST max_cycles = %d fast_period = %d slow_period = %d backoff_multiplier = %d delay_start_time = %d num_args = %d 
3423,I,NLO_CH_PREDICT_CONFIG enable %d 
3424,I,NLO ADD BCAST PROBE ssid_len:%d 
3425,IIII,NLO ADD SSID bcast_nw_type.valid:%d bcast_nw_type.type:%d num_ssid:%d ssid_len:%d 
3426,IIIII,NLO_CONFIG_3 active_dwell %d passive_dwell %d fast_max_cycle %d  rest_time %d max_rest %d 
3427,IIIII,NLO_CONFIG_2 fast_scan_period %d slow_scan_period %d delay_start_time %d probe_bundle_size %d backoff_multiplier %d 
3428,IIII,NLO_CONFIG_1 vdev_id %d no_of_ssids %d num_of_channels %d flags 0x%x 
3429,,NLO_MAWC_CONFIG_ERROR cannot alloc NLO config 
3430,IIIII,NLO_MAWC_CONFIG vdev_id = %d enable = %d ratio = %d init = %d max = %d 
3431,II,NLO_MAWC_MOTION_NOTIFY cur_motion_state = %d new_motion_state = %d (0:unknown,1:stationary,2:walk,3:transit) 
3432,III,NLO_MAWC_UPDATE_SCAN_INTERVAL mawc_motion_state = %d prev_interval = %d new_interval = %d 
3442,II,SUPPL_WPA_IE for msg 2/4: proto = %d, (len=%d) 
3441,II,SUPPL_DECRYPT_KEYDATA_INVALID LEN %d > MAX_KEYDATA_LEN %d 
3440,IIIIIII,SUPPL_IGTK_KDE: keyix %d, ipn = %x%x%x%x%x%x 
3439,I,SUPPL_DECRYPT_KEY incorrect igtk keyix = %d 
3438,IIII,SUPPL_NONCE_MISMATCH (first 4 bytes) M1 = %08x:08%x M3 = %08x:08%x 
3437,IIII,SUPPL_GET_FRM_ERR size = %d (< %d) proto = 0x%02x frm5_6: 0x%02x  -> ignore  
3436,III,SUPPL_GET_FRM_INVALID_KEY_TYPE frm_sz = %d akmp = 0x%x received wrong key_info = 0x%x -> ignore 
3435,IIIIII,SUPPL_GET_FRM_INFO size = %d akmp = %d proto = 0x%x key_info = 0x%04x keydata_len = 0x%x evt = %d 
3434,I,SUPPL_GET_FRM_NOT_EAPOL_KEY type (%d) -> hand it to host 
3433,II,SUPPL_GET_FRM_INVALID_LEN frm_sz = %d p_len_hdr= %d -> ignore 
3443,I,SUPPL_EAPOL_KEY_MIC EAPOL key_mic - ver %d  
3444,III,SUPPL_WPA_PTK derivation (akmp 0x%08x) sha%d ptk_len %d 
3445,III,SUPPL_CCKM Installing GTK to the driver (keyidx=%d tx=%d len=%d). 
3446,,SUPPL_CCKM_ERR_WPA: AES unwrap failed - could not decrypt GTK 
3447,I,SUPPL_CCKM_ERR_WPA: Unsupported pairwise cipher %d 
3448,,SUPPL_CCKM_ERR_WPA: Pairwise Cipher Suite: NONE - do not use pairwise keys 
3449,II,SUPPL_CCKM_INSTALL_GTK group_cipher 0x%x pairwise_cipher 0x%x 
3450,IIII,SUPPL_MIC_MISMATCH calc = 0x%08x%08x rcvd = 0x%08x%08x 
3451,,SUPPL_CCKM: Use HMAC-MD5 for MIC calculation 
3452,,SUPPL_CCKM: Use HMAC-SHA1 for MIC calculation 
3453,III,SUPPL_CCKM: verify_mic cie_len %d gtk_len %d data_len %d 
3454,II,SUPPL_CCKM_ERR: Invalid CCKM reassociation response element - no room for %u octet GTK (cie_len = %d) 
3455,,SUPPL_CCKM_ERR: Use own WPA/RSN IE in MIC calculation (no AP info available?!) 
3456,,SUPPL_CCKM_ERR: Use AP WPA IE in MIC calculation (proto mismatch?!) 
3457,,SUPPL_CCKM_ERR: Use AP RSN IE in MIC calculation (proto mismatch?!) 
3458,III,SUPPL_CCKM: verify_mic proto = 0x%x (1=WPA, 2=RSN) wpa_ie_len %d rsn_ie_len %d 
3459,IIIIIIII,SUPPL_CCKM: mn mic: %02x %02x %02x %02x %02x %02x %02x %02x 
3460,IIII,SUPPL_DUMP_KRK %08x:%08x:%08x:%08x 
3461,IIII,SUPPL_CCKM_BUILD Timestamp[32] 0x%08x rn 0x%x Proto 0x%02x data_len %d 
3462,I,SUPPL_CCKM: cckm RN = %02x 
3463,II,SUPPL_CCKM: Input Timestamp: 0x%x%x 
3464,IIIIII,SUPPL_CCKM: bssid: %02x:%02x:%02x:%02x:%02x:%02x 
3465,IIIIII,SUPPL_CCKM: sm->own_addr: %02x:%02x:%02x:%02x:%02x:%02x 
3466,III,SUPPL_CCKM_PROC_RSP succeed 0x%08x:%04x rn=0x%x 
3467,,SUPPL_CCKM_ERR Reassociation Response - MIC Failure 
3468,IIIII,SUPPL_CCKM_PROC_RSP_ERR eid 0x%x (exp 0x9c) oui 0x%02x%02x%02x (exp 0x00409600) 
3469,I,SUPPL_CCKM_FR_IS_COMPLETED %d 
3470,II,SUPPL_INVALID_SUITE  type %d (1 group, 2 pairwise, 3 akm) suite 0x%x 
3471,IIIII,SUPPL_FT_MIC_MISMATCH md 0x%x%x ftie_len %d rsnie_len %d ricie_len %d 
3472,IIIII,SUPPL_FT_RIC_IE_ADDED len %d 0x%x 0x%x 0x%x 0x%x 
3470,II,SUPPL_INVALID_SUITE  type %d (1 group, 2 pairwise, 3 akm) suite 0x%x 
3470,II,SUPPL_INVALID_SUITE  type %d (1 group, 2 pairwise, 3 akm) suite 0x%x 
3470,II,SUPPL_INVALID_SUITE  type %d (1 group, 2 pairwise, 3 akm) suite 0x%x 
3473,III,SUPPL_EXCEED_MAX_LEN  buf_type %d buf_len %d max_len %d 
3566,III,SUPPL_DEINIT installed_key = 0x%x timer_init=%d closing=%d 
3565,III,SUPPL_DEINIT_TIMER period = %d msec, peer = %08x%04x  
3564,II,SUPPL_NODE_NOT_FOUND auth_init_auth peer 08x:%04x already exist 
3563,II,SUPPL_CHECK_CLOSING index=%d closing=%d 
3553,,SUPPL_INIT_AUTH ALLOC NODE FAIL 
3562,IIIII,SUPPL_INIT_AUTH proto|key_mgmt = 0x%06x mgmt|group|pair_cipher = 0x%x 0x%08x peer = %08x%04x 
3562,IIIII,SUPPL_INIT_AUTH proto|key_mgmt = 0x%06x mgmt|group|pair_cipher = 0x%x 0x%08x peer = %08x%04x 
3561,IIII,SUPPL_DUMP_PMK %08x:%08x:%08x:%08x 
3560,,SUPPL_KEY_LEN_ERR_PMK 
3559,,SUPPL_REPLACE_PMK_WITH_CACHED_VAL 
3558,II,SUPPL_NODE_EXIST auth_init_cckm peer 08x:%04x 
3557,,SUPPL_INIT_FT ALLOC NODE FAIL 
3556,IIII,SUPPL_INIT_CCKM proto|key_mgmt = 0x%06x mgmt|group|pair_cipher = 0x%06x peer = %08x%04x 
3460,IIII,SUPPL_DUMP_KRK %08x:%08x:%08x:%08x 
3555,IIII,SUPPL_DUMP_BTK %08x:%08x:%08x:%08x 
3554,II,SUPPL_NODE_EXIST auth_init_ft peer 08x:%04x 
3553,,SUPPL_INIT_AUTH ALLOC NODE FAIL 
3552,I,SUPPL_PLUMB_IGKT key_id = %d 
3551,,SUPPL_RECV_EAPOL null ctxt 
3550,III,SUPPL_RECV_EAPOL_1X size = %d evt = %d (RX_1X 11/SENT_FAIL 12/OUT_OF_MEM 13) state = %d (NULL 0/INIT 1/SENT_M2 2/SENT_M4 3/CONNECTED 4) 
3549,II,SUPPL_STATE_CHANGE old_state = %d cur_state = %d 
3548,IIII,SUPPL_NODE_NOT_FOUND recv_frm sz = %d, SA = %08x:%04x evt = %d  
3547,IIIIIII,SUPPL_RECV_EAPOL recv_sz = %d evt = %d cur_state = %d proto = %d role = %d pmf=%d(1:True, 0:False) param = 0x%x 
3546,III,SUPPL_NODE_NOT_FOUND should_offload is_eapol = %d, SA = %08x:%04x 
3545,III,SUPPL_NODE_NOT_FOUND update_pmk pmk_len = %d, SA = %04x:%08x 
3544,III,SUPPL_FINISH_ERROR status = %d peer = 08x:%04x (peer not found) 
3543,III,SUPPL_FINISH_ERROR status = %d peer = 08x:%04x 
3542,II,SUPPL_NODE_NOT_FOUND parse_auth_ftie peer 08x:%04x doesn't exist 
3541,IIII,SUPPL_PARSE_FTIE_FAIL ret %d key_mgmt 0x%x ie_len %d ric_len %d 
3540,II,SUPPL_NODE_NOT_FOUND parse_cckmie peer 08x:%04x doesn't exist 
3539,II,SUPPL_NODE_NOT_FOUND parse_reassoc_ftie peer 08x:%04x doesn't exist 
3538,IIII,SUPPL_PARSE_FTIE_FAIL ret %d key_mgmt 0x%x ie_len %d refined_ie_len %d 
3537,II,SUPPL_NODE_NOT_FOUND get_ccx_ie peer 08x:%04x doesn't exist 
3536,II,SUPPL_NODE_NOT_FOUND get_ftie peer 08x:%04x doesn't exist 
3535,II,SUPPL_INSTALL_KEY [reqested|installed|resulted]_key = 0x%06x[group|pairwise]_chiper = 0x%08x  
3534,I,_suppl_pmk_cache_add_ pmk_cache->cat_flag  %d 
3533,IIIIII,_suppl_pmk_cache_add peer_addr %x %x %x %x %x %x 
3532,,_suppl_pmk_cache_add_ returning as cat flag is 0 
3531,,_suppl_pmk_cache_del_ returning as cat flag is 0 
3530,II,SUPPL_PROCESS_CONNECTED connected=%d curr_state=%d 
3529,IIIII,SUPPL_MIC_MISMATCH len = %d ucipher = 0x%x pmk_len = %d pmk(first 8 byte) = %08x:%08x 
3521,I,SUPPL_GET_BUF_FAIL M%d -> evt = OUT_OF_MEM 
3520,II,SUPPL_SEND_EAPOL_FAIL M%d status = %d 
3528,II,SUPPL_RECV_EAPOL_TIMEOUT state = %d (NULL 0/INIT 1/SENT_M2 2/SENT_M4 3/CONNECTED 4) status = %d 
3527,II,AUTHE_RECV_EAPOL_TIMEOUT state = %d (NULL 0/INIT 1/SENT_M2 2/SENT_M4 3/CONNECTED 4) status = %d 
3524,III,SUPPL_PARSE_FTIE remain_buf_len %d < ie_len %d (ie_id 0x%x) skipped to copy and break 
3526,I,SUPPL_PARSE_FTIE ric_num %d 
3525,IIII,SUPPL_PARSE_FTIE remain_buf_len %d < ie_len %d (ie_id 0x%x) ric_num = %d skipped to copy and break 
3524,III,SUPPL_PARSE_FTIE remain_buf_len %d < ie_len %d (ie_id 0x%x) skipped to copy and break 
3473,III,SUPPL_EXCEED_MAX_LEN  buf_type %d buf_len %d max_len %d 
3523,,SUPPL_SEND_EAPOL invalid param NULL 
3522,IIII,SUPPL_SEND_EAPOL send_sz = %d status = %d cur_evt = %d cur_state = %d 
3521,I,SUPPL_GET_BUF_FAIL M%d -> evt = OUT_OF_MEM 
3520,II,SUPPL_SEND_EAPOL_FAIL M%d status = %d 
3519,II,SUPPL_DEINIT peer = %08x%04x  
3518,II,SUPPL_NODE_EXIST auth_init_fils peer 08x:%04x 
3517,,SUPPL_INIT_FILS ALLOC NODE FAIL 
3516,I,SUPPL_ERP_SEQ_NUM_INVALID %d 
3515,II,SUPPL_NODE_NOT_FOUND fils reassoc decrypt peer_mac_addr 08x:%04x doesn't exist 
3514,I,FILS_DEBUG FILS AEAD decryption failed - %d 
3513,II,FILS_DEBUG aad[%d] len - %d 
3512,I,FILS_DEBUG KEK len - %d 
3511,I,FILS_DEBUG AEAD Decryption of Assoc resp successful - %d 
3510,II,SUPPL_NODE_NOT_FOUND fils get_key peer 08x:%04x doesn't exist 
3509,II,SUPPL_NODE_NOT_FOUND fils encrypt_reassoc peer_mac_addr 08x:%04x doesn't exist 
3508,IIII,FILS_DEBUG AEAD vectors aad[%d] %x aad_len[%d] - %d 
3507,I,FILS_DEBUG AEAD input - %d 
3506,I,FILS_DEBUG AEAD KEK - %d 
3505,I,FILS_DEBUG AEAD result - %d 
3504,I,FILS_DEBUG AEAD output - %d 
3503,II,SUPPL_NODE_NOT_FOUND fils cached_pmk peer 08x:%04x doesn't exist 
3502,II,SUPPL_NODE_NOT_FOUND fils key_auth_sk peer 08x:%04x doesn't exist 
3501,II,SUPPL_NODE_NOT_FOUND fils pmk_to_ptk peer 08x:%04x doesn't exist 
3500,II,SUPPL_NODE_NOT_FOUND fils rmsk_to_pmsk peer 08x:%04x doesn't exist 
3499,II,SUPPL_NODE_NOT_FOUND get_auth_fils peer 08x:%04x doesn't exist 
3498,II,SUPPL_NODE_NOT_FOUND parse fils nonce peer 08x:%04x doesn't exist 
3497,II,SUPPL_NODE_NOT_FOUND parse fils session peer 08x:%04x doesn't exist 
3496,II,FILS session element length (%d) is not of expected size -(%d) 
3495,I,FILS_DEBUG FILS session IE length is as expected - %d 
3494,, FILS session id in re-assoc rsp doesnt match the one sent in reassoc req 
3493,I,FILS session IE content is as expected - %d 
3492,I,FILS_DEBUG Key confirm IE size - %d 
3491,II,SUPPL_NODE_NOT_FOUND fils cofnfirm_ie  peer_addr 08x:%04x doesn't exist 
3490,I,FILS_DEBUG Parsing FILS Key Confirm IE - %d 
3489,II,FILS_DEBUG FILS Key Confirm IE len doesn't match expected %d actual %d 
3488,I,FILS_DEBUG FILS Key Confirm IE length matched as expected - %d 
3487,I,FILS_DEBUG FILS Key Confirm IE content doesn't match expected %d 
3486,I,FILS_DEBUG FILS Key Confirm IE content matched as expected - %d 
3485,II,SUPPL_NODE_NOT_FOUND fils delivery_ie  peer_addr 08x:%04x doesn't exist 
3484,I,suppl_parse_fils_key_delivery_ie: parsing Key Delivery IE - %d 
3483,II,suppl_parse_fils_key_delivery_ie: IE length %d is greater than available frame length %d 
3482,II,suppl_parse_fils_key_delivery_ie: IE length %d less than Key RSC Length %d 
3481,I,suppl_parse_fils_key_delivery_ie: Replay counter - %d 
3480,I,suppl_parse_fils_key_delivery_ie: Expected 0xdd at the start of KDE, found %02x 
3479,II,suppl_parse_fils_key_delivery_ie: KDE length %d greater than data_left %d 
3478,II,suppl_parse_fils_key_delivery_ie: KDE length %d less than data_left %d 
3477,II,suppl_parse_fils_key_delivery_ie: GTK Key extraction successful GTK Key Index: %d Length - %d 
3476,IIII,suppl_parse_fils_key_delivery_ie: Cannot parse KDE OUI: %02x-%02x-%02x Data type: %d 
3475,I,SUPPL_SSID_PMK_CACHE_INVALID ssid_len %d. return. 
3474,II,SUPPL_SSID_PMK_CACHE_INVALID pmk_len %d. return. 
3567,II,_wlan_eapol_process: length=%d, L3_offset=%d 
3571,I,suppl_auth_init_auth_mt alloc_size=%d 
3570,I,suppl_auth_init_auth_mt real_size=%d 
3569,II,suppl_auth_status_change_evt_mt null sa=0x%08x%04x 
3568,I,_wlan_suppl_be_thread_comm_msg_handler(): message_id = %d 
3581,I,FILS_KEY_AUTH_SK_STA returned %d 
3580,I,FILS_KEY_AUTH_SK_AP returned %d 
3579,IIIII,FILS_EAP_NODE_NOT_FOUND erp.code = 0x%x, identifier=0x%x, length = %d, peer = %08x:%04x 
3578,III,FILS_EAP_PROCESS erp_seq %d %d next_seq %d 
3577,II,FILS_EAP_INVALID_SEQ (%d) != exp_erp_seq (%d) 
3576,I,FILS_EAP_PARSE_ERR %d 
3575,,FILS_EAP_PARSE_ERR_KEYNAME 
3574,II,FILS_EAP_INVALID_TYPE pkt_type (0x%x) != EAP_ERP_TYPE_REAUTH (0x%x) 
3573,I,FILS_EAP_PARSE_ERR_KEYNAME_LEN %d >253 
3572,II,FILS_EAP_INVALID_LEN len (%d) < hdr_len+4 (%d) 
3585,III,FILS_DEBUG iv_c_len %d key_len %d num_elem %d 
3584,I,FILS_DEBUG AES tag did not match %d 
3583,I,FILS_DEBUG, aes_ctr_encrypt returned error %d 
3582,I,FILS_DEBUG, aes_s2v returned error %d 
3586,II,wlan_tdls_wmi_set_state_enable() TDLS_PASSIVE teardown_notification_ms: %d peer_rssi_monitor_period_cnt: %d 
3587,III,wlan_tdls_wmi_set_state_enable(505) TDLS_PASSIVE vdev_id=%d, rssi_teardown_threshold=%d, result=%d 
3588,III,wlan_tdls_wmi_set_state_enable(470) TDLS_PASSIVE vdev_id=%d, tdls_peer_kickout_threshold: %d result=%d 
3589,III,wlan_tdls_wmi_set_state_enable(449) TDLS_PASSIVE vdev_id=%d, traffic_response_timeout_ms=%d, result=%d 
3590,I,wlan_tdls_wmi_set_state_enable TDLS_PASSIVE offchan_enabled=%d 
3591,II,wlan_tdls_wmi_set_state_enable TDLS_PASSIVE slp_sta_support=%d buf_sta_support=%d 
3592,IIII,wlan_tdls_wmi_set_state_enable(410) TDLS_PASSIVE wal_vdev = %p vdev_id=%d, tdls_options=0x%x, result=%d 
3593,IIIIIII,wlan_tdls_wmi_peer_state_connected(323) vdev_id=%d, primary_freq=%d, center_freq1=%d, center_freq2=%d, info=0x%x, reg_info_1=0x%x, reg_info_2=0x%x 
3594,IIIII,TDLS_DBGID_WLAN_PEER_UPDATE_SET(311) vdev_id=%d, pref_offchan_num=%d, off_chan_support=%d, phymode=%d, new center_freq=%d 
3595,IIIIIII,wlan_tdls_wmi_peer_state_connected(301) vdev_id=%d, primary_freq=%d, center_freq1=%d, center_freq2=%d, info=0x%x, reg_info_1=0x%x, reg_info_2=0x%x 
3596,IIIII,wlan_tdls_wmi_peer_state_connected(280) OFFCHAN enabled, vdev_id=%d, pref_offchan_num=%d, pref_offchan_bw=0x%x, self_oper_class=%d, peer_oper_class=%d 
3597,II,wlan_tdls_wmi_peer_state_connected(260) vdev_id=%d, tdls_options=0x%x 
3598,II,_wlan_tdls_delete_instance() vdev_id = %d tdls_handle=%p 
3599,II,_wlan_tdls_create_instance() vdev_id: %d tdls_handle=%p 
3600,,_wlan_tdls_is_link_present() (!vdev) 
3601,III,_wlan_tdls_suspend_resume_offchannel() 2 offchan_temp_disabled: %d offchan_active: %d offchan_state: %d 
3602,I,_wlan_tdls_suspend_resume_offchannel() 1 offchan_temp_disabled: %d 
3603,I,_wlan_tdls_suspend_resume_offchannel() offchan_temp_disabled: %d 
3604,IIIIIIIII,_wlan_tdls_suspend_resume_offchannel() vdev_id: %d tdls: %d suspend: %d RC: %d OC_E: %d OC_temp_dis: %d OC_Active: %d OC_State: %d scan_started: %d 
3605,,_wlan_tdls_suspend_resume_offchannel() (!tdls) 
3606,,_wlan_tdls_suspend_resume_offchannel() (!vdev) 
3607,I,_wlan_tdls_suspend_resume_offchannel(): suspend: %d 
3608,III,wlan_tdls_notify_host_connection_tracker(): vdev id = %d reason = 0x%x evh = %p 
3609,IIIII,wlan_tdls_wmi_set_offchan_mode_cmd() support_offchan=%d offchan_active=%d op_class=%d offchan_num=%d chan_info=%p 
3610,I,wlan_tdls_wmi_set_offchan_mode_cmd(682) vdev_id=%d 
3611,I,wlan_tdls_wmi_set_offchan_mode_cmd(668) Peer is NULL vdev_id=%d 
3612,IIII,wlan_tdls_wmi_set_offchan_mode_cmd(654) vdev_id=%d, offchan_mode=%d, MAC(MSB=0x%x, LSB=0x%x) 
3613,III,wlan_tdls_wmi_set_offchan_mode_cmd(637) TDLS is 0x%x state %d vdev_id=%d 
3614,I,wlan_tdls_wmi_set_state_cmd() failed: result = %d 
3615,,wlan_tdls_wmi_set_state_cmd: tdls on vdev_id = %d was already disabled 
3616,I,wlan_tdls_wmi_set_state_cmd: tdls = %p 
3617,III,wlan_tdls_wmi_set_state_cmd(392) Cmd  vdev_id=%d cmd state = %d tdls = %p 
3618,IIIII,wlan_tdls_wmi_peer_update_cmd(346) Cmd state TEARDOWN, vdev_id=%d, peer = %p peer_state=%d, MAC(MSB=0x%x, LSB=0x%x) 
3619,IIIII,wlan_tdls_wmi_peer_update_cmd(285) Cmd state CONNECTED, vdev_id=%d, peer = %p peer_state=%d, MAC(MSB=0x%x, LSB=0x%x) 
3620,IIII,wlan_tdls_wmi_peer_update_cmd(276) Cmd state PEERING, vdev_id=%d, peer_state=%d, MAC(MSB=0x%x, LSB=0x%x) 
3621,I,wlan_tdls_wmi_peer_update_cmd(214) TDLS is in disabled state!!! return 
3622,,wlan_tdls_wmi_peer_update_cmd : Ignoring this command as we are not connected to AP 
3623,IIII,wlan_tdls_wmi_peer_update_cmd(256) PEER_UPDATE cmd recvd frm host, vdev_id=%d, tdls=%p tdls_state=%d peer_state=%d  
3624,III,_wlan_tdls_init() peer_max = %d sleep_sta = %d buffer_sta = %d 
3759,III,wlan_tdls_chan_switch_req_completion(2122) offchan_active=%d, abf = %p completion_status=%d 
3758,IIIII,wlan_tdls_chan_switch_resp_completion(2198) abf = %p rx_chan_switch_req=%d, offchan_active=%d, completion_status=%d, link_pause_incomplete=%d 
3757,II,wlan_tdls_chan_switch_resp_completion(2217) offchan_pause_unpause_cb_fn=0x%x, pause_unpause_cb_fn=0x%x 
3756,IIII,wlan_tdls_chan_switch_rx_complete_timer_handler(3160) peer_valid= 0x%x, offchan_enabled=0x%x, link_pause_incomplete=%d, pause_unpause_cb_fn=%p 
3755,I,wlan_tdls_chan_switch_rx_complete_timer_handler(3177) TDLS peer is NULL! link_pause_incomplete=%d 
3754,IIIII,wlan_tdls_check_sco_bandwidth(2430) host_pref_bw=0x%x, offchan offset=%d, wide_bw_ch_sw=%d, target_channel=%d, offchan_activ=%d 
3753,II,wlan_tdls_clear_peer_entry(917) vdev_id=%d, peer_connect_count=%d 
3752,III,wlan_tdls_clear_peer_entry(963) vdev_id=%d, buf_sta_handle=0x%x, num_active_buf_sta=%d 
3751,II,wlan_tdls_clear_peer_entry(990) PEER does not exist, vdev_id=%d, peer_connect_count=%d 
3750,III,wlan_tdls_create_offchan()entry=%p offchan_timers_initialized=%d offchan_active=%d 
3749,IIII,wlan_tdls_create_offchan(1075) tdls ptr=%p, entry ptr=%p, offchan_link=%p offchan_cs_req=%p 
3748,III,wlan_tdls_create_offchan()is_peer_responder=%d offchan_active=%d strict: %d 
3747,II,wlan_tdls_deconfigure_offchan(1143) tdls=0x%x, offchan_peer=0x%x 
3746,IIIII,wlan_tdls_deconfigure_offchan(1155) sifs_burst_flag=%d, offchan_init=%d, scan_started=%d, restore_offchan_state=%d offchan_peer=%p 
3745,,Enable SIFS back as offchan is removed 
3744,IIIII,wlan_tdls_delete_offchan(1177) no_of_tdls_base_pause=%d, no_of_tdls_offchan_pause=%d, duration=%d, total_offchan_time=%d, offchan_cs_req=0x%x 
3743,IIIII,wlan_tdls_delete_offchan(1195) tdls_link_pause_state = %d, link_pause_incomplete=%d, peer_paused=%d, pause_unpause_cb_fn=0x%x, offchan_pause_unpause_cb_fn=0x%x 
3742,IIIII,wlan_tdls_delete_offchan(1225) preempt_offchan_cs_req=0x%x, offchan_link=0x%x, rx_chan_switch_resp=%d, rx_chan_switch_req=%d, offchan_active=%d 
3741,I,wlan_tdls_homechan_ocs_hdlr(3420) event type=%d 
3740,I,wlan_tdls_link_ispaused(1691) TDLS base link not paused yet! pause_incomplete=%d 
3739,I,wlan_tdls_link_pause cb_fn = %p 
3738,III,wlan_tdls_link_pause(1471) index=%x, peer_cnt=%d, peer_valid=%d 
3737,II,wlan_tdls_link_pause(1478) Peer found, pausing TIDQs, entry=0x%x, wlan_peer=0x%x 
3736,II,wlan_tdls_link_pause_basic() entry->peer_paused: %d wal_connection_pause_is_peer_paused: %d 
3735,IIIIII,wlan_tdls_link_pause_offchan(1400) peer_valid=%d, wlan_peer=0x%x, offchan_enabled=%d, buf_sta_role = %d, rx_chan_switch_req=%d offchan_active=%d 
3734,I,wlan_tdls_link_pause(1417) ch_switch_sent=%d 
3733,III,wlan_tdls_link_pause_offchan() state: 0x%x CH_SW_sent: %d wal_connection_pause_is_peer_paused:0x%x 
3732,III,wlan_tdls_link_pause_offchan() state: 0x%x CH_SW_sent: %d wal_connection_pause_is_peer_paused:%0x%x 
3731,IIII,wlan_tdls_link_pause Did not send ch switch packets, change to basic TDLS pause, ch_switch_sent=%d                   offchan_peer: %p, link_pause_state=%d wal_connection_pause_is_peer_paused=0x%x 
3730,III,wlan_tdls_link_pause_sleep_sta(1366) vdev_id=%d, buf_sta_handle=0x%x, status=%d 
3729,IIIII,wlan_tdls_link_pause(1378) vdev_id=%d, buf_sta_handle=0x%x, temp_status=%d, counter=%d timeout = %d 
3728,II,wlan_tdls_link_pause_sleep_sta() entry->peer_paused: %d wal_connection_pause_is_peer_paused: %d 
3727,IIIIIII,wlan_tdls_link_pause_update_pause_state(1329)link_pause_state=%d, new_chan_mhz=%x, scan_started=%d, num_active_slp_sta=%d, t2tbtt=%d, peer_connect_count=%d, offchan_freq=%d 
3726,IIIII,wlan_tdls_link_unpause(1513) link_pause_state=%d, scan_started=%d, peer_connect_count=%d, last pause_incomplete=%d cb_fn = %p 
3725,I,wlan_tdls_link_unpause(1551) peer_switch_time=%d 
3724,II,wlan_tdls_link_unpause(1565) vdev_id=%d, timer_duration_ms=%d 
3723,IIII,wlan_tdls_link_unpause(1605) vdev_id=%d, buf_sta_handle=0x%x, status=%d, counter=%d 
3722,III,wlan_tdls_link_unpause(1618) vdev_id=%d, buf_sta_handle=0x%x, temp_status=%d 
3721,III,wlan_tdls_link_unpaus(1656) vdev_id=%d, entry=0x%x, wlan_peer=0x%x 
3720,I,wlan_tdls_link_unpause() wal_connection_pause_is_peer_paused: %d 
3719,III,wlan_tdls_offchan_link_ispaused(2955) Peer not paused yet, peer_valid=%d, peer_paused=%d, offchan_enabled=%d 
3718,IIII,wlan_tdls_offchan_link_pause(2763) 0xd00d1e03: offchan_init=%d, scan_started=%d, offchan_enabled=%d, time=%d 
3717,III,wlan_tdls_offchan_link_pause(2796) sent channel switch resp status=%d, entry=0x%x, is_peer_paused=%d 
3716,III,wlan_tdls_offchan_link_pause(2809) entry=0x%x, offchan_init=%d, is_peer_paused=%d 
3715,IIII,wlan_tdls_offchan_link_unpause(2857) 0xd00d1e02: offchan_init=%d, scan_started=%d, offchan_enabled=%d, is_peer_paused=%d 
3714,II,wlan_tdls_offchan_link_unpause(2874) cur_time=%d, peer_switch_time=%d 
3713,II,wlan_tdls_offchan_link_unpause(2902) timer_duration_ms=%d, NULL data tx_status=%d 
3712,I,wlan_tdls_offchan_link_unpause(2916) WLAN peer is NULL! entry=0x%x 
3711,I,wlan_tdls_offchan_ocs_hdlr(2987) ev=%d 
3710,I,wlan_tdls_offchan_req_receive_timeout_handler(3201) rx_chan_switch_req=%d 
3709,,wlan_tdls_offchan_req_receive_timeout_handler(3213) Unexpected, timer should have stopped earlier! 
3708,IIII,wlan_tdls_offchan_req_receive_timeout_handler()peer_ni_flags=0x%x offchan.phy_mode=%d enter_freq1=0x%x off_chan.mhz=0x%x 
3707,II,wlan_tdls_offchan_req_receive_timeout_handler(3293) Offchan request posted to OCS, offchan_cs_req=0x%x, offchan primary=%d 
3706,IIIII,wlan_tdls_offchan_responder_setup_link_chreq vdev_id=%d, peer_ni_flags=0x%x, phymode=%d, center_freq1=%d, offchan freq=%d 
3705,III,wwlan_tdls_offchan_responder_setup_link_chreq  bandwidth=%d, phymode=%d, center_freq=%d 
3704,IIIII,wlan_tdls_offchan_txrx_timer_handler(3317) last_activity=%d, now=%d, switch_timeout=%d, preempt_offchan_cs_req=%d, offchan_cs_req=%d 
3703,I,wlan_tdls_pause_traffic_timer_handler(3085) Stopping preempt request, time_to_tbtt=%d 
3702,I,wlan_tdls_pause_traffic_timer_handler(3097) Offchan is active, time_to_tbtt=%d 
3701,,wlan_tdls_pause_traffic_timer_handler(3104) Offchan is not active! 
3700,III,wlan_tdls_pause_traffic_timer_handler(3108) peer_valid=%d, offchan_enabled=%d, link_pause_incomplete=%d 
3699,I,wlan_tdls_pause_traffic_timer_handler(3121) TDLS peer is NULL! link_pause_incomplete=%d 
3698,II,wlan_tdls_pause_traffic_timer_handler(3127) pause_unpause_cb_fn=0x%x, offchan_pause_unpause_cb_fn=0x%x 
3697,II,wlan_tdls_peer_capability_update(1734) vdev_id=%d, index=%d 
3696,I,wlan_tdls_peer_capability_update(1739) Wrong index, vdev_id=%d 
3695,IIIIIIIII,wlan_tdls_peer_capability_update(1751) vdev_id=%d, peer buf_sta_supported=%d, slp_sta_supported=%d, is_peer_responder=%d, num_active_slp_sta=%d, concurrent_slp_sta_max=%d, num_active_buffer_sta=%d concurrent_buffer_sta_max=%d, self buffer_sta_supported=%d 
3694,I,wlan_tdls_peer_capability_update(1769) vdev_id=%d 
3693,I,wlan_tdls_peer_capability_update(1784) vdev_id=%d, slp_sta_handle=0x%x 
3692,III,wlan_tdls_peer_capability_update(1798) vdev_id=%d, ps_handle=0x%x, peer=0x%x 
3691,I,wlan_tdls_peer_capability_update(1826) buf_sta_handle=0x%x 
3690,IIIIII,wlan_tdls_peer_capability_update(1852) AP chan=%d, offchan_active=%d, offchannel ptr=0x%x, is_peer_responder=%d, offchan_enabled=%d, offchan_support=%d 
3689,II,wlan_tdls_peer_connect(647) vdev_id=%d, index=%d 
3688,I,wlan_tdls_peer_connect(652) Either index is negative or max peer reached, vdev_id=%d 
3687,IIIII,wlan_tdls_peer_connect(661) vdev_id=%d, entry ptr=%p, peer_valid=%d, sleep_sta_handle=0x%x, buf_sta_handle=0x%x 
3686,II,wlan_tdls_peer_connect(819) onchan_link=0x%x, home_cs_req=0x%x 
3685,I,wlan_tdls_peer_connect(842) home_cs_req=0x%x 
3684,I,wlan_tdls_peer_connect(871) vdev_id=%d 
3683,IIIIIII,wlan_tdls_peer_connect_update_peer_param(736) chan=%d, AP phymode=%d, peer phymode=%d, AP center_freq=%d, AP antenna_max=%d chan flags=0x%x vdev_bw = %d 
3682,IIIIIIIII,wlan_tdls_peer_connect_update_peer_param(764) chan_change: %d chan center_freq=%d, old peer phymode=%d, new peer phy_mode=%d, qualified phymode=%d, chan center_freq1=%d, chan center_freq2=%d, chan antenna_max=%d, new_vdev_bw=%d 
3681,IIIIII,wlan_tdls_peer_connect_update_peer_param(771) vdev_id=%d, chan=%d chan phymode=%d, center_freq=%d, chan center_freq1=%d, chan center_freq2=%d, chan flags=0x%x 
3680,IIIII,wlan_tdls_peer_connect_update_peer_param(779) vdev_id=%d, max_reg_power=%d, antenna_max=%d, max_tx_power=%d, offchan_enabled=%d 
3679,I,wlan_tdls_peer_get_index(180) vdev_id=%d 
3678,II,wlan_tdls_peer_get_index(195) vdev_id=%d, free_idx=%d 
3677,I,wlan_tdls_peer_get_index(202) vdev_id=%d 
3676,IIIII,wlan_tdls_peer_offchannel_configure(1976) offchan_enabled=%d, peer_connect_count=%d, offchannel_wmi=%p, offchan_temp_disabled=%d, host_pref_bw=0x%x 
3675,I,wlan_tdls_peer_offchannel_configure(1991) offchan_freq=%d 
3674,IIIIIIIII,wlan_tdls_peer_offchannel_configure channel = %d peer_ni_flags=0x%x, is_peer_responder=%d, offchan phymode=%d, center=%d, max_tx_pwr=%d, antenna_max=%d, max_reg_power=%d off_chan_peer=%p 
3673,,wlan_tdls_peer_offchannel_configure(2060) SIFS is enabled, disable it 
3672,III,wlan_tdls_peer_teardown(1026) Cannot proceed, vdev_id=%d, index=%d, peer_max=%d 
3671,III,wlan_tdls_peer_teardown(1032) vdev_id=%d, index=%d, peer_max=%d 
3670,I,wlan_tdls_print_peer_params(386) cid=0x%x, PTR is NULL 
3669,IIIII,wlan_tdls_print_peer_params(395) cid=0x%x, ni_flags=0x%x, ht_caps=0x%x, vht_caps=0x%x, legacy_rate_set=0x%x 
3668,III,wlan_tdls_print_peer_params(400) cid=0x%x, ht_mcs_set[0]=0x%x, ht_mcs_set[1]=0x%x 
3667,IIII,wlan_tdls_print_peer_params(406) cid=0x%x, vht_mcs_set=0x%x, tx_chainmask=0x%x, phymode=%d 
3666,IIIII,wlan_tdls_print_peer_params(413) cid=0x%x, ni_flags=0x%x, ht_caps=0x%x, vht_caps=0x%x, legacy_rate_set=0x%x 
3665,III,wlan_tdls_print_peer_params(420) cid=0x%x, ht_mcs_set[0]=0x%x, ht_mcs_set[1]=0x%x 
3664,IIIII,wlan_tdls_print_peer_params(425) cid=0x%x, vht_mcs_set=0x%x, tx_chainmask=0x%x, phymode=%d, retain_start_mcs=%d 
3663,III,wlan_tdls_requeue_offchan_timer_handler(3017) requeue_offchan_req=%d, scan_started=%d, offchan_active=%d 
3662,II,wlan_tdls_restore_ratectrl_params(462) vdev_id=%d, peer ptr=%p 
3661,III,wlan_tdls_restore_ratectrl_params(476) no need to apply rate vdev_id=%d, is_offchan=%d, offchan_rate_applied=%d 
3660,,Initialize the offchannel rate node context 
3659,I,Swap the rate node context is_offchan = %d 
3658,I,Fill rate control params: phy mode = %d 
3657,IIII,wlan_tdls_restore_ratectrl_params(603) vdev_id=%d, is_peer_paused=%d is_offchan = %d phymode = %d 
3656,III,wlan_tdls_restore_ratectrl_params(592) vdev_id=%d, is_offchan=%d, offchan_rate_applied=%d 
3655,,wlan_tdls_peer_chan_switch_event_handler(2322) VDEV is NULL! 
3654,I,wlan_tdls_rt_thread_comm_msg_handler(): unknown teardown reason code : %d 
3653,IIII,wlan_tdls_rx_chan_switch_req_frame(2392) Cannot process channel switch req frame, vdev_id=%d, tdls ptr=%p, offchan_peer=%p, peer_connect_count=%d 
3652,III,wlan_tdls_rx_chan_switch_req_frame(2399) Offchan not enabled, vdev_id=%d, offchan_enabled=%d, offchan_temp_disabled=%d 
3651,I,wlan_tdls_rx_chan_switch_req_frame : frame parsing failed!! parse_status = %u 
3650,III,wlan_tdls_rx_chan_switch_req_frame(2420) Channel switch request received with wrong BSSID mac[0]=0x%x, mac[4]=0x%x, mac[5]=0x%x 
3649,,wlan_tdls_rx_chan_switch_req_frame() chan_info NULL return 
3648,III,wlan_tdls_rx_chan_switch_req_frame()switch_time=%d time_to_tbtt=%d duration=%d 
3647,III,wlan_tdls_rx_chan_switch_req_frame()Delete & Create ocs_ch_req: switch_time=%d time_to_tbtt=%d duration=%d 
3646,IIII,wlan_tdls_rx_chan_switch_req_frame()tdls=%p channel=%d duration=%d time_to_tbtt=%d 
3645,IIII,wlan_tdls_rx_chan_switch_resp_frame(2651) Cannot process channel switch rsp frame, vdev_id=%d, tdls ptr=0x%p, offchan_peer=%p, peer_connect_count=%d 
3644,IIIIIIII,wlan_tdls_rx_chan_switch_resp_frame(2658) status_code=%d, chan_switch_resp_pending=%d, time_to_tbtt=%d, offchan_active=%d link_pause_incomplete = %d              curr_chan(mhz)=0x%x BSS(mhz)=0x%x peer_paused=0x%x 
3643,,wlan_tdls_rx_chan_switch_resp_frame(2664) Do not respond to chan switch resp offchan_init is FALSE 
3642,IIIII,wlan_tdls_rx_chan_switch_resp_frame()abort_channel_change:%d status_code=%d peer_switch_time=%d switch_time=%d switch_timeout=%d 
3641,II,wlan_tdls_rx_chan_switch_resp_frame(2744) Either offchan not active or no TDLS peer, offchan_active=%d, entry=0x%x 
3640,IIIIII,wlan_tdls_scan_evt_handler(3353) event type=0x%x, restore_offchan_state=%d, offchan_active=%d, scan_started=%d, tdls->scan_move_on_chan_req=0x%x, offchan_init=%d 
3639,III,wlan_tdls_scan_evt_handler()No need to handle scan event TDLS handle:%p event type=%d tdls state:%d 
3638,I,wlan_tdls_scan_evt_handler: scan started scan ev type: 0x%x 
3637,II,wlan_tdls_scan_evt_handler: scan ended scan ev type: 0x%x num of Pending scan req = %d 
3636,III,wlan_tdls_send_chan_switch_req_frame(2143) tdls_peer=0x%x, target_channel=%d, sec_chan_offset=%d 
3635,II,wlan_tdls_send_chan_switch_req_frame(2148) TDLS peer is NULL! target_channel=%d, sec_chan_offset=%d 
3634,II,wlan_tdls_send_chan_switch_req_frame(2165) No buffer! target_channel=%d, sec_chan_offset=%d 
3633,II,wlan_tdls_send_chan_switch_req_frame(2175) tid=%d, TX send_status=%d 
3632,III,wlan_tdls_send_chan_switch_resp_frame(2251) TDLS peer is NULL! wlan peer=0x%x, switch_time=%d, status_code=%d 
3631,III,wlan_tdls_send_chan_switch_resp_frame(2268) No buffer! wlan peer=0x%x, switch_time=%d, status_code=%d 
3630,IIIIII,wlan_tdls_send_chan_switch_resp_frame(2279) vdev_id=%d, switch_time=%d, status_code=%d, is_peer_responder=%d, is_peer_TIDQs_paused=%d, TX send_status=%d 
3629,IIIII,wlan_tdls_stats_timer_handler MAC: 0x%x 0x%x nf: %d peer_avg_rssi: %d threshold: %d 
3628,IIII,wlan_tdls_stats_timer_handler send teardown to peer: 0x%x 0x%x peer_avg_rssi: %d threshold: %d 
3627,IIIII,wlan_tdls_unit_test(128) no_of_tdls_base_pause=%d, no_of_tdls_offchan_pause=%d, duration=%d, total_offchan_time=%d, num_args=%d 
3626,I,wlan_tdls_update_tdls_peer_table: Failed to get index for the peer from tdls peer table. Index = %d 
3625,II,wlan_tdls_update_tdls_peer_table: pausing TIDQs, entry=0x%x, wlan_peer=0x%x 
3778,I,wlan_tdls_enter_exit_buf_sta_role() enter: %d 
3777,,Cannot handle PTR completion as wal peer is NULL 
3776,III,wlan_tdls_ptr_tx_completion() status: 0x%x peer: %p abf = %p 
3775,IIII,TDLS_DBGID_UAPSD_STA_PS_EVENT_HANDLER  event type: %d, status = %d ps_handle = %p, peertype: %d 
3774,I,TDLS_DBGID_UAPSD_STA_PS_EVENT_HANDLER  Don't handle event tdls_peer = %p sleep_sta_handle = %p 
3773,III,wlan_tdls_sleep_sta_ps_event_handler()  WLAN_PS_STA_PAUSE_COMPLETE: vdev_id = %d event->status: %d continous noack_cnt = %d 
3772,I,TDLS_DBGID_UAPSD_STA_PS_EVENT_HANDLER  WLAN_PS_STA_UNPAUSE_COMPLETE failed status = %d 
3771,,wlan_tdls_sleep_sta_ps_event_handler() WLAN_PS_STA_UNPAUSE_COMPLETE event when peer is in pause state !!! 
3770,I,wlan_tdls_uapsd_handle_pti_from_peer() peer_type: 0x%x tdls_peer not found return 
3769,I,Dont handle new pti frame: prev ptr completion pending (same dialog token = %d) 
3768,IIII,wlan_tdls_uapsd_handle_pti_from_peer() dialog_token: %d peer_paused: %d ps_sleep_sta_handle: 0x%x pti_frame_recvd: %d 
3767,II,wlan_tdls_uapsd_pti_frame_recvd() Not a tdls peer : peer: %p peer_type: 0x%x 
3766,III,wlan_tdls_uapsd_pti_frame_recvd() tdls_peer: %p ps_sleep_sta_handle: 0x%x is_pti_frame_recvd: %d 
3765,I,wlan_tdls_uapsd_send_ptr_frame() vdev_id: %d 
3764,,wlan_tdls_uapsd_send_ptr_frame() (!abf) failed to get ptr action frame buffer 
3763,IIII,wlan_tdls_uapsd_send_ptr_frame() vdev_id = %d status = %d dialog token = %d is_peer_paused: 0x%x 
3762,,TX completion is not received for Prev PTR. Dont Queue another PTR 
3761,II,wlan_tdls_uapsd_sleep_sta_handle() Not a Tdls (peer=%p) peer_type = %d 
3760,III,wlan_tdls_uapsd_sleep_sta_handle() return NULL: peer = %p peer type = %d tdls_vdev = %p 
3779,II,WLM config, cur:%d, wmi:%d
 
3780,I,WLM found no entry in vdev: %x
 
3781,IIII,WLM deliver notif, flags:%x,lvl:%d,ul:%d,dl:%d
 
3780,I,WLM found no entry in vdev: %x
 
3782,I,WLM vdev evt handler: %x
 
3780,I,WLM found no entry in vdev: %x
 
3783,I,WLM deregistered by module: %x
 
3780,I,WLM found no entry in vdev: %x
 
3784,I,WLM registered by module: %x
 
3780,I,WLM found no entry in vdev: %x
 
3785,I,WLM vdev had been initialized: %x
 
3788,IIIIII,WLM CONFIG unit test input: type=%d, args[1]=%d,args[2]=%d,args[3]=%d,args[4]=%d,args[5]=%d 
3787,I,wlan_vdev_latency_config_wmi_test entry:%d
 
3786,I,wlan_wlm_get_stats entry:%d
 
3789,III,WMI_EVENT_ALLOC_FAILURE vdev_id = %d EventId = 0x%x AssocId/VdevMap = 0x%x 
3790,II, WMI_EVENT_ALLOC_FAILURE EventId = 0x%x AssocId/VdevMap = 0x%x 
3789,III,WMI_EVENT_ALLOC_FAILURE vdev_id = %d EventId = 0x%x AssocId/VdevMap = 0x%x 
3791,IIIIII,WMI_CHAN_INFO_EVT chan_tx_pwr_tp = %d, rx_frm_cnt = %d, my_bss_rx_cycle_cnt = %d, rx_11b_mode_data_dur = %d, tx_frm_cnt = %d, mac_clk_mhz = %d 
3792,IIIIIII,WMI_CHAN_INFO_EVT err_code = %d, freq = %d, cmd_flags = %d, nf = %d, rx_clr_cnt = %d, cycle_cnt = %d, chan_tx_pwr_range = %d 
3793,II,WMI_CHAN_INFO_EVENT_ALLOC_FAILURE  EventId = 0x%x chan_freq = 0x%x 
3794,,BEACON_EVENT_SWBA_SEND_FAILED 
3795,II,drop mgmt as size:%d,limit:%d 
3796,II,WMI handle send WMI evt msg, evt_id:0x%x, evt_len:0x%x
 
3797,II,WMI handle send WMI evt msg fail, evt_id:0x%x, evt_len:0x%x
 
3798,,WMI handle send wmi evt msg in RT 
3799,,WOW send initial wakeup wmi cmd 
3800,IIII,wlan_debug_mesg_flush_compete stall_type:%d vdev_bmap:%d reason_code1:%d reason_code2:%d 
3801,IIIII,bdf_version = %x ref_design_id=%x, customer_id=%x, project_id=%x, board_data_rev=%x 
3802,III,wow_assert_tmr wow_asserted @ %d, wow_continus_nack_period %d first_wow_nack_time %d 
3803,,Excessive time bw consecutive NACKs 
3804,I,wow_assert_tmr start  %d 
3805,,WMI_WOW_SET_ACTION_WAKE_UP_CMDID variable length NULL returning 
3805,,WMI_WOW_SET_ACTION_WAKE_UP_CMDID variable length NULL returning 
3805,,WMI_WOW_SET_ACTION_WAKE_UP_CMDID variable length NULL returning 
3806,III,WOW wake event bitmap input:%x pdev:%x vdev:%x 
3807,II,WOW enable wake event vdevId=%d isAdd=%d 
3808,I,WOW host awake ind wake reason %x 
3809,I,wow_acked @ %d 
3810,,Wow error mac operation fail 
3811,I,WOW error mgmt tx pending %x 
3812,II,WOW event flag: idx=%d evt %x
 
3813,I,WOW CMD hdlr pause=%d 
3814,,WOW awake complete 
3815,I,WOW enter failure, wow state:%d 
3816,,WOW enter success. 
3817,I,WOW event comp handle  msg_status=%d 
3812,II,WOW event flag: idx=%d evt %x
 
3818,I,WOW data Enable failed: tx pending:%d 
3819,I,WOW data handle for msgId %d 
3820,II,WOW_IBSS_VDEV_ALLOW status = 0x%x peer_count = 0x%x 
3821,I,WOW_AP_VDEV_DISALLOW  allow_status = 0x%x 
3822,I,WOW_P2PGO_VDEV_DISALLOW  0x%x 
3823,I,WOW_STA_VDEV_DISALLOW  0x%x 
3824,I, Auto detect: Failure handling - Sending Event to Host - reason id %d 
3825,II,Not in wow entered state wow state=%d wake reason=%d 
3826,,WOW data wakeup host msg to RT 
3827,,WOW handle wakeup host msg in RT 
3828,III,WOW wakeup host wake reason=%d, packet_len:%d, len:%d 
3829,I,HTT msg type %d 
3830,II,HTT msg saved failure:%d, type %d 
3857,II,GetDpdLoopbackInfoHandler phyId %d chainMask 0x%x 
3856,II,GetDpdLoopbackInfoHandler sending response phyId %d chainIdx 0x%x 
3855,II,GetLUTTablesHandler(Phy:%d, Option:%d)
 
3854,,GetLUTTablesHandler pCmdStream NULL
 
3853,I,GetPowerTableHandler(Phy:%d)
 
3852,,GetPowerTableHandler: pCmdStream = NULL
 
3851,III,NEWXTALCALPROCHandler start phyid = %d, TrimValue = %d, ctrlFlag = %x
 
3850,I,NEWXTALCALPROCHandler readback is not same with the setting value read back trim = 0x%x 
3849,I,NEWXTALCALPROCHandler readback fail status = 0x%x 
3848,I,NEWXTALCALPROCHandler end status = %d
 
3847,I,NEWXTALCALPROCHandler store best cal value = %d
 
3846,II,NEWXTALCALPROCHandler get the trim range min = %d, max = %d
 
3845,IIII,TpcGenTool: Received parameters chanFreq : %ld nss : %d mode : %d beamforming %d 
3844,IIIIII,TpcGenTool: Received parameters chainNum: %d chainMask: %d rate: %d ctl: %d sarIndex: %d ctlrd : %x 
3843,II,TpcGenTool: sar verion %d sar flags %d 
3842,I,TpcGenTool: Power value %d 
3841,,bdGetSizeHandler
 
3840,III,bdReadHandler: bdSize %d, offset 0x%x, size %d
 
3839,I,error in bdReadHandler: status %d
 
3838,II,combCalGroupHandler(): phyId = %d; cmdid = %d 
3837,III,noiseFloorReadHandler phyid = %d, freq = %d, chainmask = %x
 
3836,IIII,nfValues[0,1,%d] = %d,%d,%d
 
3835,,Rx Gain Control
 
3834,II,Rx PDADC Value Query Req Handler(RequestId = %d, BurstId = %d)
 
3833,IIII,RxQueryStatus = %d, arrayLen = %d, numOfPdAdcValues %d  pParms->requestId %d
 
3832,II,tpc packet Log Enable Handler(phyId = %d, logEnBitMap = %d)
 
3831,IIII,Tx Gain Control:Chain %d, Gain %d, dacGain %d, forceCal %d 
 
3869,,genCALData
 
3868,I,nextCAL idxChainNew 1 %d greater than MAX_RXG_CAL_CHANS
 
3867,I,nextCAL idxChainNew 2 %d greater than MAX_RXG_CAL_CHANS
 
3866,I,nextCAL nextCAL 3 %d greater than MAX_RXG_CAL_CHANS
 
3865,I,nextCAL nextCAL 4 %d greater than MAX_RXG_CAL_CHANS
 
3864,II,HOST->rxGainCal: radioID %d, Chain %d 
3863,I,send2HostNextRxCal chanIdx 1 %d greater than MAX_RXG_CAL_CHANS
 
3862,I,send2HostNextRxCal chanIdx 2 %d greater than MAX_RXG_CAL_CHANS
 
3861,III,Before_on:  nextLoopRxCal b-c-c %d %d %d
 
3860,IIIII,ON: minCCAThreshold %d,PNFdBm %d, PNFdBr %d, rssiDBr %d temp %d
 
3859,I,siglDoneRsp calChanIdx 1 %d greater than MAX_CAL_CHANS
 
3858,I,siglDoneRsp calChanIdx 2 %d greater than MAX_CAL_CHANS
 
3913,III,band:%d,gainIdx:%d, temp:%d 
3913,III,band:%d,gainIdx:%d, temp:%d 
3912,IIIII,freq %d gIdx %d dacGain %d paCfg %d chMask %d
 
3911,,here 2 
3910,,here 1 
3909,,More than 5 calibration failures, aborting 
3908,II,greenTxGainIndGrpFlag2G:%d,greenTxGainIndGrpFlag5G:%d 
3907,II,calPwrTargetsConfigured_2G:%d calPwrTargetsConfigured_5G:%d 
3906,IIII,gtx2G[0]: %d gtx2G[1]: %d gtx2G[2]: %d gtx2G[3]: %d 
3905,IIII,gtx5G[0]: %d gtx5G[1]: %d gtx5G[2]: %d gtx5G[3]: %d 
3904,III,Max_Glut_Map[%d][%d]:%d 
3903,,Green TX combined grp gain Idx meas pts exceeds limit for TPC_5G !!! 
3902,II,tpcCfg[TPC_2G].gainIdx[1][%d]):%d 
3901,II,tpcCfg[TPC_5G].gainIdx[1][%d]):%d 
3900,II,tpcCfg[TPC_2G].tgtPwrEst[1][%d]):%d 
3899,II,tpcCfg[TPC_5G].tgtPwrEst[1][%d]):%d 
3898,,Green TX combined grp gain Idx meas pts exceeds limit for TPC_2G !!! 
3897,,numValidMeas is 0. it is abnormal 
3896,I,startHi=%d 
 
3895,II,Skipping compare of gainIdx %d and %d 
3894,IIII,Got fewer than MIN_CAL_GAINS_REQUIRED_4_GLUT:%d maxNumGainIdxToUse:%d Band:%d chan:%d 
3893,IIIII,v3Begin: Band:%d chan:%d startPwrIdxGrp:%d  endPwrIdxGrp:%d numGlutEntries:%d 
3892,IIIIII,k = %d, Idx %d: meas %d, Tgt %d,max_Tgt %d, numGainIndexes %d 
3891,IIII,m:%d numGlutEntries:%d k:%d (numGlutEntries - (k)):%d 
3890,I,PICK %d 
3889,IIII,Moving up m:%d numGlutEntries:%d k:%d (numGlutEntries - (k)):%d 
3888,II,Sending to host freq2G %d, freq5G %d
 
3887,III,Sending to host freq2G %d, freq5G %d, chain %d 
3886,IIII,gain %d pwr %d numChain %d numCalpt %d
 
3885,,Cal fail due to slope check, returning with error
 
3884,,Cal fail due to Fewer_Glut_Entries, returning with error
 
3881,I,Wait %d ms before measuring power 
3883,II,postProcessingOLPCCALData_gtx: %p,postProcessingOLPCCALData:%p 
3882,I,postProcessingOLPCCALData_ptr:%p 
3881,I,Wait %d ms before measuring power 
3880,II,###########chIdx %d, temp %d 
3879,I,GainIdx = %d 
3878,I,Using max pdadc target as %d 
3874,II,Mid range power check failed cur %d, prev %d
 
3873,II,low/hi range power check failed cur %d, prev %d
 
3877,IIIIII,GreenTXEn t1: %d t2: %d t3: %d t4: %d sl %d slHithresh %d
 
3876,IIII,band:%d, gainIdx:%d, skipSlope:%d,skipSlope_gtx_bndry:%d 
3875,III,skipping slope tpcFlag = %d, greentx = %d gainIdx = %d 
3871,I,slope Failed %d
 
3874,II,Mid range power check failed cur %d, prev %d
 
3873,II,low/hi range power check failed cur %d, prev %d
 
3872,IIIIII,t1: %d t2: %d t3: %d t4: %d sl %d slHithresh %d
 
3871,I,slope Failed %d
 
3870,III,Got Power from host %d, Read pdadc %d, nextAction %d
 
3909,,More than 5 calibration failures, aborting 
3927,I,available_gainIdxs:%d 
3926,I,Picked limiting gainidx:%d 
3925,III,Picked gainidx:%d from delta_measPwrlow :%d 
3924,II,Picked gainidx:%d  from delta_measPwrhigh :%d 
3923,,Moving up gainidxs to guarantee GLUT count! 
3922,II,currIndx:%d Updated endPwrIdxGrp:%d 
3921,,BAD CAL TARGETs CONFIGURED for 
3920,II,Picked max gainidx:%d from group :%d  
3919,,ERR: BAD CAL TARGETs CONFIGURED for:  
3918,,postProcessingOLPCCALData_gtx 
3917,III,Invalid TPC_GLUT_PWR_MAP_GRP Id ! from Band:%d Chain:%d tgtpwridx:%d 
3916,IIII,tpcCalResult[%d][%d].numValidMeas[%d]:%d 
3915,IIIII,Write to tpcCalPostProcResult[%d][%d].olpc.measPwr[%d][%d]:%d 
3914,II,glutsfilled[%d]:%d 
3929,IIIIII, ftmOnepointCALTxStart freq %d txPwr %d dacGain %d gainIdx %d paCfg %d chMask %d
 
3928,I, tpcPwr measured PWR %d
 
3948,III,TPC_2G i:%d src_GlutEntry:%d dst_GlutEntry:%d 
 
3947,III,TPC_5G i:%d src_GlutEntry:%d dst_GlutEntry:%d 
 
3941,I,ch %d:
 
3945,I,GLUT chn %d: pa gIdx pwr 
 
3942,III,%d %d %d
 
3944,II,dac %d therm %d
 
3943,,PLUT: idx pdadc pwr
 
3942,III,%d %d %d
 
3946,,utfDeviceGenCalData4BrdData_gtx
 
3945,I,GLUT chn %d: pa gIdx pwr 
 
3942,III,%d %d %d
 
3944,II,dac %d therm %d
 
3943,,PLUT: idx pdadc pwr
 
3942,III,%d %d %d
 
3941,I,ch %d:
 
3940,I,tpcPowerOffset2G %d
 
3939,I,tpcPowerOffset5G %d
 
3938,,Invalid PreTxCalGainIdxGrp requested for 2G or 5G!  
3937,,Invalid PreTxCalGainIdxGrp requested for default grp!  
3936,,Invalid PreTxCalGlutPwrMap requested for 2G or 5G!  
3935,,Invalid PreTxCalGlutPwrMap requested for default grp!  
3934,II,power est = %d is2GHz %d
 
3933,I,chanIdx %d
 
3933,I,chanIdx %d
 
3932,,corresponding ctl values are set. 
3931,,ctlvalues are set as 0. 
3930,,call finished - currentRD and CTL values updated 
3951,IIIII,freq %d chainmask 0x%x mode 0x%x tx_gain 0x%x ant_sel 0x%x
 
3950,,CW TONE for chain 0: 
3949,,CW TONE for chain 1: 
3978,III,check_band_chainmask: invalid supported band (phyId %d, boardOpFlags = %d, is2GHz = %d) 
3977,III,check_band_chainmask phyId %d invalid chain 0x%x used, validTxChainmask 0x%x 
3976,,tcmd_BackToBack_tx_complete_timer_handler BACKTOBACK TX still ongoing 
3975,II,tcmd_BackToBack_tx_complete_timer_handler ONE BURST (Burst id: %x, PDADC VALUE %x) 
3974,I,tcmd_BackToBack_tx_complete_timer_handler ALL BURST number of burst %d 
3973,II,tcmd_BackToBack_tx_complete_timer_handler (Burst id: %x, PDADC VALUE %x) 
3972,,tcmd_BackToBack_tx_complete_timer_handler start 
3971,I,tcmd_BackToBack_tx_complete_timer_handler PDADC: %x 
3970,I,tcmd_BackToBack_tx_complete_timer_handler NULL BURST PDADC: %x 
3969,I,tcmd_BackToBack_tx_complete_timer_handler stopping after BURST INDEX %d 
3968,I,tcmd_BackToBack_tx_complete_timer_handler NULL BURST INDEX %d 
3967,II,tcmd_BackToBack_tx_complete_timer_handler BURST INDEX %d Timeout %d 
3966,,tcmd_cont_data_tx_stop poll tx complete interrupt failed 
3965,I,tcmd_cont_data_tx_stop polling count %d 
3964,,tcmd_cont_rx_cmd stopped tx and started timer 
3963,III,STOPPING SINE WAVE TX:(phyId %d, boardOpFlags = %d, tcmd_default_freq = %d) 
3962,II,STOPPING SINE WAVE TX: supported band (chan.phy_mode %d, tcmd_default_freq = %d) 
3961,I,enable wal_pdev_chainmask_algo set txChain to 0x%x 
3956,I,tcmd_rx_start_timer_handler peer delete in progress phyId %d 
3960,,tcmd_set_tx_stop_acknowledged 
3959,I,tcmd_tx_complete_timer_handler phyId %d Tx stopped 
3958,,tcmd_tx_complete_timer_handler phyId %d numTxPkt is 0 existing without restarting timer 
3957,IIIII,tcmd_tx_complete_timer_handler stopping Tx. phyId %d totalPkt %d numTxPkts %d currentTx %d totalToTx %d 
3956,I,tcmd_rx_start_timer_handler peer delete in progress phyId %d 
3955,,tcmd_tx_stop_request 
3954,I,Tx Failed tcmdTxStat.totalPkt = %d 
3953,II,utfTxStartInternal phyId %d starting tcmd_tx_complete_timer, numPkts %d 
3952,II,utfTxStartInternal phyId %d starting tcmd_BackToBack_tx_complete_timer, numPkts %d 
3993,III,tcmd_add_buf_to_free_list: Enter.. tcmd_rx_refill_list_wr_idx=%d ptr_lo 0x%x ptr_hi 0x%x 
3992,II,tcmd refill list is full!!! tcmd_rx_refill_list_rd_idx %d wr_ix %d
 
3991,IIIII,tcmd refill req..refill list is empty!! req_cnt(%d) rd(%d) wr(%d) ptr_lo=0x%x ptr_hi=0x%x
 
3990,II,tcmd refill req..after refill refill_cnt = 0x%x, rd_idx %d
 
3989,IIII,tcmd refill req..before refill req_cnt = 0x%x, tcmd_rx_refill_list_depth = %d, rd(%d) wr(%d)
 
3988,II,tcmd refill..found a entry  ptr_lo 0x%x, ptr_hi 0x%x
 
3987,,tcmd rx detach
 
3986,IIII,tcmd_wal_rx_htt_handler not in Rx mode, exiting! rx_status = 0x%x msdu_cnt =%d mpdu_cnt= %d mac_id = %d
 
3985,IIII,tcmd_wal_rx_htt_handler Enter rx_status = 0x%x msdu_cnt =%d mpdu_cnt= %d mac_id = %d
 
3984,II,tcmd_htt_handler: before processing buf_lo=0x%x, buf_hi=0x%x
 
3983,I,tcmd_htt_handler: pkt_buf = 0x%x 
 
3982,,tcmd_wal_rx_htt_setup: Enter
 
3981,,tcmd do the remote ring setup
 
3980,IIIIII,tcmd_rx_setup (%d):%d,%d,%d,%d,%d 
3979,,tcmd local buf hdlr: HACK- Ath-buf list got re inited, return
 
3994,I,tcmd_wal_peer_free pdev %d 
3996,III,utf_allocram success bufIndex %d nBytes %d avaiBytes %d 
3995,III,utf_allocram failed bufIndex %d nBytes %d avaiBytes %d 
3997,I,_tcmd_peer_delete_conf_msg_hdlr pdevId %d 
3998,IIIII,RATE_UpdateRTSPer: rts_rix 0x%x def_rix 0x%x alt_rix 0x%x curr_rix 0x%x ni_legacy_rate_set 0x%x 
 
3999,IIIIIII,RATECTRL_DBGID_RATE_UPDATE: cur_rate:0x%x rate_code:0x%x currPER:%d lastPER:%d Mbps:%d bw_idx:%x tpc:0x%x 
4000,,Set INVALID!!! RTS Rate Index 
4001,III,RATECTRL_DBGID_RATE_UPDATE: _rcUpdate_HT bw_idx %d nss_idx %d xRetry %d  
4002,IIIIIII,RATECTRL_DBGID_RATE_UPDATE: _rcUpdate_HT is_gtx_tx %d ptx_rc 0x%x ptx_tpc %d nFrames %d retries %d nBad %d flags 0x%x 
4003,IIIIIIII,RATECTRL_DBGID_GTX_UPDATE: UP: tpc=0x%x last_tpc=0x%x curr_PPER:%d curr_RPER:%d rix=0x%x ratecode:%x bw_idx=0x%x (ER,RTS) 0x%x 
4004,IIII,Reset pseudo_per[%d] = %d last_tpc %d updated_tpc %d
 
4005,II,cur_min_tpc updated to %d for bw_idx %d
 
4006,IIIIIIII,RATECTRL_DBGID_GTX_UPDATE: DOWN: (packet 0x%x) tpc=0x%x last_tpc=0x%x curr_PPER=%d curr_RPER %d rix=0x%x ratecode=%x bw_idx=0x%x  
4007,IIIIII,TPC DOWN EVAL / last_tpc %d tpc_step %d,                                                        curr_min_tpc %d gtxTPCMin %d temp %d packets %d
 
4008,III,last_tpc %x curr_ratePer = %d, Reference is GTX = %d 
4009,IIIIIII,GTX disable RATECTRL_DBGID_GTX_UPDATE: 0x%x 0x%x 0x%x 0x%x 0x%x 0x%x 0x%x 
4010,,RATECTRL_DBGID_GTX_UPDATE: GTX disable, BW mis-match  
4011,,RATECTRL_DBGID_GTX_UPDATE: GTX disable, Rate change  
4012,III,RATECTRL_DBGID_GTX_UPDATE: GTX disable vdevtype:%d gtx_enable:%d pause:%d 
4013,IIIIII,RATECTRL_DBGID_GTX_UPDATE: MIN_TPC: 0x%x 0x%x 0x%x 0x%x 0x%x 0x%x 
4014,IIIIIIII,RATECTRL_DBGID_GTX_UPDATE: ENTRY: BW 0x%x / NSS 0x%x / RC 0x%x / TPC 0x%x / MAX_TPC 0x%x / NEW_PPER 0x%x / OLD_PPER 0x%x/ NEW_RPER 0x%x 
 
4015,IIII,RATECTRL_DBGID_GTX_UPDATE 0x%x 0x%x 0x%x 0x%x 
4016,II,RATECTRL_DBGID_GTX_UPDATE 0x%x 0x%x 
4017,IIIII,RATECTRL_DBGID_GTX_UPDATE 0x%x 0x%x 0x%x 0x%x 0x%x 
4018,IIIII,AUTORATE_RESET_USER_START_RATE: peer phymode %d ni_flags 0x%x ht %d vht %d user_start_rate %d 
4019,I,AUTORATE_RESET_ERR: BSS Peer has invalid phymode %d Exiting AutoRate Reset attempt 
4020,II,AUTORATE_RESET_INFO:[VDEV_ID]:%d [USER_START_RATE]:%d 
4021,I,AUTORATE_RESET_ERR: VDEV ID:%d is not an INFRA STA session, no support yet for AUTORATE RESET 
4022,I,AUTORATE_RESET_ERR: VDEV ID:%d OR bss_peer OR pSib is NULL for this VDEV 
4023,I,_RATE_GTX_dbg: INAVLID CMD: %d 
4024,I, g_pRATE->gtxRTMask[2]:%x  
4025,I, g_pRATE->gtxRTMask[1]:%x  
4026,I, g_pRATE->gtxRTMask[0]:%x  
4027,I,gtxBWMask:0x%x  
4028,I,userGtxMask:0x%x  
4029,I,gtxTPCMin:%d  
4030,I,gtxTPCstep:%d  
4031,I,gtxPERMargin:%d  
4032,I,gtxPERThreshold:%d  
4033,III,VDEV ID:%d PDEV ID:%d GTX STATUS:%d  
4034,IIII,_RATE_GTX_dbg: [0]:%d [1]:%d [2]:%d [3]:%d  
4035,I,_RATE_GTX_dbg: VDEV ID:%d wal_vdev is NULL 
4042,IIIIII,DATA_TXRX_DBGID_DUP_CHECK vdev_id = %d tcp_info=0x%x SN=0x%x Len=0x%x last_pn_valid=0x%x offset_winsize=0x%x 
4041,IIIIII,DATA_TXRX_DBGID_DUP_CHECK vdev_id = %d SN=0x%x Len=0x%x valPN=0x%x WalRxCnt=0x%x DataRxCnt=0x%x 
4040,IIII,DATA_TXRX_DBGID_RX_DATA_SEQ_LEN_INFO Invalid Peer vdev_id = %d 0x%x 0x%x 0x%x 
4039,III,DATA_TXRX_DBGID_RX_DATA_SEQ_LEN_INFO Invalid Peer vdev_id = %d 0x%x 0x%x 
4038,IIIII,DATA_TXRX_DBGID_RX_DATA_SEQ_LEN_INFO Invalid Peer vdev_id = %d 0x%x 0x%x 0x%x 0x%x 
4038,IIIII,DATA_TXRX_DBGID_RX_DATA_SEQ_LEN_INFO Invalid Peer vdev_id = %d 0x%x 0x%x 0x%x 0x%x 
4037,IIIIII,DATA_TXRX_DBGID_RX_DATA_SEQ_LEN_INFO Invalid Peer vdev_id = %d 0x%x 0x%x 0x%x 0x%x 
4036,IIII,DATA_TXRX_DBGID_RX_DATA_SEQ_LEN_INFO Inv-frag vdev_id = %d 0x%x 0x%x 0x%x 
4043,IIII,DATA_TXRX_DBGID_REPLAY_CHECK 0x%x KeyId=0x%x oldPN=0x%x newPN=0x%x 
4072,IIIIIII,blockack (pdev=%d): rcvd BAR-tid=%d,SN=0x%x,BAR#=%d,reset=0x%x,ts=0x%x/0x%x 
4071,I,blockack (pdev=%d): trigger reset 
4070,I,%s: Failed to allocate BA peer info
 
4058,II,%s: peer=%p  
4069,III,tid %d state %lld event %d
 
4068,IIII,%s: No HT/QOS/AUTH peer flags vht_support(%u) qos_en(%u) conn_state(0x%x)
 
4067,I,%s: Sending ADDBA req
 
4066,I,%s: Cannot generate ADDBA req
 
4065,I,%s: ADDBA req send successful
 
4064,I,%s: BA negotiation successful
 
4063,I,%s: BA negotiation failed
 
4062,I,%s: BA negotiation stopped
 
4048,I,%s: DELBA send successful
 
4061,I,%s: Sending DELBA
 
4060,I,%s: Teardown started
 
4059,I,%s: Teardown complete
 
4058,II,%s: peer=%p  
4057,III,tid %d state %d event %d
 
4056,IIII,%s:Rejected. HT_VHT(0x%x), QOS(0x%x) AUTH(%x)  
4055,I,ba_policy=%d  
4054,I,fixed resp_code=%d
 
4053,II,%s: Sending ADDBA resp %d
 
4052,I,%s: ADDBA resp generation failed
 
4051,I,%s: Rejecting ADDBA resp %d
 
4050,I,%s: ADDBA rsp send successful
 
4049,I,%s: BA Tearing down
 
4046,I,%s: BA restarting
 
4048,I,%s: DELBA send successful
 
4047,I,%s: BA tearing down
 
4046,I,%s: BA restarting
 
4045,,wal_ba_support_amsdu_in_2g FAILED : provide correct arguments 
4044,,bss is NULL, amsdusupported won't be 0!!!  
4073,IIIIIIIII,htt host_buff_refill_req: SHADOW_RING is EMPTY !!,shd_ring(rd-%d,wr-%d,f_s=%d,b_a=%d,r_i_p=%d,r_b_c=%d), host_ring(rd-%d, wr-%d), req_cnt-%d
 
4075,I,Total num of msdu sent on all flows for %d
 
4074,I,RFS_BATCHING_THRESHOLD:0x%x 
4076,,GCM: Tag mismatch 
4078,IIIIII,CMC_QMIC_UNIT_TEST num_args = %d, args: %d, %d, %d, %d, %d 
4077,III,CMC_QMIC_UNIT_TEST_TIMEOUT  test case = %d, args: %d, %d 
4117,II,CMC_QMIC_SENSOR_REPORT_IND sensor_status = %d, motion_state = %d 
4116,,CMC_QMIC_ERROR_WMI_OUT_OF_BUFFER skip sending wmi event 
4115,III,CMC_QMIC_MSG_CB_RESULT msg_id 0x%x sns_result_t 0x%x sns_err_t 0x%x 
4114,I,CMC_QMIC_ERROR_OUT_OF_RX_BUFFER enable_req 0x%x skipped 
4113,I,CMC_QMIC_ERROR_SEND_QMI_FAILED enable_req error = %d
 
4112,,CMC_QMIC_ENABLE_REQ 
4111,I,CMC_QMIC_ERROR_OUT_OF_RX_BUFFER update_reporting_req 0x%x skipped 
4110,I,CMC_QMIC_ERROR_SEND_QMI_FAILED update_reporting_req error = %d
 
4109,,CMC_QMIC_UPDATE_REPORTING_REQ 
4108,I,CMC_QMIC_ERROR_OUT_OF_RX_BUFFER disable_req 0x%x skipped 
4107,I,CMC_QMIC_ERROR_SEND_QMI_FAILED disable_req error = %d
 
4106,,CMC_QMIC_DISABLE_REQ 
4105,I,CMC_QMIC_IND_CB_RX_NULL_BUF msg_id 0x%x 
4104,IIII,CMC_QMIC_IND_CB_OUT_OF_BUF report_ind instance_id 0x%x timestamp %d motion_state=%d probability %d 
4103,IIII,CMC_QMIC_IND_CB report_ind instance_id 0x%x timestamp %d motion_state=%d probability %d 
4102,IIII,CMC_QMIC_IND_CB_DECODE_ERROR report_ind instance_id 0x%x timestamp %d motion_state=%d probability %d 
4101,III,CMC_QMIC_IND_CB_OUT_OF_BUF error_ind instance_id 0x%x timestamp %d error 0x%x 
4100,III,CMC_QMIC_IND_CB error_ind instance_id 0x%x timestamp %d error 0x%x 
4099,III,CMC_QMIC_IND_CB_DECODE_ERROR error_ind instance_id 0x%x timestamp %d error 0x%x 
4098,I,CMC_QMIC_IND_CB unhandled msg_id 0x%x 
4097,I,CMC_QMIC_ERROR_CB error = 0x%x 
4096,,CMC_QMIC_NOTIFY_CB: no context 
4095,III,CMC_QMIC_NOTIFY_CB service_event:%d pending_close:%d, state:%d 
4094,II,CMC_QMIC_NOTIFY_CB init state %d, handle:%d 
4093,II,CMC_QMI_CLIENT_INIT_FAIL state %d with %d 
4092,II,CMC_QMIC_NOTIFY_CB state %d with %d 
4091,II,CMC_QMIC_SIG_HANDLER rx_msg p_buf = 0x%x, msg_id = %d 
4090,,CMC_QMIC_SIG_HANDLER_DISABLE_RESP failed to disable CMC 
4089,III,CMC_QMIC_SIG_HANDLER_ERROR_IND instance_id = %d, timestamp = %d, error = %d 
4088,,CMC_QMIC_SIG_HANDLER_UPDATE_REPORTING_RESP failed to update CMC 
4087,II,CMC_QMIC_SEND_BUFFER commandId = 0x%x, state = %d 
4086,I,CMC_QMIC_ERROR_SEND_BUFFER ENABLE_SENSOR in state %d 
4085,,CMC_QMIC_ERROR_SEND_BUFFER DISABLE_SENSOR in state %d 
4084,I,CMC_QMIC_RETURN_RECV_BUF p_buf = 0x%x 
4083,I,CMC_QMIC_OPEN in state %d 
4082,I,CMC_QMIC_OPEN_ERROR 0x%x 
4081,II,CMC_QMIC_OPEN in state %d with %d 
4080,I,CMC_QMIC_CLOSE in state %d 
4079,II,CMC_QMIC_DEINIT in state %d, handle:%d 
4120,,OFLDIF no buf available for data HIFCPY 
4119,II,offload status with status buffer:%d,first_wakeup:%d 
4118,,OFLDIF no buf avail for pending HIFCPY 
4121,I,WOW error tx pending %x 
4125,IIIII,WAL_DBGID_CHANNEL_CHANGE_FORCE_RESET: mhz = %d mac_id = %d phy_mode = %d flags = 0x%x rx_stop|tx_stop = 0x%x 
4124,IIII,WAL_DBGID_CHANNEL_CHANGE: mhz = %d mac_id = %d phy_mode = %d flags = %d 
4123,IIIIII,WAL_DBGID_CHANNEL_CHANGE_COMPLETE: mhz = %d mac_id = %d chan_flags = 0x%x wal_flags = %d tx_resumed %d is_lb_cal_pending %d 
4122,, @@@@ Caling DPD SM for home channel  
4151,IIIII,Invalidate Tx DE Cache: cache_idx: 0x%x TID: 0x%x vdev: 0x%x peer: 0x%x ptid: 0x%x 
4150,IIIIIIII,Tx DE Cache: cache_idx: 0x%x TID: 0x%x valid: 0x%x vdev: 0x%x peer: 0x%x cache_vdev: 0x%x cache_peer: 0x%x  cache_tid_q: 0x%x 
4132,I,WAL_DBGID_TX_ARP Enqueue msdu_id:0x%x 
4131,I,WAL_DBGID_TX DHCP msdu_id:0x%x 
4130,IIIII,WAL_DBGID_TX_ARP (WAPI)-msdu=%x,vdev=%d,type=%d,peer=%x,tid=%d 
4129,IIIII,WAL_DBGID_TX_ARP (UAPSD)-msdu=%x,vdev=%d,type=%d,peer=%x,tid=%d 
4127,IIIII,WAL_DBGID_TX_ARP (UPASD)-msdu=%x,vdev=%d,type=%d,peer=%x,tid=%d 
4149,II,WAL_DBGID_PROCESS_4_WAY_HANDSHAKE peer_entry:0x%x msdu_id 0x%x 
4148,III,WAL_DBGID_TX_EAPOL_PKT type:0x%x tid:%d thread_id:%d
 
4147,,wapi_m2_frame  
4146,,wapi_m4_frame  
4145,IIIIII,WAL_DBGID_TX_EAPOL_KEY KeyInfo(type:%d ack:%d secure:%d)-ts=%x,peer=%x,flags=%x 
4144,III,WAL_DBGID_SECURITY_PM2_QUEUED-ts=%x,peer=%x,flags=%x 
4143,,WAL_DBGID_SECURITY_PM2: register for WAPI M2 rekey compl 
4142,III,WAL_DBGID_SECURITY_PM4_QUEUED-ts=%x,peer=%x,flags=%x 
4141,III,WAL_DBGID_SECURITY_GM2_QUEUED-ts=%x,peer=%x,flags=%x 
4140,I,WAL_DBGID_SECURITY_ALLOW_DATA peer:0x%x (Queue_G2_PTK_Installed_Set_Flag) 
4139,III,WAL_DBGID_SECURITY_PMx_QUEUED-ts=%x,peer=%x,flags=%x 
4138,III,WAL_DBGID_SECURITY_GM1_QUEUED-ts=%x,peer=%x,flags=%x 
4137,I,WAL_DBGID_SECURITY_ALLOW_DATA peer:0x%x (Queue_G1_PTK_Installed_Set_Flag) 
4136,IIIIII,peer_key_set:ts=%x,peer=%x,flags=%x,FC=0x%x,keyid=%d,mc=%d 
4135,I,WAL_DBGID_SECURITY_ALLOW_DATA peer:0x%x (Evt_Key_Set_GTK_G1_Queued_Set_Flag) 
4134,I,WAL_DBGID_SECURITY_PM4_SENT Tx_Compl_Status:%d 
4133,I,WAL_DBGID_SECURITY_ALLOW_DATA peer:0x%x (M4_Tx_Compl_Set_Flag) 
4132,I,WAL_DBGID_TX_ARP Enqueue msdu_id:0x%x 
4131,I,WAL_DBGID_TX DHCP msdu_id:0x%x 
4130,IIIII,WAL_DBGID_TX_ARP (WAPI)-msdu=%x,vdev=%d,type=%d,peer=%x,tid=%d 
4129,IIIII,WAL_DBGID_TX_ARP (UAPSD)-msdu=%x,vdev=%d,type=%d,peer=%x,tid=%d 
4128,I,TX: TDLS frame: action code = 0x%x 
4127,IIIII,WAL_DBGID_TX_ARP (UPASD)-msdu=%x,vdev=%d,type=%d,peer=%x,tid=%d 
4126,II,WAL_DBGID_PROCESS_4_WAY_HANDSHAKE peer_entry:0x%x msdu_id:0x%x 
4154,II,HCM HWM event posted bin_idx = %d bin_ptr->cur %d 
4153,II,hcm_vdev_id already allocated vdev_id %d hcm_vdev_id %d 
4152,I,hcm_vdev_id already deallocated for vdev_id %d 
4209,IIIIII,ROOT BIN        curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4208,IIIIII,VDEV_0 BIN      curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4207,IIIIII,VDEV_1 BIN      curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4206,IIIIII,VDEV_2 BIN      curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4205,IIIIII,DROPPED BIN     curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4204,IIIIII,VDEV0_BE_AC     curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4203,IIIIII,VDEV0_BK_AC     curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4202,IIIIII,VDEV0_VI_AC     curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4201,IIIIII,VDEV0_VO_AC     curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4200,IIIIII,VDEV0_PWRSAVE   curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4199,IIIIII,VDEV0_NODROP    curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4198,IIIIII,VDEV0_MCAST     curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4197,IIIIII,VDEV1_BE_AC     curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4196,IIIIII,VDEV1_BK_AC     curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4195,IIIIII,VDEV1_VI_AC     curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4194,IIIIII,VDEV1_VO_AC     curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4193,IIIIII,VDEV1_PWRSAVE   curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4192,IIIIII,VDEV1_NODROP    curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4191,IIIIII,VDEV1_MCAST     curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4190,IIIIII,VDEV2_BE_AC     curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4189,IIIIII,VDEV2_BK_AC     curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4188,IIIII,VDEV2_VI_AC     curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4187,IIIIII,VDEV2_VO_AC     curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4186,IIIIII,VDEV2_PWRSAVE   curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4185,IIIIII,VDEV2_N0DR0P    curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4184,IIIIII,VDEV2_MCAST     curr %5d 	 min %5d 	 pbb %5d 	 dropcnt %5d 	 pbbdropcnt %5d 	 preallocnt %5d 
 
4183,,HCM reset drop count 
 
4182,I,stat : %d 
4182,I,stat : %d 
4181,I,cbf_20[i] = %d
 
4180,I,cbf_40[i] = %d
 
4179,I,cbf_80[i] = %d
 
4178,IIIII,WAL_PDEV_SUSPEND_REQ req = %d, reason = %d, is_pdev_pause = %d, force_sync = %d, resume_inline = %d 
4177,,releasing antenna pdev allready suspended 
4176,I,WAL_PDEV_SUSPEND: Before clearing RXPCU flt reg, curr_filter:0x%x
 
4175,II,PDEV_SUSPEND (pdev=%d): rx suspend failed after reset-rx=%d 
4174,,releasing antenna at pdev suspend 
4173,II,WAL_PDEV_RESUME_REQ req = %d, is_pdev_pause = %d 
4172,,Don't reset as CHIP IS IN POWER DOWN STATE 
4171,IIII,PDEV_RESET (pdev=%d): reset end-rx=%d,tx=%d,reset=%d 
4170,,_wal_pdev_debug_reg_dump pdev found NULL 
 
4169,IIII,_wal_pdev_debug_reg_dump invoked for pdev_id=%d logview=%d route_type=%d reason_code=%d
 
4168,I,_wal_pdev_debug_reg_dump route_type=%d support un-available 
 
4167,III,RXPCU WDOG error interrupt on MAC-%d, mask 0x%x, total count 0x%x
 
4166,III,TXPCU WDOG error interrupt on MAC-%d, mask 0x%x, total count 0x%x
 
4165,III,TXDMA WDOG error interrupt on MAC-%d, mask 0x%x, total count 0x%x
 
4164,III,RXOLE WDOG error interrupt on MAC-%d, mask 0x%x, total count 0x%x
 
4163,III,TXOLE WDOG error interrupt on MAC-%d, mask 0x%x, total count 0x%x
 
4162,III,CRYPTO WDOG error interrupt on MAC-%d, mask 0x%x, total count 0x%x
 
4161,III,RXDMA WDOG error interrupt on MAC-%d, mask 0x%x, total count 0x%x
 
4160,III,PDG WDOG error interrupt on MAC-%d, mask 0x%x, total count 0x%x
 
4159,III,HWSCH WDOG error interrupt on MAC-%d, mask 0x%x, total count 0x%x
 
4158,III,MXI WDOG error interrupt on MAC-%d, mask 0x%x, total count 0x%x
 
4157,III,AMPI WDOG error interrupt on MAC-%d, mask 0x%x, total count 0x%x
 
4156,III,wal_tracer_pdev_event_handler 0x%x wal_pdev->pdev_id 0x%x power_state0x%x 
 
4155,IIIIII,WAL_DBGID_BB_WDOG_TRIGGERED  time_stamp:0x%x,               bb_wdog_status_a: 0x%x, bb_wdog_status_b: 0x%x,               bb_wdog_status_c: 0x%x, bb_wdog_status_d: 0x%x,               g_dbg_num_bb_timeout: 0x%x 
4228,IIII,LOCAL_FRAME_COMP: type=0x%x thread=%d/%d status=%d 
4227,IIIII,WAL_DBGID_TX_MGMT_WMI_FROM_HOST_COMP vdev_id=%d mac_id=%d desc_id=0x%x tx_status=0x%x tid=0x%x 
4226,,WAL_DBGID_TX_MGMT_HTT_FROM_HOST_COMP 
4225,IIIIIIII,WAL_DBGID_TX_MGMT_COMP_DESCID_TYPE_SEQ_STATUS vdev_id=%d mac_id=%d desc_id=0x%x type=0x%x seq_num=%d tx_status=0x%x tid=0x%x abf=0x%x 
4217,II,WAL_DBGID_TX_MGMT_ENQUEUE_FAILED vdev_id = %d tid:%d 
4224,IIIIIII,WAL_DBGID_TX_MGMT_DESCID_TYPE_SEQ_LEN vdev_id=%d mac_id=%d desc_id=0x%x type=0x%x seq_num=%d len=%d status=0x%x 
4223,IIIII,Local data send (tid=%d,%x,%x):ALLOW_DATA unset-peer=%x,flags=%x 
4222,I, Local data send: Tid doesnt exist. Alloc tid tidnum = %d 
4221,,Local data send: use default tid 
4220,I, No data TID exist, return tid_del_in_prog_bmap:%d 
4219,IIIIIII,WAL_DBGID_TX_MGMT_DESCID_TYPE_SEQ_LEN local data vdev_id=%d mac_id=%d desc_id=0x%x type=0x%x seq_num=%d len=%d status=0x%x 
4218,II,MGMT_TX_WMI_FROM_HOST flags = %x, is_wmi = %d 
4217,II,WAL_DBGID_TX_MGMT_ENQUEUE_FAILED vdev_id = %d tid:%d 
4216,IIIIIIII,WAL_DBGID_TX_MGMT_DESCID_SEQ_TYPE_LEN vdev_id=%d mac_id=%d des_id=0x%x seq_num=0x%x type=0x%x len=0x%x status =0x%x flags=0x%x 
4215,IIIII,WAL_DBGID_MGMT_TX_FAIL vdev_id=%d, err_code=%x, desc_id=%d, status=%d, fc[0]=%x 
4215,IIIII,WAL_DBGID_MGMT_TX_FAIL vdev_id=%d, err_code=%x, desc_id=%d, status=%d, fc[0]=%x 
4214,II,WAL_DBGID_MGMT_TX_FAIL vdev_id = %d  0x%x 
4213,II,send local buffer fail: status=%x, flags=%x 
4212,IIIIII,Deliver LOCAL buffer sending msg failure: tid=%x,peer=%x,abf=%x,flag=%d,target_thread=%x, is_data:%x 
4211,IIIIII,LOCAL abf completion msg:peer=%x,abf=%x,flag=%d,abf_thread=%x,cur_thread=%d,target_thread=%x 
4210,IIIII,LOCAL abf completion internal,peer=%x,abf=%x,flags=%d,abf_thread=%x,cur_thread=%d 
4234,IIIII,WAL_DBGID_AST_ADD_WDS_ENTRY  0x%x 0x%x 0x%x 0x%x 0x%x 
4234,IIIII,WAL_DBGID_AST_ADD_WDS_ENTRY  0x%x 0x%x 0x%x 0x%x 0x%x 
4234,IIIII,WAL_DBGID_AST_ADD_WDS_ENTRY  0x%x 0x%x 0x%x 0x%x 0x%x 
4233,IIII,WAL_DBGID_AST_UPDATE_WDS_ENTRY 0x%x 0x%x 0x%x 0x%x 
4233,IIII,WAL_DBGID_AST_UPDATE_WDS_ENTRY 0x%x 0x%x 0x%x 0x%x 
4232,IIII,WAL_DBGID_AST_WDS_ENTRY_PEER_CHG  0x%x 0x%x 0x%x 0x%x 
4231,,WAL_DBGID_AST_ENTRY_EXIST WAL_EEXIST 
4230,III,WAL_DBGID_AST_DEL_WDS_ENTRY  0x%x 0x%x 0x%x 
4229,,WAL_DBGID_AST_ENTRY_FULL WAL_ENOSPC 
4292,II,ADDR_TYPE_A: mac_adr_31_0=0x%x, mac_addr_32_47=0x%x 
4291,II,ADDR_TYPE_B peer: mac_adr_31_0=0x%x, mac_addr_32_47=0x%x 
4290,II,ADDR_TYPE_C self: mac_adr_31_0=0x%x, mac_addr_32_47=0x%x 
4289,IIIIII,ar_wal_peer_free_ast_entry: peer %p mac_adr_31_0=0x%x, mac_addr_32_47=0x%x, invalidate=%d, ast_index=0x%x, ast_entry_valid_bmap[ast_index] = 0x%x
 
4288,III,_wal_peer_del_msg_hdlr:  thread_id =%d, peer=%p, be_tid_bmap=0x%x
 
4287,I,_wal_peer_delete_conf_msg_hdlr: peer=%p
 
4286,II,_wal_peer_free: peer = %p, delete_in_progress = %d
 
4285,,_wal_peer_free: send peer del msg to BE to delete all BE tids
 
4284,,_wal_peer_free: Now deleting tids for RT
 
4283,IIIIII,WAL_PEER_UCAST_KEY_SET:ts=%x,peer=%x,flags=%x,FC=%x,key=%d,type=%d 
4282,IIIIII,WAL_PEER_MCAST_KEY_SET:ts=%x,peer=%x,flags=%x,FC=%x,key=%d,type=%d 
4281,I,WAL_DBGID_SECURITY_SAFE_MODE on: %d  
4279,IIIIIII,WAL_PEER_CONN_STATE(%d,%d):ts=%x,peer=%x,flags=%x,FC=%x,type=%d 
4280,I,WAL_DBGID_SECURITY_ALLOW_DATA  peer:0x%x (Set_WalPeer_Conn_State_Set_Flag) 
4279,IIIIIII,WAL_PEER_CONN_STATE(%d,%d):ts=%x,peer=%x,flags=%x,FC=%x,type=%d 
4278,IIIIII,WAL_PEER_SECURITY_ENCR_EN:thread=%d,ts=%x,val=%x,peer=%x,flags=%x,FC=0x%x 
4277,IIIIII,WAL_PEER_SECURITY_ENCR_EN:ts=%x,val=%x,peer=%x,flags=%x,FC=0x%x,key=%d 
4277,IIIIII,WAL_PEER_SECURITY_ENCR_EN:ts=%x,val=%x,peer=%x,flags=%x,FC=0x%x,key=%d 
4276,IIII,ar_wal_peer_deliver_tid_list_msg_to_tac: cmd=%d, peer=%p, tid=%p,tid_bmap=0x%x
 
4275,II,_wal_peer_tac_tid_list_op_msg_hdlr: TID_LIST_OP_DEL_TID peer=%p, tidno = %d
 
4274,I,_wal_peer_tac_tid_list_op_msg_hdlr: TID_LIST_OP_DEL_TID cleared the tid_del_in_prog_bmap for peer=%p 
 
4273,II,_wal_peer_tac_tid_list_op_msg_hdlr: TID_LIST_OP_DEL_TID_BMAP Before Processing..peer=%p, tid_bmap=0x%x
 
4272,IIII,_wal_peer_tac_tid_list_op_msg_hdlr: TID_LIST_OP_DEL_TID_BMAP After Processing.. peer=%p tid_bmap=0x%x tid_list_empty=%d, peer->peer_tid_del_req_cnt = %d
 
4271,I,_wal_peer_tac_tid_list_op_msg_hdlr: TID_LIST_OP_DEL_TID_BMAP peer del in prog, send peer del conf to RT, peer=%p 
 
4270,III,_wal_peer_tac_tid_list_op_msg_hdlr: TID_LIST_OP_INSERT cmd peer=%p, tid=%p tidno=%d
 
4269,,_wal_peer_tac_tid_list_op_msg_hdlr: removing the tid from temp tid list
 
4268,,_wal_peer_tac_tid_list_op_msg_hdlr: OOPS..shouldnt reach here
 
4267,I,_wal_peer_alloc_tid: got tid flush handle for tidno %d
 
4266,I,_wal_peer_alloc_tid: adding tid %d to temp tid list
 
4265,IIII,ar_wal_peer_free_tid_by_bitmap: thread_id=%d,peer %p,tid_bmap=0x%x, delete_in_progress =%d
 
4264,II,ar_wal_peer_free_tid_by_bitmap: sending peer flush cmd to tac tread_id=%d, tid_bmap=0x%x
 
4263,II,ar_wal_peer_free_tid: thread_id=%d, tidno=%d
 
4262,II,ar_wal_peer_free_tid: sending tid DEL message to BE thread thread_id=%d, tidno=%d
 
4261,II,ar_wal_peer_free_tid: sending tid flush cmd to tac thread_id=%d, tidno=%d
 
4260,IIII,ar_wal_peer_tid_flush_by_bitmap_comp_cb: thread_id=%d, peer=%p,delete_in_progress=%d, tid_bmap=0x%x
 
4259,III,ar_wal_peer_tid_flush_by_bitmap_comp_cb: sending TID_DELETE to tac thread_id=%d, peer %p tid_bmap=0x%x 
4258,II,ar_wal_peer_tid_flush_comp_cb: thread_id=%d, tidno=0x%x 
4257,II,ar_wal_peer_tid_flush_comp_cb: sending TID_DELETE to tac thread_id=%d, tid_bmap=0x%x 
4256,II,ar_wal_peer_tidq_empty: thread_id =%d,tidq->tid_num=%d
 
4255,II,_wal_peer_mcast_key_id_update: peer :%0x key_id:%d 
4254,,wal_peer_mcast_cfg AST entry not found for key_id:%d 
4253,III,wal_peer_fill_mcast_key_info: peer :%0x key_id:%d key_id_type:%d 
4252,III,wal_pm_mcast_cfg: enable :%d encr_en:%d decap_type:%d 
4251,,_wal_peer_state_publish: Entry  
4250,II,_wal_peer_state_publish: bytes is %d, less than output size = %d  
4249,IIII,_wal_peer_state_publish: peer_keyid0_ast_index is %d, vdev_id = %d, qos_enabled = %d, ba_tx_state_bmap = %d 
4248,IIIIII,_wal_peer_state_publish: mac_address is %d:%d:%d:%d:%d:%d  
4247,,_wal_peer_state_publish: Exit  
4246,II,_wal_peer_tid_state_publish: bytes is %d, less than output size = %d  
4245,IIII,_wal_peer_tid_state_publish: tid_start_sn is %d, tid_start_pn = %d, tid_win_size = %d, num_pending_mpdus = %d 
4244,IIII,_wal_peer_tid_state_publish: num_ppdus_in_hwq = %d,    ppdu_retries_per_txstatus = %d, short_ppdu_retries_per_txstatus = %d, long_ppdu_retries_per_txstatus = %d 
4243,III,_wal_peer_tid_state_publish: mpdu_in_reorder_list is %d, tid_win_size = %d, tid_last_sn = %d 
4242,II,tx mcs 3d Stats publish :: input buffer size = %d 3d stats buffer size = %d 
4241,II,tx mcs Stats publish :: input buffer size = %d mcs stats buffer size = %d 
4240,II,tx ofdm Stats publish :: input buffer size = %d ofdm stats buffer size = %d 
4239,II,tx cck Stats publish :: input buffer size = %d ofdm stats buffer size = %d 
4238,II,rx mcs 3d Stats publish :: input buffer size = %d 3d stats buffer size = %d 
4237,II,rx mcs Stats publish :: input buffer size = %d mcs stats buffer size = %d 
4236,II,rx ofdm Stats publish :: input buffer size = %d ofdm stats buffer size = %d 
4235,II,rx cck Stats publish :: input buffer size = %d ofdm stats buffer size = %d 
4295,,call to function cmnos_thread_find is NULL 
4294,, Auto detect: Failure handling - Silently trying to rejuvinate.. 
4293,, Auto detect: Failure handling - CRASH. 
4296,IIII,rule_num = %d ,rule_config_lsb 0x%0x , rule_config_msb 0x%0x,filter_id %d 
4297,III,super_rule_num = %d ,rule_mapping 0x%0x ,super_rule_config 0x%0x 
4298,II,Total_rules_configured = %d , Total_filters_configured = %d  
4299,,CCE Rules are not configured 
4300,,****** CCE Rules Info ************* 
4301,,_wal_cce_vdev_down_notif  
4302,III,super_rule_num = %d ,rule_ind 0x%0x , super_rule_config 0x%0x 
4302,III,super_rule_num = %d ,rule_ind 0x%0x , super_rule_config 0x%0x 
4296,IIII,rule_num = %d ,rule_config_lsb 0x%0x , rule_config_msb 0x%0x,filter_id %d 
4296,IIII,rule_num = %d ,rule_config_lsb 0x%0x , rule_config_msb 0x%0x,filter_id %d 
4303,I,In _wpm_cce_config_hw :configuring rules to hw for vdev_id : %d 
4304,I,Disabling CCE : cce_ofld_enable = %d 
4305,I,Enabling CCE : cce_ofld_enable = %d 
4306,II,CCE delete a rule for check_rule_ind :%d , rule_bitmap :%d 
4307,I,CCE delete a rule for filter_no : %d 
4308,II,CCE Filter exists? Filterid : %d , superrule id: %d 
4309,I,CCE: Pool alloc failed for rule number =%d 
4310,I,CCE: Pool alloc failed for filter id =%d 
4311,II,CCE super rule num = %d ,rule_num = %d 
4312,I,super_rule_list handle : 0x%0x  
4313,III,CCE super rule filter_id = %d , super_rule_config =  0x%0x , rule_indication = 0x%0x 
4314,III,CCE super_rule_config= %d , g_super_rule_ring_mask =  0x%0x,super_rule_negate = 0x%0x 
4315,I,CCE rule list : rule_no %d 
4316,,in CCE rule configuration : number of rules present is already out of bound - returning. 
4317,,in CCE rule configuration : rule linked list is emply but bitmap is not empty - filter not configured 
4318,,in CCE rule configuration : No free space, all rules are occupied - filter not configured. 
4319,II,in CCE rule configuration : free rule position: 0x%0x,bitmap = 0x%0x 
4320,II,in CCE rule configuration : mask_match: 0x%0x,rule_config = 0x%0x 
4321,II,returning position %d for bitmap 0x%x 
4321,II,returning position %d for bitmap 0x%x 
4321,II,returning position %d for bitmap 0x%x 
4322,I,in wal_cce : cce_global_ring_mask %d 
4323,I,CCE enable rules with filter_bitmap : 0x%0x 
4324,,List is empty 
4325,,deleting a non-existent rule 
4326,I,CCE skipping delete for shared rule: %d 
4327,II,CCE deleted rule number: %d , rule bitmap - %d 
4328,III,CCE delete rule_no start : %d , rule bitmap - %d, mac id: %d 
4329,,CCE cannot add rule as it exceeds maximum allowed 
4330,,CCE cannot add rule as it exceeds maximum allowed - refcount check 
4331,I,CCE MAC id : %d 
4332,II,wpm_cce_alloc_vdev_rule_ctxt : deallocating memory to rule handle from poolfor vdev : %d,type %d 
4333,,wpm_cce_alloc_vdev_rule_ctxt : allocating memory to rule handle from pool 
4334,I,Set Flags to default value in mac : %d 
4335,,In wal_cce_soc_init : Inited pool memory for rules and super rules 
4341,II,RATECTRL_DBGID_WAL_SET_VDEV_DATA_RX  rc=0x%x data_rc=0x%x 
4340,II,Invalid RC Entry:nss=%x and pdev_max_nss=%x
 
4339,I,wlan_rc_pdev_enable_disable_cck_allowed: rc_cck_rate_allowed = 0x%x 
4338,II,temp_cck_rate_bitmap = 0x%x module_id=%x 
4337,,WHAL_RC_FLAG_TXBF cleared for that BW
 
4336,,WHAL_RC_FLAG_TXBF enabled for that BW
 
4367,I,WAL_DBGID_RX_LOCAL_DROP_LARGE_MGMT  0x%x 
4366,IIIII,RXRESUME-BE-PROC After reaping (pdev=%d): ring=%d, #free_slots=%d, curr_idx=0x%x proc_cnt=0x%x 
4365,II,RXRESUME-BE-PROC: Cannot have unprocessed status at this time,status_buf(0x%x) num_iter_statuses(%d) 
4364,III,BE_PROC: HW_INDX(0x%x), FW_INDX(0x%x), FETCH_INDX(0x%x)
 
4363,IIIIII,WAL_DBGID_RX_REENTRY 0x%x 0x%x 0x%x 0x%x 0x%x 0x%x 
4362,IIIIIII,RXDSR: RING SWITCH (%d->%d) first=%p/%p, num=0x%x next=%p/%p 
4361,IIIIIII,RXDSR: TID SWITCH (%d->%d) first=%p/%p, num=0x%x next=%p/%p 
4360,III,phy error frame: mask0:0x%x mask1:0x%x, att_word:%x 
 
4359,IIIIII,RXDSR:found a duplicate first msdu w/o last.. prev_first(%p) cur_first(%p) num_mpdu(%d) num_msdu(%d) num_msdu_last_mpdu(%d) first_mpdu(%p)
 
4358,IIII,RXDSR: MSDU_DISCARD status_buf %p num_drop = %d num_partial_msdu = %d num_msdu = %d
 
4357,IIIIII,wal_rx_handle_pcu_ovfl: mac-id(%d) ring(%d) #free_slots=%d, Ring index(HW=0x%x, FW=0x%x, fetch=0x%x) 
4356,II,_rx_ring_setp: RX SUSPENDED, Delay ring programming pdev_id(%d),ring_indx(%d)
 
4355,IIIII,RXSUSPEND START (pdev=%d), rx_ring_setup_done(%d), rx_ctxt_flags(0x%X) suspend_mod_bitmap(0x%X), module_id(%d)
 
4354,II,RXSUSPEND pdev(%d) current Rx filter(0x%X) 
4353,II,RXSUSPEND: PCUSTOP failed on pdev(%d)!!. Suspend bitmap =0x%x
 
4352,I,RXSUSPEND (pdev=%d): fail on RXDMA 
4351,IIIIIII,RXSUSPEND SUCCESS (pdev=%d): ring(%d), free_slots(%d), mac_ring_free_slots(%d), HW(0x%x), FW(0x%x), fetch(0x%x) 
4350,IIIIIII,RXSUSPEND FAILED (pdev=%d): fail_code(%d) ring_id(%d), free_slots(%d), HW(0x%x), FW(0x%x), FETCH(0x%x) 
4349,IIIII,RXRESUME START (pdev=%d), rx_ring_setup_done(%d), rx_ctxt_flags(0x%X) suspend_mod_bitmap(0x%X), module_id(%d)
 
4348,I,RXRESUME (pdev=%d), Rx state is neither suspend success nor suspend failed, No op.
 
4347,III,RXRESUME (pdev=%d), Susupend bitmap is non-zero, bitmap(0x%X), module_id(%d)
 
4346,IIIII,RXRESUME SUCCESS: After turning on RER.. ring(%d) #free_slots=%d, Ring index(HW=0x%x, FW=0x%x, fetch=0x%x) 
4345,IIIII,WAL_DBGID_RX_BA_SETUP  0x%x 0x%x 0x%x 0x%x 0x%x 
4344,III,%s: filter0 (0x%x) filter1 (0x%x)
 
4343,IIII,wal_rx_check_remote_ring_starvation: HW_INDX(0x%x), FW_INDX(0x%x), FETCH_INDX(0x%x)
 rr_empty_cnt:%d 
4342,III,rx_ring_process_delayed_ring_setup: ring_indx(%d), pdev_id(%d), ring_flags(0x%x)
 
4371,IIIIII,WAL_DBGID_RX_ARP_FRAME pdev_id:0x%x vdev_id:0x%x src_mac_address_0_31:0x%x src_mac_address_47_32:0x%x dst_mac_address_0_32:0x%x dst_mac_address_47_32:0x%x 
4370,IIIIII,WAL_DBGID_RX_EAPOL_FRAME pdev_id:0x%x vdev_id:0x%x src_mac_address_0_31:0x%x src_mac_address_47_32:0x%x dst_mac_address_0_32:0x%x dst_mac_address_47_32:0x%x 
4369,II,WAL_RX_OFFLOAD: Received an unclassified %s packet, route(%d) 
4368,III,WAL_RX_SET_MSDU_ROUTE: Didnt process any pkt filter list for msdu(0x%x), vdev(0x%x) peer(0x%x) 
4393,I,txq_tid_flush_cb: peer 0x%x deletion in prog 
4392,II,txq_abort_peer_blocked: unblock peer 0x%x bitmap = 0x%x 
4391,III,txop_abort_peer_blocked: peer=0x%x,del=%d,block=%d 
4390,II,txop_abort_peer_blocked: created=0x%x, blocked=0x%x 
4389,IIIIIII,proc_txop_abort: tid=0x%x (%d),flags=0x%x,peer=0x%x,del=%d,block=%d/%d 
4388,I,update_data_queue_mpdu_len: peer=0x%x-delete in prog 
4387,IIII,update_data_queue_mpdu_len: peer=%x,flags=%x,FC=0x%x,keytype=%d 
4386,II,update_data_queue_mpdu_len: peer=%x,non-data tid=%d 
4385,II,update_data_queue_mpdu_len: peer=%x,tid in delete=%d 
4384,IIIIIII,update_data_queue_mpdu_len: peer=%x,flags=%x,FC=%x,tid=%x/%d,qdepth=%d/%d 
4383,IIII,update_data_queue_mpdu_len: mpdu=%x:msdus=%d,len=%d->%d 
4382,III,update_data_queue_mpdu_len: mpdu=%x,msdu_flags=%x,is_enc=%d 
4381,IIIIIIIII,tid(%x, %d): frq_num_mpdus=%d/%d, frq_last_mpdu_msdus=%d, frq_remote_num_msdus=%d, frq_local_num_msdus=%d count=%d tid_count=%d 
4380,II,#### START NEW MPDU (curr=%x, next=%x) #### 
4379,III,idx=%d,msdu=%x,next_mpdu=%x 
4378,IIII,idx=%d,msdu=%x,tmp_mpdu=%x,tmp_mpdu_next=%x 
4377,IIIIIII,idx=%d,msdu=%x,tmp_mpdu=%x,tmp_mpdu_next=%x,counts=%d,%d,%d 
4376,III,tmp_mpdu=%x,tmp_mpdu_next=%x,frq_last_msdu=%x 
4375,IIII,tmp_mpdu=%x,tmp_mpdu_next=%x,frq_first=%x, frq_last=%x 
4374,, reached deaggregation threshold so stop  
4373,IIII,before and after amsdu deaggregation mpdus %d %d %d %d 
4372,IIIIII,tid(%x, %d): frq_num_mpdus=%d, frq_remote_num_msdus=%d, frq_local_num_msdus=%d frq_num_msdus=%d 
4395,I,wal_tx_unit_test: g_delay_sched=%d 
4394,,wal_tx_unit_test FAILED: provide correct arguments 
4424,IIII,status_ring_wmark_reached (pdev=%d,cnt=%d):WHAL=0x%x/WAL=0x%x 
4423,IIIII,WAL_DBGID_TX_BA_SETUP  0x%x 0x%x 0x%x 0x%x 0x%x 
4422,IIIII,slide=%d, credit=%d, subfrms_max=%d, ppdu_bmap=%x-%x 
4421,III,WAL_DBGID_TX_LOG_FRAME_TX_COMPLETE pdev_id:0x%x msdu_id:0x%x comp_type:%d 
4420,IIII,HCM pwrsavebin last pkt comp  bin_idx = %d bin_ptr->cur %d  bin_ptr->local_max_desc_peer_pwrsave %d bin_ptr->max_desc_peer_pwrsave %d 
4419,III,adj_burst_txop (pdev=%d):burst=%d,reg=0x%x 
4418,IIII,adj_burst_txop (pdev=%d):qnum=%d,ac=%d,burst=%d 
4417,III,first flush_failure: pdev_id:%d queue_id:%d vdev_id:%d 
4416,III,first non_flush_failure : pdev_id:%d  queue_id:%d vdev_id:%d 
4415,IIIIIII,TXOP ABORT-pdev=%d,vdev=%d,peer=0x%x,tid=0x%x (flags=0x%x),consecutive failure=%d,misc=0x%x 
4414,, ### TX_ABORT_REASON_TXOP_ABORT ### 
4413,II,seq aborted (%d) due to unexp FES bmap/SSN on queue=%d 
4412,IIII,unexp_fes_bmap (%d,%d): %d, %d 
4411,IIII,unexp_fes_ssn (%d,%d): %d, %d 
4410,II,WAL_DBGID_XCESS_FAILURES  0x%x 0x%x 
4409,IIIIII,pdev=%d, vdev=%d, peer=0x%x, tid=0x%x (flags=0x%x), consecutive failure=%d -> 0 
4408,IIIIIII,pdev=%d,vdev=%d,peer=0x%x,tid=0x%x (flags=0x%x),consecutive failure=%d,kickout thresh=%d  
4407,IIIIII,pdev=%d vdev=%d peer=0x%x consecutive_failure:%d cur_time:%x elapsed_ppdu_fail_time:%x 
4406,IIII,prev_flags:%x cur_flags:%x tid_retryfailure:%x vdevtype:%x 
4405,I, MAX AGG retries reached %d, set BAR  
4404,II,WAL_DBGID_STA_KICKOUT  0x%x 0x%x 
4403,IIIII,ppdu_fail_time:%x current_time:%x delta:%x type:%x rc_flags:%x  
4402,IIII,hwsim-retry:tid=%d,festry:%d,sched_status:%x,flushst:%x  
4401,I,hwsim-retry: remaining SW retry :%d  
4400,III,nonagg-retry:tid=%d,retry=%d,first_attempt_ts=%x 
4399,IIIIII,PDEV_TX_TIMEOUT(pdev=%d,txq=%d):CCA=0x%x(0x%x),elapse=0x%x(0x%x) 
4398,II,PDEV_TX_TIMEOUT (pdev=%d,txq=%d): reset start 
4397,,Fixed rate used, Flush tried frames 
4396,I, Retried BAR for %d times, clear BAR flag 
4428,IIII,pdev=%d,ring=%d,%d paused on RBO burst-unpause (count=%d) 
4427,IIIII,enable assist on pdev=%d,curr@=0x%x,(flush@=0x%x/0x%x),#active=%d 
4426,IIII,term_assist (pdev=%d,txqid=%d): swflush @=0x%x,curr@=0x%x 
4425,IIII,disable assist on pdev=%d,@ts=0x%x,prev@=0x%x (txqid=%d) 
4429,,invalid pdev_id
 
4431,IIIIII,_ar_wal_tx_send_flush_tid(%d): flush-count tried:%d local:%d, host:%d in-swq:%d, total:%d
 
4430,III,wal_peer_flush_tids: msg from thread=%d to pdev=%d bitmap=0x%x
 
4432,II,tx_sched_enable_delay_sched: delay_sched=%d, tid_delay=%d 
4439,,WAL_POWER_STATE_FULL_SLEEP 
4438,,WAL_POWER_STATE_AWAKE 
4437,II,wal_txbf_update_txbfee_filter:en:%d,txbfee_dis_bitmap:%x 
4436,IIII,txbf_peer_setup:SU:bfee=%x,bfer=%x MU:Bfee=%x,bfer=%x 
4434,II,txbf_peer_setup:Txbfer:%x and txbfee count:%x 
4435,IIII,txbf_peer_teardown:SU:bfee=%x,bfer=%x MU:Bfee=%x,bfer=%x 
4434,II,txbf_peer_setup:Txbfer:%x and txbfee count:%x 
4433,II,cbf bw mis-match cv_flags=%x cv_bw=%x
 
4440,IIIIII,_wal_txrx_monitor_pdev_record: type %x rx msdu %x ppdu %x, tx msdu %x ppdu %x phy_mode %d
 
4450,I,WHAL_COEX_PHY_IDLE: Invalid WLAN id(%u) 
4449,IIIIIII,WHAL_COEX_BMH_ISR: Tx(%u) Rx(%u) BmhIntRaw(0x%x) BmhRxMsgRaw(0x%x) BmhInt1Raw(0x%x) invalid_hdr(%u) cont_info_to(%u) 
4448,,COEX_MCI_ISR_IntRaw: COEX MCIBasic Bus Sync Error in MCIM ISR 
4447,,COEX_MCI_ISR_IntRaw: COEX Fatal error: MCI_ISR_IntRaw 
4446,,ERROR_COEX_MCI_GPM: COEX RX_MCI_GPM_FULL_ERR_INT 
4445,,ERROR_COEX_MCI_GPM: COEX GPM_SKIP_ERR_INT 
4444,,ERROR_COEX_MCI_GPM: COEX AHB_ERR_INT 
4443,,ERROR_COEX_MCI_GPM: COEX CCU_ACCESS_ERR_INT 
4442,,COEX_MCI_ISR_IntRaw: SMH ISR overflow 
4441,IIIIII,cxc_dbg:i_mac1(%d),i_mac2(%d) result_mac1(%u) result_mac2(%u) wlan(%u) reg_status(%u) 
4490,I,WHAL_MCI_GPM_SENT: [0x%x] - CAL GRANT 
4489,I,WHAL_MCI_GPM_SENT: GPM Sent [0x%x] -  CAL REQ 
4488,I,WHAL_MCI_GPM_SENT: [0x%x] - CAL DONE 
4487,I,COEX_POLL_BT_CAL_DONE_TIMEOUT: BtCalState(0x%x) 
4486,III,COEX_WHAL_PAUSE: WlanCalState(%u) WlanMciState(%u) BtCalHwPaused(%u) 
4485,III,COEX_RX_MCI_GPM_BT_CAL_REQ: Cal Req state(0x%x) WlanCalState(0x%x) BtCalState(0x%x) 
4484,IIII,COEX_WLAN_CAL_START: BtMciState(0x%x) isFirstCal(%u) HsReqired(%u) WlanCalState(0x%x) 
4483,II,COEX_WLAN_CAL_START: WlanCalState(0x%x) i(%u) 
4482,IIIII,COEX_BtMciState: BtMciState(0x%x) BtCalState(0x%x) WlanCalState(0x%x) RxReqWakeCount(%u) RxRemoteResetCount(%u) 
4481,I,COEX_RESTART_CAL: BtCalState(0x%x) 
4480,I,COEX_GENERIC_ERROR: MCIIntfTimeout(%u) 
4479,II,WHAL_MCI_GPM_SENT: [0x%x] [0x%x]- Version query 
4478,IIII,WHAL_MCI_GPM_SENT: [0x%x] [0x%x] - WLAN Version resp. : Major(0x%x) Minor(0x%x) 
4477,IIII,WHAL_MCI_GPM_SENT: [0x%x] [0x%x]- WLAN Conn Status Report : 5G Status(0x%x) 2G Status(0x%x) 
4476,IIIIIII,WHAL_MCI_GPM_SENT: [0x%x] [0x%x]- WLAN Unused channels : 0x%x 0x%x 0x%x 0x%x 0x%x 
4475,IIII,WHAL_MCI_GPM_SENT: [0x%x] [0x%x]- Status Query : WLAN QueryType(0x%x) Source 0x%x 
4474,III,WHAL_MCI_GPM_SENT: [0x%x] [0x%x] - Disable BT GPM : State(0x%x) 
4473,IIII,WHAL_MCI_GPM_SENT: [0x%x] [0x%x] - BT Update flags : Opcode(0x%x) BT Flags(0x%x) 
4472,IIIII,WHAL_MCI_GPM_SENT: OBSOLETE[0x%x] [0x%x] - BT Pause profile : PauseSlot(0x%x) ProfileBitmap(0x%x) Data(0x%x) 
4471,IIII,WHAL_MCI_GPM_SENT: [0x%x] [0x%x] - WLAN set ACL Inactivity Report : InactivityThresh(0x%x) LinkID(0x%x) 
4470,IIIII,WHAL_MCI_GPM_SENT: [0x%x] [0x%x] - BT remote registry write : Address(0x%x) Value(0x%x) Op(0x%x) 
4469,II,WHAL_MCI_GPM_SENT: [0x%x] [0x%x] - Query BT RXSS Minimum Threshold 
4468,III,WHAL_MCI_GPM_SENT: [0x%x] [0x%x] - Set BT RXSS Minimum Threshold : Threshold(0x%x) 
4467,IIIIII,WHAL_MCI_GPM_SENT: [0x%x] [0x%x] - Sched info trigger : TriggerEnaNum(0x%x) TriggerType(0x%x) LowerBound(0x%x) UpperBound(0x%x) 
4466,IIIII,WHAL_MCI_GPM_SENT: [0x%x] [0x%x] - Send priority config : Op(0x%x) Priority(0x%x) IsRead(0x%x) 
4465,IIII,WHAL_MCI_GPM_SENT: [0x%x] [0x%x] - BT Airtime Stats Req: NumOfDelivery(0x%x) TestInterval(0x%x) 
4464,III,WHAL_MCI_GPM_SENT: [0x%x] [0x%x] - WLAN Status Update : Status(0x%x) 
4463,III,WHAL_MCI_GPM_SENT: [0x%x] [0x%x] - Read BT TX power : LinkId(0x%x) 
4462,III,WHAL_MCI_GPM_SENT: [0x%x] [0x%x] - Limit BT Max TX power : power(0x%x)dbm 
4461,III,WHAL_MCI_GPM_SENT: [0x%x] [0x%x] - Start BT RSSI Reporting: period(0x%x)second 
4460,IIIII,COEX_SENDMSG_QUEUE: MciType(%u)  IsMCIBusPaused(%u) PendingMciMsg(0x%x) SleepOverride(%u) btPmh(%u) 
4459,,NULL: Buffers not allocated 
4458,,BTCOEX_DBG_MCI_2: Trying to power up. due to POWERUP_FAILURE, return 
 
4457,IIIIIII,WAL_COEX_SCHED_INFO: i=%d Prio(%d) Tag(%d) tx(%d) Txp(%d) Link(%d) Dur(%d) 
4456,,BTCOEX_DBG_MCI_2: Calling cxc power down
 
4455,I,BTCOEX_DBG_MCI_2: _whal_mci_powerup Power up WLAN1, and band is %dG
 
4454,II,BTCOEX_DBG_MCI_2: Coex Band setting. WLAN1(%d),  WLAN2(%d)
 
4452,II,ERROR_COEX_MCI_GPM: Drop GPM, Recovery in progress: SWGpmIndex(%u) NumGPM(%u) 
4453,,ERROR_COEX_MCI_GPM: invalid GPM 
4452,II,ERROR_COEX_MCI_GPM: Drop GPM, Recovery in progress: SWGpmIndex(%u) NumGPM(%u) 
4451,IIIIIIII,WAL_COEX_CONT_INFO: Contention[INFO(%u) NACK(%u) RST(%u)]: Prio(%u), LinkId(%u) Tx(%u) Ch(%u) Rssi_pwr(%d) 
4507,IIIIII,COEX_MWS_PA_MUTE: TxG: W(%u),EV1(0x%x),EV2(0x%x),OEV(0x%x)=0x%x, Read=0x%x 
4506,IIII,COEX_MWS_PA_MUTE: [Err] : TestBus:MacDis(0x%x,0x%x),TestBus:0x%x,Type-0:0x%x  
4505,I,COEX_MWS_TYPE2_TX: Byte:0x%x 
4504,,COEX_MWS_TYPE2_TX: TX_FIFO_FLUSH 
4503,,COEX_MWS_TYPE2_TX: TX_FIFO_OVERFLOW 
4502,,COEX_MWS_PA_MUTE: [Info]:Tx_Grant_Config called when CSS is Down 
4501,,COEX_MWS_PA_MUTE: [Info]:MUTE both MACs : Event : PERMANENT_MUTE_ON_WLAN_CRASH 
4500,,COEX_MWS_PA_MUTE: [Info]:MUTE both MACs because WLAN state is CRASH 
4499,II,COEX_MWS_TYPE2_RX: [Warn] Buffer Underflow :Read after delay: init_depth:%d, Data:0x%x 
4498,I,COEX_MWS_TYPE2_TX: BMH.TRC_CTRL.TESTBUS_SELECT: %d [PMH] 
4497,II,COEX_MWS_TYPE2_TX: PMH.TBSel:0x%x --> 0x%x 
4496,I,COEX_MWS_TYPE2_TX: BMH.TRC_CTRL.TESTBUS_SELECT: %d [LMH] 
4495,II,COEX_MWS_TYPE2_TX: LMH.TBSel:0x%x --> 0x%x 
4494,I,COEX_MWS_TYPE2_TX: BMH.TRC_CTRL.TESTBUS_SELECT: %d [LCMH] 
4493,II,COEX_MWS_TYPE2_TX: LCMH.TBSel:0x%x --> 0x%x 
4492,I,COEX_MWS_TYPE2_TX: BMH.TRC_CTRL.TESTBUS_SELECT: %d [MCI] 
4491,II,COEX_MWS_TYPE2_TX: MCI.TBSel:0x%x --> 0x%x 
4520,IIIII,HWSCH_TRACER_LOG: mac(%d), tbus_index(0x%x), dbg_select(0x%x), debug_trace(0x%x.0x%x) 
4519,IIIII,TXPCU_TRACER_LOG: mac(%d), tbus_index(0x%x), dbg_select(0x%x), debug_trace(0x%x,0x%x) 
4518,IIII,RXPCU_TRACER_LOG: mac(%d), tbus_index(0x%x), dbg_select(0x%x), debug_trace(0x%x) 
4517,IIIII,PDG_TRACER_LOG: mac(%d), tbus_index(0x%x), dbg_select(0x%x), debug_trace(0x%x,0x%x) 
4516,IIIII,CRYPTO_TRACER_LOG: mac(%d), tbus_index(0x%x), dbg_select(0x%x), debug_trace(0x%x,0x%x) 
4515,IIII,TXOLE_TRACER_LOG: mac(%d), tbus_index(0x%x), dbg_select(0x%x), debug_trace(0x%x) 
4514,IIII,RXOLE_TRACER_LOG: mac(%d), tbus_index(0x%x), dbg_select(0x%x), debug_trace(0x%x) 
4513,IIII,RXDMA_TRACER_LOG: mac(%d), tbus_index(0x%x), dbg_select(0x%x), debug_trace(0x%x) 
4512,IIIII,TXDMA_TRACER_LOG: mac(%d), tbus_index(0x%x), dbg_select(0x%x), debug_trace(0x%x,0x%x) 
4511,II,CMEM0: src = 0x%08X end = 0x%08X 
4510,II,CMEM1: src = 0x%08X end = 0x%08X 
4509,II,CMEM2: src = 0x%08X end = 0x%08X 
4508,II,CMEM3: src = 0x%08X end = 0x%08X 
4528,IIIIII,MACID=%d-r0=%x,r1=%x hwsch_check_hang(ring=%d): dbg_sel=0x%x,lower=0x%x 
4527,IIII,MACID=%d-r0=%x,r1=%x hwsch_recover_hang(WHAL_HWSCH_HANG_ON_TXPCU_WAIT): ring=%d 
4526,IIII,MACID=%d-r0=%x,r1=%x hwsch_recover_hang(WHAL_HWSCH_HANG_ON_TXPCU_RESPONSE_FRAME_ERROR): ring=%d 
4525,IIIIIII,MACID=%d-r0=%x,r1=%x hwsch_check_hang(reason=%d): dbg_sel=0x%x,upper=0x%x,lower=0x%x 
4524,IIIII,MACID=%d-r0=%x,r1=%x hwsch_recover_hang: ring=%d 
4522,IIII,MACID=%d-r0=%x,r1=%x hwsch_check_hang(reason=%d): no ring stuck 
4523,IIIII,MACID=%d-r0=%x,r1=%x hwsch_check_hang(reason=%d): txpcu reg=0x%x 
4522,IIII,MACID=%d-r0=%x,r1=%x hwsch_check_hang(reason=%d): no ring stuck 
4521,IIIIII,MACID=%d-r0=%x,r1=%x hwsch_recover_hang: ring=%d idle (head=%d,tail=%d) 
4537,I,PDG_SETUP_ERR on MAC=%d  
4536,I,ERRVLD: 0x%x 
4535,I,ERR0: 0x%x 
4534,I,ERR1: 0x%x 
4533,I,ERR3: 0x%x 
4532,I,ERR4: 0x%x 
4531,I,ERR5: 0x%x 
4530,I,GetPendingInterrupts-whalPending:0x%x 
4529,IIIIIII,L2VIC status (pdev=%d):indx=%d,int=0x%x,isr=0x%x,ena=0x%x,pndg=0x%x,status=0x%x 
4538,,poll WCSS_CLK_CTRL_REG_WCSS_CSS_GDSCR/PWR_ON timeout
 
4539,,poll PMM_COMMON_IDLEREQ_CSR/WNOC_IDLE timeout
 
4539,,poll PMM_COMMON_IDLEREQ_CSR/WNOC_IDLE timeout
 
4538,,poll WCSS_CLK_CTRL_REG_WCSS_CSS_GDSCR/PWR_ON timeout
 
4600,IIIII,rxpcu_testbus:0x%x intf_tlv_bitmap:0x%x bcn1_global_cnt:0x%0x ebt_debug:0x%0x phy_intf_tlv_cnt1:0x%0x 
4599,IIIII,phy_intf_tlv_rcvd:0x%x txpcu_intf_tlv_cnt4:0x%x txpcu_intf_tlv_cnt5:0x%0x tbtt_bitmap0:0x%0x last_beacon_tsf:0x%0x 
4598,IIII,mac_idle:0x%x mcmn_isr_p:0x%x mcmn_isr_s4:0x%0x mcmn_isr_s16:0x%0x 
4597,IIII,rxsm_fsm:0x%x dpsm_fsm:0x%x tric_fsm:0x%0x phy_intf_tlv_cnt1:0x%0x 
4596,IIIII,bb_timing_controls1:0x%x bb_timing_controls2:0x%x bb_timing_controls3:0x%0x bb_settling_time:0x%0x bb_find_signal:0x%0x 
4595,IIIII,bb_agc_control:0x%x bb_cca_b0:0x%x bb_multichain_enable:0x%0x bb_gen_controls:0x%0x bb_modes_select:0x%0x 
4594,IIIII,bb_active:0x%x bb_misc_control:0x%x bb_analog_power_on_time:0x%0x bb_tlv_state_history:0x%0x bb_packet_counter:0x%0x 
4593,I,bb_pmi_debug_status:0x%x 
4591,II,cur_global:0x%x cur_tsf:0x%x
 
4590,I,MAC:%d H2S grant timeout in PMM-WLAN MAC_WAKE 
4585,III,phy_off_send:%d phy_idle:%d mac_idle:%d 
4589,II,MAC:%d PMM-WLAN stuck at:0x%x
 
4588,IIII,RRI Restore stuck, current_add:0x%x active:0x%x state:0x%x err_int_status:0x%x 
4592,I,SW_WLAN1_FORCE_IDLE:%d 
4586,III,MAC:%d H2S Grant get: pmm_wlan_off:%d pmm_wlan_on:%d 
4585,III,phy_off_send:%d phy_idle:%d mac_idle:%d 
4591,II,cur_global:0x%x cur_tsf:0x%x
 
4590,I,MAC:%d H2S grant timeout in PMM-WLAN MAC_WAKE 
4585,III,phy_off_send:%d phy_idle:%d mac_idle:%d 
4589,II,MAC:%d PMM-WLAN stuck at:0x%x
 
4588,IIII,RRI Restore stuck, current_add:0x%x active:0x%x state:0x%x err_int_status:0x%x 
4587,I,SW_WLAN2_FORCE_IDLE:%d 
4586,III,MAC:%d H2S Grant get: pmm_wlan_off:%d pmm_wlan_on:%d 
4585,III,phy_off_send:%d phy_idle:%d mac_idle:%d 
4584,II,whal_wmac_clr_rogue_ap_type_by_mask: rogue_ap_bit_mask[%d]: %d 
4583,II,whal_wmac_set_rogue_ap_type: rogue_ap_bit_mask[%d]: %d 
4582,IIIII,mac:%d curr_tsf:0x%08x_0x%08x curr_glob:0x%08x_0x%08x
 
4581,,Sleep Aborted due to close to next TBTT
 
4580,II,Sleep Aborted due to %dus close to curr TBTT, cur_bto:%d
 
4579,II,mac:%d Duration of sleep= %d
 
4578,I,Sleep Aborted due to %dus close to target wake time
 
4577,,Sleep Aborted due to stop wlan_ss fail
 
4576,I,Sleep Aborted due to %dus close to target wake time:%d
 
4575,,IMPS/SW_DTIM Sleep Aborted due to stop wlan_ss fail
 
4574,IIII,set_target_wakeup_time:i:%d m:%d, t:0x%08x_%08x 
4574,IIII,set_target_wakeup_time:i:%d m:%d, t:0x%08x_%08x 
4573,,set_target_wakeup_time fail: table full 
4572,IIIIII,calc_target_wakeup_time:i:%d m:%d left:0x%08x_%08x min:0x%08x_%08x 
4571,I,whal_phy_low_power_entry PMM_AON_INT_RAW_STAT: %X
 
4570,I,mac_id:%d phy_low_power_entry success 
4569,I,whal_wmac_get_rx_chain_mask 0x%x
 
4568,III,MAC:%d LP chain mask:0x%x dtim_synth_in_use:%d 
4567,II,mac:%d Number of chains %d 
 
4566,II,mac:%d RSSI indication %d 
 
4565,II,mac:%d DTIM type %d 
 
4564,II,mac:%d DTIM synth en %d 
 
4563,II,mac:%d RXDMA_GLOBAL_RER:0x%x 
4562,I,mac:%d enter HW-DTIM/IMPS fail
 
4561,,MAC RRI restore error
 
4560,,SW trigger RRI restore success
 
4559,I,mac:%d enter partial awake success
 
4558,II,bcn_cnt:%d, bmiss_cnt:%d 
4557,I,b:0x%08x 
4556,I,mac:%d full wake success
 
4555,I,After WLAN SS stop: MAC0 MAC_MCMN_REG_MCMN_MAC_IDLE 0x%x
 
4548,,Invalid Low Power DTIM type requested
 
4554,,Table generation error
 
4553,,Loading TXPCU Buffer failed
 
4553,,Loading TXPCU Buffer failed
 
4552,I,MAC power down failed, stuck in WAKE state due to pending WAKEUP INTR %x
 
4551,I,mac:%d enter HW-DTIM success
 
4550,I,mac:%d enter SW-DTIM success
 
4549,I,mac:%d enter IMPS success
 
4548,,Invalid Low Power DTIM type requested
 
4547,I,SHADOW_REGISTERS_PMM_SR_LSB 0x%x 
4546,I,wlan_stat %d 
4545,IIII,pwr:%d,rst:%d,last_hw_down_mac_time:0x%08x%08x
 
4544,II,cur_mac_time:0x%08x%08x
 
4543,I,MAC:%d WDOG bite error
 
4542,II,brssi_compensate dtim_rssi_offset:%d sleep:%d
 
4541,III,brssi_compensate bf cur_brssi:%d low_thresh:%d high_thresh:%d
 
4540,III,brssi_compensate af cur_brssi:%d low_thresh:%d high_thresh:%d
 
4662,III,ebt_config mac:%d ebt_en:%d thres:%d
 
4661,II,bcn_filter_config mac:%d mode:%d 
 
4660,I,curr_filter:0x%x
 
4659,III,wmac_int_config mac:%d mode:%d active_msk:0x%x
 
4658,II,en_msk:0x%x dis_mask:0x%x
 
4657,I,curr_mask:0x%x
 
4621,II,mac:%d MAC_MCMN_REG_MCMN_ISR_S4:0x%x
 
4620,II,mac:%d MAC_MCMN_REG_MCMN_IMR_S4:0x%x
 
4619,II,mac:%d MAC_MCMN_REG_MCMN_ISR_S16:0x%x
 
4618,II,mac:%d MAC_MCMN_REG_MCMN_IMR_S16:0x%x
 
4617,II,mac:%d MAC_MCMN_REG_MCMN_ISR_S2:0x%x
 
4616,II,mac:%d MAC_MCMN_REG_MCMN_IMR_S2:0x%x
 
4656,II,mac:%d MAC_MCMN_REG_MCMN_ISR_RX_OK:0x%x
 
4655,II,mac:%d MAC_MCMN_REG_MCMN_IMR_RX_OK:0x%x
 
4654,I,mac:%d PPDU_END is not SET 
4653,II,wmac_pwr_config mac:%d pwr cfg mode:%d
 
4652,II,pmm_wlan_get_sm_state mac:%d pmm_wlan state:0x%x
 
4652,II,pmm_wlan_get_sm_state mac:%d pmm_wlan state:0x%x
 
4651,II,pmm_wlan_set_h2s_req mac:%d set h2s_req thres:%d
 
4650,I,pmm_wlan_clear_h2s_req mac:%d clr h2s_req
 
4649,IIII,mac:%d flag:0x%x next_wakeup:0x%08x_%08x
 
4648,IIIII,mac:%d next_tbtt:0x%08x_%08x tsf_offset:0x%08x_%08x
 
4647,IIII,mac:%d sleep_slop:%d beaconPeriod:0x%08x_%08x
 
4646,III,mac:%d cur_tsf:0x%08x_%08x
 
4645,III,mac0: dbg_reg1: 0x%x, dbg_reg2: 0x%x, pmm_sm:0x%x
 
4644,III,mac1: dbg_reg1: 0x%x, dbg_reg2: 0x%x, pmm_sm:0x%x
 
4643,,poll RRI_RESTORE timeout
 
4642,,poll IDLE timeout
 
4642,,poll IDLE timeout
 
4641,III,mac:%d sleep_time_us:0x%08x_%08x
 
4640,I,mac:%d sleep time larger than WDOG threshold! 
4639,I,MAC_WCMN_REG_WAKEUP_INTR_RAW_STATUS_1:0x%x
 
4638,I,MAC_MCMN_REG_MCMN_ISR_P 0x%x
 
4623,I,masked MAC_MCMN_REG_MCMN_ISR_P 0x%x
 
4621,II,mac:%d MAC_MCMN_REG_MCMN_ISR_S4:0x%x
 
4620,II,mac:%d MAC_MCMN_REG_MCMN_IMR_S4:0x%x
 
4619,II,mac:%d MAC_MCMN_REG_MCMN_ISR_S16:0x%x
 
4618,II,mac:%d MAC_MCMN_REG_MCMN_IMR_S16:0x%x
 
4617,II,mac:%d MAC_MCMN_REG_MCMN_ISR_S2:0x%x
 
4616,II,mac:%d MAC_MCMN_REG_MCMN_IMR_S2:0x%x
 
4615,II,mac:%d MAC_MCMN_REG_MCMN_ISR_S8:0x%x
 
4614,II,mac:%d MAC_MCMN_REG_MCMN_IMR_S8:0x%x
 
4639,I,MAC_WCMN_REG_WAKEUP_INTR_RAW_STATUS_1:0x%x
 
4638,I,MAC_MCMN_REG_MCMN_ISR_P 0x%x
 
4637,I,MAC_MCMN_REG_MCMN_ISR_RX_OK 0x%x
 
4636,I,mac:%d WAKEUP_INTR_MASKED_STATUS_1 check timeout
 
4634,I,RRI save addr:0x%x
 
4635,I,RRI restore addr:0x%x
 
4634,I,RRI save addr:0x%x
 
4633,I,CH0 RFACTRL_REG_ARB_COMMAND 0x%x
 
4632,I,CH1 RFACTRL_REG_ARB_COMMAND 0x%x
 
4639,I,MAC_WCMN_REG_WAKEUP_INTR_RAW_STATUS_1:0x%x
 
4638,I,MAC_MCMN_REG_MCMN_ISR_P 0x%x
 
4623,I,masked MAC_MCMN_REG_MCMN_ISR_P 0x%x
 
4621,II,mac:%d MAC_MCMN_REG_MCMN_ISR_S4:0x%x
 
4620,II,mac:%d MAC_MCMN_REG_MCMN_IMR_S4:0x%x
 
4619,II,mac:%d MAC_MCMN_REG_MCMN_ISR_S16:0x%x
 
4618,II,mac:%d MAC_MCMN_REG_MCMN_IMR_S16:0x%x
 
4617,II,mac:%d MAC_MCMN_REG_MCMN_ISR_S2:0x%x
 
4616,II,mac:%d MAC_MCMN_REG_MCMN_IMR_S2:0x%x
 
4615,II,mac:%d MAC_MCMN_REG_MCMN_ISR_S8:0x%x
 
4614,II,mac:%d MAC_MCMN_REG_MCMN_IMR_S8:0x%x
 
4639,I,MAC_WCMN_REG_WAKEUP_INTR_RAW_STATUS_1:0x%x
 
4638,I,MAC_MCMN_REG_MCMN_ISR_P 0x%x
 
4637,I,MAC_MCMN_REG_MCMN_ISR_RX_OK 0x%x
 
4636,I,mac:%d WAKEUP_INTR_MASKED_STATUS_1 check timeout
 
4634,I,RRI save addr:0x%x
 
4635,I,RRI restore addr:0x%x
 
4634,I,RRI save addr:0x%x
 
4633,I,CH0 RFACTRL_REG_ARB_COMMAND 0x%x
 
4632,I,CH1 RFACTRL_REG_ARB_COMMAND 0x%x
 
4631,II,pmm_wlan_pwr_seq mac:%d pmm_wlan seq:%d
 
4609,I,stop_wlan_ss_seq mac:%d
 
4629,I,PMM WLAN MAC IDLE 0x%x
 
4628,I,MCMN MAC IDLE 0x%x
 
4629,I,PMM WLAN MAC IDLE 0x%x
 
4628,I,MCMN MAC IDLE 0x%x
 
4627,I,stop wlan_ss Aborted due to lwm interrupt is pending 0x%x
 
4630,,poll mac0 idle timeout
 
4625,,stop wlan_ss Aborted due to pending int
 
4624,III,masked ISR_RX_OK:0x%x ISR_SIFS_RESP:0x%x ISR_TX_OK:0x%x
 
4623,I,masked MAC_MCMN_REG_MCMN_ISR_P 0x%x
 
4622,,stop wlan_ss Aborted due to misc
 
4621,II,mac:%d MAC_MCMN_REG_MCMN_ISR_S4:0x%x
 
4620,II,mac:%d MAC_MCMN_REG_MCMN_IMR_S4:0x%x
 
4619,II,mac:%d MAC_MCMN_REG_MCMN_ISR_S16:0x%x
 
4618,II,mac:%d MAC_MCMN_REG_MCMN_IMR_S16:0x%x
 
4617,II,mac:%d MAC_MCMN_REG_MCMN_ISR_S2:0x%x
 
4616,II,mac:%d MAC_MCMN_REG_MCMN_IMR_S2:0x%x
 
4615,II,mac:%d MAC_MCMN_REG_MCMN_ISR_S8:0x%x
 
4614,II,mac:%d MAC_MCMN_REG_MCMN_IMR_S8:0x%x
 
4613,I,QDSP_ASIC_INTR_MASKED_STATUS 0x%x
 
4612,I,QDSP_ASIC_INTR_MASKED_STATUS_2 0x%x
 
4611,I,QDSP_ERROR_INTR_MASKED_STATUS 0x%x
 
4610,I,QDSP_ERROR_INTR_MASKED_STATUS_2 0x%x
 
4609,I,stop_wlan_ss_seq mac:%d
 
4629,I,PMM WLAN MAC IDLE 0x%x
 
4628,I,MCMN MAC IDLE 0x%x
 
4629,I,PMM WLAN MAC IDLE 0x%x
 
4628,I,MCMN MAC IDLE 0x%x
 
4627,I,stop wlan_ss Aborted due to lwm interrupt is pending 0x%x
 
4626,,poll mac1 idle timeout
 
4625,,stop wlan_ss Aborted due to pending int
 
4624,III,masked ISR_RX_OK:0x%x ISR_SIFS_RESP:0x%x ISR_TX_OK:0x%x
 
4623,I,masked MAC_MCMN_REG_MCMN_ISR_P 0x%x
 
4622,,stop wlan_ss Aborted due to misc
 
4621,II,mac:%d MAC_MCMN_REG_MCMN_ISR_S4:0x%x
 
4620,II,mac:%d MAC_MCMN_REG_MCMN_IMR_S4:0x%x
 
4619,II,mac:%d MAC_MCMN_REG_MCMN_ISR_S16:0x%x
 
4618,II,mac:%d MAC_MCMN_REG_MCMN_IMR_S16:0x%x
 
4617,II,mac:%d MAC_MCMN_REG_MCMN_ISR_S2:0x%x
 
4616,II,mac:%d MAC_MCMN_REG_MCMN_IMR_S2:0x%x
 
4615,II,mac:%d MAC_MCMN_REG_MCMN_ISR_S8:0x%x
 
4614,II,mac:%d MAC_MCMN_REG_MCMN_IMR_S8:0x%x
 
4613,I,QDSP_ASIC_INTR_MASKED_STATUS 0x%x
 
4612,I,QDSP_ASIC_INTR_MASKED_STATUS_2 0x%x
 
4611,I,QDSP_ERROR_INTR_MASKED_STATUS 0x%x
 
4610,I,QDSP_ERROR_INTR_MASKED_STATUS_2 0x%x
 
4609,I,stop_wlan_ss_seq mac:%d
 
4608,I,turn_on_wlan_ss_seq mac:%d
 
4607,I,turn_on MAC_HWSCH_REG_HWSCH_CMD_RING_PAUSE 0x%x
 
4607,I,turn_on MAC_HWSCH_REG_HWSCH_CMD_RING_PAUSE 0x%x
 
4606,II,get_seq_latency type_msk:0x%x total:%d
 
4605,II,set_seq_latency type:0x%x val:%d
 
4604,I,set_paid_match mac:%d ALL PAID match has been assigned
 
4603,I,set_rxdma_hold_bit dma_hold:0x%x
 
4602,II,WD Bite Sleep ticks %x larger than programmable, disabling WD bite, please check beacon period %x
 
4602,II,WD Bite Sleep ticks %x larger than programmable, disabling WD bite, please check beacon period %x
 
4601,IIIII,PMM WLAN SM stall state %x RRI Intr status :0x%x RRI current address:0x%x RRI active:0x%xRRI state: 0x%x
 
4663,III,poll reg:0x%x for 0x%x timeout, line:%d 
4679,I,MISC signal pending but RRI not complete %x
 
4678,III, RRI wait iteration:0x%x :0x%x :0x%x
 
4677,II, RRI Restore done, int status:0x%x iteration:%d
 
4676,IIIII, RRI Restore error, int status:0x%x iteration:%d cur_addr:0x%x active:0x%xstate:0x%x
 
4675,,call to function cmnos_this_thread is NULL 
4674,II,tbl:%d size:%d 
4671,II,tbl:%d cost:%dus 
4674,II,tbl:%d size:%d 
4673,IIII, CE dst:0x%x src:0x%x size:0x%x trc_noc_ce_remap_dis:0x%x
 
4672,III, RRI Restore addr:0x%x size:0x%x rem_size:0x%x
 
4671,II,tbl:%d cost:%dus 
4670,IIII,en:PHY1_CBCR:0x%x, PHY1_80_CBCR:0x%x, PHY1_160_CBCR:0x%x, PHY1_TDAC_CBCR:0x%x
 
4670,IIII,en:PHY1_CBCR:0x%x, PHY1_80_CBCR:0x%x, PHY1_160_CBCR:0x%x, PHY1_TDAC_CBCR:0x%x
 
4669,IIII,dis:PHY1_CBCR:0x%x, PHY1_80_CBCR:0x%x, PHY1_160_CBCR:0x%x, PHY1_TDAC_CBCR:0x%x
 
4669,IIII,dis:PHY1_CBCR:0x%x, PHY1_80_CBCR:0x%x, PHY1_160_CBCR:0x%x, PHY1_TDAC_CBCR:0x%x
 
4668,,fast_pwr_transition_mode: Dynamic Not supported, use static 
4667,II,full_save mac:%d entry, chmsk:0x%x
 
4666,II,full_save mac:%d exit, timeline=%d 
 
4665,II,full_restore mac:%d entry, chmsk:0x%x
 
4664,II,full_restore mac:%d exit, timeline=%d 
 
4706,I,CCE rule count exceeded  :%d 
4705,I,CCE Last rule valid :0x%0x 
4704,I,CCE super rule count exceeded  :%d 
4703,I,CCE prev_super_rule rule valid :0x%0x 
4702,I,CCE appended_super_rule_indication rule valid :0x%0x 
4701,II,CCE last_super_rule_valid :0x%0x,current super_rule :0x%0x 
4700,I,in _whal_drop_counters_reset: counter_no: %d 
4699,II,in _whal_cce_counter_assign: counter_no: %d, superrulenum: %d  
4698,IIII,in whal api call: cce_drop_1: %d,cce_drop_2: %d,cce_drop_3: %d,cce_drop_4: %d 
4697,IIII,in whal super rule api call: cce_rule_drop_1:  0x%0x,cce_rule_drop_2:  0x%0x,cce_rule_drop_3:  0x%0x,cce_rule_drop_4: 0x%0x 
4696,III,in whal cce disable api call:ppdu_end: 0x%0x ,idle %d,ITERATION :%d 
4693,I,RX_OLE_SM_STATUS:0x%x  
4692,I,RX_OLE_WATCHDOG:0x%x  
4691,I,CCE_SM_STATUS:0x%x  
4690,I,CCE_WATCHDOG:0x%x  
4689,I,MCMN_ISR_S14:0x%x  
4688,I,MCMN_MAC_IDLE:0x%x  
4687,I,RXDMA_FETCH_IDX_0:0x%x  
4686,I,RXDMA_FETCH_IDX_1:0x%x  
4685,I,RXDMA_FETCH_IDX_2:0x%x  
4684,I,RXDMA_IDX_0:0x%x  
4683,I,RXDMA_IDX_1:0x%x  
4682,I,RXDMA_IDX_2:0x%x  
4695,,Rx Ring full condition detected in CCE disable, going to whal reset   
4694,II,unknown whal_cce disable fail after MAX_LOOP_COUNT ,RXOLE ppdu_end: 0x%0x ,idle %d  
4693,I,RX_OLE_SM_STATUS:0x%x  
4692,I,RX_OLE_WATCHDOG:0x%x  
4691,I,CCE_SM_STATUS:0x%x  
4690,I,CCE_WATCHDOG:0x%x  
4689,I,MCMN_ISR_S14:0x%x  
4688,I,MCMN_MAC_IDLE:0x%x  
4687,I,RXDMA_FETCH_IDX_0:0x%x  
4686,I,RXDMA_FETCH_IDX_1:0x%x  
4685,I,RXDMA_FETCH_IDX_2:0x%x  
4684,I,RXDMA_IDX_0:0x%x  
4683,I,RXDMA_IDX_1:0x%x  
4682,I,RXDMA_IDX_2:0x%x  
4681,II,CCE SM status: 0x%0x ,CCE_WATCHDOG status: 0x%0x  
4680,II,Crashing in whal_cce enable after MAX_LOOP_COUNT ,RXOLE ppdu_end: 0x%0x ,idle %d  
4722,IIII, meta:%d tbl:%d txpcu_off:0x%x dwords:%d 
4721,I,load_rri_tbl msk:0x%x
 
4720,II, rri_scratch <0x%x - 0x%x>
 
4719,II, rri_cmd_tbl <0x%x - 0x%x>
 
4718,II,MAC:%d SW trig RRI func:%d
 
4717,I,MAC:%d SW trig RRI end
 
4716,I,MAC:%d SW trig RRI fail
 
4715,I,BUF_CONTROL:0x%x
 
4714,IIII,RRI Int status:0x%x cur_addr:0x%x active:0x%x state:0x%x
 
4713,I,CH0 RF_BUS_ERROR_STATUS 0x%x
 
4712,I,CH1 RF_BUS_ERROR_STATUS 0x%x
 
4711,I,CH0 RF_BUS_STATUS 0x%x
 
4710,I,CH1 RF_BUS_STATUS 0x%x
 
4709,I,CH0 ARB_COMMAND 0x%x
 
4708,I,CH1 ARB_COMMAND 0x%x
 
4707,IIII,MAC:%d debug_dump_regs, reg_start:0x%x len:0x%x txpcu_buf_ctl:0x%x
 
4732,,phy idle timeout
 
4731,I,Reset phy core %x
 
4730,I,PcuHaltRx %x
 
4726,I,Stop PCU receive %x
 
4729,IIII,RecvReset: Before turning off RER ring_id(%d) HW_INDX(0x%x) FW_INDX(0x%x) fetch(%d)
 
4728,IIII,RecvReset: Before restoring FW_INDX ring_id(%d) HW_INDX(0x%x) FW_INDX(0x%x) fetch(%d)
 
4727,II,SetHWIndx: RXDMA Set Hw index error F:0x%X, H:0x%X 
 
4726,I,Stop PCU receive %x
 
4725,II,rxole_check_hang (mac=%d): rxole_reg=0x%x 
4724,III,rxole_check_hang (mac=%d): debug_select=0x%x, testbus_val=0x%x 
4723,II,rxole_check_hang (mac=%d): invalid L4 info detected (%d times) 
4733,,whal reset done
 
4741,IIII,read_CIR: num_samples %d buff %p chain_idx %d is_ext %d 
4740,,whal_rtt_frame_prepare() HW is already prepared for RTT return !!! 
4739,III,i: %d sw selfgen_chainmask: 0x%x not same as hw conifgured value: 0x%x 
4738,,HT_VHT_ACKS enabled 
4737,,whal_rtt_frame_recover() HW was not configured for RTT!!! return 
4736,,HT_VHT_ACKS enabled  
4735,IIIII,status: %d channel_bw: %d delay_tdbl_indx: %d, pkttype: %d txrx_delay: %d 
4734,IIIIII,rtt_get_delay_tbl_indx_packetype() status: %d bw: %d, preamble: %d, delay_tdbl_indx: %d, pkttype: %d ack_dyn_bw: %d 
4745,II,XMIT Compute: phy =%d, rix =%d 
4744,I,XMIT STOPDMA SEND FLUSH =%x 
4743,II,XMIT STOPDMA RING PAUSE=%x, MAC IDLE =%x 
4743,II,XMIT STOPDMA RING PAUSE=%x, MAC IDLE =%x 
4742,II,fatal TX flush reason=%d on MAC=%d 
4746,II,buf_len:%d is greater than msg length:%d 
4760,IIII,WMI_CMD_RX handle in BE cmd=%d length=%d endPt=%d, pHTCbuf=%x 
4759,IIII,WMI_CMD_RX cmd comp. handle in RT --free buf cmd=%d length=%d endPt=%d, pHTCbuf=%x 
4758,I,WMI_EVENT_SEND EventId = 0x%x 
4757,I, pending EventId = 0x%x 
4756,IIIIIIII,WMI_CMD_PARAMS 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 
4755,I,WMI_CMD_PARAMS 0x%08x 
4754,II,WMI_CMD_PARAMS 0x%08x 0x%08x 
4753,III,WMI_CMD_PARAMS 0x%08x 0x%08x 0x%08x 
4752,IIII,WMI_CMD_PARAMS 0x%08x 0x%08x 0x%08x 0x%08x 
4751,IIIII,WMI_CMD_PARAMS 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 
4750,IIIIII,WMI_CMD_PARAMS 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 
4749,IIIIIII,WMI_CMD_PARAMS 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 
4748,II,WMI_CMD_RX CmdId = 0x%x Length = %d 
152,I,WMI_SEND_EVENT_WRONG_TLV CmdId/EventId = 0x%x 
4747,IIII,WMI_CMD_RX process inline cmd=%d length=%d endPt=%d, pHTCbuf=%x 
4766,,MXI halt  
4765,I,MAC %d MXI halt failed 
4764,,Rx dma halt  
4763,,Rx dma halt failed 
4762,I,Timestamp: %x, Rejuvenation Count = 0. 
4761,II,Timestamp: %x, Rejuvenation Count = %d. 
4767,,COEX_MWS_OTHER: modem qdi obj rec 
4786,IIIII,WAL_AP_PS_DBGID_DETECT_OUT_OF_SYNC_STA vdev_id = %d AssocID = %d Timestamp = %d OldestTxBufferedWaitingMs = %d n_buffered_mpdu = %d 
4785,IIIII,WAL_AP_PS_DBGID_DETECT_OUT_OF_SYNC_STA vdev_id = %d AssocID = %d Timestamp = %d OldestTxBufferedWaitingMs = %d QDepeth = %d 
4784,II,WAL_AP_PS_DBGID_HOST_TX_PAUSE vdev_id = %d : 0x%x 
4783,II,WAL_AP_PS_DBGID_HOST_TX_UNPAUSE vdev_id = %d : 0x%x 
4782,III,WAL_AP_PS_DBGID_PEER_CREATE vdev_id = %d AssocID = %d peer:%0x 
4781,III,WAL_AP_PS_DBGID_PEER_DELETE vdev_id = %d AssocID = %d peer:%0x 
4780,II,WAL_AP_PS_DBGID_SLEEP_STA_DEC vdev_id = %d num_sleeping_sta:%d 
4779,II,WAL_AP_PS_DBGID_SLEEP_STA_INC vdev_id = %d num_sleeping_sta:%d 
4778,II,WAL_AP_PS_DBGID_HOST_TX_PAUSE 0x%x 0x%x 
4777,II,WAL_AP_PS_DBGID_PS_DESC_BIN_LWM Bitmap = 0x%x VdevMap = 0x%x 
4776,II,WAL_AP_PS_DBGID_PS_DESC_BIN_HWM Bitmap = 0x%x VdevMap = 0x%x 
4775,II,WAL_AP_PS_DBGID_HOST_TX_UNPAUSE 0x%x 0x%x 
4774,,_wal_ps_buf_peer_create_instance() ps_psoc_handle NULL !!! 
4773,,_wal_ps_buf_peer_create_instance() TDLS peer_handle alloc failed !!! 
4772,III,_wal_ps_buf_peer_create_instance() vdev_id = %d peer_handle = %p wal_peer = %p 
4771,,invalid access 
4770,IIII,_wal_ps_buf_delete_create_instance() vdev_id = %d peer_handle = %p PM enabled: %d wal_peer = %p 
4769,IIII,WAL_AP_PS_DBGIG_SET_PARAM vdev_id = %d AssocID = %d Param = %d Value = %d 
4768,IIII,WAL_AP_PS_DBGIG_UAPSD_CFG vdev_id = %d AssocID = %d UAPSDTriggerTids = 0x%x UAPSDDeliveryTids = 0x%x 
4787,III,WAL_AP_PS_DBGID_SM vdev_id = %d assoc_id:%d SLEEP_DOZE ==> ACTIVE (num_sleeping_sta = 0x%x) 
4788,II,WAL_AP_PS_DBGID_SM: vdev_id = %d assoc_id:%d SLEEP_DOZE <-- SEND_N_COMP 
4789,II,WAL_AP_PS_DBGID_SM: vdev_id = %d assoc_id:%d SLEEP_DOZE <-- SEND_COMP 
4790,II,WAL_AP_PS_DBGID_SM: vdev_id = %d assoc_id:%d SLEEP_DOZE <-- RX 
4791,III,WAL_AP_PS_DBGID_SM vdev_id = %d assoc_id:%d SLEEP_DOZE <-- PM_STATE_CHANGE (num_sleeping_sta = 0x%x) 
4792,III,WAL_AP_PS_DBGID_SM vdev_id = %d assoc_id:%d ACTIVE ==> SLEEP_DOZE(num_sleeping_sta = 0x%x) 
4793,III,WAL_AP_PS_DBGID_SM vdev_id = %d assoc_id:%d ACTIVE <-- PM_STATE_CHANGE(num_sleeping_sta = 0x%x) 
4794,IIII,WAL_AP_PS_DBGID_SYNC_TIM vdev_id = %d AssocID = %d Tids = 0x%x TimSet = %d 
4795,III,WAL_AP_PS_DBGID_UPDATE_TIM vdev_id = %d AssocID = %d IsTimSet = %d 
4796,IIII,WAL_AP_PS_DBGID_SEND_N_COMPLETE vdev_id = %d AssocID = %d USPActive = %d PendingPollResp = %d 
4797,IIIIII,WAL_AP_PS_DBGID_SEND_COMPLETE vdev_id = %d AssocID = %d FrameCtrl = 0x%x QoSCtrl = 0x%x USPActive = %d PendingPollResp = %d 
4798,IIII,WAL_AP_PS_DBGID_COMPLETED_EOSP vdev_id = %d AssocID = %d Timestamp = %d LastRxTriggerTime = %d 
4799,IIII,WAL_AP_PS_DBGID_START_SP vdev_id = %d AssocID = %d Timestamp = %d Mark = %d 
4800,IIIII,WAL_AP_PS_DBGID_NEXT_RESPONSE vdev_id = %d AssocID = %d USPActive = %d PendingUSP = %d PendingPollResp = %d 
4801,IIIII,WAL_AP_PS_DBGID_DUPLICATE_TRIGGER vdev_id = %d AssocID = %d Timestamp = %d SeqNO = %d Tid = %d 
4802,IIIII,WAL_AP_PS_DBGID_PSPOLL_REQ vdev id = %d AssocID = %d Aid = %d PeerPSEnabled = %d SendNInProgress = %d 
4799,IIII,WAL_AP_PS_DBGID_START_SP vdev_id = %d AssocID = %d Timestamp = %d Mark = %d 
4803,IIIII,WAL_AP_PS_DBGID_TRIGGER vdev_id = %d AssocID = %d Timestamp = %d USPActive = %d SendNInProgress = %d 
4804,IIIIII,WAL_AP_PS_DBGID_UAPSD_RESPONSE_ERROR vdev_id = %d AssocID = %d Tid/Paused = 0x%x AllowedUAPSDTidMask = 0x%x PendingTidMap = 0x%x SPLength = 0x%x 
4805,IIIIIIII,WAL_AP_PS_DBGID_UAPSD_RESPONSE vdev_id = %d AssocID = %d Tid = %d NumMPDUToSend = %d need_extra_qnull = %d Flags = %d allow_n_flags_qnull = %d SPLength = 0x%x 
4806,IIIII,WAL_AP_PS_DBGID_PSPOLL_ERROR vdev_id = %d AssocID = %d TidPaused = %d AllowdLegacyTidMask = 0x%x LegacyTidMask = 0x%x 
4807,IIIIIII,WAL_AP_PS_DBGID_PSPOLL vdev_id = %d AssocID = %d Tid = %d Flags = 0x%x legacy_tidmask = 0x%x allowed_legacy_tidmask = 0x%x pending_legacy_tidmap = 0x%x 
4813,II,_wal_ps_de_initialize_tdls_buf_sta_instance (peer=%p vdev = %p) 
4812,III,wal_ps_initialize_tdls_buf_sta_instance() failed (peer=%p caps = %p vdev = %p) failed 
4811,,wal_ps_initialize_tdls_buf_sta_instance() buf_sta create failed 
4810,IIII,wal_ps_initialize_tdls_buf_sta_instance() (peer=%p caps = %p vdev = %p slp_sta_support = %d) 
4809,III,wal_ps_tdls_init_default_configs() assoc_id = %d uapsd_trigger_tids = 0x%x default_legacy_ac = 0x%x 
4808,,wal_ps_tdls_wal_peer_event_handler()  buf_sta_handle NULL return 
4815,III,_wal_ps_sta_process_rx_event: frame_control=%0x, qos_control=%0x, thread_id=%d 
4814,,_wal_ps_sta_process_rx_event: leaky AP detected 
4826,I,_wal_egap_disable_event invalid frame event = %d  
 
4825,II,_wal_egap_disable_event frame event = %d egap_psoc_handle->event_bitmap = %d 
 
4824,I,_wal_egap_enable_event invalid frame event = %d  
 
4823,II,_wal_egap_enable_event frame event = %d egap_psoc_handle->event_bitmap = %d 
 
4822,I,_wal_egap_is_event_enabled invalid frame event = %d  
 
4821,I,_wal_egap_is_event_enabled egap_psoc_handle->event_bitmap = %d 
 
4820,II,_wal_egap_notify_sta_sleep num_sta_asleep = %d num clients = %d** 
 
4819,I,_wal_egap_pdev_event_handler event->event_type  = 0x%x  
 
4818,,_wal_egap_pdev_event_handler send RT the phyerr event  
 
4817,I,_wal_egap_update_peer_connections num_clients = %d 
 
4816,I,wal_egap_is_powersave_frame powersave_frame = %d 
 
4842,IIIII,_ar_wal_tdls_attach() tdls_psoc_handle = %p                              pdev = %p, num_vdevs = %d                              num_conn_table = %d tdls_pool ptr = %p 
4841,IIII,_ar_wal_tdls_psoc_init()                              tdls_psoc_handle = %p num_vdevs = %d num_conn_table = %d tdls_pool ptr = %p 
4840,II,_ar_wal_tdls_vattach() vdev_id = %d vdev flags: 0x%x 
4839,,_ar_wal_tdls_vattach(): failure: no memory left for vdev tdls handle, must be at max tdls vdevs  
4838,II,_ar_wal_tdls_vdetach() vdev_id = %d vdev flags = 0x%x  
4837,,_tdls_process_rx_frame(): wal_pdev NULL 
4836,,_tdls_process_rx_frame(): wal_peer NULL 
4835,,_tdls_process_rx_frame():L3 invalid 
4834,,_tdls_process_rx_frame(): tdls payload is NULL 
4833,I,_tdls_process_rx_frame(): action code = %d 
4832,I,_tdls_process_rx_frame(): tdls payload size is incorrect: %d 
4831,I,_tdls_wlan_action_notif: notif_type = %d 
4830,II,TDLS_DBGID_WAL_GET  Tdls9: vdev_id = 0x%x param_type = %d 
4829,II,TDLS_DBGID_WAL_GET not handled in switch vdev_id = 0x%x param_type = %d 
4828,III,TDLS_DBGID_WAL_SET  Tdls8: vdev_id = %d param_type = %d value = 0x%x 
4827,II,TDLS_DBGID_WAL_SET not handled in switch vdev_id = 0x%x param_type = %d 
4855,I,tdls_pti_tx_completion() completion_status = %x 
4854,II,_tdls_uapsd_cancel_ptr_recv_timer() dialog_token = 0x%x ia_action = 0x%x 
4853,I,_tdls_uapsd_cancel_ptr_recv_timer() RX Event pwrmgmt = %d 
4852,I,_tdls_uapsd_cancel_ptr_recv_timer() RX Event 2 pwrmgmt = %d 
4851,I,_tdls_uapsd_enter_exit_buf_sta_role() enter: %d 
4850,I,_tdls_uapsd_ptr_recv_notif_handler() ptr frame not received issue tear down peer_handle = %p 
4849,I,_tdls_uapsd_send_pti_frame() wal_peer = 0x%x 
4848,II,_tdls_uapsd_send_pti_frame(): get pti frame buffer failed vdev_id = %d peer_type = 0x%x 
4847,IIII,_tdls_uapsd_send_pti_frame():  vdev_id = %d status = 0x%x dialog token = 0x%x buf_bitmask = 0x%x 
4846,II,_tdls_uapsd_send_pti_frame() vdev_id = %d peer_type =0x%x 
4845,III,_tdls_uapsd_send_pti_frame() failed buf_bitmask is zero vdev_id = %d peer_type = 0x%x tid_bitmap = 0x%x 
4844,II,_tdls_uapsd_send_pti_frame_to_peer  failure buf_sta_handle = %p ptr_timer running = 0x%x 
4843,I,tdls_uapsd_send_pti_frame failed: status = %d 
4857,I,invalid type:%x
 
4865,I,not register type when insert:%x
 
4864,II,insert:type:%x,id:%x
 
4863,II,found dup when insert:type:%x,id:%x
 
4862,II,pool exhausted when insert:type:%x,id:%x
 
4857,I,invalid type:%x
 
4861,I,already registered type:%x
 
4857,I,invalid type:%x
 
4860,I,not register type when remove:%x
 
4859,II,remove:type:%x,id:%x
 
4858,II,not found when remove: type:%x, id:%x
 
4857,I,invalid type:%x
 
4856,I,not registered type:%x
 
4868,IIIII,timeout detected,type:%x,id:%x, cur_ms:%x, insert_ms:%x, insert_tick:%lx
 
4867,I,timeout detected, list is empty, type:%x 
4866,III,timeout detected, timeout:%x, total insert cnt:%x, total remove cnt:%x 
4876,IIIIII,swba_intr: misc=0x%x,period=%u,tsf=%u,tbtt-curr=%u/next=%u,diff=%u 
4875,I,cur_tsf %u 
4874,II,Burst beacon drift: next_beacon = %u, next_hw_tbtt = %u 
4873,III,Burst beacon drift recover: next_beacon = %u,                                         beacon_period = %u, until_next_tbtt = %u 
4872,II,Staggered beacon drift: next_beacon = %u, next_hw_tbtt = %u 
4871,III,Staggered beacon drift recover: next_beacon = %u,                                 beacon_period = %u, until_next_tbtt = %u 
4870,I,next_beacon_wal_swba_restore=%d 
4869,III,_wal_swba_set_and_fire: cur_tsf=0x%x sta_offset=0x%x next_beacon=0x%x 
4878,II,WAL_DBGID_GET_HW_CHAINMASK  Tx:0x%x Rx:0x%x 
4877,III,WAL_DBGID_SET_HW_CHAINMASK 0x%x 0x%x 0x%x 
4879,I,_wal_set_home_channel : num home chans = %d 
4943,II,COEX_MWS_ANT_DIVERSITY: chnmsk completed rx=%d tx=%d 
4942,,COEX_MWS_ANT_DIVERSITY: UnMuting after init chanmask change 
4923,,COEX_MWS_ANT_DIVERSITY: PA_Muting: 2G Ch1 UnMute 
4941,I,COEX_MWS_ANT_DIVERSITY: Updating chainmask. tx_chm=0x1, rx_chm=0x1, rx_nss=0x%x, defer_smps = 0 
4940,I,COEX_MWS_ANT_DIVERSITY: PwrOnTimer, AntShState = 0x%x  
4939,,COEX_MWS_ANT_DIVERSITY: PA_UNMUTE on PwrOnTimer because AntShState is SWITCH_ON_WLAN 
4938,,COEX_MWS_ANT_DIVERSITY: Antenna Sharing feature is disabled 
4937,,COEX_MWS_ANT_DIVERSITY: Duplicate power down event 
4936,,COEX_MWS_ANT_DIVERSITY: Powering down... 
4935,,COEX_MWS_ANT_DIVERSITY: Powering down before power on timeout 
4934,,COEX_MWS_ANT_DIVERSITY: Duplicate power up event 
4933,,COEX_MWS_ANT_DIVERSITY: Powering up... 
4932,,COEX_MWS_ANT_DIVERSITY: On power up, WLAN in 2x2 and Antenna state has changed 
4931,,COEX_MWS_ANT_DIVERSITY: PA_Muting: 2G Ch1 Mute 
4930,,COEX_MWS_ANT_DIVERSITY: Cancelling early Release timer 
4929,II,COEX_MWS_ANT_DIVERSITY: Entering FAS opmode %d, vdevid %d 
4928,,COEX_MWS_ANT_DIVERSITY: In power save mode, cache state changes 
4927,IIIIII,COEX_MWS_ANT_DIVERSITY: (0x%x) (0x%x) (0x%x) (0x%x) (%d) (0x%x) 
4927,IIIIII,COEX_MWS_ANT_DIVERSITY: (0x%x) (0x%x) (0x%x) (0x%x) (%d) (0x%x) 
4926,III,COEX_MWS_ANT_DIVERSITY: 0x6666 AntShareConf: %d , target: %d wlanOwn:%d 
4925,IIII,COEX_MWS_ANT_DIVERSITY: Updating chainmask. tx_chm=0x%x, rx_chm=0x%x, rx_nss=0x%x, defer_smps=%d 
4924,II,COEX_MWS_ANT_DIVERSITY: 0x6670, ShDur: %d timeout: %d 
4923,,COEX_MWS_ANT_DIVERSITY: PA_Muting: 2G Ch1 UnMute 
4922,IIII,COEX_MWS_ANT_DIVERSITY: RSSI Threshold met. Type= %d rssi= %d, threshold= %d (BRssi=%d) 
4921,III,COEX_CONFIG_MGR: WlanConfigManager(0x%x) Stimulus(%u) CurBand(%u) 
4920,IIIIIIII,WAL_COEX_RC_CHAINMASK: pdev_id(%u) RFBand(%u) ShareIndx(%u) NumWlanRfChains(%u) bdf_chm(0x%x) nss1(%u) nss2(%u) nss3(%u) 
4919,,COEX_SET_COEX_WEIGHT: Setting coex weight group to 4 as BT A2DP became NORMAL ! 
4918,,COEX_SET_WEIGHT_GROUP6: Setting coex weight group 6 as BT A2DP became CRITICAL 
4917,II,COEX_SET_COEX_WEIGHT: CoExTimerHandler - End of WLAN interval. Resetting the WLAN Weight from %d to %d for BT Interval ! 
4916,II,COEX_CSS_PWR: CSS power change: css_id(%u) event_id(%u) 
4915,I,COEX_MWS_TYPE2_TX: Tx_FiFo Depth: %d 
4914,,COEX_SET_WEIGHT_GROUP3: Setting coex weight group to 3 BT became normal 
4913,,COEX_SET_WEIGHT_GROUP3: Setting coex weight group to 3 due because 2G vdev is Paused 
4912,I,COEX_SET_WEIGHT_GROUP6: Setting coex weight group 6 due to reason %d 
4911,II,COEX_ENTER_CRITICAL_OCS:  Error in starting OCS Status = 0x%x, TransState(0x%x) 
4910,IIII,COEX_ENTER_CRITICAL_OCS: Dur(%u) Intrvl(%u) TransState(0x%x) Status(%u) 
4909,III,COEX_ENTER_OCS: OCSTransitionState(%u) Status(%u) DynOCSStatus(%u) 
4908,II,COEX_ENTER_OCS:  Error in starting OCS Status = 0x%x, TransState(0x%x) 
4907,IIII,COEX_ENTER_OCS: Dur(%u) Intrvl(%u) TranState(0x%x) Status(%u) 
4906,II,WAL_COEX_ENTER_PSP: Error(0x%x) TX_SEND_BURST disabled (0x%x) 
4905,II,COEX_EXIT_CRITICAL_OCS: TransState(%u) Status(%u) 
4904,II,COEX_EXIT_OCS: OCSTransitionState(0x%x) DynOCSStatus(%u) 
4903,II,COEX_EXIT_OCS: TranState(%u) Status(%u) 
4902,II,WAL_COEX_EXIT_PSP: Error(0x%llx) TX_SEND_BURST enabled (0x%x) 
4901,IIIIII,COEX_CTS2S_RESULT: result(%u) pdev(%u) ts(%u) cts2s_tx_latency(%u) cts2s_max_time(%u) dut_nav(%u) 
4900,IIIIIII,WAL_COEX_HALPHY: event(%u) param(%u) total_req(%u) rej_cnt(%u) fail_cnt(%u) in_prog(%u) switch_cntr(%u) 
4899,II,COEX_MWS_ANT_DIVERSITY: Antenna Sharing low RSSI Threshold from BDF= %d and Actual= %d 
4898,II,WAL_COEX_BDF: Flags(0x%x) Config(0x%x) 
4897,IIIII,WAL_COEX_MNGR: Error(0x%x) Stimulus(%u) BTSMState(0x%x) SysUpdateResult(%u) ConfigMngr(0x%x) 
4896,IIIIIII,WAL_COEX_ALT_CHM: pdev(%u) chm(0x%x) enable_alt(%u) is_2gchan(%u) alt_chm(%u) selfgenAltChm (%u) pending(%u) 
4895,,WAL_COEX_ALT_CHM: pdev is NULL 
4894,II,WAL_COEX_PSP: Error(0x%x) MinInterval(%u) BtIdleTime(%u) 
4893,,COEX_RESET_WEIGHT_GROUP:  Group6 exceeded the programmed timeout 
4892,II,COEX_SET_NSS: VdevId(%u) NumStreams(%u) 
4891,III,COEX_SELF_GEN_MASK: Selfgen(%u) RFBand(%u) MaxChains(%u) 
4890,III,COEX_CTS2S_SEND: Dur(%u) Time2Discard(%u) CurrTime(%u) 
4889,IIIIIIIII,COEX_SYSTEM_MONITOR: bt(%u) pmh(%u) num_prof(%u), non_link(%u) acl_int(%u) passive_bt(%u) wlanrx_crit(%u) wlanrx(0x%x) 2g_pdev_idle(%u) 
4888,II,COEX_SYSTEM_UPDATE: Three Antenna BTC: ConfigMode(%u) RunningMode(%u) 
4887,IIIIIIII,COEX_SYSTEM_UPDATE: status(%u) stimulus(%u) hw_mode(%u) wlan0_state(0x%x) wlan1_state(0x%x) algo(%u) num_chains(%u) aggr_lim(%u) 
4886,III,COEX_MWS_WBTMR_SYNC: T2NonWlan(%u) Now(%u) Now+NonWlanDuration(%u) 
4885,IIII,COEX_UPDATE_CRITICAL_OCS: Dur(%u) Intrvl(%u) TransState(0x%x) Status(%u) 
4884,IIII,COEX_UPDATE_OCS: Dur(%u) Intrvl(%u) TransState(0x%x) Status(%u) 
4883,,COEX_MWS_TYPE2_RX: Schedule read after 500us  
4882,I,COEX_MWS_ERROR: excced buffer size:length=%d 
4881,I,WAL_COEX_WSI: Error(0x%x) 
4880,I,WAL_COEX_WSI_TMR: enable(%u) 
4983,III,WAL_COEX_BTPROF_ADD: Status(%u) RemoteId(%u) ProfileType(%u) 
4982,IIII,WAL_COEX_BT_ALLOC: Ret(%u) LocalId(%u) Remote_Id(%u) MinFreeLinkId(%u) 
4981,III,WAL_COEX_BT_DEALLOC: LocalId(%u) Remote_Id(%u) MinFreeLinkId(%u) 
4980,II,COEX_HWQ_EMPTY_CB: PauseState(0x%x) pdev(%u) 
4979,IIIIII,WAL_COEX_SCHED_INTERVAL: Error(0x%x) bt_grant(%u) bt_duration(%u) interval(%u) bt_traffic_status(%u) is_bt_heavy(%u) 
4978,IIII,WAL_COEX_PROC_GPM: Error(0x%x) status(%d) type(%u) subtype(%u) 
4977,II,COEX_MCI_RECOVER: StimulusState(0x%x) RecoveryState(0x%x) 
4976,I,COEX_MCI_TIMER_HANDLER: Recovery(0x%x) 
4975,II,COEX_WAL_PAUSE_RESUME: Pause(%u) State(0x%x) 
4974,I,COEX_GENERIC_ERROR: COEX_BT_GPM_OVERFLOW NumBtGpmOverflow(%u) 
4973,I,COEX_GENERIC_ERROR: Alloc Failed: Exceeds max num BT links: LinkId(%u) 
4972,I,COEX_GENERIC_ERROR: Exceeds max num BT links: LinkId(%u) 
4971,III,COEX_GENERIC_ERROR: Invalid GPM: MCI_GPM_BT_SCAN_UPDATE  En(%u) Window(%u) Int(%u) 
4970,II,COEX_GENERIC_ERROR: No record for existing link (%u) 
4969,I,COEX_GENERIC_ERROR: Exceeds max num BT links- LinkId:(%u) 
4968,I,COEX_GENERIC_ERROR: Exceeds max BT links- LinkId(%u) 
4967,II,COEX_GENERIC_ERROR: Link rate overshoots: Rate(%u) Id(%u) 
4966,I,COEX_GENERIC_ERROR: Alloc Fail: Exceeds max num BT links- Link(%u) 
4965,I,COEX_GENERIC_ERROR: Exceeds max num BT links- Link(%u) 
4964,I,COEX_GENERIC_ERROR: BT RXSS lower threshold is out of range Thresold(%d) 
4963,,COEX_GENERIC_ERROR: COEX_BT_LINKID_ERROR 
4962,I,COEX_GENERIC_ERROR: COEX_BT_LINKID_INVALID LinkId(%u) 
4961,III,WAL_COEX_BTPROF_DEL: Status(%u) RemoteId(%u) ProfileType(%u) 
4957,I,COEX_GENERIC_ERROR: Cannot Alloc link, Exceeds max BT links: LinkId(%u) 
4960,III,COEX_GENERIC_ERROR: BT removing invalid link: Type(%u) State(0x%x), NumProf(%u) 
4959,I,COEX_GENERIC_ERROR: Exceeds max BT links: LinkId(%u) 
4958,I,COEX_GENERIC_ERROR: CCK Rate Config 0x121212 (%u) 
4957,I,COEX_GENERIC_ERROR: Cannot Alloc link, Exceeds max BT links: LinkId(%u) 
4956,,WAL_COEX_WGT2PRIO: Invalid Weight Group 
4955,III,COEX_BT_INTERVAL_START: bt_intrvl_cnt(%u) duration(%u) enable_bt_bw_lim(%u) 
4954,,COEX_START_PRIO_TIMER: Warning! Coex start prio timer already running 
4953,II,COEX_WLAN_POSTPAUSE_INTERVAL_START: Dur(%u) Wght(%u) 
4952,II,COEX_WLAN_INTERVAL_START: wlan_intrvl_cnt(%u) duration(%u) 
4951,IIIIIII,WAL_COEX_PROFILES: NumBTProfiles(%u) ACL(%u) PwrSaveACL(%u) A2DP(%u) HID(%u) Voice(%u) BA(%u) 
4950,IIII,COEX_UPDATE_AFH: IsAdd(%u) Freq(%u), 2G(%u) HT20(%u) 
4949,II,COEX_BT_RXSS_THRES: NewRSSI(%d) 1 LowerThresh(%d) 
4948,I,COEX_GENERIC_ERROR: COEX_DUPLICATE_LINK_ERROR BtNonLinkCriticalNum(%u) 
4947,I,COEX_GENERIC_ERROR: COEX_NUM_LINK_OVERFLOW_ERROR BtNonLinkCriticalNum(%u) 
4946,,WAL_COEX_BT_BA: Interval is 0 
4945,III,COEX_BT_PRIO_BUDGET: BTIdleTime(%u) BtLowPrioBudget(%u) BtHiPrioBudget(%u) 
4944,II,COEX_BT_PRIO_BUDGET: pBtCoexInfoDev->bt_prof_prev_bitmap(%d) pBtCoexInfoDev->bt_prof_bitmap(%d) 
5232,II,COEX_MWS_ASM: [ASM_CHMASK] Req(TxChMask:0x%x, RxChMask:0x%x)  
5231,,COEX_MWS_ASM: [Err]ASM ChMask Client is not registered 
5230,III,COEX_MWS_REMOTE_EVENT: [Error] chavd_group_start: %u, wlan_freq_start: %u, wlan_freq_stop: %u 
5229,III,COEX_MWS_REMOTE_EVENT: [Error] chavd_group_stop: %u, wlan_freq_start: %u, wlan_freq_stop: %u 
5228,,COEX_MWS_REMOTE_EVENT: [Error] The range reported by modem is not valid 
5227,IIIII,COEX_MWS_REMOTE_EVENT: [POTENTIAL_CONFLICT] Freqs:(%d->%d), chavd_group:0x%x, chavd_1_0:0x%x, chavd_3_2:0x%x, 
5226,IIIIIII,COEX_MWS_ANT_DIVERSITY: AntShare Stats1, StartPos=0x%02x, EndPos=0x%02x, GrantCnt=%d, RelCnt=%d, Dur=%dms, WLAN=%dms, WAN=%dms 
5225,IIII,COEX_MWS_ANT_DIVERSITY: AntShare Stats2, MinWLAN=%dms, MaxWLAN=%dms, MinWAN=%dms, MaxWAN=%dms 
5224,I,COEX_MWS_ASM: [Err]:Dummy Client Reg Fail: %d 
5223,I,COEX_MWS_ASM: [Info]:Dummy Client Reg Success: Handle=%d 
5222,I,COEX_MWS_ASM: Dummy Client Notification GRANT Duration = %d ms 
5221,I,COEX_MWS_ASM: Dummy Client Notification NACK Duration = %d ms 
5220,,COEX_MWS_ASM: Dummy Client Notification RELEASE_IND 
5219,II,COEX_MWS_ASM: Dummy Client Notification ANT_STATUS_UPDATE Mask = 0x%x, Duration = %d 
5218,I,COEX_MWS_ASM: Invalid Client Notification Evt:%d 
5217,I,COEX_MWS_ASM: [Err]:Dummy Client request Failed: %d 
5216,,COEX_MWS_ASM: [Info]:Virtual Sync(ARB_NOT_REQUIRED,CH_NONE) from Acquisition Client 
5215,I,COEX_MWS_ASM: [Err][WLAN->ASM]:Illegal Cancel: Client_id(%d) not registered 
5214,II,COEX_MWS_ASM: [WLAN->ASM]:Cancel: Client_id(%d), Cancel_mask[0x%x] 
5213,I,COEX_MWS_ASM: [Err][WLAN->ASM]:Illegal Release: Client_id(%d) not registered 
5212,III,COEX_MWS_ASM: [Err][WLAN->ASM]:Illegal Release: Client_id(%d) Rel_mask[0x%x] is Different thn Req_mask[0x%x] 
5211,II,COEX_MWS_ASM: [WLAN->ASM]:Release: Client_id(%d), Rel_mask[0x%x] 
5210,I,COEX_MWS_ASM: [Err]:Illegal Request: Client_id(%d) not registered 
5209,II,COEX_MWS_ASM: [Err]:Illegal Request state(%d): Client_id(%d) 
5208,I,COEX_MWS_ASM: [Err]:Illegal Request: ChainMask(%d) not valid 
5207,II,COEX_MWS_ASM: [WLAN->ASM]:Request: Client_id(%d), ChMask[0x%x] 
5206,I,COEX_MWS_ASM: [WLAN->ASM] Cli Request Return Val=%d 
5205,II,COEX_MWS_ASM: [ASM_CHMASK][Err] Unexpected ChMask Completed(TxChMask:0x%x, RxChMask:0x%x) 
5204,II,COEX_MWS_ASM: [ASM_CHMASK] Completed(TxChMask:0x%x, RxChMask:0x%x)  
5203,II,COEX_MWS_ASM: [Err][ASM_CHMASK] Requested chmask(0x%x) is different then Nofication chmask(0x%x) 
5202,I,COEX_MWS_ASM: [Info][ASM_CHMASK]Pending Msg Count:%d 
5201,,COEX_MWS_ASM: [Err]: Stuck in While loop 
5200,I,COEX_MWS_ASM: [ASM_CHMASK]Target ChMask is same as Present ChMask (0x%x) 
5199,,COEX_MWS_ASM: [Info]:ASM DE-INIT Done 
5198,I,COEX_MWS_ASM: [Warning][WLAN->ASM]:Illegal deregister W/o register: Client_id(%d) 
5197,II,COEX_MWS_ASM: [Warning][WLAN->ASM]:Illegal deregister: Client_id(%d) :Request_state(%d) 
5196,I,COEX_MWS_ASM: [WLAN->ASM]:Deregister: Client_id(%d) 
5195,III,COEX_MWS_ASM: [WLAN->ASM]:Get_Ant_State:(0x%x, %d): handle(%d) 
5194,II,COEX_MWS_ASM: [Err]:Illegal WAN Grant: GrantMask[0x%x], ASM State[0x%x] 
5193,,COEX_MWS_ASM: [Warning] Grant during: Chain mask update in process 
5192,II,COEX_MWS_ASM: [Err]Wrong State:%d, GrantMask:0x%x 
5191,I,COEX_MWS_ASM: [Err]:Illegal WAN Nack: ASM State[0x%x] 
5190,,COEX_MWS_ASM: [Warning] Nack during: Chain mask update in process 
5189,II,COEX_MWS_ASM: [Err]Wrong State:%d, ReqMask:0x%x 
5188,II,COEX_MWS_ASM: [Warning]:State Diff[CH_1=%d, CH_Both=%d] 
5187,I,COEX_MWS_ASM: [Warning]Illegal Cancel when ASM_STATE is %d 
5186,,COEX_MWS_ASM: [Info][CH_1] Cancel msg not send to WAN as other client are waiting from Grant 
5185,,COEX_MWS_ASM: [Info] Send cancel msg to WAN 
5184,,COEX_MWS_ASM: [Info][CH_Both] Cancel msg not send to WAN as other client are waiting from Grant 
5183,,COEX_MWS_ASM: [Info] WLAN_CANCEL during: Chain mask update in process 
5182,II,COEX_MWS_ASM: [Err]Wrong State:%d, CancelMask:0x%x 
5181,,COEX_MWS_ASM: [Info] Release : ASM_STATE is ANT_OWN_NO_ARB 
5180,I,COEX_MWS_ASM: [Warning]Illegal Release when ASM_STATE is %d 
5179,,COEX_MWS_ASM: [Info] Keep Ant with Wlan as few requests are still open 
5178,,COEX_MWS_ASM: [Info] Rel Ant[0x2] to WAN 
5177,,COEX_MWS_ASM: [Info] Keep Ant[0x3] with Wlan as few request are still open 
5176,,COEX_MWS_ASM: [Warning]Illegal Release during Hold state 
5175,,COEX_MWS_ASM: [Warning]Illegal Release during: Chain mask update in process 
5174,II,COEX_MWS_ASM: [Err]Wrong State:%d, RelChainmask:0x%x 
5173,I,COEX_MWS_ASM: [Info]Req is on Hold for Cliend_id(%d) 
5172,I,COEX_MWS_ASM: [Err]Illegal ASM_STATE_HOLD for Resource[0x%x] 
5171,,COEX_MWS_ASM: [Info] WLAN_REQUEST during: Chain mask update in process 
5170,II,COEX_MWS_ASM: [Err]Wrong State:%d, RequestChainMask:0x%x 
5169,I,COEX_MWS_ASM: [Info]: 5G Antenna Sharing is Disable, plat_is_wtr_missing = %d  
5168,I,COEX_MWS_ASM: [Info]: 5G Antenna Sharing is Enable, plat_is_wtr_missing = %d  
5167,,COEX_MWS_ASM: [Info]:ASM INIT Done 
5166,III,COEX_MWS_ASM: [Info]Pull Pending Msg (%d,%d): Count:%d 
5165,,COEX_MWS_ASM: [Info]No Pending Msg 
5164,III,COEX_MWS_ASM: [Info]Push Pending Msg (%d,%d): Count:%d 
5163,,COEX_MWS_ASM: [Err]Pending Msg Q Full 
5162,,COEX_MWS_ASM: [Warning][Modem->ASM]Wan Grant received W/o Req, So sending Rel to Wan 
5161,II,COEX_MWS_ASM: [Err][Modem->ASM]Grant ChMask[0x%x] is Diff then Req ChMask[0x%x] 
5160,,COEX_MWS_ASM: [Warning][Modem->ASM]Multiple Grant for One Req; Ignore this Grant 
5159,II,COEX_MWS_ASM: [Modem->ASM]:Grant:Mask:0x%x, Duration:%d 
5158,I,COEX_MWS_ASM: [Err][Modem->ASM]Grant Duration (%d ms) is too less for WLAN operation 
5157,,COEX_MWS_ASM: [Warning][Modem->ASM]Wan Nack received W/o Req, So sending Rel to Wan 
5156,I,COEX_MWS_ASM: [Modem->ASM]:Nack:Duration:%d 
5155,II,COEX_MWS_ASM: [Warning][Modem->ASM]ASM State not Init.State(%d,%d) 
5154,,COEX_MWS_ASM: [Warning][Modem->ASM]Back to Back Sync Msg 
5153,I,COEX_MWS_ASM: [Err][WLAN->ASM]:Illegal Register: Client_id(%d) already registered 
5152,I,COEX_MWS_ASM: [WLAN->ASM]:Register Client_id(%d) 
5151,I,COEX_MWS_ASM: [Err][WLAN->ASM]:Illegal register notify: Client_id(%d) not registered 
5150,III,COEX_MWS_ASM: [WLAN->ASM]:Register notification event: Client_id(%d) Event:0x%x, Ant_State[0x%x] 
5149,I,COEX_MWS_ASM: [Err]Client_id[%d]: Cb is NULL 
5148,IIII,COEX_MWS_ASM: [ASM->WLAN]: CB_Event:%d, Param1: %d, Param2: %d Client_id[%d]  
5133,,COEX_MWS_ASM: [Warning]5G Ant sharing is not enabled: Cancel msg not send 
5147,,COEX_MWS_ASM: [Warning]Cancel W/o Request 
5146,,COEX_MWS_ASM: [Err]Illegal Cancel for Granted Request, Release is expected instead of Cancel 
5145,,COEX_MWS_ASM: [Info]Canceling the Nacked Request 
5144,,COEX_MWS_ASM: [Info]Canceling the Request, because No response from WAN 
5143,,COEX_MWS_ASM: [ASM->Modem]:Cancel 
5142,,COEX_MWS_ASM: [Warning]5G Ant sharing is not enabled: Extend msg not send 
5141,II,COEX_MWS_ASM: [ASM->Modem]:Extend Duration(%d ms),Granted Duration(%d ms) 
5140,,COEX_MWS_ASM: [Warning]5G Ant sharing is not enabled: Release msg not send 
5139,,COEX_MWS_ASM: [Warning]Rel W/o Grant 
5138,II,COEX_MWS_ASM: [Warning]Rel_mask[0x%x] is Diff thn Grant_Mask[0x%x] 
5137,I,COEX_MWS_ASM: [ASM->Modem]:Rel[0x%x] 
5136,,COEX_MWS_ASM: [Warning]5G Ant sharing is not enabled: Request msg not send 
5135,II,COEX_MWS_ASM: [Warning]Back to Back Qsoc Req. Old Req Granted(%d), Nacked(%d) 
5134,III,COEX_MWS_ASM: [ASM->Modem]:Req: Mask[0x%x], Type[%d], Reason[%d] 
5133,,COEX_MWS_ASM: [Warning]5G Ant sharing is not enabled: Cancel msg not send 
5132,,COEX_MWS_ASM: [Err][ASM->Modem]:Sync Req W/o Resp from Modem 
5131,I,COEX_MWS_ASM: [ASM->Modem]:Sync Req, WLAN State: %d 
5130,,COEX_MWS_ASM: [Warning]5G Ant sharing is not enabled: Sync resp msg not send 
5129,II,COEX_MWS_ASM: [ASM->ASM]:Virtual Sync Resp:Arb(%d),AntOwn(%d) 
5128,II,COEX_MWS_ASM: [Modem->ASM]:Sync Resp:Arb(%d),AntOwn(%d) 
5127,II,COEX_MWS_ASM: [Modem->ASM]:Sync Req:Arb(%d),AntOwn(%d) 
5126,I,COEX_MWS_ASM: [ASM->Modem]:Sync Resp, WLAN State: %d 
5125,II,COEX_MWS_ASM: [Info] Client(%d) Granted (%d ms) 
5124,,COEX_MWS_ASM: [ASM_STATE_UPDATE]Resource Mask(0x3) is put On Hold 
5123,I,COEX_MWS_ASM: [Err]ASM_STATE_UPDATE:Illegal state(%d) of CH_1 
5122,I,COEX_MWS_ASM: [Err]ASM_STATE_UPDATE:Illegal resource mask(%d) 
5121,IIIIII,COEX_MWS_ASM: [ASM_STATE_UPDATE](0x%x,%d):CH_1[%d->%d], CH_BOTH[%d->%d] 
5120,IIIIII,COEX_MWS_WWAN_STATE: [FILL_BAND_INFO] tech:%u, freq:%u, dir:%u, bw:%u, token_state:%d, token_token:%d 
5119,IIIIII,COEX_MWS_WWAN_STATE: [LPL] Fill band info: %d, %d, %d, %d, %d, %d, 
5118,II,COEX_MWS_WWAN_STATE: [Error] cannot append new tech (tech:%d freq) to Band_info_table, all entries used 
5117,IIIIII,COEX_MWS_WWAN_STATE: [Error] Fill band info failed, tech_info[] full: %d, %d, %d, %d, %d,%d 
5116,I,COEX_MWS_OTHER: WAL_MWSCOEX_CHAVD_RPT_ALLOW_FLAG value = %d 
5115,,COEX_MWS_OTHER: [SAP_CHAVD_DEBUG] CoexFreqAvoid function was NULL 
5114,,COEX_MWS_OTHER: Modem is considered offline, as there is no response to Active conflict req 
5113,III,COEX_MWS_ENCODE_SEND: [WIFI_STATE_INFO] token:%u, hp_evnt_len:%u, conn_len:%u 
5112,II,COEX_MWS_ENCODE_SEND: [WIFI_STATE_INFO-HP] freq:%d, bw_dir:%u 
5111,II,COEX_MWS_ENCODE_SEND: [WIFI_STATE_INFO-Conn] freq:%d, bw_dir:%u 
5110,III,COEX_MWS_ENCODE_SEND: [SYNC_REQ], Tech:%u, token(state:%u, token:%u) 
5109,,COEX_MWS_ENCODE_SEND: [ACTIVE_CONFLICT_REQ] 
5108,,COEX_MWS_ENCODE_SEND: [SYNC_RESP] 
5107,I,COEX_MWS_ENCODE_SEND: [Err]msgid(0x%x) 
5106,II,COEX_MWS_ERROR: excced buffer size:msg=%d, length=%d 
5105,,COEX_MWS_OTHER: [Err] LTE index is invalid when sending SYNC_UPDATE_IND 
5104,III,COEX_MWS_ENCODE_SEND: [SINR_START_IND] Tech:0x%x, Carrier:0x%x, Alpha:%d 
5103,II,COEX_MWS_ENCODE_SEND: [SINR_READ_REQ] Tech:0x%x, Carrier:0x%x 
5102,II,COEX_MWS_ENCODE_SEND: [SINR_STOP_IND] Tech:0x%x, Carrier:0x%x 
5101,I,COEX_MWS_ENCODE_SEND: [Err] SINR_FillTX : Unknown cmd(0x%x) 
5100,IIIIIII,COEX_MWS_OTHER: [DETECT_TIMER] TxThr:%u,Flags:0x%x,Curr:%u,TDM = %d,RSSI_TDM:%d,SINR_TDM:%d,low rx rate = %d 
5099,,COEX_MWS_OTHER: [DETECT_TIMER] Modem is considered offline by WLAN now 
5098,IIIIII,COEX_MWS_PA_MUTE: TX_Grant[%d][%d]: wlan(%d),value(%d), thre(%d), time(%u) 
5097,I,COEX_MWS_ERROR: [LPL] [ERR] SUB %d is trying to blank TX twice! 
5096,I,COEX_MWS_PWB: [LPL] SUB %d is entering TXB 
5095,II,COEX_MWS_PWB: [LPL] SUB %d is entering TXB - wlanid %d 
5094,I,COEX_MWS_ERROR: [LPL] [ERR] SUB %d is trying to exit TXB without entering TXB policy! 
5093,I,COEX_MWS_PWB: [LPL] SUB %d is exiting TXB 
5092,II,COEX_MWS_PWB: [LPL] SUB %d is exiting TXB - wlanid %d 
5090,I,COEX_MWS_OTHER: [SAR] Error: invalid active index set (%d) 
5091,II,COEX_MWS_OTHER: [SAR] Error: number of limits doesn't match (%d!=%d) 
5090,I,COEX_MWS_OTHER: [SAR] Error: invalid active index set (%d) 
5089,IIIII,COEX_MWS_OTHER: [SAR][Error] counted more SAR limit rows (%d) than recorded (%d) band(%d) mod(%d) chain(%d) 
5088,IIIIII,COEX_MWS_OTHER: [SAR] %d get sar_limits[%d](chain,band, mod, limit)=(%d,0x%x,0x%x,0x%x) 
5087,I,COEX_MWS_OTHER: [SAR]returning from get_sar_limit_rows (%d) 
5086,I,COEX_MWS_ERROR: msgid(0x%x) 
5085,III,COEX_MWS_CP_UNFRAME: Ret(%u), CRC [Err] (rcvd:%d,Calc:%d) 
5084,I,COEX_MWS_CP_UNFRAME: Ret(%u) 
5083,II,COEX_MWS_ERROR: SUB %d is trying to sleep but no policy to exit, current policy = %d 
5082,III,COEX_MWS_ERROR: [LPL] [Err] SUB %d timer expired!, now = %u, end %u 
5081,I,COEX_MWS_ERROR: [LPL][Err] Recovering because missing sleep ind (%u)ms 
5080,II,COEX_MWS_INIT: LTE_PHY_EXIST = %d ;coex_flags:0x%x 
5079,I,COEX_MWS_INIT: COEX_MWS_2G_ANT_SHARE = %d 
5078,I,COEX_MWS_INIT: COEX_BT_THIRD_ANT = %d 
5077,I,COEX_MWS_INIT: COEX_LTEU_ANT_CONF = %d 
5076,,COEX_MWS_INIT: MWS Init Done 
5075,II,COEX_MWS_WWAN_STATE: [QMI_LTE_STATE_IND] valid:%u, ca_valid:%d  
5074,II,COEX_MWS_WWAN_STATE: [QMI_LTE2_STATE_IND] valid:%u, ca_valid:%d  
5073,IIII,COEX_MWS_WWAN_STATE: [QMI_LTE_STATE_CC_INFO] band-idx:0x%x, dimension:%u, frame_offset:%d, tdd_config:%d 
5072,III,COEX_MWS_REMOTE_EVENT: [Err] **major** error (i:%d, band_index:0x%x, len:0x%x) 
5071,IIII,COEX_MWS_PWB: [PWB_CALC] cc_id=%d, sinrWLANOFFAve=%d, sinrWLANONAve=%d, deltaN=%d 
5070,III,COEX_MWS_PWB: [PWB_CALC] TURN ON FORCED TDM : RSSI: (RSSI[%d] + P(n)[%d]) < RSSI_Threshold[%d] 
5069,IIIIIII,COEX_MWS_PWB: [PWB_CALC] Max_delta_N=%d, P(n+1):%d, P(n)=%d, P(Max)=%d, needUpdate=%d, F TDM = %d, RSSI:%d 
5068,III,COEX_MWS_PWB: [PWB_CALC] TURN ON FORCED TDM : SINR: Max_Sinr_Diff=%d, P(n)=%d, needUpdate=%d 
5067,,COEX_MWS_PWB: [PWB_Err]: TX Grant : Block during Active Conflict = 0 
5066,II,COEX_MWS_PWB: [PWB_Helper]:Active Conflict:0, Action:%d, Value:%d 
5065,,COEX_MWS_OTHER: [Err][SINR_RESP_TIMER] 
5064,I,COEX_MWS_PWB: PWB WLAN ON static power = %d 
5063,,COEX_MWS_PWB: [PWB_UPDATE]Event[PWB_PAUSE] State[PWB_HALTED] 
5062,,COEX_MWS_PWB: [PWB_UPDATE]Event[PWB_RESUME] State[WLAN_ON_SINR_START] 
5061,I,COEX_MWS_PWB: [PWB_UPDATE]Event[PWB_SCHEME_ENABLE] State[UNINIT->SINR_START] UN-BLOCK_WLAN for %d usec 
5060,,COEX_MWS_CST_AUTOMATION: *****CXM_LTE_SET_WLAN_POWERBACKOFF_ACTIVE(Client)***** 
5059,II,COEX_MWS_PWB: [PWB_UPDATE]Event[SINR_READ] c_id=%d SINR_ON=%d 
5058,I,COEX_MWS_PWB: [PWB_UPDATE][Err]Event[SINR_RESP_TIMEOUT] before SINR_UPDATE, wlan_on_resped_bitmap= 0x%x 
5057,I,COEX_MWS_PWB: [PWB_UPDATE] SINR_OFF Duration (%d usec) 
5056,II,COEX_MWS_PWB: [PWB_UPDATE]Event[SINR_READ] c_id=%d, SINR_OFF=%d 
5055,I,COEX_MWS_PWB: [PWB_UPDATE][Err]Event[SINR_RESP_TIMEOUT] before SINR_UPDATE, wlan_off_resped_bitmap= 0x%x 
5054,,COEX_MWS_PWB: [PWB_UPDATE]State[WLAN_OFF_WAIT_RESP->WLAN_OFF_SINR_STOP] 
5053,,COEX_MWS_PWB: [PWB_UPDATE]Event[PWB_RSSI_CHANGE] 
5052,,COEX_MWS_PWB: [PWB_UPDATE]Event[PWB_DISABLE] 
5051,II,COEX_MWS_PWB: [PWB_UPDATE]State[FORCED_TDM_ENABLED] RSSI_TDM:%d, SINR_TDM:%d 
5050,,COEX_MWS_CST_AUTOMATION: [PWB_UPDATE]CxM_CP_WLAN_Power_Backoff_DeInit 
5049,I,COEX_MWS_PWB: [PWB_UPDATE] SINR_ON  Duration (%d usec) 
5048,III,COEX_MWS_PWB: [PWB_UPDATE] Event=%d, State(%d->%d) 
5047,IIII,COEX_MWS_REMOTE_EVENT: [Err]WAL_MWSCOEX_LTE_PHY_EXIST_FLAG:%d, Stimulus:%d, Flag:0x%x Bytes: %d 
5046,IIIII,COEX_MWS_REMOTE_EVENT: stimulation:0x%x, Time_Diff:%d, Flag:0x%x, ArmTimer=0x%x, PsSavedTimer=0x%x 
5045,,COEX_MWS_REMOTE_EVENT: [SYNC_REQ] 
5044,I,COEX_MWS_REMOTE_EVENT: [SYNC_RESP] len:%u 
5043,I,COEX_MWS_REMOTE_EVENT: [SYNC_REQ] len:%u 
5042,IIII,COEX_MWS_REMOTE_EVENT: [SYNC_RESP] id:%u, Token(state:%u, token:%u), WlanToken:%d 
5041,IIII,COEX_MWS_REMOTE_EVENT: [SYNC_REQ] id:%u, Token(state:%u, token:%u), WlanToken:%d 
5040,I,COEX_MWS_REMOTE_EVENT: [SYNC_RESP] NeedExg:%u 
5039,I,COEX_MWS_REMOTE_EVENT: [SYNC_REQ] NeedExg:%u 
5038,III,COEX_MWS_REMOTE_EVENT: [SYNC_UPDATE_IND], id:%u, Token(state:%u, token:%u) 
5037,I,COEX_MWS_REMOTE_EVENT: [TECH_STATE_UPDATE] Stimulus:%u 
5036,I,COEX_MWS_REMOTE_EVENT: [WWAN_STATE_IND] Stimulus:%u 
5035,II,COEX_MWS_REMOTE_EVENT: [SINR_READ_RESP] sinr:%d, cc_id:%u 
5034,III,COEX_MWS_REMOTE_EVENT: [Error] Stimulus(0x%x) cc_id (0x%x) >= MAX value (0x%x). MPSS mismatch? 
5033,,COEX_MWS_REMOTE_EVENT: [Err][SINR_READ_RESP] E_TECH_NOT_ACTIVE 
5032,I,COEX_MWS_REMOTE_EVENT: [Err][SINR_READ_RESP] report is not valid (%d) 
5031,III,COEX_MWS_REMOTE_EVENT: [ACTIVE_CONFLICT] valid:%u, len:%u, Conflict = %d 
5026,I,COEX_MWS_REMOTE_EVENT: [Error] Stimulus(0x%x) incorrect Victim Table Style MWS_VICTIM_TABLE_STYLE_V1. MPSS mismatch? 
5030,II,COEX_MWS_REMOTE_EVENT: [ACTIVE_CONFLICT][Err] wlan_active_conflicts_len (%d) > %d 
5029,II,COEX_MWS_REMOTE_EVENT: [ACTIVE_CONFLICT][Err] too many retries: wlan_active_conflicts_len (%d) > %d 
5028,IIII,COEX_MWS_REMOTE_EVENT: [ACTIVE_CONFLICT] index:0x%x, carrier:%d, Mws_Tech:0x%x, Victim_idx:%d 
5027,II,COEX_MWS_REMOTE_EVENT: [POTENTIAL_CONFLICT] valid:%u, len:%u 
5026,I,COEX_MWS_REMOTE_EVENT: [Error] Stimulus(0x%x) incorrect Victim Table Style MWS_VICTIM_TABLE_STYLE_V1. MPSS mismatch? 
5025,II,COEX_MWS_REMOTE_EVENT: [Error] Stimulus(0x%x) Too many Potential Conflicts (%d) 
5024,III,COEX_MWS_REMOTE_EVENT: [Err]QSocK : WAL_MWSCOEX_LTE_PHY_EXIST_FLAG:%d, msg:%d, Flag:0x%x 
5023,I,COEX_MWS_ANT_DIVERSITY: COEX_ANTENNA_SHARING_IND & wan_state=%d 
5022,III,COEX_MWS_ANT_DIVERSITY: Received Ant Share GRANT with duration=%d. AntShState=0x%x, wan_state=%d 
5021,II,COEX_MWS_ANT_DIVERSITY: Received Ant Share RELEASE. AntShState=0x%x, wan_state=%d 
5020,IIII,COEX_MWS_ANT_DIVERSITY: [Qsock_Rcvd] Modem ACQ Msg:%u, Curr ACQ State:%u, Paused:%u, Hyst:%u 
5019,,COEX_MWS_ANT_DIVERSITY: [Qsock_Rcvd] Unexpected Modem ACQ msg during Paused State 
5018,I,COEX_MWS_ANT_DIVERSITY: [Qsock_Rcvd] Modem ACQ NONE :%d 
5017,III,COEX_MWS_REMOTE_EVENT: [METRICS_REPORT] sinr_system:%d, cc_id:%u, param:0x%x  
5016,I,COEX_MWS_REMOTE_EVENT: [SAR] Modem requested power reports every %dms 
5015,,COEX_MWS_REMOTE_EVENT: [SAR] Modem requested turning off RT SAR feature 
5014,I,COEX_MWS_REMOTE_EVENT: [SAR] Limit Receivend from modem: %d 
5013,IIIII,COEX_MWS_REMOTE_EVENT: [LPL] Tech: %d, Sleeping: %d, Critical: %d, RSSI: %d, Duration: %d 
5012,I,COEX_MWS_ERROR: [LPL][Warning] Back2Back Wakeup ind Ignored: Last_Ind:%d 
5011,III,COEX_MWS_ERROR: [LPL][ERR] Tech-id 0x%x  and sub-id %d is not matching with corresponding tech 0x%x 
5010,I,COEX_MWS_ERROR: [LPL][ERR] Tech-id %d is not matching with any LTE-sub tech id! 
5009,I,COEX_MWS_ERROR: [LPL][ERR] SLEEP/WAKEUP indication is received for non-LTE tech: tech_id = %d 
5008,,COEX_MWS_REMOTE_EVENT: [METRICS_CMD] 
5007,,COEX_MWS_REMOTE_EVENT: Received GNSS coex msg 
5006,I,COEX_MWS_REMOTE_EVENT: [Err]Unknown QSocket message: %d 
5005,II,COEX_MWS_OTHER: [SAR] RT-SAR: applied limit reason (%d) MIMO limits? (%d) 
5004,IIIII,COEX_MWS_OTHER: [SAR] Calc done. reason (0x%x) measurements((0x%x,0x%x)(0x%x,0x%x)) 
5003,IIII,COEX_MWS_OTHER: [SAR] RTSAR averages calc done ((0x%x,0x%x),(0x%x,0x%x)) 
5002,,COEX_MWS_OTHER: [SAR] RTSAR Averages encountered error, not returning an average 
5001,III,COEX_MWS_SAR: chain0=%x, chain1=%x, result=%x 
5000,IIII,COEX_MWS_SAR: cmd=%d, rows=%d, commit=%d, version=%d 
4999,IIIII,COEX_MWS_SCHEME_UPDATE: chavd_1_0:0x%x, chavd_3_2:0x%x, tdm_pb:0x%x, Final_scheme:0x%x, High duty cycle = %d 
4998,IIII,COEX_WCI2_TYPE3: [Err] Fail to send Type3_Msg:0x%x, W2G:0x%x, W5G:0x%x, Param:%d 
4997,IIII,COEX_WCI2_TYPE3: Sent Type3_Msg:0x%x, W2G:0x%x, W5G:0x%x, Param:%d 
4996,IIII,COEX_MWS_WWAN_STATE: [LPL] WLAN_FREQ: %d, WWAN_FREQ: %d, SUB_id: %d, Combo_id: %d 
4995,I,COEX_MWS_ERROR: [ERR] Invalid TDD config is received from modem: 0x%x 
4994,IIII,COEX_MWS_TDM: [TDM_EVENT] Event(%d) Type(%d) TDM Running(%d) Sticky(%d) 
4993,,COEX_MWS_TYPE2_TX: [Err] mws tx tdm failed. wait and retry 
4992,I,COEX_MWS_TYPE2_TX: [Err] mws tx tdm full:%d 
4991,II,COEX_MWS_TYPE2_TX: mws tx tdm remain:%d, Tx_FiFo Depth: %d 
4990,,COEX_MWS_ANT_DIVERSITY: Updating ant share chmask during init 
4989,IIIIIII,COEX_MWS_WLAN_EVENT: stimulation:%u, W_state:0x%x, WlanWorstFreq:%d, WlanToken:%u, Freq:%d, W2G:0x%x, W5G:0x%x 
4988,IIIIIII,COEX_MWS_PWB: [PWR_LIMIT_SET] PrevPwrLimit:%u, finalPwr:%u, sarPwr:%u, pwb_power:%u pwb_static_power:%u, MaxPwrLimit:%u, SPB:%d 
4987,I,COEX_MWS_ERROR: [LPL] SUB %d is trying to set static power limit twice! 
4986,II,COEX_MWS_PWB: [LPL] SUB %d is entering SPWB with PWR %d 
4985,I,COEX_MWS_ERROR: [LPL] SUB %d is trying to reset static power without entering SPWB 
4984,I,COEX_MWS_PWB: [LPL] SUB %d is exiting SPWB 
5279,,COEX_GENERIC_ERROR: COEX_LIST_OVERFLOW_ERROR 
5278,II,COEX_GENERIC_ERROR: id(%u) isPaused(%u) 
5277,,COEX_GENERIC_ERROR: COEX_ERROR_GET_RSSI 
5276,,COEX_GENERIC_ERROR: COEX_ERROR_GET_RSSI_SEQ 
5275,IIIII,COEX_FORCE_OCS: wlan_dur(%u) bt_dur(%u)  wlan_wght(%u) bt_wght(%u) algo(%u) 
5274,III,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [Version query] 
5273,IIIIII,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [BT system reset] sub sys bit(0x%x) rst reason(0x%x) id(0x%x) 
5272,IIIII,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [Report reg] address(0x%x) value(0x%x) 
5271,III,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [BT queue overflow] 
5270,IIII,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [Request WLAN update BT flags] reason(0x%x) 
5269,IIIII,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [Additional BT link info] id(0x%x) A2DP sink(0x%x) 
5268,IIIIII,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [BT Airtime Stats Response] status(%d) start(0x%x) interval(0x%x) 
5267,IIIIIIIII,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [BT Airtime Stats Status] status(%d) page(%d) cnt1(0x%x) cnt2(0x%x) cnt3(0x%x) cnt4(0x%x) 
5266,IIIIIII,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [ACL Interactive] id(%u) reason(%u) timeslice(%u) start(%u) 
5265,IIIIIIII,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [Adv BT Prof Info] type:prof(%u) rsvd(%u) grpId(%u) cfg(%u) conn(%u) 
5264,IIIIIIIII,WAL_COEX_GPM_RECV: [0x0C] [0x30] timer[%u]: [Adv BT Connect Stat] type:prof(%u) rsvd(%u) grpId(%u) cfg(%u) conn(%u) sniff(%u) win(%u) intvl(%u) 
5263,IIIIIIIII,WAL_COEX_GPM_RECV: [0x0C] [0x%x] timer[%u]: [Adv BT Status Update] type:prof(%u) rsvd(%u) grpId(%u) status(%u) reason(%u) piconet(%u) 
5262,IIIIIII,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [BT QoS Update] id(0x%x) Link Bandwidth(%u) Non-link Bandwidth(%u) MaxLatency (%u) 
5261,IIIII,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [BT report TX power] LinkId(0x%x) Power(0x%x) 
5260,IIIII,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [BT report RSSI] LinkId(0x%x) RSSI(0x%x) 
5254,III,COEX_INVALID_GPM: [0x%x] [0x%x] timer[%u] : [Unknown GPM type subtype] 
5259,III,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u] : [BT calibration request] 
5258,III,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u] : [BT calibration grant] 
5257,III,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u] : [BT calibration done] 
5256,III,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u] : [ANT message] 
5255,III,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u] : [BT Debug Msg] 
5254,III,COEX_INVALID_GPM: [0x%x] [0x%x] timer[%u] : [Unknown GPM type subtype] 
5253,IIIII,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [Version resp] major(0x%x) minor(0x%x) 
5252,IIIII,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [Status query] BT bmap(0x%x) WLAN bmap(0x%x) 
5251,III,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [BT prof info] 
5250,IIIIIIIII,WAL_COEX_GPM_RECV: [BT prof info] type(0x%x) id(0x%x) state(0x%x) role(0x%x) rate(0x%x) voice(0x%x) T(0x%x) W(0x%x) A(0x%x) 
5249,IIIIIIII,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [Status update] type(0x%x) id(0x%x) state(0x%x) optype(0x%x) reason(0x%x) 
5248,IIIIII,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [BT scan activity report] type(0x%x) start(0x%x) id(0x%x) 
5247,IIII,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [Scan activity bitmap] bitmap(0x%x) 
5246,IIIIII,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [BT ACL inactivity report] id(0x%x) rsvd(0x%x) slots(0x%x) 
5245,IIII,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [RXSS min threshold] RXSS min(0x%x) 
5244,IIIIIII,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [Sched msg trigger resp] type(0x%x) id(0x%x) prio(0x%x) time2trig(0x%x) 
5243,IIIII,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [Scan op] type(0x%x) time2scan(0x%x) 
5242,III,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [BT connect status] 
5241,IIIIIII,WAL_COEX_GPM_RECV: [BT connect status] op(0x%x) id(0x%x) role(0x%x) win(0x%x) TO/winoff(0x%x) intvl(0x%x) conn latency(0x%x) 
5240,III,WAL_COEX_GPM_RECV: [0x%x] [0x%x] timer[%u]: [BT scan update] 
5239,IIIIIII,WAL_COEX_GPM_RECV: [BT scan update] page(0x%x) type(0x%x) intrvl(0x%x) win(0x%x) id(0x%x) status(0x%x) timeout(0x%x) 
5238,IIIIIIII,WAL_COEX_WGHTS: Static: W0[wl_idle(%d) sw_ctrl3(%d) sw_ctrl2(%d) sw_ctrl1(%d)] W1[sw_ctrl0(%d) wait_bcn(%d) wait_ack_cts(%d) selfgen(%d] 
5237,IIIIIIII,WAL_COEX_WGHTS: FES Tx: W4[null(%d) data(%d) qos(%d) rsvd(%d)] W5[om(%d) oc(%d) od(%d) oo(%d)] 
5236,IIIIIIII,WAL_COEX_WGHTS: FES Rx: W6[bcn(%d) conn(%d) scan(%d) ibss(%d)] W7[psp(%d) bar(%d) cts(%d) rsvd(%d)] 
5235,IIIIIIII,WAL_COEX_WGHTS: FES Rx: W8[null(%d) data(%d) qos(%d) rsvd(%d)] W9[om(%d) oc(%d) od(%d) oo(%d)] 
5234,IIII,WAL_COEX_WGHTS: Static: W10[rx_lvl3(%d) rx_lvl2(%d) rx_lvl1(%d) (%d)] 
5233,IIIIIIII,WAL_COEX_WGHTS: FES Tx: W2[bcn(%d) conn(%d) scan(%d) ibss(%d)] W3[psp(%d) bar(%d) cts(%d) rsvd(%d)] 
4956,,WAL_COEX_WGT2PRIO: Invalid Weight Group 
5281,IIIIIIIII,COEX_SET_COEX_WEIGHT: wght_grp(%u) reason(%u) wlan_idle(%u) hid_con_tx_o(%u) bcon_tx_o(%u) bcon_rx_o(%u) prio_wlan_fc(%u) flow_ctrl(0x%x) concur_tx(%u) 
5280,IIII,WAL_COEX_80211_FRAME: tx_qid(%u) type[%d] subtype[%d] pwr[%u] 
5302,IIIII,WAL_COEX_BAND_CHANGE: Pdev(%u) NewFreq(%u) WLANSysState(0x%x) CurBand(%u) HWMode(%u) 
5301,I,COEX_CHANNEL_CHANGE: Invalid pdev_id %u was passed 
5300,IIIIIII,WAL_COEX_MODE_CHANGE: new_mode(%u) old_mode(%u) band_mac_map(0x%x) mac0_settings(0x%x) mac1_settings(0x%x) mac0_band(%u) mac1_band(%u) 
5299,IIIII,COEX_RX_RATE_THRESHOLD: RSSIType(%u) LowKpbsThresh(%u) UpperKpbsThresh(%u) NumPPDUsBelowThresh(%u) NumPPDUsAboveThresh(%u) 
5298,IIIIII,COEX_MWS_PA_MUTE: src(%u) event(%u) wlan(%u) mode(%u) mac0(%d), mac1(%d) 
5297,III,COEX_MWS_PA_MUTE: Error(0x%x) mac0(%d), mac1(%d) 
5296,IIII,COEX_RX_RATE_THRESHOLD: ChWidth(0xFF) TriggRate(%u) XputMonitorActiveNum(%u) TotalCoexIntrvls(%u) EventType(%u) 
5295,IIIII,COEX_RX_RATE_THRESHOLD: ChWidth(%u) TriggRate(%u) XputMonitorActiveNum(%u) TotalCoexIntrvls(%u) EventType(%u) 
5294,IIIIII,WAL_COEX_POWER_CHANGE: mac(%u) event_type(%u) cur_state(0x%x) new_state(0x%x) macs_up(0x%x) mac_woke(0x%x) 
5293,II,COEX_GENERIC_ERROR: ErrCode(%u) RSSIType(%u) 
5292,I,COEX_GENERIC_ERROR: ErrCode(%u) 
5291,II,UPDATE_SPECIFIC_AP_STATE: connected:%u, behaviour:%u 
5290,I,WAL_COEX_VDEV_STATE: Error(0x%x) 
5289,,COEX_VDEV_STATE: 2g vdev not paused 
5288,,COEX_VDEV_STATE: 2g vdev not unpaused 
5287,III,WAL_COEX_VDEV_STATE: VDEV_MIGRATE: old_mac_id %u, new_mac_id %u, old_mac_sleep_state %u ! 
5286,II,WAL_COEX_VDEV_STATE: VDEV_MIGRATE: ERROR - Invalid old_mac_id %u / new_mac_id %u was passed ! 
5285,IIIIIIIII,WAL_COEX_VDEV_STATE: Error(0x%x) id(%u) stimulus(%u) vdev_state(0x%x) strict_dur_scan(%u) num_peers(%u) pdev(%u) chan(%u) op(%u) 
5284,II,COEX_POWER_CHANGE: Swapping the MAC id for SLEEP_VOTE from %d to %d due to possible SYNC DBS SCAN 
5283,I,COEX_POWER_CHANGE: ERROR - Invalid mac_id %u was passed 
5282,I,COEX_POWER_CHANGE: PHY is ON - Coex recipe change is best effort. mac_id(%d) 
4956,,WAL_COEX_WGT2PRIO: Invalid Weight Group 
4956,,WAL_COEX_WGT2PRIO: Invalid Weight Group 
5316,III,COEX_GET_T2BT: t2bt(%u) sched_time(%u) curr_time(%u) 
5315,I,COEX_EXIT_OCS: Error - Switching to FREE_RUN for %u msecs due to ENTER_DYNAMIC_OCS failure 
5314,I,COEX_EXIT_CRITICAL_OCS: Error - Switching to FREE_RUN for %u msecs due to UPDATE_CRITICAL_OCS failure 
5313,I,COEX_EXIT_CRITICAL_OCS: Error - Switching to FREE_RUN for %u msecs due to ENTER_CRITICAL_OCS failure 
5312,IIIIIII,WAL_COEX_SCHED_RESULT: Error(0x%x) SchedulerReq(%u) Algo(%u) PrevAlgo(%u) Policy(%u) NextInterval(%u) WlanRxState(%u) 
5311,I,COEX_EXIT_OCS: Error - Switching to FREE_RUN for %u msecs due to UPDATE_OCS failure 
5310,I,COEX_EXIT_OCS: Error - Switching to FREE_RUN for %u msecs due to ENTER_OCS failure 
5309,IIIIIIIII,COEX_TRF_SHAPE_OCS: interval(%u) Dur(%u) Latency(%u) VdevPauseDelay(%u) ConcurrState(0x%x) nonlinkExtraIntervals(%u) wlan_2g(%u) a2dp_crit(%u) bt_qos_pct(%u) 
5308,II,COEX_SET_WEIGHT_GROUP3: Setting coex weight group 3 BT hasn't been non-critical pCoexDev->DynamicOcsSchedReq = %d  pBtCoexWeightDev->resetWtVdevPause= %d 
5307,I,COEX_SET_WEIGHT_GROUP6: Setting coex weight group six pCoexDev->DynamicOcsSchedReq %d 
5306,II,COEX_SET_WEIGHT_GROUP3: Else part pCoexDev->DynamicOcsSchedReq = %d  pBtCoexWeightDev->resetWtVdevPause= %d 
5305,IIIII,COEX_TRF_FREERUN: NextIntvl(%u) AllocatedBtIntervals(%u) BtIntervalCnt(%u) AllocatedWlanIntervals(%u) WlanIntervalCnt(%u) 
5304,IIIII,COEX_TRF_SHAPE_OCS: interval(%u) Dur(%u) Latency(%u) ConcurrState(0x%x) wlan_2g(%u) 
5303,IIIIII,COEX_TRF_SHAPE_PSP: Error(0x%x) NextInterval(%u) wght(%u) IntrvalDur(%u) BtTriggerRecieved(%u) IS_PSP_ALG_WLAN_CRITICAL(%u) 
5320,,COEX_MWS_QSOCK: Unable to send as socket is in closed state 
5319,I,COEX_MWS_QSOCK: ipcr_find_name failed with rc=0x%x 
5318,I,COEX_MWS_QSOCK: Sending QSock msg (%d) 
5317,I,COEX_MWS_QSOCK: qsendto failed with rc=0x%x 
5320,,COEX_MWS_QSOCK: Unable to send as socket is in closed state 
5319,I,COEX_MWS_QSOCK: ipcr_find_name failed with rc=0x%x 
5318,I,COEX_MWS_QSOCK: Sending QSock msg (%d) 
5317,I,COEX_MWS_QSOCK: qsendto failed with rc=0x%x 
5318,I,COEX_MWS_QSOCK: Sending QSock msg (%d) 
5317,I,COEX_MWS_QSOCK: qsendto failed with rc=0x%x 
5329,,COEX_MWS_QSOCK: closing the socket 
5328,I,COEX_MWS_QSOCK: [Err]rcvd invalid version. expected=0x%x 
5327,I,COEX_MWS_QSOCK: qsocket() failed, rc=%d 
5326,I,COEX_MWS_QSOCK: qbind() failed, rc=%d, closing the socket 
5325,,COEX_MWS_QSOCK: qsocket open success
 
5324,I,COEX_MWS_QSOCK: qsetsockopt() failed, rc=%d, closing the socket 
5323,I,COEX_MWS_QSOCK: qrecv() taking too long. Time taken = %d ms
 
5322,I,COEX_MWS_QSOCK: wal_coex_qsock_recv -> qrecv() returned err %d
 
5321,I,COEX_MWS_QSOCK: Received QSock msg (%d) 
5365,II,COEX_MWS_PA_MUTE: 2g CH0 Mute Wlan:%d, Mask:0x%x 
5364,II,COEX_MWS_PA_MUTE: 2g CH0 UnMute Wlan:%d, Mask:0x%x 
5363,II,COEX_MWS_PA_MUTE: 2g CH1 Mute Wlan:%d, Mask:0x%x 
5362,,COEX_MWS_PA_MUTE: Skipping 2g CH1 Mute since antenna is with WAN 
5361,II,COEX_MWS_PA_MUTE: 2g CH1 UnMute Wlan:%d, Mask:0x%x 
5360,II,COEX_MWS_PA_MUTE: 5g CH0 Mute Wlan:%d, Mask:0x%x 
5359,II,COEX_MWS_PA_MUTE: 5g CH0 UnMute Wlan:%d, Mask:0x%x 
5358,II,COEX_MWS_PA_MUTE: 5g CH1 Mute Wlan:%d, Mask:0x%x 
5357,II,COEX_MWS_PA_MUTE: 5g CH1 UnMute Wlan:%d, Mask:0x%x 
5356,,COEX_MWS_PA_MUTE: PA thread exit close qdi 
5355,,COEX_MWS_PA_MUTE: PA thread handle null 
5354,,COEX_MWS_PA_MUTE: De-Reg Pre STM Crash Handler : Success 
5353,,COEX_MWS_PA_MUTE: De-Reg Pre STM Crash Handler : Fail 
5352,,COEX_MWS_PA_MUTE: QDI open success 
5351,,COEX_MWS_PA_MUTE: Reg Pre STM Crash Handler : Success 
5350,,COEX_MWS_PA_MUTE: Reg Pre STM Crash Handler : Fail 
5349,,COEX_MWS_PA_MUTE: QDI open fail 
5348,III,COEX_MWS_PA_MUTE: Invalid wlan id. wlan=%d, req=%d, client=%d 
5347,I,COEX_MWS_PA_MUTE: WLAN-2.4GHz: Unable to unmute because client=%d muted it! 
5344,I,COEX_MWS_PA_MUTE: Invalid client id.client=%d 
5346,,COEX_MWS_PA_MUTE: 2.4Ghz-MUTE Req from SUB1/SUB2/PWB, so don't unmute 
5345,III,COEX_MWS_PA_MUTE: Invalid wlan id. wlan=%d, req %d, client %d 
5344,I,COEX_MWS_PA_MUTE: Invalid client id.client=%d 
5343,,COEX_MWS_PA_MUTE: 5Ghz-MUTE Req from SUB1/SUB2/PWB, so don't unmute 
5342,I,COEX_MWS_PA_MUTE: WLAN-5GHz: Unable to unmute because client=%d muted it! 
5341,IIIII,COEX_MWS_PA_MUTE: macid:%d,event:%d,band:%d,src:%d,Other:0x%x 
5340,I,COEX_MWS_PA_MUTE: Muting on power up 2g-MacId:%d 
5339,I,COEX_MWS_PA_MUTE: Muting on power up 5G-MacId:%d 
5338,,COEX_MWS_PA_MUTE: Invalid Band 
5337,,COEX_MWS_PA_MUTE: wal_coex_pa_pre_stm_crash_handler: CXM_QDI_INTF_WLAN_CRASH_IND Sent 
5336,I,COEX_MWS_PA_MUTE: [Err]: Invalid wlan id:%d 
5334,,COEX_MWS_PA_MUTE: $$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$ 
5335,II,COEX_MWS_PA_MUTE: $$$$$$$$$$      PA_MUTE_RECOVERY for MAC:%u Client:%u      $$$$$$$$ 
5334,,COEX_MWS_PA_MUTE: $$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$ 
5334,,COEX_MWS_PA_MUTE: $$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$ 
5335,II,COEX_MWS_PA_MUTE: $$$$$$$$$$      PA_MUTE_RECOVERY for MAC:%u Client:%u      $$$$$$$$ 
5334,,COEX_MWS_PA_MUTE: $$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$ 
5330,,COEX_MWS_PA_MUTE: ******************************************************************* 
5330,,COEX_MWS_PA_MUTE: ******************************************************************* 
5333,II,COEX_MWS_PA_MUTE: ***** Error MAC[%u] Muted for more than %d ms ***************** 
5332,II,COEX_MWS_PA_MUTE: ***** From [%u] --> Now [%u]  
5331,IIIIII,COEX_MWS_PA_MUTE: ***** TX_Grant[%d][%d]: wlan(%d),value(%d), thre(%d), time(%u) 
5330,,COEX_MWS_PA_MUTE: ******************************************************************* 
5330,,COEX_MWS_PA_MUTE: ******************************************************************* 
5366,IIII,SUPPORT_COEX_NAN20: Profile Requires time Share = %d, ULW queued = %d, ULW sent %d, ALGO(%d) 
5368,IIIIIIII,WAL_COEX_VERSION: coex_ver(0x%x) wlan[major(%u) minor(%u)] bt[major(%u) minor(%u)] rom(%u) soc(%u) bt_features(0x%x) 
5367,,WAL_COEX_VERSION: Bluetooth version information is not available. 
5369,III,WAL_COEX_TWS_GPM: error(0x%x) status(%d) tws_linkid(%u) 
5369,III,WAL_COEX_TWS_GPM: error(0x%x) status(%d) tws_linkid(%u) 
5369,III,WAL_COEX_TWS_GPM: error(0x%x) status(%d) tws_linkid(%u) 
5370,I,: pdev=%d 
5381,IIIIIII,tsf_alloc: pdev_id = %d vdev_id = %d type = %d tsf_id = 0x%x bss_id = 0x%x pdev_tsf_id_map = 0x%x pdev_bss_id_map = 0x%x 
5380,IIIIIIII,staid_alloc: pdev_id = %d vdev_id = %d (%x.%x.%x) type = %d sta_id = 0x%x pdev_sta_id_map = 0x%x 
5379,IIIIIIII,staid_free: pdev_id = %d vdev_id = %d (%x.%x.%x) type = %d sta_id = 0x%x pdev_sta_id_map = 0x%x 
5378,I,Do bss2 context switch %d  
5377,IIIIIII,tsf_free: pdev_id = %d vdev_id = %d type = %d tsf_id = 0x%x bss_id = 0x%x pdev_tsf_id_map = 0x%x pdev_bss_id_map = 0x%x 
5376,IIIII,wal_vdev_add_random_mac_addr: pdev_id = %d vdev_id = %d spoof_mac=%x.%x.%x 
5375,IIIII,wal_vdev_del_random_mac_addr: pdev_id = %d vdev_id = %d spoof_mac=%x.%x.%x 
5374,IIIIIII,tsf_realloc (flag=0x%x): pdev_id = %d vdev_id = %d type = %d tsf_id = 0x%x bss_id = 0x%x pdev_tsf_id_map = 0x%x pdev_bss_id_map = 0x%x 
5373,IIIII,wal_vdev_restore_mac: pdev_id = %d vdev_id = %d spoof_type = %d sta_id = 0x%x spoof_sta_id=0x%x 
5372,IIIIIIII,wal_vdev_set_mac_addr: pdev_id = %d vdev_id = %d mac=%02x:%02x:%02x:%02x:%02x:%02x 
5371,IIIIIIII,wal_vdev_set_spoofed_mac_addr: pdev_id = %d vdev_id = %d spoof_mac=%x.%x.%x spoof_type=%d sta_id = 0x%x spoof_sta_id=0x%x 
5395,IIIIII,_wal_dev_reset: mode=%x,c0=%lx,c1=%lx,inprog=%d,dis=%d,en=%x 
5394,I,wal_get_mac_addresses:Halphy num_macaddr =%d,Defaulting to max WAL_NUM_MAC_ADDRESSES 
5393,IIIIII,datastall type:2 
                                 SU_RESPONSE_TYPE_MISMATCH_FAIL_CNT:%d WIFI_CBF_MIMO_CTRL_MISMATCH_FAIL_CNT:%d
                                LIFESPAN_EXPIRY_FAIL_CNT:%d MAX_SCHEDULE_RETRY_COUNT_FAIL_CNT:%d
                                WIFI_QCU_FILTERED_CNT:%d WIFI_LOWER_CBF_BW_FAIL_CNT:%d
  
5392,IIII,WIFI_LOWER_CBF_BW_FAIL_CNT:%d
                                WIFI_IBSS_NAN_STALL:%d WIFI_SW_STALL:%d WIFI_BA_ASSIST_STALL:%d 
5391,I,datastall type:3 WIFI_FLUSH_RCVD_CNT:%d 
5390,II,WAL_DBGID_STA_KICKOUT:                     peer=0x%x consecutive_null_failure=%d 
5389,III,WAL_DBGID_STA_KICKOUT:                     null_ppdu_fail_time:%dms delta:%dms vdev_type:%d 
5388,II,wal_pdev_dstall_detection_pause pdev_id:%d pause_countdown:%d 
5387,III,wal_pdev_dstall_mon_timer_timeout: pdev_id:%d dstall_pause_countdown:%d total_active_vdev_cnt%d 
5386,II,data stall time rssi:%d vdev_id:%d 
5385,II, WAL_DBGID_SET_POWER_STATE  current = 0x%x desired = 0x%x 
5384,,Quiet functionality not supported 
 
5383,II,WAL_PDEV_REG_DOMAIN (pdev=%d): reg=0x%x 
5382,II,Set PN_SHIFT_FACTOR: old_pn_shift = %d new_pn_shift = %d 
5433,I,start hwbmiss delay wake tmr, timeout:%d 
5421,I,%s: NULL pointer 
 
5432,I,%s: invalid addr_type 
 
5429,I,%s: no buf in pool 
 
5431,I,%s: inserting at head 
 
5430,I,%s: update the existing filter 
 
5429,I,%s: no buf in pool 
 
5428,I,%s: Inserting in the list 
 
5427,I,SW_DTIM: Improper Beacon due to invalid usRemBufLen 1 for vdev:%d 
5426,III,SW_DTIM: Improper Beacon due to invalid usRemBufLen (%d<%d) for vdev:%d 
5425,III,SW_DTIM: Improper Beacon line due to invalid Dtim count (%d) and period (%d) for vdev :%d 
5421,I,%s: NULL pointer 
 
5421,I,%s: NULL pointer 
 
5420,I,%s: Invalid addr_type 
 
5419,I,%s: List is empty
 
5424,I,%s: removing from the head 
 
5423,I,%s: removing from the middle 
 
5422,IIIII,wal_vdev_down pdev_id %d vdev_id %d vdev_type %d flags 0x%x cnt_per_opmode %d 
5421,I,%s: NULL pointer 
 
5421,I,%s: NULL pointer 
 
5420,I,%s: Invalid addr_type 
 
5419,I,%s: List is empty
 
5418,IIIIII,wal_vdev_migrate (%d, 0x%x): pdev %d->%d, active=%d/%d 
5417,II,_wal_vdev_migrate_bring_up: vdev_id = %d rssi_beacon = %d 
5416,IIII,_wal_vdev_migrate_bring_up: vdev_id = %d cur_tsf_64 = 0x%x sta_bss_tstamp = 0x%x time_at_sta_bss_tstamp = 0x%x 
5415,II,_wal_vdev_migrate_tear_down: vdev_id = %d rssi_beacon = %d 
5414,III,_wal_vdev_migrate_tear_down: vdev_id = %d sta_bss_tstamp = 0x%x time_at_sta_bss_tstamp = 0x%x 
5413,IIII,wal_vdev_event_handler (vdev=0x%x,%d): add peer (0x%x)-count=%d 
5412,IIII,wal_vdev_event_handler (vdev=0x%x,%d): del peer (0x%x)-count=%d 
5411,II,wal_vdev_post_migrate - old_pdev is %d, new_pdev is = %d 
5410,,wal_vdev_post_migrate - Calling rx_resume 
5409,II,wal_vdev_pre_migrate - old_pdev is %d, new_pdev is = %d 
5408,II,wal_vdev_reconfig vdev_id %d  tsf_id is %d 
5407,III,[ERP_PROTECTION]: param_val %d default profile 0x%x new profile 0x%x 
5406,IIII,WAL_DBGID_SETUP_RSSI_INTERRUPTS vdev_id = %d 0x%x 0x%x 0x%x 
5405,IIII,wal_vdev_start vdev_id %d vdev_type %d vdev's mac %dbss_peer %d 
5404,,_wal_vdev_state_publish: Entry  
5403,II,_wal_vdev_state_publish: vdev_type_state is %d, vdev_id_state = %d  
5402,IIIIII,_wal_vdev_state_publish: mac_address is %d:%d:%d:%d:%d:%d  
5401,,_wal_vdev_state_publish: Exit  
5400,II,_wal_vdev_state_publish: bytes is %d, less than output size = %d  
5399,I,_wal_vdev_state_publish: vdev_id_map %d  
5398,I,_wal_vdev_state_publish: vdev  %d  
5397,II,wal_vdev_stop vdev_id %d vdev_type %d 
5396,IIIII,wal_vdev_up: pdev_id %d vdev_id %d, vdev_type %d flags 0x%x cnt_per_opmode %d 
5454,I,nss_chainmaks:array=%x 
5453,IIII,num_tids=%d,num_mpdu=%d,num_msdu=%d
 
5452,IIII,tid_sz=%d,mpdu_sz=%d,msdu_sz=%d
 
5451,,_wal_soc_pkt_info_run_algo: No monitored phy mode or device in sleep mode, enabled pktlog.
 
5450,IIIIII,pktlog from %d to %d: tx_msdu %d, threshold %d, tx_ppdu %d, threshold %d.
 
5449,IIIIII,pktlog from %d to %d: rx_msdu %d, threshold %d, rx_ppdu %d, threshold %d.
 
5448,IIIIII,pktlog from %d to %d: tx_msdu %d, sum_msdu %d, threshold %d, sum_ppdu %d, threshold %d.
 
5447,III,_wal_soc_register_pkt_info_handler 0x%x, 0x%x, 0x%x 
5446,II,wal_soc_switch_mode: nss applied for mac0 -  %d and %d 
5445,, Caling DPD SM for home channel  
5444,IIII,_wal_soc_switch_mode: mhz = %d mac_id = %d  tx_resumed %d last_pdev_state %d 
5443,II,_wal_soc_state_publish: bytes is %d, less than output size = %d  
5442,II,_wal_soc_state_publish: correct return num_mac %d soc mode %d 
5441,,_wal_soc_state_publish: gp_wal_soc is null 
5440,I,wal_soc_switch_mode: Start switching to mode = %d 
5439,I,wal_soc_switch_mode: Not switching to mode = %d 
5438,II,wal_soc_switch_mode: tx chainmask [%d] from protocol %d 
5437,II,wal_soc_switch_mode: rx chainmask [%d] from protocol %d 
5436,II,wal_soc_switch_mode: pdev_state[%d] = %d 
5435,I,wal_soc_switch_mode: Switched to Mode = %d 
5434,III,_wal_soc_unregister_pkt_info_handler 0x%x, 0x%x, 0x%x 
5467,I,crc32_calc: CRC=0x%08x 
5466,I,tx_send_disa_frame: vdev_id=%d 
5465,,DISA: Invalid pdev_id 
5464,I,DISA PPDU setup failed!!! Status=%d 
5463,I,tx_send_disa_frame: Seq No = 0x%x 
5462,I,DISA HW configuration failed!!! Status=%d 
5461,,No MEMORY for DISA frame!!! 
5460,,wal_sw_peer_key allocation failed...!!! 
5459,,disa_frm_buf allocation failed...!!! 
5458,,disa_frag_desc allocation failed...!!! 
5458,,disa_frag_desc allocation failed...!!! 
5457,,wal_sw_peer_key allocation SUCCESS 
5456,,disa_ppdu_desc allocation failed...!!! 
5455,,_wal_disa_prepare_80211_frame: QoS frame with order bit set to 1 
5501,II,Tx_Pause: WAL_PEER_EVENT_SEND_N_COMPLETE sent: peer:0X%x, tid_num:%d 
5500,IIII,Tx_Pause: WAL_PEER_SEND_N_REQ rcvd: peer:0X%x, tidno:%d, num_frames:%d, flags:0X%x [No_Resp] 
5499,IIII,Tx_Pause: WAL_PEER_PS_PRE_REQ rcvd: peer:0X%x, force_ps:%d, pm_ts:%d, paused_tidmask:0X%x  [No_Resp] 
5498,I,Tx_Pause: WAL_VDEV_TX_PAUSE_RESET_IND rcvd: vdev_id:%d [No_Resp] 
5497,II,Tx_Pause: WAL_TX_PAUSE_TID_CREATE rcvd: peer:0X%x, tid_num:%d [No_Resp] 
5496,I,Tx_Pause: WAL_TX_PAUSE_VDEV_CREATE rcvd: vdev_id:%d [No_Resp] 
5495,I,Tx_Pause: WAL_TX_PAUSE_PEER_CREATE rcvd: peer:0X%x [No_Resp] 
5494,I,Tx_Pause: WAL_TX_PAUSE_HWQ_EMPTY rcvd: tid_num:%d [No_Resp] 
5493,I,Tx_Pause: unsupported no-resp request id:%d 
5492,IIII,Tx_Pause: WAL_PDEV_TX_PAUSE_REQ rcvd: pdev_id:%d, module_id:%d, block:%d, filter:%d 
5491,III,Tx_Pause: WAL_PDEV_TX_UNPAUSE_REQ rcvd: pdev_id:%d, module_id:%d, block:%d 
5490,I,Tx_Pause: unsupported pdev request id:%d 
5489,IIIII,Tx_Pause: WAL_PEER_TX_PAUSE_UNPAUSE_REQ rcvd: peer:0X%x, module_id:%d, tids_to_pause:0X%x, tids_to_unpause:0X%x, filter:%d 
5488,IIIII,Tx_Pause: WAL_PEER_TX_BLOCK_UNBLOCK_REQ rcvd: peer:0X%x, module_id:%d, tids_to_block:0X%x, tids_to_unblock:0X%x, filter:%d 
5487,I,Tx_Pause: unsupported peer request id:%d 
5486,IIII,Tx_Pause: WAL_PEER_TX_PAUSE_UNPAUSE_COMPLETE sent: peer:0X%x, module_id:%d, tids_to_pause:0X%x, tids_to_unpause:0X%x 
5485,IIII,Tx_Pause: WAL_PEER_TX_BLOCK_UNBLOCK_COMPLETE sent: peer:0X%x, module_id:%d, tids_to_block:0X%x, tids_to_unblock:0X%x 
5484,III,Tx_Pause: WAL_VDEV_TX_PAUSE_COMPLETE sent: vdev_id:%d, module_id:%d, block:%d 
5483,III,Tx_Pause: WAL_VDEV_TX_UNPAUSE_COMPLETE sent: vdev_id:%d, module_id:%d, block:%d 
5482,III,Tx_Pause: WAL_PDEV_TX_PAUSE_COMPLETE sent: pdev_id:%d, module_id:%d, block:%d 
5481,III,Tx_Pause: WAL_PDEV_TX_UNPAUSE_COMPLETE sent: pdev_id:%d, module_id:%d, block:%d 
5480,IIII,Tx_Pause: WAL_PEER_TX_PAUSE_UNPAUSE_REQ comp: peer:0X%x, module_id:%d, tids_to_pause:0X%x, tids_to_unpause:0X%x 
5479,IIII,Tx_Pause: WAL_PEER_TX_BLOCK_UNBLOCK_REQ comp: peer:0X%x, module_id:%d, tids_to_block:0X%x, tids_to_unblock:0X%x 
5478,III,Tx_Pause: WAL_VDEV_TX_PAUSE_REQ comp: vdev_id:%d, module_id:%d, block:%d 
5477,III,Tx_Pause: WAL_VDEV_TX_UNPAUSE_REQ comp: vdev_id:%d, module_id:%d, block:%d 
5476,III,Tx_Pause: WAL_PDEV_TX_PAUSE_REQ comp: pdev_id:%d, module_id:%d, block:%d 
5475,III,Tx_Pause: WAL_PDEV_TX_UNPAUSE_REQ comp: pdev_id:%d, module_id:%d, block:%d 
5474,IIII,Tx_Pause: WAL_VDEV_TX_PAUSE_REQ rcvd: vdev_id:%d, module_id:%d, block:%d, filter:%d 
5473,III,Tx_Pause: WAL_VDEV_TX_UNPAUSE_REQ rcvd: vdev_id:%d, module_id:%d, block:%d 
5472,I,Tx_Pause: unsupported vdev request id:%d 
5471,IIII,tid_pause_data_stall tid_num:%d pause_module_id_map:%d block_module_id_map:%d peer:0X%x 
5470,I,Tx_Pause: Pdev event PEER_CREATE for peer:0X%x rcvd 
5469,I,Tx_Pause: Pdev event PEER_DELETE for peer:0X%x rcvd 
5468,I,Tx_Pause: unsupported request id:%d 
5502,II,WAL_DBGID_SMPS_SET_HW_MODE: new=0x%x old=0x%x 
5503,I,actual min early_rx:%d 
5517,IIII,wal_wdcvs_boost_disable: Boost released mod:%d mac_id:%d ref_cnt:%d ref_cnt_totoal:%d 
5516,I,wal_wdcvs_boost_disable: mod:%d boost without enable 
5515,,wal_wdcvs_boost_enable fail: boost module ref_cnt table full 
5514,IIII,wal_wdcvs_boost_enable: Boost requested mod:%d mac_id:%d ref_cnt:%d ref_cnt_totoal:%d 
5513,,WDCVS adaptive algorithm disabled
 
5512,,WDCVS adaptive algorithm enabled
 
5511,IIIIIII,WDCVSRX-MAC%d %x %x %x %x %x %x 
5510,IIIIIII,WDCVSTX-MAC%d %x %x %x %x %x %x 
5509,IIIII,WDCVSTXMSDU-MAC%d %x %x %x %x 
5508,IIIII,rx_rate_index-MAC%d %x rx_aggr_index %x tx_rate_index %x tx_aggr_index %x
 
5507,II,wal_wdcvs_state_change_notify mac:%d: state %x 
5506,II,wal_wdcvs_swdtim_notification mac:%d: state %x 
5505,IIII,wal_wdcvs_update_bw: Mac Id: %x  BW mode updated: %x Old WDCVS state: %x New WDCVS state: %x
 
5504,IIII,wal_wdcvs_update_opmode: Mac Id: %x OPMODE updated: %x Old WDCVS state: %x New WDCVS state: %x
 
5597,II,wal_correct_tsf_for_go_vdev: current_offset (%d) < (%d) 
5596,I,RRI interrupt received for MAC ID %d 
5595,IIII,wal_pm_chain_imbalance: min:%d max:%d chmsk:0x%x thres:%d 
5594,II,evaluate_dtim: current_state=%d, new_state=%d 
5593,I,evaluate_dtim: force_swdtim=%d 
5592,I,wal_pm_evaluate_dtim_type sleep validation with invalid TSF id %d 
5591,I,exit hwdtim awake msg handler: pdev_id=%u 
5590,II,wal_pm_h2s_intr_hdlr: REQ: %d GRANT :%d 
5589,II,wal_pm_h2s_wait: start REQ: %d GRANT :%d 
5588,II,wal_pm_h2s_wait: select exit %u %x 
5587,II,wal_wmac_pm_h2s select got signal: %d h2s_grant: %d
 
5586,,wal_pm_h2s_wait: Invalid select status
 
5585,,wal_wmac_pm_h2s timed out 
5584,II,wal_pm_handle_swdtim_pending_op: pdev_id:%u, pending_op:%u 
5583,,wal_pm_get_band_config: Invalid Channel config, Assume 5G 
5582,III,wal_pm_power_thread_msg_handler: mac=%u, power msg_id=%d pending_op=0x%x 
5581,II,wal_pm_power_thread_msg_handler: mac=%u, unsupported request id:%d 
5580,II,mac:%d wal_pm_reset_wow_awake_hdlr, wow_awake_to_cnt:%d 
5579,,wal_pm_sm_state_change_request_extn : Invalid power_state full sleep 
5578,I,stay on partial awake request cnt:%d 
5577,,wal_pm_sm_state_change_request_extn: Invalid power state 
5576,I,stay on partial awake release cnt:%d 
5575,III,wal_pm_state_active_entry_timestamp : %lu mac_id: %d active_entry_count: %lu 
5574,,!!!!wal_pm_state_active_entry:                 incorrect previous state from hw_dtim Exit sleep !!!!
 
5544,,H2S Grant Check Failed 
5543,,Disabling CCE : Reseting Mac as CCE Disabled failed  
5542,,Disabling CCE : WHAL_PMAC_DTIM_AWAKE disable 
5573,,wal_pm_state_active_entry:                 from hw_dtim_awake Exit sleep
 
5572,,wal_pm_state_active_entry: from IMPS sleep Exit
 
5571,,wal_pm_state_active_entry:                 from partial_awake Exit sleep
 
5570,, Previous SM state is not valid. n 
5569,,wal_pm_state_active_event: Already Awake, Do nothing 
5568,,wal_pm_state_active_event: Active to HW DTIM Transition 
5567,,wal_pm_state_active_event: Active to SW DTIM Transition 
5566,,wal_pm_state_active_event: Active to IMPS Transition 
5565,II,wal_pm_state_hw_dtim_awake_entry_timestamp: %lu mac_id: %d 
5545,I,H2S request set status %d 
5544,,H2S Grant Check Failed 
5543,,Disabling CCE : Reseting Mac as CCE Disabled failed  
5542,,Disabling CCE : WHAL_PMAC_DTIM_AWAKE disable 
5564,,wal_pm_state_hw_dtim_awake_event: HW_DTIM_AWAKE to HW DTIM Transition 
5563,,wal_pm_state_hw_dtim_awake_event: HW_DTIM_AWAKE to Active Transition 
5562,,wal_pm_state_hw_dtim_awake_event: HW_DTIM_AWAKE to partial awake Transition 
5561,III,wal_pm_state_hw_dtim_entry_timestamp : %lu mac_id: %d hw_dtim_entry_count: %lu 
5560,,wal_pm_state_hw_dtim_entry: Previous SM state is invalid 
5559,,wal_pm_state_hw_dtim_entry: dtim entry guard time breached 
5558,,wal_pm_state_hw_dtim_event: event type invalid. 
5557,,wal_pm_state_hw_dtim_event: HW DTIM to HW_DTIM_AWAKE Transition 
5556,,wal_pm_state_hw_dtim_event: HW DTIM to Partial_awake Transition 
5555,II,wal_pm_state_hw_dtim_exit_timestamp : %lu Mac_Id: %d 
5554,,wal_pm_state_imps_entry: STATE 
5553,III,wal_pm_state_imps_entry_timestamp : %lu mac_id: %d imps_entry_count: %lu 
5552,,wal_pm_state_imps_event: IMPS to Active Transition 
5551,,wal_pm_state_imps_event: IMPS to partial awake Transition 
5550,,wal_pm_state_imps_event: Invalid event type 
5549,II,wal_pm_state_imps_exit_timestamp : %lu Mac_Id: %d 
5548,II,wal_pm_state_init_entry_timestamp : %lu mac_id: %d 
5547,II,wal_pm_state_init_exit_timestamp : %lu Mac_Id: %d  
5546,,wal_pm_state_partial_awake_entry: STATE 
5545,I,H2S request set status %d 
5544,,H2S Grant Check Failed 
5543,,Disabling CCE : Reseting Mac as CCE Disabled failed  
5542,,Disabling CCE : WHAL_PMAC_DTIM_AWAKE disable 
5541,,wal_pm_state_partial_awake_event: Partial_awake to HW DTIM Transition 
5540,,wal_pm_state_partial_awake_event: Partial_awake to Active Transition 
5539,,wal_pm_state_partial_awake_event: Partial_awake to HW_DTIM_AWAKE Transition 
5538,,wal_pm_state_partial_awake_event: Partial_awake to IMPS Transition 
5537,II,wal_pm_state_sw_dtim_entry_timestamp : %lu mac_id: %d 
5536,I,wal_pm_update_spm: WAL_SPM_BW_MODE_UPDATE : %d 
5535,I,RSSI_IND wal_pm_update_soc_mgr: WAL_PM_MAC_PARAM_RSSI_INDICATION, rssi indication  ->%d  
5534,I,wal_pm_update_spm: WAL_PM_MAC_PARAM_RX_CHAINS_COUNT, chain count ->%d  
5533,I,wal_pm_update_spm: WAL_SPM_BAND_UPDATE  :%d 
5533,I,wal_pm_update_spm: WAL_SPM_BAND_UPDATE  :%d 
5532,I,wal_pm_update_spm: WAL_PM_MAC_PARAM_LATENCY_MODE :%d 
5531,I, wal_pm_update_spm invalid param: param_id %d 
5530,II,wal_pm_update_spm: chain_mask->%d, dtim_period -> %d  
5529,III,WDOG mac:%d global_count:0x%08x_%08x
 
5528,III,WDOG mac:%d cur_tsf:0x%08x_%08x
 
5527,,hwdtim awake in non-hwdtim 
5526,II,mac:%d Triggering fake TSF OOR 
5525,IIIIII,mac:%d curr_tsf:0x%08x_0x%08x next_tbtt:0x%08x_0x%08x dtim_period:%0x 
5524,,enter hwdtim in non-hwdtim-awake 
5523,II,wal_pm_state_active_initial_timestamp_%d : %lu 
5522,,Enabling CCE : WHAL_PMAC_PARAM_DTIM_HW  
5521,I,mac:%d wal_pm_wow_awake_to_hdlr 
5520,I,consective_wow_awake_to_cnt:%d 
5519,,long mac awake detect!!! 
5518,I,Waiting for 10 secs more to check null failure threshold, waiting for STA_KICKOUT, cnt %d 
5638,I,_wal_spm_css_pwr_down : state: %d 
5637,I,wal_spm_css_state_change_notify: ccpm_request_wlan_pwr failed with error code: %d 
5636,I,wal_spm_css_state_change_notify :ccpm_request_wlan_ccvs failed with error code: %d 
5636,I,wal_spm_css_state_change_notify :ccpm_request_wlan_ccvs failed with error code: %d 
5635,I,_wal_spm_css_pwr_down : ccpm_request_wlan_pwr failed with error code: %d 
5634,I,_wal_spm_init : ccpm_request_wlan_pwr failed with error code: %d 
5632,,Invalid mac_id 
5633,I,_wal_spm_set_params_cfg update_mask 0%x 
5632,,Invalid mac_id 
5631,I,_wal_spm_set_params_cfg op mode selected: %d 
5630,I,_wal_spm_set_params_cfg invalid op mode selected: %d 
5629,I,_wal_spm_set_params_cfg bw mode selected: %d 
5628,I,_wal_spm_set_params_cfg invalid bw mode selected: %d 
5627,I,_wal_spm_set_params_cfg band selected: %d 
5626,I,_wal_spm_set_params_cfg invalid band selected: %d 
5625,I,_wal_spm_set_params_cfg apply_wlan_params.flags 0%x 
5624,I,_wal_spm_set_wpm_params_cfg : ccpm_request_wlan_pwr failed with error code: %d 
5623,,wal_spm_dump_votes: mac 0/1 Param configuration 
5614,I,q6_to_ddr.ib -> %d 
5613,I,q6_to_wlan.ab -> %d 
5611,I,q6_to_wlan.ib -> %d 
5610,I,wlan_to_ddr.ab -> %d 
5609,I,wlan_to_ddr.ib -> %d 
5608,I,q6_clk_freq_kHz -> %d 
5599,I,q6_mpps -> %d 
5622,I,bw_mode -> %d 
5621,I,n_chain_mask -> %d 
5620,I,dtim_period -> %d 
5619,I,opmode -> %d 
5618,I,ccpm ->opmode -> %d 
5617,I,lp_state -> %d 
5616,I,css_down -> %d 
5615,I,band -> %d 
5598,I,q6_to_ddr.ab -> %d 
5614,I,q6_to_ddr.ib -> %d 
5613,I,q6_to_wlan.ab -> %d 
5612,I,**** wal_spm_dump_votes: for mac id : %d 
5611,I,q6_to_wlan.ib -> %d 
5610,I,wlan_to_ddr.ab -> %d 
5609,I,wlan_to_ddr.ib -> %d 
5608,I,q6_clk_freq_kHz -> %d 
5607,I, bw_mode -> %d 
5606,I, n_chain_mask -> %d 
5605,I, dtim_period -> %d 
5604,I, opmode -> %d 
5603,I, lp_state -> %d 
5602,I, band -> %d 
5600,I,q6_cpp -> %d 
5601,,wal_spm_dump_votes: Applid param configuration 
5600,I,q6_cpp -> %d 
5599,I,q6_mpps -> %d 
5598,I,q6_to_ddr.ab -> %d 
5642,I,wal_pm_arbiter_request request Type 0x%x
 
5641,,wal_pm_arbiter_request:ERROR: wal_pm_arbiter_request_type_t req invalid 
5640,,wal_pm_arbiter_request:ERROR: Double Sleep request without awake done  
5639,III,wal_pm_arbiter_resolve_mac_pm_state: pdev %d mac_id %d, Resolved state:%d 
5675,,wal_pm_debug_log_init done 
 
5674,,wal_pm_gpio_pwr_profile request is for MAC0 
5673,,wal_pm_gpio_pwr_profile request is for MAC1 
5672,I,wal_pm_gpio_pwr_profile request is wrong MAC id %d 
5671,,wal_pm_lock_stats  
5670,III,  wal_pm_lock_stats holding by WAL(MAC#0) request : %d, pm_requester :%d, ref_cnt %d
 
5669,III,  wal_pm_lock_stats holding by WAL(MAC#1) request : %d, pm_requester :%d, ref_cnt %d
 
5668,II,wmi_cce_cmd request %d is for MAC%d 
5667,,cce_cmd FAILED : provide correct arguments 
5666,,cce_counter_cmd FAILED : provide correct arguments 
5665,I,debug command triggered for  %d 
5664,II,wmi_conf_nth_bcn mac id-%d nth becn threshold: %d 
5663,,wal_power_debug_css_pwr_ctrl_cmd FAILED : in-correct arguments 
5662,II,wmi_dtim_rf_chain_ctrl_cmd request %d is for MAC%d 
5661,,wal_power_debug_dtim_rf_chain_ctrl_cmd FAILED : in correct arguments 
5660,II,wmi_dtim_synth_cmd request %d is for MAC%d 
5659,,dtim_synth_cmd FAILED : provide correct arguments 
5650,II,force_swdtim request %d is for MAC%d 
5648,,force_swdtim FAILED : provide correct arguments 
5658,III,chain_imbalance_1ch_dtim request %d val:%d for MAC%d 
5657,,chain_imbalance_1ch_dtim FAILED : provide correct arguments 
5656,II,wmi_hwdtim_cmd request %d is for MAC%d 
5655,,hwdtim_cmd FAILED : provide correct arguments 
5654,II,wmi_imps_cmd request %d is for MAC%d 
5653,,IMPS_cmd FAILED : provide correct arguments 
5652,II,fast_wake_cmd request %d is for MAC%d 
5651,,fast_wake_cmd FAILED : provide correct arguments 
5650,II,force_swdtim request %d is for MAC%d 
5649,II,sim rogue ap request %d is for MAC%d 
5649,II,sim rogue ap request %d is for MAC%d 
5648,,force_swdtim FAILED : provide correct arguments 
5647,II,wmi_wcvs_cmd request %d is for MAC%d 
5646,,wcvs_cmd FAILED : in-correct arguments 
5645,,wal_power_debug_wow_long_wake_detect_cmd FAILED : in-correct arguments 
5644,,setUnitTestcmd FAILED : wal_vdev is NULL 
5643,,setUnitTestcmd FAILED : pdev is NULL 
5681,II,sw_dtim_peer_event: DATA, fc:%0x, more:%u 
5680,II,sw_dtim_peer_event: Unexpeted unicast packet received for vdev=%d in state=%d 
5679,II,sw_dtim_power_msg_handler: mac=%u, power msg_id=%d 
5678,II,sw_dtim_power_msg_handler: mac=%u, unsupported request id:%d 
5677,III,sw_dtim_power_msg_handler: mac=%u, Beacon RX for vdev=%d, DTIM_set=%u 
5676,I,sw_dtim_power_msg_handler: mac=%u, Beacon RX but vdev is NULL 
5690,II,sw_dtim_wmac_is_safe_to_power_up(FALSE): mac=%d, !vdev_is_safe_to_sleep(%d) 
5689,III,sw_dtim_wmac_is_safe_to_power_up(FALSE): mac=%d, min_time_till_tbtt=%u, back_off=%u 
5688,I,sw_dtim_wmac_is_safe_to_power_up(TRUE): mac=%d 
5687,II,sw_dtim_wmac_power_req: mac=%u, cmd_id=%u 
5686,I,sw_dtim_wmac_validate_swdtim_entry(FALSE): non-supported vdev, mac=%u 
5685,I,sw_dtim_wmac_validate_swdtim_entry(FALSE): validate_imps_swdtim failing, mac=%u 
5684,IIII,sw_dtim_wmac_validate_swdtim_entry(TRUE): mac=%u, timeout=%u, min_tbtt=%u, sleep_exit_sys_time=%u 
5683,I,sw_dtim_wmac_validate_swdtim_entry(FALSE): start reeval timer, mac=%u 
5682,IIIIII,sw_dtim_wmac_validate_swdtim_entry(FALSE): close to tbtt, mac=%u, timeout=%d, powerdown=%u, min_tbtt=%u, powerup=%u, back_off=%u 
5695,III,sw_dtim_vdev_is_safe_to_sleep(FALSE): vdev_id=%d, cur_state:%d, next_state:%d 
5694,IIIIIIII,sw_dtim_vdev_is_safe_to_sleep(TRUE): vdev_id=%d, tsf_id=%u, bss_id=%u, nTBTT=%0x-%0x, tsf=%0x-%0x, time_till_TBTT=%u 
5693,IIIIII,sw_dtim_vdev_start_sm: tbtt=%0x-%0x < tsf=%0x-%0x for vdev=%d tsf_id=%u 
5692,II,sw_dtim_vdev_start_sm: vdev:%d, next_state:%d 
5691,IIIIII,sw_dtim_vdev_start_tbtt_timer: vdev_id=%d, nTBTT=%0x-%0x, tsf=%0x-%0x, time_till_TBTT=%u 
5697,,_wal_rmc_deliver_event: Deliver RMC event 
5696,I,RMC event handler: event_type = 0x%x
 
5746,IIIIII,DEBUG-TKNS: %d,%d,%lu,%lu,%lu,%lu 
5745,IIIIIIIII,DEBUG-PERF: %lu,%lu,%lu,%lu,%lu,%lu,%lu,%lu,%d 
5744,IIIIIIII,DEBUG-PERF: %d,%d,%lu,%lu,%lu,%lu,%lu,%lu 
5743,II,_wal_collect_report_info: pre %d bw %d 
5742,III,_wal_report_type2_buffer_done() buff = %p, curr: %p len: %d 
5741,IIII,_wal_report_type2_buffer_init buff = %p cur_p = %p chan = %d report_type = %d 
5740,IIIIII,_wal_report_type2_collect_report_info:  total_time = %d num_frms = %d info1 = %d info2 = %d info3 = %d start_ts = %d 
5739,,DISCARDING MEASUREMENT!! T3 not captured 
5731,II,RTT_INITR_TSTAMP: t2= %lu fac= %d 
5738,IIII,_wal_report_type2_collect_report_info: tx_rate_info1 = 0x%x tx_rate_info2= 0x%x rx_rate_info1=0x%x, rx_rate_info2 = 0x%x 
5737,IIIIII,_wal_report_type2_collect_report_info: meas_cnt=%d num_rtt_per_frame_info_saved: %d tx_preamble=%d tx_bw=%d, rssi=0x%x, rtt=0x%x 
5736,II,RTT_INITR_TSTAMP: t3= %lu  t3_del= %ld 
5735,III,RTT_RSPDR_TSTAMP:  t1= %lu t4= %lu t4_del= %ld 
5734,III,COMPUTED_RTT: rtt=%d meas_count=%d num_rtt_per_frame_info_saved: %d 
5733,IIII,_wal_report_type2_collect_report_info:  tx_rate_info1=0x%x, tx_rate_info2 =0x%x, rx_rate_info1=0x%x, rx_rate_info2=0x%x 
5732,III,_wal_report_type2_collect_report_info: rx_preamble=%d, bw=%d rssi = 0x%x 
5731,II,RTT_INITR_TSTAMP: t2= %lu fac= %d 
5730,IIIIII,index: %d saved_count: %d rtt_ps: %d sum_rtt: %d tx_bw: %d, rx_bw: %d 
5729,II,_wal_report_type2_update_start_ts: start_ts(rtt_ctxt) start_ts(peer_head) %d 
5728,III,_wal_rtt_attach() pdev = %p rtt_pdev_ctxt = %p wal_rtt_ctxt = %p 
5727,II,num_meas: %d num_rtt_per_frame_info_saved: %d 
5726,IIII,Detected Outlier. i: %d rtt: %d mean_rtt: %d bw: %d 
5725,,No filtered measurements 
5724,II,cumilative_rtt: %d filtered meas count: %d 
5723,,Zero measurements. Skip distance computation 
5722,II,i: %d bw: %d is wrong. skip!! 
5721,IIII,_wal_rtt_ctxt_init() :freq: %d is_qca: %d force_legacy_ack: %d enable_ht_vht_ack :%d 
5720,IIIIII,_wal_rtt_get_buffer_ptr:max_len:0x%x rem_len:0x%x reqd_len:0x%x buff:0x%x buf_p:0x%x cur_p:0x%x 
5719,I,_wal_rtt_get_dyn_bw:%d 
5718,IIIII,_wal_rtt_init() pdev_id = %d rtt_ctxt: %p  alloc_buff = %p buff = %p max_buff_len = %d 
5717,IIIII,_wal_rtt_local_frame_send_with_rate: acks%d tid_num 0x%x rate_info 0x%x flags 0x%x report %d 
5716,IIIII,_wal_rtt_mt_cb: msg:0x%x id:0x%x s_thr:%d d_thr:%d ticks:0x%x 
5711,,TX completion message was dropped. Report failure 
5715,,_wal_rtt_null_ack_hdl() is called after RTT session is completed !!! 
5714,III,_wal_rtt_psoc_init() wal_rtt_ctxt idx in rtt_psoc_handle: %d rtt_ctxt: %p alloc_buff_p: %p 
5713,IIII,_wal_rtt_psoc_init() psoc_rtt handle: %p sizes rtt_tx_pool: %d rtt_rx_pool handle: %d, rtt_rx_ofld_pool: %d 
5712,IIIIIII,t3_report_buff_addr=0x%x, t3_32=0x%x t3_0=0x%x t2_32=0x%x t2_0=0x%x, t3_del=0x%x len= 
5711,,TX completion message was dropped. Report failure 
5710,,_wal_rtt_tm_ack_hdl() is called after RTT session is completed !!! 
5709,II,Ignore TM ack for stale entry: ath_buf: %p: last queued TM frame ath_buf: %p 
5708,,_wal_rtt_tm_rx_hdl: TM frame not directed to me. Don't process 
5707,,_wal_rtt_tm_rx_hdl: Not a valid TM frame. Don't process 
5706,I,_wal_rtt_tm_rx_hdl: HT_VHT ack enable RTT_TM_FTM1 %d 
5705,III,_wal_rtt_tm_rx_hdl:  expect_token=%d, dia_token=%d, follow_token=%d 
5704,IIII,_wal_rtt_tm_rx_hdl:  t1_32=0x%x, t1_0=0x%x, t4_32=0x%x, t4_0=0x%x 
5703,,wal_rtt_tx_ppdu_done(): rx_location_info is found to be invalid 
5702,III,_wal_rtt_tx_ppdu_done: rtt_type=%d, tx_preamble=%d, retries=%d 
5701,IIII,_wal_rtt_tx_ppdu_done: abf: %p rtt_type=%d, tx_preamble=%d, retries=%d 
5700,IIIIII,_wal_rtt_tx_ppdu_done: tod_32= 0x%x tod_0= 0x%x toa_32= 0x%x toa_0= 0x%x fac_valid: %d fac= 0x%x 
5699,II,_wal_rtt_tx_ppdu_done:  RSSI = 0x%x chain_idx = 0x%x 
5698,II,report type 0 size: %d %d 
5760,III,WMMAC_PAUSE_CB: peer=0x%x blocked tids=0x%x/0x%x 
5759,IIII,WMMAC_Q_REPRIO: peer=0x%x tid=%d qid:%d->%d 
5758,II,WMMAC_PAUSE_CB: unblock tid(%d)=0x%x 
5757,IIII,WMMAC_Q_DEPRIO: peer=0x%x tid=%d qid:%d->%d 
5756,III,WMMAC_Q_DROP: peer=0x%x tid(%d)=0x%x 
5755,IIIIII,WMMAC_STATUS: peer=0x%x, used=%d, admitted=%d, txq_sts=%d/%d, downgrade=%d 
5754,IIIII,WMMAC_TXQ_STATUS ac=%d txq_status=0x%02x used=%d admitted=%d downgrade=%d 
5753,IIII,WMMAC_PERIODIC_UPDATE 0x%x 0x%x 0x%x 0x%x 
5752,I,WMMAC_NO_DOWNGRADE: unblock tid mask=0x%x 
5751,III,WMMAC_PERIODIC_UPDATE (VO): peer=0x%x, used=%d, admitted=%d 
5750,III,WMMAC_PERIODIC_UPDATE (VI): peer=0x%x, used=%d, admitted=%d 
5749,IIII,WMMAC_USED_TIME_EXCEED: used=%d admitted=%d tx_sts=%d wmmac_q=%d 
5748,IIIII,WMMAC_ADD_DELTS: ac=%d admitted=%d acm=%d block=0x%x downgrade=0x%x 
5747,III,WMMAC_UPDATE: used_time=%d admitted_time=%d, downgrade=%d 
5777,II,MGMT buf get failure: mgmtbufCnt = %d, bsmall = %d 
5776,II,MGMT buf get beacon: mac_id:%d, rsvd:%d 
5775,III,MGMT buf abf failure: smgmtbufCnt = %d, bsmall = %d mgmtBufCnt = %d 
5774,IIIII,MGMT buf get success: abf = 0x%x  mgmtBufCnt = %d smgmtbuffcnt = %d bsmall = %d flags = 0x%x 
5772,III,MGMT buf get failure: thread:%d,bufCnt:%d, bsmall:%d 
5773,IIII,MGMT buf get success, abf:0x%x,thread:%d,bufCnt:%d, bsmall:%d 
5772,III,MGMT buf get failure: thread:%d,bufCnt:%d, bsmall:%d 
5771,IIII,MGMT buf get success, abf:0x%x,thread:%d,bufCnt:%d, bsmall%d 
5770,,wlan_buf_mac_buffer_dispatcher no buffers available in chain 
5769,I,wlan_buf_mac_buffer_dispatcher mac_id=%d
 
5761,,wlan_buf_mac_buffer_dispatcher oops 
5761,,wlan_buf_mac_buffer_dispatcher oops 
5768,III,buf free: free the reused abf:0x%x, thread:%d, cb flags:0x%x 
5763,IIII,SMGMT buf free,small:%d,abf:0x%x,thread:%d,bufCnt:%d 
5767,IIII,MGMT buf free,small:%d,abf:0x%x,thread:%d,bufCnt:%d 
5766,IIII,TXDATA buf free,small:%d,abf:0x%x,thread:%d,bufCnt:%d 
5765,IIII,SMTXDATA buf free,small:%d,abf:0x%x,thread:%d,bufCnt:%d 
5764,IIII,free beacon abf:0x%x, thread:%d, cb flags:0x%x,rsvd:%d 
5763,IIII,SMGMT buf free,small:%d,abf:0x%x,thread:%d,bufCnt:%d 
5762,I,wlan_buf_rxbuf_requeue mac_id=%d
 
5761,,wlan_buf_mac_buffer_dispatcher oops 
5761,,wlan_buf_mac_buffer_dispatcher oops 
5784,IIII,arena_flags: 0x%x, bytes:%d, call1:0x%x, call2:0x%x
 
5783,IIII,unknown proxy_flag:0x%x, ret:0x%x, ret1:0x%x,ret2:0x%x 
5782,,BEGIN: cmnos_allocram_info_dump() 
5781,IIIII,max: %d, idx: %d, total_num: %d, total_bytes: %d, length: %d 
5780,,HEX_DUMP: 
5779,,END: cmnos_allocram_info_dump() 
5778,IIIIII,arena: %d, start: 0x%p, current: 0x%p, used = %d, remaining: %d, num_allocs: %d
 
5792,III,APP THREAD ID %d thread stack: %dB used, %dB unused
 
5791,,cmnos_threads_delete
 
5790,I,cmnos_threads_delete: wait for thread app id 0x%x to exit
 
5789,I,cmnos_threads_delete: thread app id 0x%x is done
 
5788,,cmnos_threads_delete: clean up mutex locks
 
5787,,cmnos_threads_delete: clean up thread barriers
 
5786,,cmnos_threads_delete: do global cleanups
 
5785,I,cmnos_threads_delete: send exit to 0x%x thread app id
 
5793,I,product resulting in buffer overflow: num_of_elem * elem_sz = 0x%x 
5794,I,profile_report: could not alloc, size=%d 
5795,I,profile_report: #profiles enabled > WMI limit (=%d) 
5801,III,SM: %d:%p : allocation from event pool failed for event %d 
5800,IIIIIIII,[SM:ChgSta] CurS:%x --> NextS:%x mod_id=%d vapid =%d make_sm = 0x%x extra = 0x%x extra2 = 0x%x extra3 = 0x%x 
5799,III,SM: %d:%p : invalid event %d 
5798,IIIIIIII,[SM:RcvEvt] CurS:%x <-- Event:%x mod_id=%d vapid =%d make_sm = 0x%x extra = 0x%x extra2 = 0x%x extra3 = 0x%x 
5797,IIII,SM: %d:%p : event %d not handled in state %d 
5796,IIIIIIII,[SM:RcvEvt] Evt:%d not handled in CurS:%d mod_id=%d vapid =%d make_sm = 0x%x extra = 0x%x extra2 = 0x%x extra3 = 0x%x 
5806,IIIII,ANI_DBGID_POLL phyId %d listen_time 0x%x 0x%x 0x%x 0x%x 
5805,IIIIIIII,ANI_DBGID_POLL phyId %d listen_time %d-%d ofdmPhyErrCnt %d cckPhyErrCnt %d ofdmPhyErrRate %d cckPhyErrRate %d level %d 
5804,II,EnableAni phyId %d enable %d 
5803,I,ANI_DBGID_LISTEN_PERIOD: 0x%x 
5802,I,ANI_DBGID_POLL_PERIOD: 0x%x 
5813,III,halphy_bdf_ActivateSARLimitSet  enable = %d, Index = %d, chainNum = %d
  
5812,I,SetPerChainSARLimit failed,  phyId ​%d in power down, will be applied on wake 
5811,I,TpcGenTool: rate-index %d  
5810,I,TPC Final Power :%d 
5809,III,### Setting Reg domain pCfgCtl[0] %d pCfgCtl[1] %d regDom %d 
5808,IIII,TGT_VER: %08X
RegDomain: %X, CfgCtl: %d - %d
 
5807,IIII,halphy_bdf_SetUserSARValues SARUserLimits[%d] : CCK2gLimit %x  Ofdm2gLimit %x Ofdm5gLimit %x
  
5828,IIIII,hw_bdf_info: bdf_version %x ref_design_id %x customer_id %x project_id %x board_data_rev %x 
 
5827,IIII,g_gtx_cfg.gtxTPCstepDown %x  g_gtx_cfg.gtxTPCMinCck %x g_gtx_cfg.gtxTPCMin5G %x g_gtx_cfg.gtxMACEnable %x 
 
5826,,cckTxFirCh14 bdf settings all zero, do not apply 
5825,,cckTxFirCommon bdf settings all zero, do not apply 
5824,,Warning: No valid ATE temperture characterized info in OTP, returns as 25C always. 
5823,II,GetNFMaxCCAPwr freqIdx %x freqIdx2 %d 
5822,I,halphy_bdf_device_GetRTT dyn_bw=%d is not valid
 
5822,I,halphy_bdf_device_GetRTT dyn_bw=%d is not valid
 
5822,I,halphy_bdf_device_GetRTT dyn_bw=%d is not valid
 
5822,I,halphy_bdf_device_GetRTT dyn_bw=%d is not valid
 
5822,I,halphy_bdf_device_GetRTT dyn_bw=%d is not valid
 
5822,I,halphy_bdf_device_GetRTT dyn_bw=%d is not valid
 
5822,I,halphy_bdf_device_GetRTT dyn_bw=%d is not valid
 
5822,I,halphy_bdf_device_GetRTT dyn_bw=%d is not valid
 
5822,I,halphy_bdf_device_GetRTT dyn_bw=%d is not valid
 
5822,I,halphy_bdf_device_GetRTT dyn_bw=%d is not valid
 
5822,I,halphy_bdf_device_GetRTT dyn_bw=%d is not valid
 
5822,I,halphy_bdf_device_GetRTT dyn_bw=%d is not valid
 
5822,I,halphy_bdf_device_GetRTT dyn_bw=%d is not valid
 
5822,I,halphy_bdf_device_GetRTT dyn_bw=%d is not valid
 
5822,I,halphy_bdf_device_GetRTT dyn_bw=%d is not valid
 
5822,I,halphy_bdf_device_GetRTT dyn_bw=%d is not valid
 
5821,I,halphy_bdf_device_GetRTTTxiqOn TxiqOffset=%d 
 
5820,I,halphy_bdf_device_GetRTTRxiqOn RxiqOffset=%d 
 
5819,I,halphy_bdf_device_GetRTT apply 2G 6us offset
 
5818,I,halphy_bdf_device_GetRTT ret=%d final
 
5817,I,halphy_bdf_device_GetRTTRxiqOn dyn_bw=%d is not valid
 
5817,I,halphy_bdf_device_GetRTTRxiqOn dyn_bw=%d is not valid
 
5817,I,halphy_bdf_device_GetRTTRxiqOn dyn_bw=%d is not valid
 
5817,I,halphy_bdf_device_GetRTTRxiqOn dyn_bw=%d is not valid
 
5817,I,halphy_bdf_device_GetRTTRxiqOn dyn_bw=%d is not valid
 
5817,I,halphy_bdf_device_GetRTTRxiqOn dyn_bw=%d is not valid
 
5817,I,halphy_bdf_device_GetRTTRxiqOn dyn_bw=%d is not valid
 
5817,I,halphy_bdf_device_GetRTTRxiqOn dyn_bw=%d is not valid
 
5817,I,halphy_bdf_device_GetRTTRxiqOn dyn_bw=%d is not valid
 
5817,I,halphy_bdf_device_GetRTTRxiqOn dyn_bw=%d is not valid
 
5817,I,halphy_bdf_device_GetRTTRxiqOn dyn_bw=%d is not valid
 
5817,I,halphy_bdf_device_GetRTTRxiqOn dyn_bw=%d is not valid
 
5817,I,halphy_bdf_device_GetRTTRxiqOn dyn_bw=%d is not valid
 
5817,I,halphy_bdf_device_GetRTTRxiqOn dyn_bw=%d is not valid
 
5817,I,halphy_bdf_device_GetRTTRxiqOn dyn_bw=%d is not valid
 
5817,I,halphy_bdf_device_GetRTTRxiqOn dyn_bw=%d is not valid
 
5816,I,halphy_bdf_device_GetRTTTxiqOn dyn_bw=%d is not valid
 
5816,I,halphy_bdf_device_GetRTTTxiqOn dyn_bw=%d is not valid
 
5816,I,halphy_bdf_device_GetRTTTxiqOn dyn_bw=%d is not valid
 
5816,I,halphy_bdf_device_GetRTTTxiqOn dyn_bw=%d is not valid
 
5816,I,halphy_bdf_device_GetRTTTxiqOn dyn_bw=%d is not valid
 
5816,I,halphy_bdf_device_GetRTTTxiqOn dyn_bw=%d is not valid
 
5816,I,halphy_bdf_device_GetRTTTxiqOn dyn_bw=%d is not valid
 
5816,I,halphy_bdf_device_GetRTTTxiqOn dyn_bw=%d is not valid
 
5816,I,halphy_bdf_device_GetRTTTxiqOn dyn_bw=%d is not valid
 
5816,I,halphy_bdf_device_GetRTTTxiqOn dyn_bw=%d is not valid
 
5816,I,halphy_bdf_device_GetRTTTxiqOn dyn_bw=%d is not valid
 
5816,I,halphy_bdf_device_GetRTTTxiqOn dyn_bw=%d is not valid
 
5816,I,halphy_bdf_device_GetRTTTxiqOn dyn_bw=%d is not valid
 
5816,I,halphy_bdf_device_GetRTTTxiqOn dyn_bw=%d is not valid
 
5816,I,halphy_bdf_device_GetRTTTxiqOn dyn_bw=%d is not valid
 
5816,I,halphy_bdf_device_GetRTTTxiqOn dyn_bw=%d is not valid
 
5815,I,halphy_bdf_device_ProcessConfigAddr skipping write pHeader->addres %x 
 
5815,I,halphy_bdf_device_ProcessConfigAddr skipping write pHeader->addres %x 
 
5814,I,halphy_bdf_device_ProcessConfigAddr writing to pHeader->addres %x 
 
5833,IIII,cal_SM_Main: 0x%x, (pHandle=0x%x, smInput=0x%x, pCalSmTable=0x%x) 
5832,IIII,CC::: cal type idx=%d, ptrStandalone=%x, pIn=%x, pOut=%x  
5831,III,CC::: generateCalSmTable=0x%x, callingContext=%d, curCalTypeIdx=%d 
5830,II,CC::: genCalTable calType=%d hwCalMask 0x%x 
5829,,VdetCal: only support for apache family now -> return 
5834,IIII,CC::: combCalIQ calType=%d, callingContext=%d, phymode = 0x%08x, bandwidth=%d 
5889,I,CB: in FTM mode and hwCalMask=%x 
5888,I,CB::: IS_FTM_MODE() : %x, DISALBE_RESTORE_FOR_FTM is defined 
5887,II,CC: spot A, NOT_APPLICABLE, testResult=%d, lifeTime=%d 
5886,II,CC: spot B, APPLICALBE_RESUBMISSION_ONLY, testResult=%d, lifeTime=%d 
5885,I,CC: spot C, NOMIMAL_APPLICABLE, testResult=%d 
5884,II,address1 %x, address0 %x 
5881,I,***INVALID RF SUB returned. Needs investigation rfsub %d ** 
5881,I,***INVALID RF SUB returned. Needs investigation rfsub %d ** 
5881,I,***INVALID RF SUB returned. Needs investigation rfsub %d ** 
5881,I,***INVALID RF SUB returned. Needs investigation rfsub %d ** 
5883,IIIII,CB: DPD cal: freq1=%d, freq2=%d, band code=%d, calValid=%d, caltime=%d 
5881,I,***INVALID RF SUB returned. Needs investigation rfsub %d ** 
5881,I,***INVALID RF SUB returned. Needs investigation rfsub %d ** 
5882,I,HW disable for DPD, band = %d
 
5881,I,***INVALID RF SUB returned. Needs investigation rfsub %d ** 
5880,III,TEMPSEN::: caldb_tempBinFile->data.cal_80p80_RF0_synth0_5G_RxIq[bandw=%d][rfsubIdx=%d]=%x  
5879,III,TEMPSEN::: caldb_tempBinFile->data.cal_80p80_RF0_synth0_5G_TxIq[bandw=%d][rfsubIdx=%d]=%x  
5878,III,TEMPSEN::: caldb_tempBinFile->data.cal_80p80_RF0_synth0_5G_TxLoNormal[bandw=%d][rfsubIdx=%d]=%x  
5877,IIII,TEMPSEN::: (caldb_tempBinFile->data.cal_RxIq[bandw=%d][rfChainIdx=%d][rfsubIdx=%d])=%x  
5876,IIII,TEMPSEN::: (caldb_tempBinFile->data.cal_TxIq[bandw=%d][rfChainIdx=%d][rfsubIdx=%d])=%x 
5875,IIII,TEMPSEN::: (caldb_tempBinFile->data.cal_TxLoNormal[bandw=%d][rfChainIdx=%d][rfsubIdx=%d])=%x  
5874,IIIIII,TEMPSEN:::  combined cal: validBitMask[0][2][%d]=%x	validBitMask[1][2][%d]=%x	validBitMask[2][2][%d]=%x 
5873,III,CALDB:::  DPD_MASTER:validBitMask[bw:%d][rfChain:%d]=%x  
5872,IIIII,HWtbl: hwCbFCSTracking[%d][HWID:%d].tableAddress[0][i:%d][chainIdx:%d] = %x 
5871,IIIII,HWtbl: hwCbFCSTracking[%d][HWID:%d].tableValid[1][i:%d][chainIdx:%d] = %d 
5870,IIIII,HWtbl: hwCbFCSTracking[%d][HWID:%d].tableAddress[2][i:%d][chainIdx:%d] = %x 
5869,IIIII,HWtbl: hwCbFCSTracking[%d][HWID:%d].tableValid[2][i:%d][chainIdx:%d] = %d 
5868,,HWtbl: =================================================================== 
5867,IIIII,HWtbl: hwCbFCSTracking[%d][HWID:%d].tableValid[0][i:%d][chainIdx:%d] = %d 
5866,IIIII,HWtbl: hwCbFCSTracking[%d][HWID:%d].tableAddress[1][i:%d][chainIdx:%d] = %x 
5865,IIII,HWtbl: hwRxDcoFCSTracking[HWID:%d].tableAddress[i:%d][chainIdx:%d] = %x 
5864,IIII,HWtbl: hwRxDcoFCSTracking[HWID:%d].tableValid[i:%d][chainIdx:%d] = %d 
5863,III,TEMPSEN:::gValidBitMask[bw:%d][rfChain:%d]=%x  
5862,III,TEMPSEN:::gDtimValidBitMask[bw:%d][rfChain:%d]=%x  
5861,III,TEMPSEN:::  RXDCO_MASTER:validBitMask[bw:%d][rfChain:%d]=%x  
5860,III,TEMPSEN:::  RXDCO_MASTER:validDTIMBitMask[bw:%d][rfChain:%d]=%x  
5859,IIIIIIII,TEMPSEN:::   chainIdx = %d, CBNormalizedOffset=%d, CBTempInC=%d, LastTempInC=%d, LastRawTempInC %d, getTime=%u, curTempID=%d, CBtempeID=%d 
5858,IIIII,findNearestValidBitIdx:::bandCode=%d, bandw=%d, curBitIndex = %d, idx_left=%d,idx_right=%d 
5857,IIII,findNearestValidBitIdx:::bandCode=%d, bandw=%d, curBitIndex = %d, selectValidBitIndex=%d 
5856,III,CC::: rxiqStart: %x, txiqStart: %x, txloStart: %x 
5852,I,ERROR: invalid band of %d
 
5855,II,ERROR: Out of band frequency, %d MHz at %d bandwidth
 
5854,I,WARNING, bad offset in checksum... %d
 
5853,II,checksum returns 0x%x
 for length %d
 
5852,I,ERROR: invalid band of %d
 
5851,II,ERROR: table index never found for frequency %d at %d bandwidth
 
5850,I,binToGet = 0x%x
 
5849,II,Warning: tempBin file incorrect size, %d should be %d
 
5848,III,Warning: tempBin %d not available on host. (availability: 0x%02x) ,filesize = %d
 
5847,I,data retrieved from host. fileSize = %d 
 
5846,,error: checksum creation failure...
 
5845,II,error: 0x%x bytes writen to host instead of 0x%x (file structure size)...
 
5844,I,*** halphy_get_caldb_clpc_error_status INVALID RF SUB returned. Needs investigation rfsub %d ** 
5843,I,*** halphy_read_caldb_clpc_error INVALID RF SUB received. Needs investigation rfsub %d ** 
5842,II,cur_tbl_idx %d halphy_update_caldb_dpd_calValidBit %d 
5841,I,***INVALID RF SUB returned. Needs investigation rawRfSubBand %d ** 
5841,I,***INVALID RF SUB returned. Needs investigation rawRfSubBand %d ** 
5840,II,RFSUB SCAN REMAP:: rfsub=%d, rawRfSubBand=%d 
5839,II,requiredAdjustRxDcoTimeOut lifeTime = %d for chainIdx= %d! 
5838,I,NO t_caldb_context found for chainIdx = %d! 
5837,IIIIII,bandCode=%d, bw =%d, BitBegin(subBegin)=%d(%d),BitEnd(subEnd)=%d(%d) 
5836,IIIIII,Reused calType =%d, rfSubIdx =%d rfSubIdx =%d bcode=%d bw=%d chIdx =%d 
5835,IIIII,TEMPSEN:::  calType=%d alt  rfPath = %d,chainIdx=%d, globalCallingContext=%d,useAltTableAllowed=%d  
5912,II,halphyDpdGetLoopBackInfo wrong chain or table index passed in: txChain %d tableIndex %d 
5911,II,halphyDpdMarkLoopBackFailure wrong chain index passed in: txChain %d tableIndex %d 
5910,II,halphyDpdMarkLoopBackFailure txChain %d tableIndex %d 
5909,II,halphyDpdUpdateLoopBackInfo wrong chain index passed in: txChain %d tableIndex %d 
5908,IIIIIII,zero_sq=%d,max_bin = %d,maxbin2db = %d,AGC2_PWR=%d,force=%d,new_rx_gain=%d,retry_cnt=%d 
5907,II,minSQ %d, SqIdx %d
 
5906,III,Rx Gain Index for chain %d, Table %d:%d 
5905,IIII,%d %d Small Signal Gain %d max index %d
 
5904,I,change to tableIndex=%d, clear all force rx gain state 
5903,III,mask %d Change training position to chain index %d and dpd table index %d 
 
5902,,Start writing AMAM AMPM curves data to file
 
5901,I,small signal gain is %d
 
5900,II, %d	%d
 
5899,,Finished writing AMAM AMPM curves data to file
 
5890,I,Channel %d is not in valid range
 
5898,I,halphy_core_PaprdEnableDPD: Channel %d
 
5897,I,Error: Invalid channel %d
 
5896,I,Unsupported bandwidth %d
 
5896,I,Unsupported bandwidth %d
 
5890,I,Channel %d is not in valid range
 
5895,IIII, %d %d Training quality is %d , warm %d
 
5894,III, %d %d Training quality is %d 
 
5894,III, %d %d Training quality is %d 
 
5893,,Will Recal with ForceAGC due to sq=0! 
5892,,Will Recal with ForceAGC due to max_bin/agc2_pwr violates! 
5891,I,Best SQ is %d and update DPD table 
 
5890,I,Channel %d is not in valid range
 
5936,III,2: max attempts %d Cal attemps chain 0 %d chain1 %d 
5935,III,3: max attempts %d Cal attemps chain 0 %d chain1 %d 
5934,II,DPD calibration is aborted on channel %d, state %d
 
5933,I, DPD calibration is aborted on channel %d
 
5932,,No DPD cal is in progress
 
5931,III,%s %d, channel %d
 
5930,II,Cant initiate DPD cal with DPD enable flag %d on at freq %d
 
5929,I,Total early exit retry %d 
5929,I,Total early exit retry %d 
5928,IIII,Error : %d %d DPD Cal hits a critical error and abort chan %d state %d
 
5927,,DPD Cal hits an critical error and abort
 
5926,I,DPD total cal time is %d
 
5925,I,DPD MAC core cal ime is %d
 
5924,I, Invalid state machine state %d
 
5923,I,Error : DPD Cal, going to tear down state g_dpd_hw_stuck %d
 
5922,III,halphyPaprdConfig: smState %d, channel %d, enable %d
 
5921,II,2. finalCase %d globalCallingContext %d 
5920,I,No available DPD slot for channel %d and deny cal request
 
5919,II,halphyPaprdEnableCal: Channel = %d, dpd_enable = %d
 
5918,III,halphyPaprdForceTxPaDacGain: Chain = %d, txgainIdx = %d, dacgain = %d
 
5917,,Err:DPD structure pointer is not initialized 
 
5916,I,DPD cal is already running on channel %d 
 
5915,I,This channel %d is already cal'ed
 
5914,,DPD has no home channel registered
 
5913,,DPD thermal recal is rejected
 
5937,II,EnableCckTxFirOvd phyId %d enable %d 
5942,,Invalid country code. Setting to "US". 
5941,,Invalid country_code/domain_code. No currentRD or ctl value change. 
5940,I,returned rdval: %d 
5939,,SetCTLVal call finished 
5938,IIII,regDmnBdf (internal): %d, regulatoryDomainVal: %d, ctlVal 1: %d, ctlVal 2: %d 
5972,II,BEGIN: halphy_reset_ChangeChainMask txChainMask %d rxChainMask %d 
5971,,halphy_reset_ChangeChainMask parameter validation successfull 
5970,II,halphy_reset_ChangeChainMask TX %d Rx %d chainmask 
5969,,NULL phy handle passed 
5968,,END: halphy_reset_ChangeChainMask 
5967,III,STOPPING PRECAL TIMER phyID = %d , caltimerStarted[] = %d %d 
5966,II,STOPPING PRECAL TIMER  end caltimerStarted[] = %d %d 
5965,IIIIII,HalphyResetSetup phyId %d resetFlags 0x%x resetCause 0x%x chan_max_tx_power %d limit %d maxTxPower %d 
5964,,In halphy_reset_PeriodicTemperatureRead 
5963,,In halphy_reset_PeriodicTemperatureRead, data == NULL 
5962,,In halphy_reset_PostAwakeTempCal 
5961,I,Enter halphy_reset_ReadTemperature, phyId = %d 
5960,,In halphy_reset_ReadTemperature, pResetStruct == NULL 
5959,II,Calling callback function in halphy_reset_ReadTemperature, pHandle->phyId = %d, cal_time_us = %d 
5958,IIII,ReleaseHomeChannel phyId %d index %d mhz %d freq1 %d 
5957,IIII,halphyRetentionSetChannel phyId %d txChainMask 0x%x rxChainMask 0x%x wakeup %d 
5956,IIIII,halphyRetentionSetChannel    chan %d freq1 %d freq2 %d phy_mode %d flags 0x%x 
5955,IIIII,halphyRetentionSetChannel curChan %d freq1 %d freq2 %d phy_mode %d flags 0x%x 
5954,I,change sw rxChainMask to 0x%x 
5953,II,halphyRetentionWlanASctl txChainMask 0x%x enable %d  
5952,I,1x1 board detected Updating phy specific devCaps RF_MODE = %d 
5951,IIIII,SetHomeChannel phyId %d bSet %d mhz %d freq1 %d i %d 
5950,,SetHomeChannel shouldn't get here, no more space for home channel. 
5949,IIII,halphySetTxChannelPowerLimit phyId %d limit %d maxTxPower %d curChan->mhz %d 
5948,IIIII,halphySetTxPowerLimit phyId %d chan %d limit %d is2GHz %d maxTxPower %d 
5947,IIII,HalphySetTxPowerScale phyId %d chan %d tpscale %d maxTxPower %d 
5946,III,halphy_reset_StartCalTimer  phyID %d , caltimerStarted[] = %d %d 
5945,III,halphy_reset_StartCalTimer end phyID %d , caltimerStarted[] = %d %d 
5944,I,STARTING PRECAL TIMER phyID %d 
5943,II,%s, chan = %d
 
5977,I,$$ STOPPING TPC TIMER phyID = %d $$ 
5976,I,$$ STOPPING TRAVERSE MISS TPC TIMER phyID = %d $$ 
5975,II,setting plut and alut for 160 chan1 %d chan2 %d 
5974,I,$$ STARTING TPC TIMER phyID %d $$ 
5973,I,$$ STARTING TRAVERSE MISS TPC TIMER phyID %d $$ 
5983,II,setting GLUT for 160, chan1 %d chan2 %d 
5982,II, halphy_tpc_device_ClpcPlutAlutUpdate tpcPowerOffset[%d] %d 
5981,II,halphy_tpc_device_GetOnePointTpcOffset channel %d chosen_chanid = %d 
5980,I,Programming GLUT channel %d 
5979,II,GlutUpdate chain %d: got clpcError %d from bdf 
5978,II,%s:chan 0x%x
 
5984,IIIIII,Configured ADC Capture for PhyID: %d, Chain: %d, Compression: %d, Mode: %d, Trigger: %d, Capture size: %d 
5988,II,Setting Phy %d AGC History Control to %d (0 = Disable, 1 = Enable) 
5987,II,AGC History Dump for Phy %d, chainmask %x 
5986,,AGC History logging not enabled, nothing to dump 
5985,, CHA IDX SEQ  TIME RSSI_P RSSI_E RSSI_C XLNA_N GcMode BBSAT RFSAT MBGAIN RFGAIN    Trig Reason/Details 
5999,IIII,ANI_DBGID_RESET  phyId %d resetFlags 0x%x resetCause 0x%x curChan 0x%x 
5998,II,ANI_DBGID_OFDM_LEVEL  0x%x 0x%x 
5997,I,ANI_DBGID_CCK_LEVEL  0x%x 
5996,,ANI_DBGID_CCK_LEVEL_CFG: ANI_CCK_DISABLE 
5995,I,ANI_DBGID_CCK_LEVEL_CFG: 0x%x 
5994,I,ANI_DBGID_OFDM_LEVEL_CFG: 0x%x 
5993,II,ANI_DBGID_CCK_LEVEL phyId %d 0x%x 
5992,III,ANI_DBGID_OFDM_LEVEL  phyId %d 0x%x 0x%x 
5991,IIIIII,StoreBandDependentIniValues 0x%x 0x%x 0x%x 0x%x 0x%x 0x%x 
5990,IIIIII,StoreBwDependentIniValues 0x%x 0x%x 0x%x 0x%x 0x%x 0x%x 
5989,IIIIII,StoreCommonIniValues 0x%x 0x%x 0x%x 0x%x 0x%x 0x%x 
6040,,*** ADC Timer Expired, Capture not triggered *** 
6039,I,*** ADC Timer Expired, Dumping ADC Data, Trigger Mode: 0x%X *** 
6038,II,GLUT pData[%d] =  0x%08X 
6037,II,PLUT pData[%d] =  0x%08X 
6036,II,ALUT pData[%d] =  0x%08X 
6035,,yet to get the resgisters list 
6034,I,GetLUTTablesDump Invalid dumpOption = %d 
6033,,GetPowerTableDump
 
6032,,RATE INDEX 	POWER 
6031,II,%d 	 	 %d
 
6030,,GetPowerTableDump complete
 
6029,I,Invalid device, vdev_id = %d 
6019,I,WDOG CTRL_1 Readback, 0x003463F8:0x%08X 
6018,I,WDOG CTRL_2 Readback, 0x003463FC:0x%08X 
6028,IIII,WDOG: status = 0x%x status_b = 0x%x status_c = 0x%x status_d = 0x%x 
6027,II,Invalid # of args for Report WDOG Status, expecting iwpriv <dev> setUnitTestCmd %d 1 %d 
6026,I,Invalid halphy debug sub command: %d 
6025,I,ADC dump timer set timer for %d ms 
6024,II,Invalid # of args for ADC Capture, expecting iwpriv <dev> setUnitTestCmd %d 5 %d <chain> <comp_mode> <trig> 
6023,II,Addr:Value, 0x%08X:0x%08X 
6022,,CSS Retention Check failed, cannot read 
6021,II,Invalid # of args for Reg Read, expecting iwpriv <dev> setUnitTestCmd %d 2 %d <addr> 
6020,II,Invalid # of args for AGC history Report, expecting iwpriv <dev> setUnitTestCmd %d 1 %d 
6019,I,WDOG CTRL_1 Readback, 0x003463F8:0x%08X 
6018,I,WDOG CTRL_2 Readback, 0x003463FC:0x%08X 
6017,II,Invalid # of args for Config WDOG, expecting iwpriv <dev> setUnitTestCmd %d 3 %d <idle time> <non-idle time> 
6016,I,Phy Debug Dump: waiting for capture to complete...%d of 10
 
6015,,error: failed to access dump memory
 
6014,II,Phy Debug Dump: num of samples: %d, Output Mode: 0x%x 
6013,III, Index %03d: 0x%08x%08x 
6012,IIIII,halphy_debug_device_RxGain_control(PhyID=%d, xlnaCtrl=%d, gainCtrlMode=%d, band=%d, gainIdx=%d) 
6011,,Rx gain control: Invalid index selected
 
6011,,Rx gain control: Invalid index selected
 
6010,,rxGainCtrlHandler: Rx gain control: Invalid band selected
 
6009,I,Rx gain control: Set automatic gain control with xlna = %d
 
6008,IIII,Force Tx Gain: Chain: %d, Ana Gain: %d, Digi Gain: %d, Force Cal Index: %d 
6007,,TxGainCtrl: Calling Rx Abort 
6006,I,utfEnableKoKg disable=%d 
6005,I,utfReadPDADC pdadc=%d 
6004,II,utfSetPDADC_BIAS current pdadc_bias=%d, new value=%d 
6003,I,utfSetPDADC_BIAS pdadc_bias=%d 
3951,IIIII,freq %d chainmask 0x%x mode 0x%x tx_gain 0x%x ant_sel 0x%x
 
3951,IIIII,freq %d chainmask 0x%x mode 0x%x tx_gain 0x%x ant_sel 0x%x
 
6002,IIII,ADC capture::: Index %03d: %08x, I=%d, Q=%d
 
6001,IIIIIIII,ADC capture::: minI=%d, maxI=%d, averageI=%d, varI=%d, minQ=%d, maxQ=%d, averageQ=%d, varQ=%d 
6000,I,Time taken = %d uSecs 
6045,,Disabling 2xDAC interpolation 
6044,,2xDAC interpolation already enabled 
6043,,BLACKBOLT CHIP: SDM636/SDA636 
6042,,NOT BLACKBOLT CHIP 
6041,I,halphySetPhyRfMode %d 
6180,I,DPD training Done %d 
 
6179,I,DPD training AGC2 size %d 
 
6178,I,DPD training AGC2 pwr %d 
 
6177,I,DPD training rx gain %d 
 
6176,I,DPD training active %d 
 
6175,I,DPD training incomplete %d 
 
6174,I,DPD training corr err %d 
 
6173,I,STAT3:  %8x
 
6172,I,SQ Idx %d 
 
6171,I,DC estimate I %d 
 
6170,I,DC estimate Q %d 
 
6169,I,STAT4: tx_max %d 
 
6168,I,STAT4: tx_min %d 
 
6167,I, PAPRD_SQ_VAL : %d
 
6166,III,dpdDisable Channel: %d Found@ chain %d! check bdf arrayIdx %d 
6165,IIIII,channel %d agc2_pwr %d rx_gain %d SQ Idx %d agc_size %d
 
6164,II,DC estimate I %d , Q %d
 
6132,I,Error: %s  DPD table address 
6163,I,  Chain %d 
 
6162,II,  B0_CTRL0 0x%8x,  B0_CTRL0 0x%8x
 
6161,II,  B0_CTRL1 0x%8x,  B0_CTRL1 0x%8x
 
6160,II,  B0_CTRL2 0x%8x,  B0_CTRL2 0x%8x
 
6159,II,  B0_CTRL3 0x%8x,  B0_CTRL3 0x%8x
 
6158,II,  CH0 Tbl 0 0x%8x,  CH1 Tbl 0 %d
 
6157,II,  CH0 Tbl 1 0x%8x,  CH1 Tbl 1 %d
 
6156,II,  CH0 Tbl 2 0x%8x,  CH1 Tbl 2 %d
 
6155,II,  CH0 Tbl 3 0x%8x,  CH1 Tbl 3 %d
 
6059,II,  dc_i      0x%8x,  dc_i      %d
 
6058,II,  dc_q      0x%8x,  dc_q      %d
 
6057,II,  sq_idx    0x%8x,  sq_idx     %d
 
6055,II,  agc2_pwr  0x%8x,  agc2_pwr   %d
 
6054,II,  rx_gain   0x%8x,  rx_gain    %d
 
6154,II,  Channel   0x%8x,  channel    %d
 
6153,IIII, dump_dpd_table phyId %d , start %d end %d, cur_tbl_idx %d
 !! 
6095,III,DPD LUT[%d] reg addr 0x%8x, val = %d 
 
6095,III,DPD LUT[%d] reg addr 0x%8x, val = %d 
 
6152,I, B0_CTRL0 %x
 
6151,I, B0_CTRL1 %x
 
6150,I, B0_CTRL2 %x
 
6149,I, B0_CTRL3 %x
 
6148,I, B1_CTRL0 %x
 
6147,I, B1_CTRL1 %x
 
6146,I, B1_CTRL2 %x
 
6145,I, B1_CTRL3 %x
 
6144,IIII, halphyDumpPaprdCtrl phyId %d , start %d end %d, cur_tbl_idx %d
 !! 
6136,I,  B0_CTRL0 0x%8x,  
 
6135,I,  B0_CTRL1 0x%8x,  
 
6134,I,  B0_CTRL2 0x%8x,  
 
6133,I,  B0_CTRL3 0x%8x,  
 
6079,I, (0 4) small signal gain %d, 
 
6078,I, (0 5) small signal gain %d, 
 
6077,I, (0 6) small signal gain %d, 
 
6076,I, (0 7) small signal gain %d, 
 
6074,I, (0 0) small signal gain %d, 
 
6073,I, (0 1) small signal gain %d, 
 
6072,I, (0 2) small signal gain %d, 
 
6071,I, (0 3) small signal gain %d, 
 
6131,I,  B1_CTRL0 0x%8x,  
 
6130,I,  B1_CTRL1 0x%8x,  
 
6129,I,  B1_CTRL2 0x%8x,  
 
6128,I,  B1_CTRL3 0x%8x,  
 
6127,I, (1 4) small signal gain %d, 
 
6126,I, (1 5) small signal gain %d, 
 
6125,I, (1 6) small signal gain %d, 
 
6124,I, (1 7) small signal gain %d, 
 
6123,I, (1 0) small signal gain %d, 
 
6122,I, (1 1) small signal gain %d, 
 
6121,I, (1 2) small signal gain %d, 
 
6120,I, (1 3) small signal gain %d, 
 
6143,,watchdog disabled 
6142,,watchdog enabled 
6141,II,(prev) GLUT %d Programming GLUT channel DPD channel %d 
6140,I,  AMAM 0x%8x,  
 
6139,I,  AMPM 0x%8x,  
 
6138,I,  HT40 0x%8x,  
 
6137,I,  HT80 0x%8x,  
 
6132,I,Error: %s  DPD table address 
6136,I,  B0_CTRL0 0x%8x,  
 
6135,I,  B0_CTRL1 0x%8x,  
 
6134,I,  B0_CTRL2 0x%8x,  
 
6133,I,  B0_CTRL3 0x%8x,  
 
6082,III, chain %d table %d Small signal gain  %d
 
6081,I,Invalid table index %d
 
6079,I, (0 4) small signal gain %d, 
 
6078,I, (0 5) small signal gain %d, 
 
6077,I, (0 6) small signal gain %d, 
 
6076,I, (0 7) small signal gain %d, 
 
6074,I, (0 0) small signal gain %d, 
 
6073,I, (0 1) small signal gain %d, 
 
6072,I, (0 2) small signal gain %d, 
 
6071,I, (0 3) small signal gain %d, 
 
6070,I,  SSQ 0 0x%8x,  
 
6069,I,  SSQ 1 0x%8x,  
 
6067,I,  SSQ 2 0x%8x,  
 
6132,I,Error: %s  DPD table address 
6131,I,  B1_CTRL0 0x%8x,  
 
6130,I,  B1_CTRL1 0x%8x,  
 
6129,I,  B1_CTRL2 0x%8x,  
 
6128,I,  B1_CTRL3 0x%8x,  
 
6082,III, chain %d table %d Small signal gain  %d
 
6081,I,Invalid table index %d
 
6127,I, (1 4) small signal gain %d, 
 
6126,I, (1 5) small signal gain %d, 
 
6125,I, (1 6) small signal gain %d, 
 
6124,I, (1 7) small signal gain %d, 
 
6123,I, (1 0) small signal gain %d, 
 
6122,I, (1 1) small signal gain %d, 
 
6121,I, (1 2) small signal gain %d, 
 
6120,I, (1 3) small signal gain %d, 
 
6070,I,  SSQ 0 0x%8x,  
 
6069,I,  SSQ 1 0x%8x,  
 
6067,I,  SSQ 2 0x%8x,  
 
6066,I,Invalid digital chain number %d
 
6051,I,Error: %s Invalid DPD table address 
6049,I,Error: %s  Invalid DPD table address 
6113,I,Invalid chain number %d
 
6119,IIIII,force gain: pa_cfg = %d, gain_index = %d, 1dbgain = %d, 6dbgain = %d, mxgain = %d 
 
6118,IIII,Chan %d halphy_paprd_device_GetComplete phyId %d, (%d %d) 
6117,I,Chan %d , dpd not requested 
 
6117,I,Chan %d , dpd not requested 
 
6116,II,Chan %d halphy_paprd_device_GetComplete %d 
6115,IIII,dpdBit[0] %d validBit[0] %x, dpdBit[1] %d validBit[1] %x 
6114,IIII,cur idx %d Chan %d halphy_paprd_device_GetComplete %d %d 
6113,I,Invalid chain number %d
 
6112,II,dpd enable 2G  %d  5G %d
 
6111,III,Disable HW search timing : forceSqEnable %d , hw_search_sq_timing %d sq_idx %d
 
6110,I,Unsupported PEF rf mode %d 
 
6109,III,read back DPD LUT[%d] val= %d; org= %d
 
6109,III,read back DPD LUT[%d] val= %d; org= %d
 
6108,I,Invalid analog chain number %d
 
6107,I,PAPRD_VALID_GAIN_5_0_0 = 0x%x
 
6106,I,PAPRD_VALID_PA_SETTING_0 = 0x%x
 
6105,I,PAPRD_ADAPTIVE_TABLE_VALID_0 =0x%x
 
6104,I,PAPRD_TABLE_RFBMODE_0 =0x%x
 
6103,I,valid_tx_gain_readback_dpdlut_5_0 = 0x%x
 
6102,I,valid_tx_gain_readback_dpdlut_7_6 = 0x%x
 
6101,I,valid_PA_cfg_readback = 0x%x
 
6100,I,dpd_lut_validity_flag_readback =0x%x
 
6066,I,Invalid digital chain number %d
 
6099,IIIII,Chain = %d, dpd_table_index = %d, glut_offset %x txgain_index = %d, pa_cfg = %d 
 
6098,III, Restore Paprd Tables %d , start %d end %d
 !! 
6082,III, chain %d table %d Small signal gain  %d
 
6081,I,Invalid table index %d
 
6079,I, (0 4) small signal gain %d, 
 
6078,I, (0 5) small signal gain %d, 
 
6077,I, (0 6) small signal gain %d, 
 
6076,I, (0 7) small signal gain %d, 
 
6097,IIIII, Restore (%d %d) dpdStart 0x%8x dpdCtrlStart 0x%8x, dpdTrgStart 0x%8x
 
6074,I, (0 0) small signal gain %d, 
 
6073,I, (0 1) small signal gain %d, 
 
6072,I, (0 2) small signal gain %d, 
 
6071,I, (0 3) small signal gain %d, 
 
6070,I,  SSQ 0 0x%8x,  
 
6069,I,  SSQ 1 0x%8x,  
 
6067,I,  SSQ 2 0x%8x,  
 
6051,I,Error: %s Invalid DPD table address 
6056,II, halphy_get_caldb_dpd_calValidBit %d, chain %d
 !! 
6096,IIII, Restore (%d %d) dpdStart 0x%8x dpdCtrlStart 0x%8x
 
6095,III,DPD LUT[%d] reg addr 0x%8x, val = %d 
 
6094,III,Chain %d tableIdx %d, tmpdpdStart 0x%8x
 
6093,IIIII,DPD LUT[%d] reg addr 0x%8x, val = %d DB 0x%8x, val = %d 
 
6085,, DPD database CTRL registers contens  
 
6092,II,  B1_CTRL0 0x%8x,  B1_CTRL0 0x%8x
 
6091,II,  B1_CTRL1 0x%8x,  B1_CTRL1 0x%8x
 
6090,II,  B1_CTRL2 0x%8x,  B1_CTRL2 0x%8x
 
6089,II,  B1_CTRL3 0x%8x,  B1_CTRL3 0x%8x
 
6088,II,  CH1 Tbl 0 0x%8x,  CH1 Tbl 0 %d
 
6087,II,  CH1 Tbl 1 0x%8x,  CH1 Tbl 1 %d
 
6086,II,  CH1 Tbl 2 0x%8x,  CH1 Tbl 2 %d
 
6085,, DPD database CTRL registers contens  
 
6084,II,  CH1 Tbl 3 0x%8x,  CH1 Tbl 3 %d
 
6059,II,  dc_i      0x%8x,  dc_i      %d
 
6058,II,  dc_q      0x%8x,  dc_q      %d
 
6057,II,  sq_idx    0x%8x,  sq_idx     %d
 
6055,II,  agc2_pwr  0x%8x,  agc2_pwr   %d
 
6054,II,  rx_gain   0x%8x,  rx_gain    %d
 
6083,II, Ch1: Channel   0x%8x,  channel    %d
 
6052,IIII, tmpTbl %x  gain %d, pa %d valid %d
 
6082,III, chain %d table %d Small signal gain  %d
 
6081,I,Invalid table index %d
 
6080,II,  B0_CTRL0 0x%8x,  B0_CTRL0 %x
 
6079,I, (0 4) small signal gain %d, 
 
6078,I, (0 5) small signal gain %d, 
 
6077,I, (0 6) small signal gain %d, 
 
6076,I, (0 7) small signal gain %d, 
 
6075,I,Error: %s  DDR, Invalid DPD table address 
6074,I, (0 0) small signal gain %d, 
 
6073,I, (0 1) small signal gain %d, 
 
6072,I, (0 2) small signal gain %d, 
 
6071,I, (0 3) small signal gain %d, 
 
6070,I,  SSQ 0 0x%8x,  
 
6069,I,  SSQ 1 0x%8x,  
 
6068,II,  B0_CTRL1 0x%8x,  B0_CTRL1 %x
 
6067,I,  SSQ 2 0x%8x,  
 
6066,I,Invalid digital chain number %d
 
6065,II,  B0_CTRL2 0x%8x,  B0_CTRL2 %x
 
6064,II,  B0_CTRL3 0x%8x,  B0_CTRL3 %x
 
6063,II,  CH0 Tbl 0 0x%8x,  CH0 Tbl 0 %d
 
6062,II,  CH0 Tbl 1 0x%8x,  CH0 Tbl 1 %d
 
6061,II,  CH0 Tbl 2 0x%8x,  CH0 Tbl 2 %d
 
6060,II,  CH0 Tbl 3 0x%8x,  CH0 Tbl 3 %d
 
6059,II,  dc_i      0x%8x,  dc_i      %d
 
6058,II,  dc_q      0x%8x,  dc_q      %d
 
6057,II,  sq_idx    0x%8x,  sq_idx     %d
 
6056,II, halphy_get_caldb_dpd_calValidBit %d, chain %d
 !! 
6055,II,  agc2_pwr  0x%8x,  agc2_pwr   %d
 
6054,II,  rx_gain   0x%8x,  rx_gain    %d
 
6053,II, Ch0: Channel   0x%8x,  channel    %d
 
6052,IIII, tmpTbl %x  gain %d, pa %d valid %d
 
6051,I,Error: %s Invalid DPD table address 
6048,IIII, Store (%d %d) dpdStart 0x%8x dpdCtrlStart 0x%8x
 
6050,III, Store (%d %d) dpdStart 0x%8x dpdCtrlStart 0x%8x
 
6047,III,[%d] reg addr 0x%8x, val = %d  
 
6049,I,Error: %s  Invalid DPD table address 
6048,IIII, Store (%d %d) dpdStart 0x%8x dpdCtrlStart 0x%8x
 
6047,III,[%d] reg addr 0x%8x, val = %d  
 
6046,II, gain idx %x, existing %x
 
6046,II, gain idx %x, existing %x
 
6181,IIIIII,apply txFirOvd: common(0x%x 0x%x 0x%x) ch14(0x%x 0x%x 0x%x) 
6182,I,halphy_rtt_device_DoAdaptScaling  RSFD_REG_MAP_BB_RTT_CNTL =%x 
 
6201,,halphy_is_Pmm_Clk_Enabled 
6200,II,Config BB WDog: Param %X, Value: %X 
6199,I,bb_wdog_ctrl_2_status = %d 
6198,,Unsupported config for Phy BB Watchdog 
6197,,ADC: halphy_reset_device_ClkGenSwReset CLK RESET NAPALI  
6196,I,11ac is remains un affected register write address: %x 
6195,I,Phy Id is %d when RF_MODE is HALPHY_RF_MODE_NON_DBS_PHY0 
6194,I,Original Devcap11Ac CAPACITY PASSED : %x 
6193,I,11ac is DISABLED. NEW CAPABILITY value: %x 
6192,I,11ac is remains un affected . Original value: %x 
6191,I,halphy_reset_device_PostChainMaskChangeProcessing: BEGIN FREq: %d 
6190,I,halphy_reset_device_PostChainMaskChangeProcessing: END dtimEnable %d 
6189,,recover xbar_mode to 0 
6188,I,CM=1, changing xbar_mode to %d 
6187,I,CM=2, changing xbar_mode to %d 
6186,III,halphyDeviceRetentionSetChannel phyId %d aniOFDMLevel 0x%x wakeup %d 
6185,I,halphyDeviceRetentionSetChannel beaconRSSI %d 
6184,III,PostCal tunning off unused chain#%d, txChainmask 0x%x rxChainmask 0x%x 
6183,,STARLORD Max BW support set to 80MHz in NON_DBS_PHYA mode 
6205,I,80P80::: iterativeCnt=%d subset ar6000ChannelSwitch stage cal done 
6184,III,PostCal tunning off unused chain#%d, txChainmask 0x%x rxChainmask 0x%x 
6204,I,preCal set chainmask to 0x%x 
6203,III,PHY %d Setting hw table: %d rxChainMask %d 
6202,II,CCK Blocker Detect State: %X, is Home Channel:%d 
6210,IIII,NfAddTempOffset is2G %d latestTemp %d maxCCApwr[%d] + %d 
6209,IIII,NfForceNFValue phyId %d chain_mask 0x%x maxCCApwr[0] = %d  maxCCApwr[1] = %d 
6208,II,startcal:%d doNoiseFloorCal failed BB_agc_control is 0x%08x 
6207,III,NfStartCal chain_mask 0x%x ch_idx = %d  NF = %d 
6206,III,NfStartCal NF readback chain_mask 0x%x ch_idx = %d  NF = %d 
6212,I,halphyRfaCtrlErrorHandler: Invalid chain %d 
6211,IIII,halphyRfaCtrlErrorHandler: CH%d    Bus Error status 0x%08x    BP_TIMEOUT_ERROR_count %d    NAK_ERROR_count %d 
6213,,RXDCO: GO BEYOND ALLOCATED BUF!  
6214,II,RXDCO: cal_time(us): %d cal_status %d 
6215,III,RXDCO: bwCode:%d, rxdco_cal_mode:%d, isDTIM:%d  
6216,IIII,RXDCO: phyId:%d, rxChMask:%d, homeCh:%d,  bandCode:%d 
6217,,Rxdco CAL HW enable for finalCase = 0 
6218,III,RXDCO LUT is disabled for phyId = %d, rxChMask = %d, bandCode=%d !!!!! 
6219,II,DCO_LUT_RF[%d] = %d 
6220,II,DCO_LUT_BB[%d] = %d 
6221,II,tempRF_shifted[%d] = %d 
6222,I,RXDCO: Kmeas_min_bits; = %d 
6219,II,DCO_LUT_RF[%d] = %d 
6220,II,DCO_LUT_BB[%d] = %d 
6223,I,RXDCO: over flow with rnge2-rnge = %d 
6224,I,RXDCO: Quantize function input over flow: 2	 shift = %d 
6225,I,Quantize function input over flow: 1	 shift = %d 
6226,I,Quantize function input over flow: 0	 shift = %d 
6227,I,RXDCO: ODAC_GAIN_RATIO_BB failure! pIn->chCal = %d! 
6228,,RXDCO: ODAC_GAIN_RATIO_RF failure!  
6229,,RXDCO: BB_dcoc_range out of max range. need debug! 
6230,IIIII,RXDCO: pIn->RF_first=%d, Binary search failed due to ODAC out of range!chidx = %d, d= %d,pHwResults->bI=%d, pHwResults->bQ=%d! 
6231,IIIII,RXDCO: pIn->RF_first=%d, chidx = %d, d= %d,pHwResults->bI=%d, pHwResults->bQ=%d with the previous good gain result! 
6232,II,RXDCO: Binary search failed @chidx = %d, d= %d! 
6233,IIIII,RXDCO: phyId = %d bandCode = %d	 W/R cal_gain[%d] = 0x%08x : 0x%08x 
6234,II,apache RXDCO_CAL_MODE_LPBK_IQ mode %d chain %d 
6235,,RXDCO: cal_done time out 
6236,IIIIIIII,turbo_data[%d][%d][%d]: aI %d, aQ=%d, bI=%d, bQ=%d, bS=%d 
6237,IIII,HQ::: Normal CAL turbo_iter=%d, in->num_gain = %d, BS_I=%d, BS_Q=%d 
6238,IIII,HQ::: Comb CAL turbo_iter=%d, in->num_gain = %d, BS_I=%d, BS_Q=%d 
6239,III,HQ::: DPD in->num_gain = %d, BS_I=%d, BS_Q=%d 
6240,III,HQ::: DTIM in->num_gain =%d, BS_I=%d, BS_Q=%d 
6241,,RXDCO Rxdco detected it was running in noisy env! 
6242,II,RXDCO: calDeltaTime = %d > calTimeThresold = %d 
6214,II,RXDCO: cal_time(us): %d cal_status %d 
6243,,RXDCO CAL failure!!! 
6244,,RXDCO CAL early exits in noisy environment!!! 
6245,IIIIIIIII,HQ::: cal_status=%d, %d, %d, %d, %d, %d, %d, %d, %d 
6246,,RXDCO: CAL Failure!!!!!!!! 
6247,,RXDCO: CAL Failure!!!!!!!! Write default value to 256. 
6248,,Error: write to DDR Invalid table address found!!!!! 
6249,III,HQ::: i = %d, BB_DCO_LUT_i = %d, BB_DCO_LUT_q = %d 
6250,II,HQ::: DPD Gain_LUT[%d] = 0x%08x 
6251,II,RXDCO: RF_DCO_LUT i: %d  q %d   
6252,II,RXDCO: BB_DCO_LUT i: %d  q %d   
6253,,RXDCO DPD: HWCAL_AFTER_ODAC_GAIN_RATIO failure!  
6254,,RXDCO DPD: FIND_ODAC_GAIN_RATIO failure!  
6255,,RXDCO: HWCAL_AFTER_ODAC_GAIN_RATIO failure!  
6256,II,RXDCO: calDeltaTime = %d > calTimeThresold 
6257,,RXDCO: FIND_ODAC_GAIN_RATIO failure!  
6258,II, failed: odac_ratio0I=%d, odac_ratio0Q=%d 
6259,IIII,RXDCO: calDeltaTime = %d > calTimeThresold =%d, rxChMask=%d, sp_rxdco.chCal=%d 
6260,IIIIIII,RXDCO: phyId:%d, rxChMask:%d, homeCh:%d, bandCode:%d, bwCode:%d, rxdco_cal_mode:%d, lpbk_mode:%d 
6261,III,RXDCO: Rxdco cal support for board_version = 0x%x, XLNA_PRESENT = %d, IPA_PRESENT = %d 
6262,I,RXDCO: V%x Rxdco cal is not supported in this build!  
6263,,RXDCO: DTIM RxDCO cal is supported in this build!  
6287,II,RXDCO 0_0::: rxdco_cal_mode B (18 DTIM):%d	 finalCase=:%d 
6286,I,set Rxdco LUT lifeTime =%d 
6282,,Restore Rxdco LUT from the previous valid one! 
6285,II,RXDCO 0_0::: rxdco_cal_mode A:%d	 finalCase=:%d 
6267,,Error: restore from DDR, invalid table address found! 
6284,IIIIIIII,RXDCOSM:::pHdl=%x, phyRfMode=%d, phyID=%d, 2/5G=%d,bw=%d, rxCM=%d, homeCh=%d, cur_tbl_idx=%d 
6283,II,set Rxdco: AAA -->LUT ((requiredAdjustRxDcoTimeOut(pIn->pHandle,  pIn->rxChMask, RXDCO) =%d and set liftTime = %d 
6282,,Restore Rxdco LUT from the previous valid one! 
6281,,Previous and current Rxdco all failed! 
6280,,absolutely fail 
6279,I,RXDCOSM:::RXDCO_CAL for DPD SPLIT CAL DONE. Recovery complete. iSrxdcoDpdCalConducted %d  
6278,I,RXDCOSM::: EXIT globalCallingContext %d  
6277,,RXDCOSM:::RXDCO_CAL_MODE_LPBK_DPD will be carried out 
6276,IIII,RXDCO 0_1::: rxdco_cal_mode(0: Normal, 1: DTIM, 2, Comb, 7: DPD) B:%d	 finalCase=:%d, globalCallingContext=%d, iSrxdcoDpdCalConducted %d  
6275,,RXDCO 0_1::: DPD_SPLIT_CAL RXDCO,NOMIMAL_APPLICABLE 
6273,I,DPD_SPLIT_CAL RXDCO finalCase:%d 
6274,,RXDCO 0_1::: DPD_SPLIT_CAL RXDCO,NOT NOMIMAL_APPLICABLE 
6273,I,DPD_SPLIT_CAL RXDCO finalCase:%d 
6272,II,RXDCO 0_1::: rxdco_cal_mode(0: Normal, 1: DTIM, 2, Comb, 7: DPD) A:%d	 finalCase=:%d 
6271,I,RXSM:::POWER_SAVE_WAKE_UP finalcase = %d 
6270,I,RXDCO 0_1::: final decsion (final case) = %d 
6269,,Disable Rxdco LUT 
6268,IIIII, RxDCO Restored Data of Chain:%d, %d, %d, %d, %d 
6267,,Error: restore from DDR, invalid table address found! 
6266,I,Rxdco cal not allowed prevTimeStamp =%d 
6265,II,set Rxdco LUT lifeTime =%d, pOutput->rxdcoExecutionTime=%d 
6264,I,set Rxdco :BBB -->LUT ((requiredAdjustRxDcoTimeOut(pIn->pHandle,  pIn->rxChMask, RXDCO) =%d 
6288,I,TEMPSEN::: read Total time (us)  :%d 
6300,IIIIIIIII,CC:::pHdl=%x, phyRfMode=%d, phyID=%d, 2/5G=%d,bw=%d, txCM=%d, rxCM=%d, hwTblIdx=%d(%d)  
6299,IIII,CC::: globalCallingContext = %x, freqIdx=%d, Running DPD RxIQ 5G IPA for 80p80 freq1=%d and freq2=%d 
6298,IIII,CC::: globalCallingContext = %x, freqIdx=%d, Writing DPD RxIQ coeffs for ch#0 f1=%d and ch#1 f2=%d 
6297,IIII,CC::: globalCallingContext = %x, freqIdx=%d, Running DPD RxIQ for 5G IPA for BW=%d freq=%d 
6296,III,CC:::calAtScan=%x, globalCallingContext=%d, finalCase=%d 
6295,I,CC::: phyRfMode = %x, in DPD split cal, cannot do RxIQ cal therefore disable correction 
6294,,CC::: 80+80 check, f1!=f2 can't do comb cal.... 
6293,,CC::: Cal, Nothing to do, just reenable 
6292,,CC:: RX IQ Coeff. Dumping Coeff of All 16 gain indexes.Each gain index has Taps - 7 
6291,,CC:::  Cal, Restore and re-enable 
6290,II,CC::: Total time (us) (cal op: %d) :%d 
6289,I,CC::: phyRfMode = %x, cannot do cal and disable 
6343,I,CC::: RxCorr Cal data in registers set to %d 
6342,I,CC::: TxCorr Cal data in registers set to %d 
6341,II,CC::: TxLO Cal data in registers set to %d for mode %d (0=Dig, 1=Ana) 
6340,I,TxIQ correction enabed = %d 
6339,I,RxIQ correction enabed = %d 
6338,I,PHYA_BB_RX_OCGAIN_0_ADDRESS = %x 
6337,I,PHYA_BB_RX_OCGAIN_1_ADDRESS = %x 
6336,I,PHYA_BB_RX_OCGAIN_2_ADDRESS = %x 
6335,I,PHYA_BB_RX_OCGAIN_3_ADDRESS = %x 
6334,I,PHYA_BB_RX_OCGAIN_4_ADDRESS = %x 
6333,I,PHYA_BB_RX_OCGAIN_5_ADDRESS = %x 
6332,I,PHYA_BB_RX_OCGAIN_6_ADDRESS = %x 
6331,I,PHYA_BB_RX_OCGAIN_7_ADDRESS = %x 
6330,I,PHYA_BB_RX_OCGAIN_8_ADDRESS = %x 
6329,III,CC::: rxGainIdx %d rx_gain_idx_mapping %d rx_gain_deltax2 %d
 
6328,III,PhyId = %d, Chain = %d, LB = %d
 
6327,III,rxiq: idx = %d, 	mag = %d	 phs = %d
 
6327,III,rxiq: idx = %d, 	mag = %d	 phs = %d
 
6327,III,rxiq: idx = %d, 	mag = %d	 phs = %d
 
6327,III,rxiq: idx = %d, 	mag = %d	 phs = %d
 
6326,III,txiq: idx = %d, 	mag = %d	 phs = %d
 
6326,III,txiq: idx = %d, 	mag = %d	 phs = %d
 
6326,III,txiq: idx = %d, 	mag = %d	 phs = %d
 
6326,III,txiq: idx = %d, 	mag = %d	 phs = %d
 
6325,III,PhyId: %d, HW table idx = %d, TxIQ correction enabed = %d 
6324,III,PhyId: %d, HW table idx = %d, RxIQ correction enabed = %d 
6323,IIIII,chain %d rxiq corr: idx = %d, 	I = %d	 Q = %d
 
6323,IIIII,chain %d rxiq corr: idx = %d, 	I = %d	 Q = %d
 
6322,IIII,chain %d txiq corr: idx = %d, 	I = %d	 Q = %d
 
6321,II,SP::tbl0 restored:idx = %d, gain_lut = 0x%4x
 
6320,II,SP::tbl0:idx = %d, gain_lut = 0x%4x
 
6319,II,SP::tbl1:idx = %d, gain_lut = 0x%4x
 
6318,II,SP::tbl0 again:idx = %d, gain_lut = 0x%4x
 
6317,III,CC::: PhyId = %d, Chain = %d, loc = %d
 
6316,III,txlo:idx = %d, 	cl_I = %d	 cl_Q = %d
 
6315,,HW measurement failing 
6310,I,CC::: Using Correction value: %d 
6314,I,CC::: Started Combined Cal (%d) 
6313,I,Disabling LO and IQ correction due to HW failure count = %d 
6312,I,CC::: Completed Combined Cal (%d) 
6311,I,Tone idx = %d
 
6311,I,Tone idx = %d
 
6310,I,CC::: Using Correction value: %d 
6309,IIIIII,CC::: pIn->dir=%d, pIn->chn=%d, pIn->homeChannel=%x, rxiqStart=%x,txiqStart=%x, txloStart=%x 
6306,I,CC::: %s restore from DDR, Invalid table address found 
6308,I,CC::: %s write to DDR, Invalid table address found 
6307,IIIII,CC::: pIn->homeChannel=%x, pIn->chn=%d, rxiqStart=%x,txiqStart=%x, txloStart=%x 
6306,I,CC::: %s restore from DDR, Invalid table address found 
6305,I,Error: %s write to DDR Invalid table address found 
6304,I,CC::: Reg_Tx_Lo (Ana): Data: %x 
6303,,Error: restore from Invalid table address found 
6302,,Error: write to DDR Invalid table address found 
6301,I,CC::: Reg_Tx_Lo (Dig): Data: %x 
6349,I,Invalid channel %d 
6348,II,xPA %d Channel %d 
6347,III,max attempts %d Cals attempted chain 0 %d chain1 %d 
6346,I,DPD Cal::: phyRfMode = %x, cannot do cal and disable 
6345,IIIII,DPD:::pHdl=%x, phyRfMode=%d, phyID=%d, txCM=%d, rxCM=%d  
6344,II,1. finalCase %d globalCallingContext %d 
6350,I,ADC::: End of cal, calSuccess = %d 
6351,II,done = 0x%3x, error = 0x%3x
 
6352,,ADC run_adc_cal: ONLY NAPALI  
6353,III,ADC::: AdcCalhadBeenPassed = %d, time=%d, (%d) no cal needed, and enable ADC to use restore values 
6354,IIII,ADC::: cal is allowed (%d, %d, %d, %d) 
6355,IIII,ADC::: not allowed (%d, %d, %d, %d) 
6356,I,ADC::: not passed before and curent PHY = %d 
6357,,DAc:::DAC Do cal entry 
6358,II,DAC:::DAC cal entry, doneYet=%d (%d) 
6362,IIIIIII,DAC Playback: Phy Id:%d, mode:%d, options:%d, radar on/off:%d/%d, chain mask:%d, count: %d
 
6361,II,DAC Playback Load: Chain Mask: %d, Count: %d
 
6360,,DAC Playback: Loaded memory with waveform data
 
6359,I,DAC Playback: Stop/Pause playback with chain mask %d
 
6363,II,PDET::: restore: overrideVal=%d, rfChainIdx=%x: 
6364,III,PDET::: restore: bandcode=%d, rfChainIdx=%x, isValid=%d: 
6365,II,PDET::: txChainMask=%d, chainIdx=%x: 
6366,I,PDET::: cal time = %d 
6367,III,PDET::: calPass=%d, calChainValuePass[%d]=%d 
6368,IIIII,PDET::: phyRfMode=%d, phyId=%d, bandcode=%d, chain %d cal value=%d
 
6368,IIIII,PDET::: phyRfMode=%d, phyId=%d, bandcode=%d, chain %d cal value=%d
 
6369,,PDET::: Unsupported configuration: 
6370,III,PDET::: RFPDET_RESTORE: calStatus=%d, bandcode=%x, chainIdx=%x: 
6371,III,PDET::: restore: bandcode=%d, txChainMask=%d, chainIdx=%x: 
6372,IIII,PDET::: etnry: bandcode=%d, txChainMask=%d, chainIdx=%x, calStatus=%d 
6373,I,TPC::: entry function: pHandle=%x 
6374,,TPC::: entry function: pHandle=NULL 
6394,III,DPD RxIQ: PhyId = %d, Chain = %d, LB = %d
 
6393,III,dpd rxiq: idx = %d, mag = %d, phs = %d
 
6393,III,dpd rxiq: idx = %d, mag = %d, phs = %d
 
6392,I,Normal path TxLO correction enabled: %d 
6391,I,Normal path TxIQ correction enabled: %d 
6390,I,Normal path RxIQ correction enabled: %d 
6389,I,Loopback path RxIQ correction enabled: %d 
6388,III,chain %d rxiq lb corr: gainidx = %d, data=0x%x
 
6387,II,Rx_gain_table: idx = %d, gain_word = 0x%8x
 
6387,II,Rx_gain_table: idx = %d, gain_word = 0x%8x
 
6386,I,
dpdRxiq_rdbk_txgain_index: Tx gain idx rdbk from HW GLUT = %d 
6385,,dpdRxiq_rdbk_txgain_index: Invalid Tx gain idx rdbk from TPC_GLUT_WORD 
6384,I,dpdRxiq_rdbk_txgain_index: isRunCalTx = 0x%x 
6383,III,PhyId = %d, Chain = %d, loc = %d
 
6382,III,txlo:idx = %d, cl_I = %d, cl_Q = %d
 
6381,,RxIQ for DPD lpbk path failure: DO_CALIBRATE in HW did not clear! 
6380,II,temp=%d and tempIdx=%d 
6379,I,iter = %d
 
6378,,RxIQ Cal for DPD path done ...... 
 
6377,II,DPD RXIQ: Band = %d, IPA_PRESENT = %d 
6376,I,Incorrect freqIdx!!! freqIdx=%d 
6375,IIII,chain %d freqIdx %d rxiq lb corr: gainidx = %d, data=0x%x
 
6401,IIIII,VdetCal: pdadc_bias ={%d,%d}, pHandle %x, mhz = %d, flags= %x 
6400,I,VdetCal:, pdadc=%d 
6399,IIII,VdetCal: pdadc = %d, dc_offset_adj = %d, -> pdadc_bias= {%d, %d} 
6398,,already run Vdet on this band 
6397,I,VdetCalibration: run time = %d (usec) 
6396,IIIII,VdetCal: vdetCalFlag = %x, offset_adj = %d, kokg_disable = %d, tx_gain_index= %d, tx_bbf_gain_pgao=%d 
6395,,VdetCal: vdet is not enabled in bdf for this band -> return 
6420,IIIII,chain %d pwrValid %d pwr %d clpcErr %d Status %d 
6419,,CLPC dup process required 
5881,I,***INVALID RF SUB returned. Needs investigation rfsub %d ** 
6418,IIII,Update tpcDb status %d, data %x, rfsub %d, bandw %d 
6417,IIIII,update Reg from DB mask %x, data[0] %x data [1] %x, rfsub %d, bandw %d 
6416,,***COLD Boot detected*** 
6415,I,Doing pDetCal for chainMask %x 
6414,I,Phy %d CLPC duplication process completed 
6413,IIII,got freq %d chain %d clpc_error %d from sub-band %d 
6412,IIIIIII,got freq %d chainIdx %d clpc_error %d from nearest sub-band %d, own subband is %d, range %d to %d 
6412,IIIIIII,got freq %d chainIdx %d clpc_error %d from nearest sub-band %d, own subband is %d, range %d to %d 
6411,IIIII,@@@@@@@@@@@@@@i %d, chmask in %x ch0: valid %d, pwr %d, reg32 = %x fb_stat_b0 %d 
6410,IIIII,@@@@@@@@@@@@@@i %d, chmask in %x ch1: valid %d, pwr %d, reg32 = %x 
6409,III,chain %d Record current averaged CLPC error %d to rfsub %d 
6408,IIIIIIII,Glut CLPC error %d %d %d %d %d %d %d %d 
6407,, $$$$$ CLPC TraverseMiss Error Recovery End $$$$$ 
6406,I,##### CLPC TraverseMiss Error Recovery Triggered, PHY HANDLE:%d ##### 
6405,IIIIII,TPC_STAT_B0B1Reg:Val when triggered, B0_LOW:%d, B0_MID:%d, B0_HIGH:%d, B1_LOW:%d, B1_MID:%d, B1_HIGH:%d 
6404,III,chain %d clpcDupValidPwrCount %d clpcDupSucceed %d 
6403,III,************** PHYA ************* stat_3 %x stat_5 %x phyA no valid counter %d 
6402,III,######### PHYB ######### stat_3 %x stat_5 %x, phyB no valid counter %d 
6431,,BLACKBOLT CHIP: SDM636/SDA636. Initializing chain mask to 0x1 and enabling NON DBS PHY 0 mode only 
6430,II,##########bdf thermCode %d, calTemp %d
 
6429,I,##########bdf temp slope %d
 
6428,I,##########bdf num_phy = %d
 
6427,IIII,tempCode ch%d = %d, calTemp %d, tempSlope %d
 
6426,II,Get per chain priority SAR limit Chain: %d PhyMode : %d 
6425,I,abnorm,  idx = 0x%x 
6424,IIII,halphyBdfComponentSetCCAThresh: %x %x %x %x 
 
6423,IIII,SetPerChainSARLimit  phyId = %d, chainIdx = %d, is2GHz = %d tx_pwr_max = %d
  
6422,,clpcPowerOffsetChan channel is not set, skip channel offset 
6421,IIIII,chain %d final: HI %d, MI %d, LO %d CCK %d 
6435,IIIII,IM2 chain %d i offset 0x%x value 0x%x q offset 0x%x value 0x%x 
6434,,wcn3950_rfa_config_device_GetXOSettleTime OUT OF BOUND XO SETTLE time returned by HW. limiting it to 100 TICKS 
6433,IIIII,wcn3950_rfa_config_device_SetChannel maxChainMask 0x%x mhz %d freq1 %d freq2 %d dtimEnable %d 
6432,IIII, is_5g_synth_updated = 0x%x is_2g5g_synth_updated = 0x%x is_2g5g_synth_in_5g_mode = 0x%x was_in_2x2_mode = 0x%x
 
6441,,EfuseInit 
6440,IIII,EfuseInit Completed boardId 0x%x 0x%x otpVersion %d chipIdExt 0x%x 
6439,II,Error: buffer is out of bounds. offset = 0x%x, numBytes = 0x%x
 
6439,II,Error: buffer is out of bounds. offset = 0x%x, numBytes = 0x%x
 
6438,II,Error: %d/%d bytes were not written to eFuse correctly.
 
6437,II,efuseW[0x%x] = 0x%x
 
6436,III,efuseR[0x%x] = 0x%x != 0x%x
 
6445,II,calData[0] %x, dac1Val %x  
6444,, @@@@ No Ko @@@ 
6442,,=== wcn3950_rfa_tpc_device_EnableHwPdetCal failed 
6443,II,WL_TPC_TPC_FB_1, PDACC_MODE = %x, adcCompRef %d
 
6442,,=== wcn3950_rfa_tpc_device_EnableHwPdetCal failed 
6446,I,RXDCO OK: RX_DCOC_LUT_OUT_EN: %d 
6447,,invalid operation mode specified!
 
6447,,invalid operation mode specified!
 
6448,I,Invalid cal path number %d
 
6457,,Clock Mode: PMIC enabled 
6456,,Clock Mode: WCN clock enabled 
6435,IIIII,IM2 chain %d i offset 0x%x value 0x%x q offset 0x%x value 0x%x 
6455,,halphy_rfa_config_device_GetXOSettleTime OUT OF BOUND XO SETTLE time returned by HW. limiting it to 100 TICKS 
6454,IIIII,halphy_rfa_config_device_SetChannel maxChainMask 0x%x mhz %d freq1 %d freq2 %d dtimEnable %d 
6453,IIII, is_5g_synth_updated = 0x%x is_2g5g_synth_updated = 0x%x is_2g5g_synth_in_5g_mode = 0x%x was_in_2x2_mode = 0x%x 
6452,IIIII,halphy_rfa_config_device_SetChannel_1x maxChainMask 0x%x mhz %d freq1 %d freq2 %d dtimEnable %d 
6451,I,halphy_rfa_config_device_WLReset  %x
 
6450,I,halphy_rfa_config_device_WLReset %x
 
6449,I,halphy_rfa_config_device_WLReset writing %x
 
6450,I,halphy_rfa_config_device_WLReset %x
 
6449,I,halphy_rfa_config_device_WLReset writing %x
 
6474,II,Enable5GXFem chainIdx %d enable %d 
6473,I,halphy_rfa_fem_ctrl_device_EnableWlanAS Before setting AON_XFEM_GPO_CFG = 0x%08x 
  
6472,I,halphy_rfa_fem_ctrl_device_EnableWlanAS Before setting AON_XFEM_PIN_CFG1.XFEM_PIN_CFG_5 = 0x%08x 
  
6471,I,halphy_rfa_fem_ctrl_device_EnableWlanAS Before setting AON_XFEM_PIN_CFG0.XFEM_PIN_CFG_1 = 0x%08x 
  
6470,,WLAN AS featured disabled in BDF 
6469,II,Enable WLAN AS chainIdx %d enable %d 
6468,I,halphy_rfa_fem_ctrl_device_EnableWlanAS After setting AON_XFEM_GPO_CFG = 0x%08x 
  
6467,I,halphy_rfa_fem_ctrl_device_EnableWlanAS After setting AON_XFEM_PIN_CFG1.XFEM_PIN_CFG_5 = 0x%08x 
  
6466,I,halphy_rfa_fem_ctrl_device_EnableWlanAS After setting AON_XFEM_PIN_CFG0.XFEM_PIN_CFG_1 = 0x%08x 
  
6465,I,EnableWLASCtrl COLD BOOT MODE chainMask %d 
6464,I,EnableWLASCtrl 2GHz chainMask %d 
6463,I,EnableWLASCtrl 5GHz IMPS Entry chainMask %d 
6462,I,EnableWLASCtrl 5GHz IMPS Exit or Channelchange chainMask %d  
6461,II,pabiasTrim0 %d pabiasTrimOffset_0 %d 
6460,,pabiasTrim offset overflow 
6460,,pabiasTrim offset overflow 
6459,II,pabiasTrim1 %d pabiasTrimOffset_1 %d 
6458,IIII,SetTxRxMode: chain %d PA mode %d lna mode %d xtrCfg %d 
6441,,EfuseInit 
6440,IIII,EfuseInit Completed boardId 0x%x 0x%x otpVersion %d chipIdExt 0x%x 
6477,I,PdetTerminationRes50OhmTrim chain 0 adj 0x%x 
6476,I,PdetTerminationRes50OhmTrim chain 1 adj 0x%x 
6439,II,Error: buffer is out of bounds. offset = 0x%x, numBytes = 0x%x
 
6475,II,TPCKgKoUpdate ko 0x%x kg 0x%x 
6439,II,Error: buffer is out of bounds. offset = 0x%x, numBytes = 0x%x
 
6438,II,Error: %d/%d bytes were not written to eFuse correctly.
 
6437,II,efuseW[0x%x] = 0x%x
 
6436,III,efuseR[0x%x] = 0x%x != 0x%x
 
6481,IIII,calData[0] %x, calData[1] %x dac1Val %x dac2Val %x 
6480,II,GTX ON, IPA, temp thr %d, cur temp %d 
6479,I, ##### ko = %d 
6478,,=== halphy_rfa_tpc_device_EnableHwPdetCal failed 
6478,,=== halphy_rfa_tpc_device_EnableHwPdetCal failed 
6444,, @@@@ No Ko @@@ 
6443,II,WL_TPC_TPC_FB_1, PDACC_MODE = %x, adcCompRef %d
 
6448,I,Invalid cal path number %d
 
6447,,invalid operation mode specified!
 
6447,,invalid operation mode specified!
 
6446,I,RXDCO OK: RX_DCOC_LUT_OUT_EN: %d 
6482,I,STA_KICKOUT: Reason=%d 
6488,I,_htt_tgt_stats_reset: g_rst_stats_types_mask : 0x%x  
6487,I,htt_tgt_stats_reset: calling fucntion : 0x%x  
6486,II,htt_tgt_stats_upload: upl_stats_types_mask : 0x%x rst_stats_types_mask 0x%x 
6485,,wdiag_cmd_get_tx_rx_stats_handle: request pointer is NULL  
6484,II,wdiag_cmd_get_tx_rx_stats_handle: pkt_len is not %d, pkt_len = %d  
6483,I,wdiag_cmd_get_tx_rx_stats_handle: Invalid stats type :%d  
6495,III,PACKET_LOG_SVC: svc_id %d, pipe_id %d, pipe_width %d 
6494,,_pktlog_enable: failed to enable packet log, was not initialised 
6493,I,_pktlog_enable: already enabled, bmap=0x%x 
6492,II,_pktlog_enable: enable %u evlist %08x 
6491,I,_pktlog_disable: already disabled, bmap=0x%x 
6490,I,_pktlog_htc_connect: ep %d 
6489,III,_pktlog_getbuf: pool_list_alloc failed with size %u type=%u missed=%d 
6533,IIII,ar_wal_rtt_ack_rx_time(): mcs: %d preamble: %d bw: %d ack_time: %d 
6532,II,rtt_get_tx_rate: rate: %d bit_rate_kbps: %d 
6531,I,TX filtered TLV:%d 
6530,I,rx_location_info_status: :%d 
6529,I,rtt_get_rx_frame_len:  reported_mpdu_length = %d 
6528,I,rtt_send_sta_get_rxpreamble: rtt_preamble_type=0x%x 
6527,I,_wal_fac_handler: report type %d  
6526,IIIIIII,timing_backoff_rssi(L: %d M: %d h: %d) timing_backoff_sel: %d timing_backoff_err: %d fac_bo_err_adj: %d str_rx_chain: %d 
6525,II,recv sta rssi 0x%x chain:%d 
6524,II,send sta rssi 0x%x chain:%d 
6523,IIIII,rtt_get_toda: toda_type=0x%x  toda_upper = 0x%x, toda_lower = 0x%x toda_80Mhz = %lu toda = %lu 
6522,I,rtt_get_toda:: unknown toda_type: %d 
6521,II,rtt_get_toda after ps: toda_upper = 0x%x, toda_lower = 0x%x 
6520,III,rtt_get_toda txrx_delay=%d toda_ajusted upper: 0x%x lower: 0x%x 
6519,,CFR status is NULL return 
6518,IIIII,collecting CFR dump from chain:%d ext:%d aln_sz:%d, sz:%d cfr_status:%d 
6517,IIIIIIII,tone %d,%d,%d,%d,%d,%d,%d,%d 
6516,II,finished CFR dump from chain:%d ext:%d 
6515,II,rtt_recv_sta_get_rxbw: rx_bw=%d rx_preamble=%d 
6514,I,rtt_send_sta_get_txbw: packet_bw=0x%x 
6513,I,rtt_send_sta_get_rxbw: rtt_pkt_bw=0x%x 
6512,II,Deliver RX Ind msg s_thr:%d to RT at ticks:0x%x 
6511,,Thread msg buff alloc failed: Failed to report RTT T3 
6510,,Failed to get rtt_mt_msg_tx 
6509,,fac_invalid 
6508,I,rtt_fac_handler:  fac_value_in_ts=%d 
6507,I,rtt_fac_handler:  fac_value_converted=%d 
6506,IIIIIIII,RXLocInf1 %d,%d,%d,%d,%d,%d,%d,%d 
6505,IIIIIIII,RXLocInf2 %d,%d,%d,%d,%d,%d,%d,%d 
6504,IIIIIIII,RXLocInf3 %d,%d,%d,%d,%d,%d,%d,%d 
6503,,rtt_get_fac_results: fac_invalid! Returning! 
6502,III,rtt_get_fac_results: fac_leg_status=0x%x fac_vht_status=0x%x fac=%d 
6501,I,_wal_log_CIR: p_CIR_buf %p 
6500,II,read_CIR: CIR status %d CIR buff %p  
6499,IIII,read_CIR: num_samples %d bw %d size %d is_ext %d 
6498,IIIIIIII,index %d,%d,%d,%d,%d,%d,%d,%d 
6497,IIIIIII,calc_tx_frame_time(): tx preamble: %d bw: %d rate_code: %d tx_preamble_duration: %d f_len: %d txrate: %d f_time: %d 
6496,IIIIIIIII,tm_rx_frame_time(): f_len: %d del: %d rate: %d f_time: %d preamble type: %d mcs: %d bw: %d nss: %d sgi: %d 
6553,,enable_gipo_profiling:BT is ON, Turnoff BT to have this feature
 
6552,,enable_gipo_profiling USE_COEX_WSI_DATA_EN set
 
6551,,enable_gipo_profiling Disabled
 
6550,I,enable_gipo_profiling PMM_GPIO_PWR_CSR:0x%x
 
6549,,enable_gipo_profiling PMM_CX_PWRDN_REQ_MSK set
 
6548,,enable_gipo_profiling PMM_CX_SEND_XO_DISABLE set
 
6547,,enable_gipo_profiling PMM_CX_DISABLE_PLL_MSK set
 
6546,,enable_gipo_profiling PMM_CX_DETECT_PLL_LOCK_MSK set
 
6545,,enable_gipo_profiling PMM_CX_ENABLE_PLL_MSK set
 
6544,,enable_gipo_profiling PMM_CX_SEND_XO_EN_MSK set
 
6543,,enable_gipo_profiling PMM_CX_GET_WAKEUP_INT_MSK set
 
6542,I,enable_gipo_profiling PMM_WLAN%d_OFF_STS_MSK set
 
6541,I,enable_gipo_profiling PMM_WLAN%d_OFF_REQ_MSK set
 
6540,I,enable_gipo_profiling PMM_WLAN%d_RX_BEACON_END_MSK set
 
6539,I,enable_gipo_profiling PMM_WLAN%d_RX_BEACON_START_MSK set
 
6538,I,enable_gipo_profiling PMM_WLAN%d_RRI_DONE_MSK set
 
6537,I,enable_gipo_profiling PMM_WLAN%d_START_RRI_MSK set
 
6536,I,enable_gipo_profiling PMM_WLAN%d_ENABLE_MSK set
 
6535,I,enable_gipo_profiling PMM_WLAN1_GPIO_PWR_MSK:0x%x
 
6534,I,enable_gipo_profiling PMM_WLAN2_GPIO_PWR_MSK:0x%x
 
6554,IIIIIII,iniAg_RfConfig: chain %d PA mode %d bandChng %d bandwChng %d freqChng %d rfmodeChng %d fcstablefreqChng %d 
6590,III,RF_LOAD_TXFE_5G_CH1 index %d freqIdx %d fcsTable %d
 
6589,I,RF_LOAD_TXFE_5G_CH1 index =  %d , not supported 
 
6588,IIII,RF_LOAD_TXFE_GTX_OVERRIDE band %d chain %d freqIdx %d fcsTable %d 
6587,I,RF_LOAD_TX_BBF index =  %d , not supported 
 
6586,,Error: cannot commit NULL table!
 
6585,II,Note: table filtered out. table[%d].filter = %c 
6584,IIII,loadBBtable - table: %d, phy: %d, column: %d, filt: %c 
6583,I,loadBBtable: invalid phy %d
 
6582,I,loadBBtable: invalid table %d
 
6581,IIII,loadDFStable - table: %d, phy: %d, column: %d, filt: %c
 
6580,I,loadDFStable: invalid table %d
 
6579,I,loadDFStable: invalid phy %d
 
6578,I,halphy_iniAg_LoadExtraRFtable index = %d  
6577,IIIII,loadRFtable - pa_mode: %d, table: %d, chain: %d, column: %d, filt: %c 
6576,I,loadRFtable: invalid table index %d
 
6575,I,loadRFtable: invalid chain %d
 
6574,,Error: iniAg_masterJoined_simple_tables is null... iniAg not init correctly 
6568,,Error: iniAg_masterJoined_tables is null... iniAg not init correctly 
6573,I,loadSplitBbRfTable: invalid bbTable %d
 
6572,I,loadSplitBbRfTable: invalid phy %d
 
6571,I,loadSplitBbRfTable: invalid chain %d
 
6570,IIIIIIII,loadSplitBbRfTable - bb:%d rf:%d phy:%d band:%d pa_mode:%d, chn:%d, col:%d, filt:%c 
6569,,loadSplitBbRfTable: No addr rfTable given.
 
6568,,Error: iniAg_masterJoined_tables is null... iniAg not init correctly 
6567,,Error: iniAg_masterJoined_tables_rxgain is null... iniAg not init correctly
 
6566,I,loadSplitBbRfTable: invalid rfTable index %d
 
6565,,bb has address, rf has data 
6564,,bb has data, rf has address 
6563,,Error: conflict merging BB and RF tables.  
6562,III,rows in table's addr %d less than rows in data %d. table index %d 
6561,,Error: row number issue in merging BB and RF tables, skip table index 
6560,I,Warning: Leftover tables while joining! All remainders skipped after index %d 
6559,II,revision index %d for rf_revision 0x%x 
6558,I,Error: no table found for rev:0x%x, using index:0 
6557,III,Note: No table found for rev:0x%x instead using tables for rev:0x%x index:%d 
6556,II,device index %d for id 0x%x
 
6555,I,ERROR: device ID %d not found in lookup list... analog master tables not set!!! 
